Cross Section Report
C:/srf04/Agama/Agama_Lite_EM_Designs/CC1311-P3EM-7XD7793-PA915/cadence/allegro/CC1311-P3EM-7XD7793-PA915.brd
Tue Feb 23 16:58:22 2021

Design Cross Section
Subclass Name,Type,Material,Thickness (MM),Tol +,Tol -,Conductivity (mho/cm),Dielectric Constant,Loss Tangent,Negative Artwork,Shield,Width (MM),Unused Pin Pad Suppression,Unused Via Pad Suppression
,SURFACE,AIR,,,,0,1,0,,,,,
TOP,CONDUCTOR,COPPER,0.035,0,0,595900,4.5,0,,,0.127,,
,DIELECTRIC,FR-4,0.175,0,0,0,3.8,0.035,,,,,
L2,PLANE,COPPER,0.0175,0,0,595900,4.5,0.035,,Yes,,,
,DIELECTRIC,FR-4,1.140000,0,0,0,4.2,0.035,,,,,
L3,PLANE,COPPER,0.0175,0,0,595900,4.5,0.035,,Yes,,,
,DIELECTRIC,FR-4,0.175,0,0,0,3.8,0.035,,,,,
BOTTOM,CONDUCTOR,COPPER,0.035,0,0,595900,4.5,0,,,0.127,,
,SURFACE,AIR,,,,0,1,0,,,,,

Total Thickness: 1.595 MM
