CC26xx Driver Library |

- Main Page
- Related Pages
- CC26xx APIs
- Register Descriptions
- Online Resources

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Modules Pages
Macros | Functions
ioc.h File Reference
`#include <stdbool.h>`
`#include <stdint.h>`
`#include <inc/hw_types.h>`
`#include <inc/hw_memmap.h>`
`#include <inc/hw_ioc.h>`
`#include <inc/hw_ints.h>`
`#include <driverlib/interrupt.h>`
`#include <driverlib/debug.h>`
`#include <driverlib/gpio.h>`

Go to the source code of this file.

## Macros
#define | NUM_IO_MAX 32
#define | IOID_0 0x00000000
#define | IOID_1 0x00000001
#define | IOID_2 0x00000002
#define | IOID_3 0x00000003
#define | IOID_4 0x00000004
#define | IOID_5 0x00000005
#define | IOID_6 0x00000006
#define | IOID_7 0x00000007
#define | IOID_8 0x00000008
#define | IOID_9 0x00000009
#define | IOID_10 0x0000000A
#define | IOID_11 0x0000000B
#define | IOID_12 0x0000000C
#define | IOID_13 0x0000000D
#define | IOID_14 0x0000000E
#define | IOID_15 0x0000000F
#define | IOID_16 0x00000010
#define | IOID_17 0x00000011
#define | IOID_18 0x00000012
#define | IOID_19 0x00000013
#define | IOID_20 0x00000014
#define | IOID_21 0x00000015
#define | IOID_22 0x00000016
#define | IOID_23 0x00000017
#define | IOID_24 0x00000018
#define | IOID_25 0x00000019
#define | IOID_26 0x0000001A
#define | IOID_27 0x0000001B
#define | IOID_28 0x0000001C
#define | IOID_29 0x0000001D
#define | IOID_30 0x0000001E
#define | IOID_31 0x0000001F
#define | IOID_UNUSED 0xFFFFFFFF
#define | IOC_IOID_MASK 0x000000FF
#define | NUM_IO_PORTS 56
#define | IOC_PORT_GPIO 0x00000000
#define | IOC_PORT_AON_SCS 0x00000001
#define | IOC_PORT_AON_SCK 0x00000002
#define | IOC_PORT_AON_SDI 0x00000003
#define | IOC_PORT_AON_SDO 0x00000004
#define | IOC_PORT_AON_CLK32K 0x00000007
#define | IOC_PORT_AUX_IO 0x00000008
#define | IOC_PORT_MCU_SSI0_RX 0x00000009
#define | IOC_PORT_MCU_SSI0_TX 0x0000000A
#define | IOC_PORT_MCU_SSI0_FSS 0x0000000B
#define | IOC_PORT_MCU_SSI0_CLK 0x0000000C
#define | IOC_PORT_MCU_I2C_MSSDA 0x0000000D
#define | IOC_PORT_MCU_I2C_MSSCL 0x0000000E
#define | IOC_PORT_MCU_UART0_RX 0x0000000F
#define | IOC_PORT_MCU_UART0_TX 0x00000010
#define | IOC_PORT_MCU_UART0_CTS 0x00000011
#define | IOC_PORT_MCU_UART0_RTS 0x00000012
#define | IOC_PORT_MCU_PORT_EVENT0 0x00000017
#define | IOC_PORT_MCU_PORT_EVENT1 0x00000018
#define | IOC_PORT_MCU_PORT_EVENT2 0x00000019
#define | IOC_PORT_MCU_PORT_EVENT3 0x0000001A
#define | IOC_PORT_MCU_PORT_EVENT4 0x0000001B
#define | IOC_PORT_MCU_PORT_EVENT5 0x0000001C
#define | IOC_PORT_MCU_PORT_EVENT6 0x0000001D
#define | IOC_PORT_MCU_PORT_EVENT7 0x0000001E
#define | IOC_PORT_MCU_SWV 0x00000020
#define | IOC_PORT_MCU_SSI1_RX 0x00000021
#define | IOC_PORT_MCU_SSI1_TX 0x00000022
#define | IOC_PORT_MCU_SSI1_FSS 0x00000023
#define | IOC_PORT_MCU_SSI1_CLK 0x00000024
#define | IOC_PORT_MCU_I2S_AD0 0x00000025
#define | IOC_PORT_MCU_I2S_AD1 0x00000026
#define | IOC_PORT_MCU_I2S_WCLK 0x00000027
#define | IOC_PORT_MCU_I2S_BCLK 0x00000028
#define | IOC_PORT_MCU_I2S_MCLK 0x00000029
#define | IOC_PORT_RFC_TRC 0x0000002E
#define | IOC_PORT_RFC_GPO0 0x0000002F
#define | IOC_PORT_RFC_GPO1 0x00000030
#define | IOC_PORT_RFC_GPO2 0x00000031
#define | IOC_PORT_RFC_GPO3 0x00000032
#define | IOC_PORT_RFC_GPI0 0x00000033
#define | IOC_PORT_RFC_GPI1 0x00000034
#define | IOC_SLEW_ENABLE 0x00001000
#define | IOC_SLEW_DISABLE 0x00000000
#define | IOC_INPUT_ENABLE 0x20000000
#define | IOC_INPUT_DISABLE 0x00000000
#define | IOC_HYST_ENABLE 0x40000000
#define | IOC_HYST_DISABLE 0x00000000
#define | IOC_JTAG_TDO_ENABLE 0x00080000
#define | IOC_JTAG_TDI_ENABLE 0x00100000
#define | IOC_JTAG_DISABLE 0x00000000
#define | IOC_NO_WAKE_UP 0x00000000
#define | IOC_WAKE_ON_LOW 0x10000000
#define | IOC_WAKE_ON_HIGH 0x18000000
#define | IOC_IOMODE_NORMAL 0x00000000
#define | IOC_IOMODE_INV 0x01000000
#define | IOC_IOMODE_OPEN_DRAIN_NORMAL 0x04000000
#define | IOC_IOMODE_OPEN_DRAIN_INV 0x05000000
#define | IOC_IOMODE_OPEN_SRC_NORMAL 0x06000000
#define | IOC_IOMODE_OPEN_SRC_INV 0x07000000
#define | IOC_NO_EDGE 0x00000000
#define | IOC_FALLING_EDGE 0x00010000
#define | IOC_RISING_EDGE 0x00020000
#define | IOC_BOTH_EDGES 0x00030000
#define | IOC_INT_ENABLE 0x00040000
#define | IOC_INT_DISABLE 0x00000000
#define | IOC_INT_M 0x00070000
#define | IOC_NO_IOPULL 0x00006000
#define | IOC_IOPULL_UP 0x00004000
#define | IOC_IOPULL_DOWN 0x00002000
#define | IOC_IOPULL_M 0x00006000
#define | IOC_CURRENT_2MA 0x00000000
#define | IOC_CURRENT_4MA 0x00000400
#define | IOC_CURRENT_8MA 0x00000800
#define | IOC_CURRENT_16MA 0x00000C00
#define | IOC_STRENGTH_AUTO 0x00000000
#define | IOC_STRENGTH_MAX 0x00000300
#define | IOC_STRENGTH_MED 0x00000200
#define | IOC_STRENGTH_MIN 0x00000100
#define | IOC_STD_INPUT
#define | IOC_STD_OUTPUT

## Functions
void | IOCPortConfigureSet (uint32_t ui32IOId, uint32_t ui32PortId, uint32_t ui32IOConfig)
| Set the configuration of an IO port. More...
uint32_t | IOCPortConfigureGet (uint32_t ui32IOId)
| Get the configuration of an IO port. More...
void | IOCIOShutdownSet (uint32_t ui32IOId, uint32_t ui32IOShutdown)
| Set wake-up on an IO port. More...
void | IOCIOJTagSet (uint32_t ui32IOId, uint32_t ui32IOJTag)
| Set wake-up on an IO port. More...
void | IOCIOModeSet (uint32_t ui32IOId, uint32_t ui32IOMode)
| Set the IO Mode of an IO Port. More...
void | IOCIOIntSet (uint32_t ui32IOId, uint32_t ui32Int, uint32_t ui32EdgeDet)
| Setup interrupt detection on an IO Port. More...
void | IOCIOPortPullSet (uint32_t ui32IOId, uint32_t ui32Pull)
| Set the pull on an IO port. More...
void | IOCIOHystSet (uint32_t ui32IOId, uint32_t ui32Hysteresis)
| Configure hysteresis on and IO port. More...
void | IOCIOInputSet (uint32_t ui32IOId, uint32_t ui32Input)
| Enable/disable IO port as input. More...
void | IOCIOSlewCtrlSet (uint32_t ui32IOId, uint32_t ui32SlewEnable)
| Enable/disable the slew control on an IO port. More...
void | IOCIODrvStrengthSet (uint32_t ui32IOId, uint32_t ui32IOCurrent, uint32_t ui32DrvStrength)
| Configure the drive strength and maxium current of an IO port. More...
void | IOCIOPortIdSet (uint32_t ui32IOId, uint32_t ui32PortId)
| Setup the Port ID for this IO. More...
__STATIC_INLINE void | IOCIntRegister (void(*pfnHandler)(void))
| Register an interrupt handler for an IO edge interrupt. More...
__STATIC_INLINE void | IOCIntUnregister (void)
| Unregisters an interrupt handler for a IO edge interrupt. More...
void | IOCIntEnable (uint32_t ui32IOId)
| Enables individual IO edge detect interrupt. More...
void | IOCIntDisable (uint32_t ui32IOId)
| Disables individual IO edge interrupt sources. More...
__STATIC_INLINE void | IOCIntClear (uint32_t ui32IOId)
| Clears the IO edge interrupt source. More...
__STATIC_INLINE uint32_t | IOCIntStatus (uint32_t ui32IOId)
| Returns the status of the IO interrupts. More...
void | IOCPinTypeGpioInput (uint32_t ui32IOId)
| Setup an IO for standard GPIO input. More...
void | IOCPinTypeGpioOutput (uint32_t ui32IOId)
| Setup an IO for standard GPIO output. More...
void | IOCPinTypeUart (uint32_t ui32Base, uint32_t ui32Rx, uint32_t ui32Tx, uint32_t ui32Cts, uint32_t ui32Rts)
| Configure a set of IOs for standard UART peripheral control. More...
void | IOCPinTypeSsiMaster (uint32_t ui32Base, uint32_t ui32Rx, uint32_t ui32Tx, uint32_t ui32Fss, uint32_t ui32Clk)
| Configure a set of IOs for standard SSI peripheral master control. More...
void | IOCPinTypeSsiSlave (uint32_t ui32Base, uint32_t ui32Rx, uint32_t ui32Tx, uint32_t ui32Fss, uint32_t ui32Clk)
| Configure a set of IOs for standard SSI peripheral slave control. More...
void | IOCPinTypeI2c (uint32_t ui32Base, uint32_t ui32Data, uint32_t ui32Clk)
| Configure a set of IOs for standard I2C peripheral control. More...
void | IOCPinTypeSpis (uint32_t ui32Rx, uint32_t ui32Tx, uint32_t ui32Fss, uint32_t ui32Clk)
| Configure a set of IOs for standard SPIS peripheral control. More...
void | IOCPinTypeAux (uint32_t ui32IOId)
| Configure an IO for AUX control. More...