CC26xx Driver Library |

- Main Page
- Related Pages
- CC26xx APIs
- Register Descriptions
- Online Resources

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Macros

- _
- a
- b
- c
- d
- e
- f
- g
- h
- i
- k
- l
- m
- n
- o
- p
- r
- s
- t
- u
- v
- w
- x

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Modules Pages
Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - a -

- ADC_COMPB_IN_AUXIO0 : rom.h
- ADC_COMPB_IN_AUXIO1 : rom.h
- ADC_COMPB_IN_AUXIO2 : rom.h
- ADC_COMPB_IN_AUXIO3 : rom.h
- ADC_COMPB_IN_AUXIO4 : rom.h
- ADC_COMPB_IN_AUXIO5 : rom.h
- ADC_COMPB_IN_AUXIO6 : rom.h
- ADC_COMPB_IN_AUXIO7 : rom.h
- ADC_COMPB_IN_NC : rom.h
- ADC_COMPB_IN_VDD1P2V : rom.h
- ADC_COMPB_IN_VDDA3P3V : rom.h
- ADC_COMPB_IN_VSSA : rom.h
- ADDR_OFFSET : flash.h
- ADI16BitsClear() : adi.h
- ADI16BitsSet() : adi.h
- ADI16RegRead() : adi.h
- ADI16RegWrite() : adi.h
- ADI16SetValBit() : adi.h
- ADI32BitsClear() : adi.h
- ADI32BitsSet() : adi.h
- ADI32RegRead() : adi.h
- ADI32RegWrite() : adi.h
- ADI4SetValBit() : adi.h
- ADI8BitsClear() : adi.h
- ADI8BitsSet() : adi.h
- ADI8RegRead() : adi.h
- ADI8RegWrite() : adi.h
- ADI8SetValBit() : adi.h
- ADI_ACK : adi.h
- ADI_CONFIG_MASK : adi.h
- ADI_NO_WAIT : adi.h
- ADI_PROTECT : adi.h
- ADI_SLAVE_REGS : adi.h
- ADI_SPEED_16 : adi.h
- ADI_SPEED_2 : adi.h
- ADI_SPEED_4 : adi.h
- ADI_SPEED_8 : adi.h
- ADI_SYNC : adi.h
- ADI_WAIT_FOR_ACK : adi.h
- ADIConfigSet() : adi.h
- ADIProtect() : adi.h
- ADIStatusGet() : adi.h
- ADISync() : adi.h
- AES_CCM_TEST_ERROR : crypto.h
- AES_DMA_BSY : crypto.h
- AES_DMA_BUS_ERROR : crypto.h
- AES_ECB_LENGTH : crypto.h
- AES_ECB_TEST_ERROR : crypto.h
- AES_KEYSTORE_READ_ERROR : crypto.h
- AES_KEYSTORE_WRITE_ERROR : crypto.h
- AES_NULL_ERROR : crypto.h
- AES_SUCCESS : crypto.h
- AON_BATMON_CYCLE_16 : aon_batmon.h
- AON_BATMON_CYCLE_32 : aon_batmon.h
- AON_BATMON_CYCLE_8 : aon_batmon.h
- AON_BATMON_CYCLE_CONT : aon_batmon.h
- AON_BATMON_TEMP_INT_FIELD_WIDTH : aon_batmon.c
- AON_BatmonTempGetDegC() : aon_batmon.c , aon_batmon.h
- AON_EVENT_AUX0 : aon_event.h
- AON_EVENT_AUX1 : aon_event.h
- AON_EVENT_AUX2 : aon_event.h
- AON_EVENT_AUX_ADC_DONE : aon_event.h
- AON_EVENT_AUX_CMPA : aon_event.h
- AON_EVENT_AUX_CMPB : aon_event.h
- AON_EVENT_AUX_TDC_DONE : aon_event.h
- AON_EVENT_AUX_TIMER0 : aon_event.h
- AON_EVENT_AUX_TIMER1 : aon_event.h
- AON_EVENT_AUX_WU0 : aon_event.h
- AON_EVENT_AUX_WU1 : aon_event.h
- AON_EVENT_AUX_WU2 : aon_event.h
- AON_EVENT_BATMON_TEMP : aon_event.h
- AON_EVENT_BATMON_VOLT : aon_event.h
- AON_EVENT_IO : aon_event.h
- AON_EVENT_IO0 : aon_event.h
- AON_EVENT_IO1 : aon_event.h
- AON_EVENT_IO10 : aon_event.h
- AON_EVENT_IO11 : aon_event.h
- AON_EVENT_IO12 : aon_event.h
- AON_EVENT_IO13 : aon_event.h
- AON_EVENT_IO14 : aon_event.h
- AON_EVENT_IO15 : aon_event.h
- AON_EVENT_IO16 : aon_event.h
- AON_EVENT_IO17 : aon_event.h
- AON_EVENT_IO18 : aon_event.h
- AON_EVENT_IO19 : aon_event.h
- AON_EVENT_IO2 : aon_event.h
- AON_EVENT_IO20 : aon_event.h
- AON_EVENT_IO21 : aon_event.h
- AON_EVENT_IO22 : aon_event.h
- AON_EVENT_IO23 : aon_event.h
- AON_EVENT_IO24 : aon_event.h
- AON_EVENT_IO25 : aon_event.h
- AON_EVENT_IO26 : aon_event.h
- AON_EVENT_IO27 : aon_event.h
- AON_EVENT_IO28 : aon_event.h
- AON_EVENT_IO29 : aon_event.h
- AON_EVENT_IO3 : aon_event.h
- AON_EVENT_IO30 : aon_event.h
- AON_EVENT_IO31 : aon_event.h
- AON_EVENT_IO4 : aon_event.h
- AON_EVENT_IO5 : aon_event.h
- AON_EVENT_IO6 : aon_event.h
- AON_EVENT_IO7 : aon_event.h
- AON_EVENT_IO8 : aon_event.h
- AON_EVENT_IO9 : aon_event.h
- AON_EVENT_JTAG : aon_event.h
- AON_EVENT_MCU_EVENT0 : aon_event.h
- AON_EVENT_MCU_EVENT1 : aon_event.h
- AON_EVENT_MCU_EVENT2 : aon_event.h
- AON_EVENT_MCU_WU0 : aon_event.h
- AON_EVENT_MCU_WU1 : aon_event.h
- AON_EVENT_MCU_WU2 : aon_event.h
- AON_EVENT_MCU_WU3 : aon_event.h
- AON_EVENT_NULL : aon_event.h
- AON_EVENT_RTC0 : aon_event.h
- AON_EVENT_RTC0DLY : aon_event.h
- AON_EVENT_RTC1 : aon_event.h
- AON_EVENT_RTC1DLY : aon_event.h
- AON_EVENT_RTC2 : aon_event.h
- AON_EVENT_RTC2DLY : aon_event.h
- AON_EVENT_RTCDLYC : aon_event.h
- AON_EVENT_SPISCS : aon_event.h
- AON_EVENT_SPISRTX : aon_event.h
- AON_RTC_ACTIVE : aon_rtc.h
- AON_RTC_CH0 : aon_rtc.h
- AON_RTC_CH1 : aon_rtc.h
- AON_RTC_CH2 : aon_rtc.h
- AON_RTC_CH_NONE : aon_rtc.h
- AON_RTC_CONFIG_DELAY_1 : aon_rtc.h
- AON_RTC_CONFIG_DELAY_112 : aon_rtc.h
- AON_RTC_CONFIG_DELAY_128 : aon_rtc.h
- AON_RTC_CONFIG_DELAY_144 : aon_rtc.h
- AON_RTC_CONFIG_DELAY_16 : aon_rtc.h
- AON_RTC_CONFIG_DELAY_160 : aon_rtc.h
- AON_RTC_CONFIG_DELAY_176 : aon_rtc.h
- AON_RTC_CONFIG_DELAY_2 : aon_rtc.h
- AON_RTC_CONFIG_DELAY_32 : aon_rtc.h
- AON_RTC_CONFIG_DELAY_4 : aon_rtc.h
- AON_RTC_CONFIG_DELAY_48 : aon_rtc.h
- AON_RTC_CONFIG_DELAY_64 : aon_rtc.h
- AON_RTC_CONFIG_DELAY_8 : aon_rtc.h
- AON_RTC_CONFIG_DELAY_80 : aon_rtc.h
- AON_RTC_CONFIG_DELAY_96 : aon_rtc.h
- AON_RTC_CONFIG_DELAY_NODELAY : aon_rtc.h
- AON_RTC_MODE_CH1_CAPTURE : aon_rtc.h
- AON_RTC_MODE_CH1_COMPARE : aon_rtc.h
- AON_RTC_MODE_CH2_CONTINUOUS : aon_rtc.h
- AON_RTC_MODE_CH2_NORMALCOMPARE : aon_rtc.h
- AONBatMonBatteryTrimSet() : aon_batmon.h
- AONBatMonBatteryVoltageGet() : aon_batmon.h
- AONBatMonDisable() : aon_batmon.h
- AONBatMonEnable() : aon_batmon.h
- AONBatMonMeasurementCycleGet() : aon_batmon.h
- AONBatMonMeasurementCycleSet() : aon_batmon.h
- AONBatMonNewBatteryMeasureReady() : aon_batmon.h
- AONBatMonNewTempMeasureReady() : aon_batmon.h
- AONBatMonTemperatureGet() : aon_batmon.h
- AONBatMonTemperatureTrimSet() : aon_batmon.h
- AONEventAuxWakeUpGet() : aon_event.c , aon_event.h
- AONEventAuxWakeUpSet() : aon_event.c , aon_event.h
- AONEventMcuGet() : aon_event.c , aon_event.h
- AONEventMcuSet() : aon_event.c , aon_event.h
- AONEventMcuWakeUpGet() : aon_event.c , aon_event.h
- AONEventMcuWakeUpSet() : aon_event.c , aon_event.h
- AONEventRtcGet() : aon_event.h
- AONEventRtcSet() : aon_event.h
- AONIOC32kHzOutputDisable() : aon_ioc.h
- AONIOC32kHzOutputEnable() : aon_ioc.h
- AONIOC_DRV_STR10_20_40 : aon_ioc.h
- AONIOC_DRV_STR14_28_56 : aon_ioc.h
- AONIOC_DRV_STR20_40_80 : aon_ioc.h
- AONIOC_DRV_STR28_56_112 : aon_ioc.h
- AONIOC_DRV_STR40_80_112 : aon_ioc.h
- AONIOC_DRV_STR5_10_20 : aon_ioc.h
- AONIOC_DRV_STR5_7_14 : aon_ioc.h
- AONIOC_DRV_STR7_14_28 : aon_ioc.h
- AONIOC_MAX_DRIVE : aon_ioc.h
- AONIOC_MED_DRIVE : aon_ioc.h
- AONIOC_MIN_DRIVE : aon_ioc.h
- AONIOCDriveStrengthGet() : aon_ioc.c , aon_ioc.h
- AONIOCDriveStrengthSet() : aon_ioc.c , aon_ioc.h
- AONIOCFreezeDisable() : aon_ioc.h
- AONIOCFreezeEnable() : aon_ioc.h
- AONRTCCaptureValueCh1Get() : aon_rtc.h
- AONRTCChannelDisable() : aon_rtc.c , aon_rtc.h
- AONRTCChannelEnable() : aon_rtc.c , aon_rtc.h
- AONRTCCombinedEventConfig() : aon_rtc.h
- AONRTCCompareValueGet() : aon_rtc.c , aon_rtc.h
- AONRTCCompareValueSet() : aon_rtc.c , aon_rtc.h
- AONRTCCurrentCompareValueGet() : aon_rtc.h
- AONRTCDelayConfig() : aon_rtc.h
- AONRTCDisable() : aon_rtc.h
- AONRTCEnable() : aon_rtc.h
- AONRTCEventClear() : aon_rtc.c , aon_rtc.h
- AONRTCEventGet() : aon_rtc.c , aon_rtc.h
- AONRTCFractionGet() : aon_rtc.h
- AONRTCIncValueCh2Get() : aon_rtc.h
- AONRTCIncValueCh2Set() : aon_rtc.h
- AONRTCModeCh1Get() : aon_rtc.c , aon_rtc.h
- AONRTCModeCh1Set() : aon_rtc.c , aon_rtc.h
- AONRTCModeCh2Get() : aon_rtc.c , aon_rtc.h
- AONRTCModeCh2Set() : aon_rtc.c , aon_rtc.h
- AONRTCReset() : aon_rtc.h
- AONRTCSecGet() : aon_rtc.h
- AONRTCStatus() : aon_rtc.c , aon_rtc.h
- AONRTCSubSecIncrGet() : aon_rtc.h
- AONWUC_AUX_ALLOW_SLEEP : aon_wuc.h
- AONWUC_AUX_BGAP_REQ : aon_wuc.h
- AONWUC_AUX_GBIAS_REQ : aon_wuc.h
- AONWUC_AUX_POWER_DOWN : aon_wuc.h
- AONWUC_AUX_POWER_ON : aon_wuc.h
- AONWUC_AUX_WAKEUP : aon_wuc.h
- AONWUC_AUX_WAKEUP_SWEVT : aon_wuc.h
- AONWUC_BGAP_ON : aon_wuc.h
- AONWUC_CLOCK_SRC_HF : aon_wuc.h
- AONWUC_CLOCK_SRC_LF : aon_wuc.h
- AONWUC_CLOCK_SRC_MF : aon_wuc.h
- AONWUC_FULL_FLASH_ERASE : aon_wuc.h
- AONWUC_GBIAS_ON : aon_wuc.h
- AONWUC_JTAG_CPUDAP : aon_wuc.h
- AONWUC_JTAG_EFUSETAP : aon_wuc.h
- AONWUC_JTAG_FORCE_ON : aon_wuc.h
- AONWUC_JTAG_ICE : aon_wuc.h
- AONWUC_JTAG_MASK : aon_wuc.h
- AONWUC_JTAG_PBIST1TAP : aon_wuc.h
- AONWUC_JTAG_PBIST2TAP : aon_wuc.h
- AONWUC_JTAG_POWER_ON : aon_wuc.h
- AONWUC_JTAG_PRCMTAP : aon_wuc.h
- AONWUC_JTAG_TESTTAP : aon_wuc.h
- AONWUC_JTAG_WUCTAP : aon_wuc.h
- AONWUC_MCU_BGAP_REQ : aon_wuc.h
- AONWUC_MCU_GBIAS_REQ : aon_wuc.h
- AONWUC_MCU_POWER_DOWN : aon_wuc.h
- AONWUC_MCU_POWER_ON : aon_wuc.h
- AONWUC_MCU_RESET_SRC : aon_wuc.h
- AONWUC_MCU_RESET_TYPE : aon_wuc.h
- AONWUC_NO_CLOCK : aon_wuc.h
- AONWUC_OSC_BGAP_REQ : aon_wuc.h
- AONWUC_OSC_GBIAS_REQ : aon_wuc.h
- AONWUC_SPLY_POWER_DOWN : aon_wuc.h
- AONWUC_TOTAL_FLASH_ERASE : aon_wuc.h
- AONWUCAuxClockConfigGet() : aon_wuc.h
- AONWUCAuxClockConfigSet() : aon_wuc.c , aon_wuc.h
- AONWUCAuxImageInvalid() : aon_wuc.h
- AONWUCAuxImageValid() : aon_wuc.h
- AONWUCAuxPowerDownConfig() : aon_wuc.h
- AONWUCAuxPowerOffConfig() : aon_wuc.h
- AONWUCAuxReset() : aon_wuc.c , aon_wuc.h
- AONWUCAuxSRamConfig() : aon_wuc.c , aon_wuc.h
- AONWUCAuxWakeUpConfig() : aon_wuc.h
- AONWUCAuxWakeupEvent() : aon_wuc.c , aon_wuc.h
- AONWUCDomainPowerDownDisable() : aon_wuc.h
- AONWUCDomainPowerDownEnable() : aon_wuc.h
- AONWUCJtagPowerOff() : aon_wuc.h
- AONWUCMcuPowerDownConfig() : aon_wuc.h
- AONWUCMcuPowerOffConfig() : aon_wuc.h
- AONWUCMcuResetClear() : aon_wuc.h
- AONWUCMcuResetStatus() : aon_wuc.h
- AONWUCMcuSRamConfig() : aon_wuc.h
- AONWUCMcuWakeUpConfig() : aon_wuc.h
- AONWUCOscConfig() : aon_wuc.c , aon_wuc.h
- AONWUCPowerStatus() : aon_wuc.h
- AONWUCRechargeCtrlConfigGet() : aon_wuc.h
- AONWUCRechargeCtrlConfigSet() : aon_wuc.c , aon_wuc.h
- AONWUCShutDownEnable() : aon_wuc.h
- ASSERT : debug.h
- AUX_CLOCK_DIV_128 : aon_wuc.h
- AUX_CLOCK_DIV_16 : aon_wuc.h
- AUX_CLOCK_DIV_2 : aon_wuc.h
- AUX_CLOCK_DIV_256 : aon_wuc.h
- AUX_CLOCK_DIV_32 : aon_wuc.h
- AUX_CLOCK_DIV_4 : aon_wuc.h
- AUX_CLOCK_DIV_64 : aon_wuc.h
- AUX_CLOCK_DIV_8 : aon_wuc.h
- AUX_CLOCK_DIV_M : aon_wuc.h
- AUX_CLOCK_DIV_UNUSED : aon_wuc.h
- AUX_FIXED_WAKE_UP : aon_wuc.h
- AUX_IMM_WAKE_UP : aon_wuc.h
- AUX_RAMREPAIR_DONE : aon_wuc.h
- AUX_SMPH_0 : aux_smph.h
- AUX_SMPH_1 : aux_smph.h
- AUX_SMPH_2 : aux_smph.h
- AUX_SMPH_3 : aux_smph.h
- AUX_SMPH_4 : aux_smph.h
- AUX_SMPH_5 : aux_smph.h
- AUX_SMPH_6 : aux_smph.h
- AUX_SMPH_7 : aux_smph.h
- AUX_SMPH_CLAIMED : aux_smph.h
- AUX_SMPH_FREE : aux_smph.h
- AUX_TDC_ABORT : aux_tdc.h
- AUX_TDC_BUSY : aux_tdc.h
- AUX_TDC_DONE : aux_tdc.h
- AUX_TDC_RUN : aux_tdc.h
- AUX_TDC_RUNSYNC : aux_tdc.h
- AUX_TDC_TIMEOUT : aux_tdc.h
- AUX_TIMER_0 : aux_timer.h
- AUX_TIMER_1 : aux_timer.h
- AUX_TIMER_BOTH : aux_timer.h
- AUX_TIMER_CFG_FALLING_EDGE : aux_timer.h
- AUX_TIMER_CFG_ONE_SHOT : aux_timer.h
- AUX_TIMER_CFG_ONE_SHOT_EDGE_COUNT : aux_timer.h
- AUX_TIMER_CFG_PERIODIC : aux_timer.h
- AUX_TIMER_CFG_PERIODIC_EDGE_COUNT : aux_timer.h
- AUX_TIMER_CFG_RISING_EDGE : aux_timer.h
- AUX_TIMER_CFG_TICK_SRC_ACLK_REF : aux_timer.h
- AUX_TIMER_CFG_TICK_SRC_ADC_DONE : aux_timer.h
- AUX_TIMER_CFG_TICK_SRC_ADC_IRQ : aux_timer.h
- AUX_TIMER_CFG_TICK_SRC_AIO0 : aux_timer.h
- AUX_TIMER_CFG_TICK_SRC_AIO1 : aux_timer.h
- AUX_TIMER_CFG_TICK_SRC_AIO10 : aux_timer.h
- AUX_TIMER_CFG_TICK_SRC_AIO11 : aux_timer.h
- AUX_TIMER_CFG_TICK_SRC_AIO12 : aux_timer.h
- AUX_TIMER_CFG_TICK_SRC_AIO13 : aux_timer.h
- AUX_TIMER_CFG_TICK_SRC_AIO14 : aux_timer.h
- AUX_TIMER_CFG_TICK_SRC_AIO15 : aux_timer.h
- AUX_TIMER_CFG_TICK_SRC_AIO2 : aux_timer.h
- AUX_TIMER_CFG_TICK_SRC_AIO3 : aux_timer.h
- AUX_TIMER_CFG_TICK_SRC_AIO4 : aux_timer.h
- AUX_TIMER_CFG_TICK_SRC_AIO5 : aux_timer.h
- AUX_TIMER_CFG_TICK_SRC_AIO6 : aux_timer.h
- AUX_TIMER_CFG_TICK_SRC_AIO7 : aux_timer.h
- AUX_TIMER_CFG_TICK_SRC_AIO8 : aux_timer.h
- AUX_TIMER_CFG_TICK_SRC_AIO9 : aux_timer.h
- AUX_TIMER_CFG_TICK_SRC_CMP_A : aux_timer.h
- AUX_TIMER_CFG_TICK_SRC_CMP_B : aux_timer.h
- AUX_TIMER_CFG_TICK_SRC_MCU_EVENT : aux_timer.h
- AUX_TIMER_CFG_TICK_SRC_RTC_EVENT : aux_timer.h
- AUX_TIMER_CFG_TICK_SRC_SMPH_RELEASE : aux_timer.h
- AUX_TIMER_CFG_TICK_SRC_TDCDONE : aux_timer.h
- AUX_TIMER_CFG_TICK_SRC_TIMER0_EVENT : aux_timer.h
- AUX_TIMER_CFG_TICK_SRC_TIMER1_EVENT : aux_timer.h
- AUX_TIMER_PRESCALE_DIV_1 : aux_timer.h
- AUX_TIMER_PRESCALE_DIV_1028 : aux_timer.h
- AUX_TIMER_PRESCALE_DIV_128 : aux_timer.h
- AUX_TIMER_PRESCALE_DIV_16 : aux_timer.h
- AUX_TIMER_PRESCALE_DIV_16384 : aux_timer.h
- AUX_TIMER_PRESCALE_DIV_2 : aux_timer.h
- AUX_TIMER_PRESCALE_DIV_2048 : aux_timer.h
- AUX_TIMER_PRESCALE_DIV_256 : aux_timer.h
- AUX_TIMER_PRESCALE_DIV_32 : aux_timer.h
- AUX_TIMER_PRESCALE_DIV_32768 : aux_timer.h
- AUX_TIMER_PRESCALE_DIV_4 : aux_timer.h
- AUX_TIMER_PRESCALE_DIV_4096 : aux_timer.h
- AUX_TIMER_PRESCALE_DIV_512 : aux_timer.h
- AUX_TIMER_PRESCALE_DIV_64 : aux_timer.h
- AUX_TIMER_PRESCALE_DIV_8 : aux_timer.h
- AUX_TIMER_PRESCALE_DIV_8192 : aux_timer.h
- AUX_VIRT_PWOFF_DISABLE : aon_wuc.h
- AUX_VIRT_PWOFF_ENABLE : aon_wuc.h
- AUX_WUC_ADC_CLOCK : aux_wuc.h
- AUX_WUC_ADI_CLOCK : aux_wuc.h
- AUX_WUC_AIODIO0_CLOCK : aux_wuc.h
- AUX_WUC_AIODIO1_CLOCK : aux_wuc.h
- AUX_WUC_CLOCK_HIFREQ : aux_wuc.h
- AUX_WUC_CLOCK_LOFREQ : aux_wuc.h
- AUX_WUC_CLOCK_OFF : aux_wuc.h
- AUX_WUC_CLOCK_READY : aux_wuc.h
- AUX_WUC_CLOCK_UNSTABLE : aux_wuc.h
- AUX_WUC_MODCLK_MASK : aux_wuc.h
- AUX_WUC_OSCCTRL_CLOCK : aux_wuc.h
- AUX_WUC_POWER_ACTIVE : aux_wuc.h
- AUX_WUC_POWER_DOWN : aux_wuc.h
- AUX_WUC_POWER_OFF : aux_wuc.h
- AUX_WUC_REF_CLOCK : aux_wuc.h
- AUX_WUC_SMPH_CLOCK : aux_wuc.h
- AUX_WUC_SOC_CLOCK : aux_wuc.h
- AUX_WUC_TDC_CLOCK : aux_wuc.h
- AUX_WUC_TDCIF_CLOCK : aux_wuc.h
- AUX_WUC_TIMER_CLOCK : aux_wuc.h
- AUXADC_FIFO_ALMOST_FULL_M : aux_adc.h
- AUXADC_FIFO_EMPTY_M : aux_adc.h
- AUXADC_FIFO_FULL_M : aux_adc.h
- AUXADC_FIFO_OVERFLOW_M : aux_adc.h
- AUXADC_FIFO_UNDERFLOW_M : aux_adc.h
- AUXADC_REF_FIXED : aux_adc.h
- AUXADC_REF_VDDA_REL : aux_adc.h
- AUXADC_SAMPLE_TIME_10P6_US : aux_adc.h
- AUXADC_SAMPLE_TIME_10P9_MS : aux_adc.h
- AUXADC_SAMPLE_TIME_170_US : aux_adc.h
- AUXADC_SAMPLE_TIME_1P37_MS : aux_adc.h
- AUXADC_SAMPLE_TIME_21P3_US : aux_adc.h
- AUXADC_SAMPLE_TIME_2P73_MS : aux_adc.h
- AUXADC_SAMPLE_TIME_2P7_US : aux_adc.h
- AUXADC_SAMPLE_TIME_341_US : aux_adc.h
- AUXADC_SAMPLE_TIME_42P6_US : aux_adc.h
- AUXADC_SAMPLE_TIME_5P3_US : aux_adc.h
- AUXADC_SAMPLE_TIME_5P46_MS : aux_adc.h
- AUXADC_SAMPLE_TIME_682_US : aux_adc.h
- AUXADC_SAMPLE_TIME_85P3_US : aux_adc.h
- AUXADC_TRIGGER_GPT0A : aux_adc.h
- AUXADC_TRIGGER_GPT0B : aux_adc.h
- AUXADC_TRIGGER_GPT1A : aux_adc.h
- AUXADC_TRIGGER_GPT1B : aux_adc.h
- AUXADC_TRIGGER_GPT2A : aux_adc.h
- AUXADC_TRIGGER_GPT2B : aux_adc.h
- AUXADC_TRIGGER_GPT3A : aux_adc.h
- AUXADC_TRIGGER_GPT3B : aux_adc.h
- AUXADC_TRIGGER_MANUAL : aux_adc.h
- AUXADCDisable() : aux_adc.h , aux_adc.c
- AUXADCEnableAsync() : aux_adc.h , aux_adc.c
- AUXADCEnableSync() : aux_adc.h , aux_adc.c
- AUXADCFlushFifo() : aux_adc.c , aux_adc.h
- AUXADCGenManualTrigger() : aux_adc.h
- AUXADCGetFifoStatus() : aux_adc.h
- AUXADCReadFifo() : aux_adc.h , aux_adc.c
- AUXADCSelectInput() : aux_adc.h
- AuxAdiDdiSafeRead() : ddi.h
- AuxAdiDdiSafeWrite() : ddi.h
- AUXSMPHAcquire() : aux_smph.h
- AUXSMPHRelease() : aux_smph.h
- AUXSMPHTryAcquire() : aux_smph.h
- AUXTDC_CLRCNT : aux_tdc.h
- AUXTDC_FORCE_STOP : aux_tdc.h
- AUXTDC_GETRESULTS : aux_tdc.h
- AUXTDC_IDLE : aux_tdc.h
- AUXTDC_NUM_SAT_VALS : aux_tdc.h
- AUXTDC_POR : aux_tdc.h
- AUXTDC_SAT_1024 : aux_tdc.h
- AUXTDC_SAT_1048576 : aux_tdc.h
- AUXTDC_SAT_131072 : aux_tdc.h
- AUXTDC_SAT_16384 : aux_tdc.h
- AUXTDC_SAT_2048 : aux_tdc.h
- AUXTDC_SAT_2097152 : aux_tdc.h
- AUXTDC_SAT_262144 : aux_tdc.h
- AUXTDC_SAT_32768 : aux_tdc.h
- AUXTDC_SAT_4096 : aux_tdc.h
- AUXTDC_SAT_4194304 : aux_tdc.h
- AUXTDC_SAT_512 : aux_tdc.h
- AUXTDC_SAT_524288 : aux_tdc.h
- AUXTDC_SAT_65536 : aux_tdc.h
- AUXTDC_SAT_8192 : aux_tdc.h
- AUXTDC_SAT_8388608 : aux_tdc.h
- AUXTDC_SAT_WRAP_AROUND : aux_tdc.h
- AUXTDC_START_ACLK : aux_tdc.h
- AUXTDC_START_ADC_DONE : aux_tdc.h
- AUXTDC_START_AIO0 : aux_tdc.h
- AUXTDC_START_AIO1 : aux_tdc.h
- AUXTDC_START_AIO10 : aux_tdc.h
- AUXTDC_START_AIO11 : aux_tdc.h
- AUXTDC_START_AIO12 : aux_tdc.h
- AUXTDC_START_AIO13 : aux_tdc.h
- AUXTDC_START_AIO14 : aux_tdc.h
- AUXTDC_START_AIO15 : aux_tdc.h
- AUXTDC_START_AIO2 : aux_tdc.h
- AUXTDC_START_AIO3 : aux_tdc.h
- AUXTDC_START_AIO4 : aux_tdc.h
- AUXTDC_START_AIO5 : aux_tdc.h
- AUXTDC_START_AIO6 : aux_tdc.h
- AUXTDC_START_AIO7 : aux_tdc.h
- AUXTDC_START_AIO8 : aux_tdc.h
- AUXTDC_START_AIO9 : aux_tdc.h
- AUXTDC_START_AON_WUC : aux_tdc.h
- AUXTDC_START_CMP_A : aux_tdc.h
- AUXTDC_START_CMP_B : aux_tdc.h
- AUXTDC_START_CS_RESET : aux_tdc.h
- AUXTDC_START_FALL : aux_tdc.h
- AUXTDC_START_MCU_EVT : aux_tdc.h
- AUXTDC_START_PRESCALER : aux_tdc.h
- AUXTDC_START_TIMER0 : aux_tdc.h
- AUXTDC_START_TIMER1 : aux_tdc.h
- AUXTDC_STARTPOL_FALL : aux_tdc.h
- AUXTDC_STARTPOL_RIS : aux_tdc.h
- AUXTDC_STOP_ACLK : aux_tdc.h
- AUXTDC_STOP_ADC_DONE : aux_tdc.h
- AUXTDC_STOP_AIO0 : aux_tdc.h
- AUXTDC_STOP_AIO1 : aux_tdc.h
- AUXTDC_STOP_AIO10 : aux_tdc.h
- AUXTDC_STOP_AIO11 : aux_tdc.h
- AUXTDC_STOP_AIO12 : aux_tdc.h
- AUXTDC_STOP_AIO13 : aux_tdc.h
- AUXTDC_STOP_AIO14 : aux_tdc.h
- AUXTDC_STOP_AIO15 : aux_tdc.h
- AUXTDC_STOP_AIO2 : aux_tdc.h
- AUXTDC_STOP_AIO3 : aux_tdc.h
- AUXTDC_STOP_AIO4 : aux_tdc.h
- AUXTDC_STOP_AIO5 : aux_tdc.h
- AUXTDC_STOP_AIO6 : aux_tdc.h
- AUXTDC_STOP_AIO7 : aux_tdc.h
- AUXTDC_STOP_AIO8 : aux_tdc.h
- AUXTDC_STOP_AIO9 : aux_tdc.h
- AUXTDC_STOP_AON_WUC : aux_tdc.h
- AUXTDC_STOP_CMP_A : aux_tdc.h
- AUXTDC_STOP_CMP_B : aux_tdc.h
- AUXTDC_STOP_CS_RESET : aux_tdc.h
- AUXTDC_STOP_MCU_EVT : aux_tdc.h
- AUXTDC_STOP_PRESCALER : aux_tdc.h
- AUXTDC_STOP_TIMER0 : aux_tdc.h
- AUXTDC_STOP_TIMER1 : aux_tdc.h
- AUXTDC_STOPPOL_FALL : aux_tdc.h
- AUXTDC_STOPPOL_RIS : aux_tdc.h
- AUXTDC_WAIT_CLRCNT_DONE : aux_tdc.h
- AUXTDC_WAIT_START : aux_tdc.h
- AUXTDC_WAIT_START_CNTEN : aux_tdc.h
- AUXTDC_WAIT_STOP : aux_tdc.h
- AUXTDC_WAIT_STOP_CNTDOWN : aux_tdc.h
- AUXTDCConfigSet() : aux_tdc.h , aux_tdc.c
- AUXTDCCounterDisable() : aux_tdc.h
- AUXTDCCounterEnable() : aux_tdc.h
- AUXTDCCounterGet() : aux_tdc.h
- AUXTDCCounterSet() : aux_tdc.h
- AUXTDCEnable() : aux_tdc.h
- AUXTDCIdle() : aux_tdc.h
- AUXTDCIdleForce() : aux_tdc.h
- AUXTDCLimitGet() : aux_tdc.h
- AUXTDCLimitSet() : aux_tdc.h
- AUXTDCMeasurementDone() : aux_tdc.h , aux_tdc.c
- AUXTDCMeasurementGet() : aux_tdc.h
- AUXTDCStatusGet() : aux_tdc.h
- AUXTimerConfigure() : aux_timer.c , aux_timer.h
- AUXTimerPrescaleGet() : aux_timer.c , aux_timer.h
- AUXTimerPrescaleSet() : aux_timer.c , aux_timer.h
- AUXTimerStart() : aux_timer.c , aux_timer.h
- AUXTimerStop() : aux_timer.h , aux_timer.c
- AUXTimerTargetValGet() : aux_timer.h
- AUXTimerTargetValSet() : aux_timer.h
- AUXWUCClockDisable() : aux_wuc.h , aux_wuc.c
- AUXWUCClockEnable() : aux_wuc.h , aux_wuc.c
- AUXWUCClockFreqReq() : aux_wuc.h
- AUXWUCClockStatus() : aux_wuc.h , aux_wuc.c
- AUXWUCFreezeDisable() : aux_wuc.h
- AUXWUCFreezeEnable() : aux_wuc.h
- AUXWUCPowerCtrl() : aux_wuc.c , aux_wuc.h