# cc26_chameleon JTAG_TAP

This document presents a summary of the hardware interface for the JTAG_TAP interface on cc26_chameleon product. Each module instance within the design is shown below, together with the module register map and bit definitions for each bitfield.

## cc26_chameleon Instance Summary

The table below shows the base address and address space for this memorymap.

Module Name | Base Address | Size
EFUSE | 0x10000000 | 256 Bytes
PRCM | 0x40000000 | 32 Bytes
TEST | 0x50000000 | 384 Bytes
AON | 0x60000000 | 56 Bytes

Add som trailing text about who built the page and with what configspec.