CC26xx Driver Library |

- Main Page
- Related Pages
- CC26xx APIs
- Register Descriptions
- Online Resources

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Modules Pages
Macros | Functions
aux_wuc.h File Reference
`#include <stdbool.h>`
`#include <stdint.h>`
`#include <inc/hw_types.h>`
`#include <inc/hw_memmap.h>`
`#include <inc/hw_aux_wuc.h>`
`#include <driverlib/debug.h>`

Go to the source code of this file.

## Macros
#define | AUX_WUC_POWER_OFF 0x00000001
#define | AUX_WUC_POWER_DOWN 0x00000002
#define | AUX_WUC_POWER_ACTIVE 0x00000004
#define | AUX_WUC_SMPH_CLOCK 0x00000001
#define | AUX_WUC_AIODIO0_CLOCK 0x00000002
#define | AUX_WUC_AIODIO1_CLOCK 0x00000004
#define | AUX_WUC_TIMER_CLOCK 0x00000008
#define | AUX_WUC_SOC_CLOCK 0x00000010
#define | AUX_WUC_TDCIF_CLOCK 0x00000020
#define | AUX_WUC_OSCCTRL_CLOCK 0x00000040
#define | AUX_WUC_ADI_CLOCK 0x00000080
#define | AUX_WUC_MODCLK_MASK 0x000000FF
#define | AUX_WUC_TDC_CLOCK 0x00000100
#define | AUX_WUC_ADC_CLOCK 0x00000200
#define | AUX_WUC_REF_CLOCK 0x00000400
#define | AUX_WUC_CLOCK_OFF 0x00000000
#define | AUX_WUC_CLOCK_UNSTABLE 0x00000001
#define | AUX_WUC_CLOCK_READY 0x00000011
#define | AUX_WUC_CLOCK_HIFREQ 0x00000000
#define | AUX_WUC_CLOCK_LOFREQ 0x00000001

## Functions
void | AUXWUCClockEnable (uint32_t ui32Clocks)
| Enable clocks for peripherals in the AUX domain. More...
void | AUXWUCClockDisable (uint32_t ui32Clocks)
| Disable clocks for peripherals in the AUX domain. More...
uint32_t | AUXWUCClockStatus (uint32_t ui32Clocks)
| Get the status of a clock. More...
__STATIC_INLINE void | AUXWUCClockFreqReq (uint32_t ui32ClockFreq)
| Request a high or low frequency clock source. More...
void | AUXWUCPowerCtrl (uint32_t ui32PowerMode)
| Control the power to the AUX domain. More...
__STATIC_INLINE void | AUXWUCFreezeEnable (void)
| Freeze the AUX IOs. More...
__STATIC_INLINE void | AUXWUCFreezeDisable (void)
| Unfreeze the AUX IOs. More...