CC26xx Driver Library |

- Main Page
- Related Pages
- CC26xx APIs
- Register Descriptions
- Online Resources

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Modules Pages
Macros | Typedefs | Enumerations | Functions
flash.h File Reference
`#include <stdbool.h>`
`#include <stdint.h>`
`#include <inc/hw_types.h>`
`#include <inc/hw_flash.h>`
`#include <inc/hw_memmap.h>`
`#include <inc/hw_ints.h>`
`#include <inc/hw_aon_sysctl.h>`
`#include <inc/hw_fcfg1.h>`
`#include <driverlib/interrupt.h>`
`#include <driverlib/debug.h>`

Go to the source code of this file.

## Macros
#define | FAPI_STATUS_SUCCESS 0x00000000
#define | FAPI_STATUS_FSM_BUSY 0x00000001
#define | FAPI_STATUS_FSM_READY 0x00000002
#define | FAPI_STATUS_INCORRECT_DATABUFFER_LENGTH 0x00000003
#define | FAPI_STATUS_FSM_ERROR 0x00000004
#define | FLASH_INT_FSM_DONE 0x00400000
#define | FLASH_INT_RV 0x00010000
#define | FLASH_PWR_ACTIVE_MODE 0x00000000
#define | FLASH_PWR_OFF_MODE 0x00000001
#define | FLASH_PWR_DEEP_STDBY_MODE 0x00000002
#define | FLASH_NO_PROTECT 0x00000000
#define | FLASH_WRITE_PROTECT 0x00000001
#define | ADDR_OFFSET (0x1F800000 - FLASHMEM_BASE)
#define | FCFG1_OFFSET 0x1000
#define | FLASH_MODULE_CLK_FREQ 48
#define | FSM_REG_WRT_ENABLE 5
#define | FSM_REG_WRT_DISABLE 2
#define | FBFALLBACK_SLEEP 0
#define | FBFALLBACK_DEEP_STDBY 1
#define | FBFALLBACK_ACTIVE 3
#define | FLASH_BAGP 0x14
#define | FLASH_PAGP 0x14
#define | PATTERN_BITS 0x20
#define | FW_WRT_TRIMMED 0x00000001
#define | FWPWRITE_BYTE_ADDRESS ((tFwpWriteByte *)((FLASH_BASE + FLASH_O_FWPWRITE0)))
#define | DUMPWORD_INSTR 0x04
#define | FLASH_CMD_EXEC 0x15
#define | CCFG_OFFSET_SECURITY 0x00000FD8
#define | CCFG_OFFSET_SECT_PROT 0x00000FF0
#define | CCFG_SIZE_SECURITY 0x00000014
#define | CCFG_SIZE_SECT_PROT 0x00000004

## Typedefs
typedef volatile uint8_t | tFwpWriteByte

## Enumerations
enum | tFlashStateCommandsType { FAPI_PROGRAM_DATA = 0x0002, FAPI_ERASE_SECTOR = 0x0006, FAPI_ERASE_BANK = 0x0008, FAPI_VALIDATE_SECTOR = 0x000E, FAPI_CLEAR_STATUS = 0x0010, FAPI_PROGRAM_RESUME = 0x0014, FAPI_ERASE_RESUME = 0x0016, FAPI_CLEAR_MORE = 0x0018, FAPI_PROGRAM_SECTOR = 0x0020, FAPI_ERASE_OTP = 0x0030 }
| Defined values for Flash State Machine commands. More...

## Functions
__STATIC_INLINE uint32_t | FlashSectorSizeGet (void)
| Get size of a flash sector in number of bytes. More...
__STATIC_INLINE uint32_t | FlashSizeGet (void)
| Get the size of the flash. More...
void | FlashPowerModeSet (uint32_t ui32PowerMode, uint32_t ui32BankGracePeriode, uint32_t ui32PumpGracePeriode)
| Set power mode. More...
uint32_t | FlashPowerModeGet (void)
| Get current configured power mode. More...
void | FlashProtectionSet (uint32_t ui32SectorAddress, uint32_t ui32ProtectMode)
| Set sector protection. More...
uint32_t | FlashProtectionGet (uint32_t ui32SectorAddress)
| Get sector protection. More...
uint32_t | FlashProtectionSave (uint32_t ui32SectorAddress)
| Save sector protection to make it permanent. More...
__STATIC_INLINE uint32_t | FlashCheckFsmForError (void)
| Checks if the Flash state machine has detected an error. More...
__STATIC_INLINE uint32_t | FlashCheckFsmForReady (void)
| Checks if the Flash state machine is ready. More...
__STATIC_INLINE void | FlashIntRegister (void(*pfnHandler)(void))
| Registers an interrupt handler for the flash interrupt. More...
__STATIC_INLINE void | FlashIntUnregister (void)
| Unregisters the interrupt handler for the flash interrupt. More...
__STATIC_INLINE void | FlashIntEnable (uint32_t ui32IntFlags)
| Enables flash controller interrupt sources. More...
__STATIC_INLINE void | FlashIntDisable (uint32_t ui32IntFlags)
| Disables individual flash controller interrupt sources. More...
__STATIC_INLINE uint32_t | FlashIntStatus (void)
| Gets the current interrupt status. More...
__STATIC_INLINE void | FlashIntClear (uint32_t ui32IntFlags)
| Clears flash controller interrupt source. More...
uint32_t | FlashSectorErase (uint32_t ui32SectorAddress)
| Erase a flash sector. More...
uint32_t | FlashProgram (uint8_t *pui8DataBuffer, uint32_t ui32Address, uint32_t ui32Count)
| Programs unprotected main bank flash sectors. More...
bool | FlashEfuseReadRow (uint32_t *pui32EfuseData, uint32_t ui32RowAddress)
| Reads efuse data from specified row. More...
void | FlashDisableSectorsForWrite (void)
| Disables all sectors for erase and programming on the active bank. More...