# cc26_chameleon ANATOP_MMAP

This document presents a summary of the hardware interface for the ANATOP_MMAP interface on cc26_chameleon product. Each module instance within the design is shown below, together with the module register map and bit definitions for each bitfield.

## cc26_chameleon Instance Summary

The table below shows the base address and address space for this memorymap.

Module Name | Base Address | Size
ADI_0_RF | 0x00000000 | 128 Bytes
ADI_1_SYNTH | 0x10000000 | 64 Bytes
DLO_DTX | 0x40044000 | 512 Bytes
ADI_2_REFSYS | 0x40086000 | 64 Bytes
ADI_3_REFSYS | 0x40086200 | 64 Bytes
DDI_0_OSC | 0x400CA000 | 256 Bytes
ADI_4_AUX | 0x400CB000 | 64 Bytes

Add som trailing text about who built the page and with what configspec.