CC26xx Driver Library |

- Main Page
- Related Pages
- CC26xx APIs
- Register Descriptions
- Online Resources

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Modules Pages
Functions
aux_adc.c File Reference
`#include <driverlib/aux_adc.h>`
`#include <inc/hw_memmap.h>`
`#include <inc/hw_aux_wuc.h>`
`#include <driverlib/adi.h>`
`#include <driverlib/event.h>`

Go to the source code of this file.

## Functions
void | AUXADCDisable (void)
| Disables the ADC. More...
void | AUXADCEnableAsync (uint32_t refSource, uint32_t trigger)
| Enables the ADC for asynchronous operation. More...
void | AUXADCEnableSync (uint32_t refSource, uint32_t sampleTime, uint32_t trigger)
| Enables the ADC for synchronous operation. More...
void | AUXADCFlushFifo (void)
| Flushes the ADC FIFO. More...
uint32_t | AUXADCReadFifo (void)
| Waits for and returns the first sample in the ADC FIFO. More...