CC26xx Driver Library |

- Main Page
- Related Pages
- CC26xx APIs
- Register Descriptions
- Online Resources

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Modules Pages
Macros | Functions
flashsafe.h File Reference
`#include <stdbool.h>`
`#include <stdint.h>`
`#include <inc/hw_types.h>`
`#include <inc/hw_flash.h>`
`#include <inc/hw_memmap.h>`
`#include <inc/hw_ints.h>`
`#include <inc/hw_fcfg1.h>`
`#include <driverlib/interrupt.h>`
`#include <driverlib/debug.h>`
`#include <driverlib/flash.h>`
`#include <driverlib/rom.h>`
`#include <driverlib/smph.h>`

Go to the source code of this file.

## Macros
#define | FLASHSAFE_ACCESS_DENIED 0x000000ff
#define | FLASHSAFE_ACCESS_OK 0x000000ee
#define | SMPH_ALLOC_FLASH 1
#define | FAPI_STATUS_SUCCESS 0x00000000
#define | FAPI_STATUS_FSM_BUSY 0x00000001
#define | FAPI_STATUS_FSM_READY 0x00000002
#define | FAPI_STATUS_INCORRECT_DATABUFFER_LENGTH 0x00000003
#define | FAPI_STATUS_FSM_ERROR 0x00000004
#define | FLASH_INT_FSM_DONE 0x00400000
#define | FLASH_INT_RV 0x00010000
#define | FLASH_PWR_ACTIVE_MODE 0x00000000
#define | FLASH_PWR_OFF_MODE 0x00000001
#define | FLASH_PWR_DEEP_STDBY_MODE 0x00000002
#define | FLASH_NO_PROTECT 0x00000000
#define | FLASH_WRITE_PROTECT 0x00000001
#define | FSM_REG_WRT_ENABLE 5
#define | FSM_REG_WRT_DISABLE 2

## Functions
__STATIC_INLINE bool | FlashsafeSMPHTryAcquire (void)
| Aquire the flash semaphore. More...
__STATIC_INLINE void | FlashsafeSMPHRelease (void)
| Release the flash semaphore. More...
uint32_t | FlashsafeSizeGet (void)
| Get the size of the flash. More...
uint32_t | FlashsafeSectorSizeGet (void)
| Get size of a flash sector in no of bytes. More...
uint32_t | FlashsafePowerModeSet (uint32_t ui32PowerMode, uint32_t ui32BankGracePeriode, uint32_t ui32PumpGracePeriode)
| Set power mode. More...
uint32_t | FlashsafePowerModeGet (void)
| Get current configured power mode. More...
uint32_t | FlashsafeProtectionSet (uint32_t ui32SectorAddress, uint32_t ui32ProtectMode)
| Set sector protection. More...
uint32_t | FlashsafeProtectionGet (uint32_t ui32SectorAddress)
| Get sector protection. More...
uint32_t | FlashsafeProtectionSave (uint32_t ui32SectorAddress)
| Save sector protection to make it permanent. More...
uint32_t | FlashsafeCheckFsmForError (void)
| Checks if the Flashsafe state machine has detected an error. More...
uint32_t | FlashsafeCheckFsmForReady (void)
| Checks if the Flash state machine is ready. More...
uint32_t | FlashsafeIntRegister (void(*pfnHandler)(void))
| Registers an interrupt handler for the flash interrupt. More...
uint32_t | FlashsafeIntUnregister (void)
| Unregisters the interrupt handler for the flash interrupt. More...
uint32_t | FlashsafeIntEnable (uint32_t ui32IntFlags)
| Enables flash controller interrupt sources. More...
uint32_t | FlashsafeIntDisable (uint32_t ui32IntFlags)
| Disables individual flash controller interrupt sources. More...
uint32_t | FlashsafeIntStatus (void)
| Gets the current interrupt status. More...
uint32_t | FlashsafeIntClear (uint32_t ui32IntFlags)
| Clears flash controller interrupt source. More...
uint32_t | FlashsafeSectorErase (uint32_t ui32SectorAddress)
| Erase a flash sector. More...
uint32_t | FlashsafeProgram (uint8_t *pui8DataBuffer, uint32_t ui32Address, uint32_t ui32Count)
| Programs unprotected main bank flash sectors. More...
uint32_t | FlashsafeDisableSectorsForWrite (void)
| Disables all sectors for erase and programming on the active bank. More...