CC26xx Driver Library |

- Main Page
- Related Pages
- CC26xx APIs
- Register Descriptions
- Online Resources

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Modules Pages
Macros | Functions
prcm.h File Reference
`#include <stdbool.h>`
`#include <stdint.h>`
`#include <inc/hw_types.h>`
`#include <inc/hw_memmap.h>`
`#include <inc/hw_ints.h>`
`#include <inc/hw_prcm.h>`
`#include <inc/hw_nvic.h>`
`#include <inc/hw_aon_rtc.h>`
`#include <driverlib/interrupt.h>`
`#include <driverlib/debug.h>`
`#include <driverlib/cpu.h>`

Go to the source code of this file.

## Macros
#define | PRCM_RUN_MODE 0x00000001
#define | PRCM_SLEEP_MODE 0x00000002
#define | PRCM_DEEP_SLEEP_MODE 0x00000004
#define | PRCM_CLOCK_DIV_1 0x0000000
#define | PRCM_CLOCK_DIV_2 0x0000001
#define | PRCM_CLOCK_DIV_4 0x0000002
#define | PRCM_CLOCK_DIV_8 0x0000003
#define | PRCM_CLOCK_DIV_16 0x0000004
#define | PRCM_CLOCK_DIV_32 0x0000005
#define | PRCM_CLOCK_DIV_64 0x0000006
#define | PRCM_CLOCK_DIV_128 0x0000007
#define | PRCM_CLOCK_DIV_256 0x0000008
#define | PRCM_DOMAIN_RFCORE 0x00000001
#define | PRCM_DOMAIN_SERIAL 0x00000002
#define | PRCM_DOMAIN_PERIPH 0x00000004
#define | PRCM_DOMAIN_SYSBUS 0x00000008
#define | PRCM_DOMAIN_VIMS 0x00000010
#define | PRCM_DOMAIN_CPU 0x00000020
#define | PRCM_DOMAIN_TIMER 0x00000040
#define | PRCM_DOMAIN_CLKCTRL 0x00000080
#define | PRCM_DOMAIN_MCU 0x00000100
#define | PRCM_DOMAIN_POWER_OFF 0x00000002
#define | PRCM_DOMAIN_POWER_ON 0x00000001
#define | PRCM_DOMAIN_POWER_DOWN_READY 0x00000000
#define | PRCM_WCLK_NEG_EDGE 0x00000008
#define | PRCM_WCLK_POS_EDGE 0x00000000
#define | PRCM_WCLK_SINGLE_PHASE 0x00000000
#define | PRCM_WCLK_DUAL_PHASE 0x00000002
#define | PRCM_WCLK_USER_DEF 0x00000004
#define | I2S_SAMPLE_RATE_16K 0x00000001
#define | I2S_SAMPLE_RATE_24K 0x00000002
#define | I2S_SAMPLE_RATE_32K 0x00000004
#define | I2S_SAMPLE_RATE_48K 0x00000008
#define | PRCM_PERIPH_TIMER0 0x00000000
#define | PRCM_PERIPH_TIMER1 0x00000001
#define | PRCM_PERIPH_TIMER2 0x00000002
#define | PRCM_PERIPH_TIMER3 0x00000003
#define | PRCM_PERIPH_SSI0 0x00000100
#define | PRCM_PERIPH_SSI1 0x00000101
#define | PRCM_PERIPH_UART0 0x00000200
#define | PRCM_PERIPH_UART1 0x00000201
#define | PRCM_PERIPH_I2C0 0x00000300
#define | PRCM_PERIPH_I2C1 0x00000301
#define | PRCM_PERIPH_CRYPTO 0x00000400
#define | PRCM_PERIPH_TRNG 0x00000401
#define | PRCM_PERIPH_UDMA 0x00000408
#define | PRCM_PERIPH_GPIO 0x00000500
#define | PRCM_PERIPH_I2S 0x00000600

## Functions
void | PRCMInfClockConfigureSet (uint32_t ui32ClkDiv, uint32_t ui32PowerMode)
| Configure the infrastructure clock. More...
uint32_t | PRCMInfClockConfigureGet (uint32_t ui32PowerMode)
| Use this function to retreive the set infrastructure clock configuration. More...
__STATIC_INLINE void | PRCMMcuPowerOff (void)
| Request a power off of the MCU voltage domain. More...
__STATIC_INLINE void | PRCMMcuPowerOffCancel (void)
| Cancel a request for a power off of the MCU voltage domain. More...
__STATIC_INLINE void | PRCMMcuUldoConfigure (uint32_t ui32Enable)
| Assert or deassert a request for the uLDO. More...
void | PRCMClockConfigureSet (uint32_t ui32Domains, uint32_t ui32ClkDiv)
| Setup the clock division factor for a subsystem in the MCU voltage domain. More...
uint32_t | PRCMClockConfigureGet (uint32_t ui32Domain)
| Get the clock configuration for a specific sub system in the MCU Voltage Domain. More...
__STATIC_INLINE void | PRCMAudioClockEnable (void)
| Enable the audio clock generation. More...
__STATIC_INLINE void | PRCMAudioClockDisable (void)
| Disable the audio clock generation. More...
void | PRCMAudioClockConfigSet (uint32_t ui32ClkConfig, uint32_t ui32SampleRate)
| Configure the audio clock generation. More...
void | PRCMAudioClockConfigSetOverride (uint32_t ui32ClkConfig, uint32_t ui32MstDiv, uint32_t ui32BitDiv, uint32_t ui32WordDiv)
| Configure the audio clock generation with manual setting of clock divider. More...
__STATIC_INLINE void | PRCMLoadSet (void)
| Use this function to synchronize the load settings. More...
__STATIC_INLINE bool | PRCMLoadGet (void)
| Check if any of the load sensitive register has been updated. More...
__STATIC_INLINE void | PRCMDomainEnable (uint32_t ui32Domains)
| Enable clock domains in the MCU voltage domain. More...
__STATIC_INLINE void | PRCMDomainDisable (uint32_t ui32Domains)
| Disable clock domains in the MCU voltage domain. More...
void | PRCMPowerDomainOn (uint32_t ui32Domains)
| Turn power on in power domains in the MCU domain. More...
void | PRCMPowerDomainOff (uint32_t ui32Domains)
| Turn off a specific power domain. More...
__STATIC_INLINE void | PRCMRfPowerDownWhenIdle (void)
| Configure RF core to power down when idle. More...
void | PRCMPeripheralRunEnable (uint32_t ui32Peripheral)
| Enables a peripheral in Run mode. More...
void | PRCMPeripheralRunDisable (uint32_t ui32Peripheral)
| Disables a peripheral in Run mode. More...
void | PRCMPeripheralSleepEnable (uint32_t ui32Peripheral)
| Enables a peripheral in sleep mode. More...
void | PRCMPeripheralSleepDisable (uint32_t ui32Peripheral)
| Disables a peripheral in sleep mode. More...
void | PRCMPeripheralDeepSleepEnable (uint32_t ui32Peripheral)
| Enables a peripheral in deep-sleep mode. More...
void | PRCMPeripheralDeepSleepDisable (uint32_t ui32Peripheral)
| Disables a peripheral in deep-sleep mode. More...
uint32_t | PRCMPowerDomainStatus (uint32_t ui32Domains)
| Get the status for a specific power domain. More...
__STATIC_INLINE bool | PRCMRfReady (void)
| Return the access status of the RF Core. More...
__STATIC_INLINE bool | PRCMWdtResetStatus (void)
| Read reset status for WatchDog Timer. More...
__STATIC_INLINE void | PRCMSleep (void)
| Put the processor into sleep mode. More...
void | PRCMDeepSleep (void)
| Put the processor into deep-sleep mode. More...
void | PRCMRetentionEnable (uint32_t ui32PowerDomain)
| Enable retention on specific power domains. More...
void | PRCMRetentionDisable (uint32_t ui32PowerDomain)
| Disable retention on power domains. More...