# cc26_chameleon CPU_MMAP

This document presents a summary of the hardware interface for the CPU_MMAP interface on cc26_chameleon product. Each module instance within the design is shown below, together with the module register map and bit definitions for each bitfield.

## cc26_chameleon Instance Summary

The table below shows the base address and address space for this memorymap.

Module Name | Base Address | Size
FLASHMEM | 0x00000000 | 512 KBytes
BROM | 0x10000000 | 512 KBytes
GPRAM | 0x11000000 | 32 KBytes
SRAM | 0x20000000 | 128 KBytes
RFC_RAM | 0x21000000 | 16 KBytes
SSI0 | 0x40000000 | 16 KBytes
UART0 | 0x40001000 | 16 KBytes
I2C0 | 0x40002000 | 16 KBytes
SSI1 | 0x40008000 | 16 KBytes
GPT0 | 0x40010000 | 16 KBytes
GPT1 | 0x40011000 | 16 KBytes
GPT2 | 0x40012000 | 16 KBytes
GPT3 | 0x40013000 | 16 KBytes
UDMA0 | 0x40020000 | 16 KBytes
I2S0 | 0x40021000 | 16 KBytes
GPIO | 0x40022000 | 4 KBytes
CRYPTO | 0x40024000 | 8 KBytes
TRNG | 0x40028000 | 32 KBytes
FLASH | 0x40030000 | 64 KBytes
VIMS | 0x40034000 | 4 KBytes
RFC_PWR | 0x40040000 | 16 Bytes
RFC_DBELL | 0x40041000 | 256 Bytes
RFC_PHA | 0x40042000 | 4 KBytes
RFC_RAT | 0x40043000 | 1 KBytes
RFC_FSCA | 0x40044000 | 2 KBytes
RFC_MDM | 0x40045000 | 4 KBytes
RFC_RFE | 0x40046000 | 1 KBytes
RFC_TRC | 0x40047000 | 256 Bytes
RFC_S2R | 0x40048000 | 64 Bytes
WDT | 0x40080000 | 16 KBytes
IOC | 0x40081000 | 16 KBytes
PRCM | 0x40082000 | 16 KBytes
EVENT | 0x40083000 | 16 KBytes
SMPH | 0x40084000 | 16 KBytes
SPIS | 0x40085000 | 6 KBytes
ADI2 | 0x40086000 | 2 KBytes
ADI3 | 0x40086200 | 2 KBytes
AON_SYSCTL | 0x40090000 | 4 KBytes
AON_WUC | 0x40091000 | 16 KBytes
AON_RTC | 0x40092000 | 4 KBytes
AON_EVENT | 0x40093000 | 4 KBytes
AON_IOC | 0x40094000 | 4 KBytes
AON_BATMON | 0x40095000 | 4 KBytes
AUX_AIODIO0 | 0x400C1000 | 16 KBytes
AUX_AIODIO1 | 0x400C2000 | 16 KBytes
AUX_TDCIF | 0x400C4000 | 16 KBytes
AUX_EVCTL | 0x400C5000 | 16 KBytes
AUX_WUC | 0x400C6000 | 16 KBytes
AUX_TIMER | 0x400C7000 | 16 KBytes
AUX_SMPH | 0x400C8000 | 16 KBytes
AUX_ANAIF | 0x400C9000 | 16 KBytes
AUX_DDI0_OSC | 0x400CA000 | 16 KBytes
AUX_ADI4 | 0x400CB000 | 2 KBytes
AUX_RAM | 0x400E0000 | 16 KBytes
AUX_SCE | 0x400E1000 | 16 KBytes
FCFG1 | 0x50001000 | 4 KBytes
FCFG2 | 0x50002000 | 4 KBytes
CCFG | 0x50003000 | 16 KBytes
CPU_ITM | 0xE0000000 | 16 KBytes
CPU_DWT | 0xE0001000 | 16 KBytes
CPU_FPB | 0xE0002000 | 16 KBytes
CPU_SCS | 0xE000E000 | 16 KBytes
CPU_TPIU | 0xE0040000 | 16 KBytes
CPU_TIPROP | 0xE00FE000 | 16 KBytes
CPU_ROM_TABLE | 0xE00FF000 | 16 KBytes

Add som trailing text about who built the page and with what configspec.