## AUX_ADI4

Instance: AUX_ADI4
Component: ADI
Base address: 0x400cb000

Analog Digital Interface
This is a generic module for handling register information between digital and analog domain.
To see the actual contents connected on the analog side, please see:
ADI2: ADI_2_REFSYS:ADI_2_REFSYS
ADI3: ADI_3_REFSYS:ADI_3_REFSYS
ADI4: ADI_4_AUX:ADI4_AUX

### TOP:AUX_ADI4 Register Summary

Register Name | Type | Register Width (Bits) | Register Reset | Address Offset | Physical Address
DIR03 | RW | 32 | 0x0000 0000 | 0x0000 0000 | 0x400C B000
DIR47 | RW | 32 | 0x0000 0000 | 0x0000 0004 | 0x400C B004
DIR811 | RW | 32 | 0x0000 0000 | 0x0000 0008 | 0x400C B008
DIR1215 | RW | 32 | 0x0000 0000 | 0x0000 000C | 0x400C B00C
SET03 | WO | 32 | 0x0000 0000 | 0x0000 0010 | 0x400C B010
SET47 | WO | 32 | 0x0000 0000 | 0x0000 0014 | 0x400C B014
SET811 | WO | 32 | 0x0000 0000 | 0x0000 0018 | 0x400C B018
SET1215 | WO | 32 | 0x0000 0000 | 0x0000 001C | 0x400C B01C
CLR03 | WO | 32 | 0x0000 0000 | 0x0000 0020 | 0x400C B020
CLR47 | WO | 32 | 0x0000 0000 | 0x0000 0024 | 0x400C B024
CLR811 | WO | 32 | 0x0000 0000 | 0x0000 0028 | 0x400C B028
CLR1215 | WO | 32 | 0x0000 0000 | 0x0000 002C | 0x400C B02C
SLAVESTAT | RW | 32 | 0x0000 0000 | 0x0000 0030 | 0x400C B030
SLAVECONF | RW | 32 | 0x0000 0004 | 0x0000 0038 | 0x400C B038
MASK4B01 | WO | 32 | 0x0000 0000 | 0x0000 0040 | 0x400C B040
MASK4B23 | WO | 32 | 0x0000 0000 | 0x0000 0044 | 0x400C B044
MASK4B45 | WO | 32 | 0x0000 0000 | 0x0000 0048 | 0x400C B048
MASK4B67 | WO | 32 | 0x0000 0000 | 0x0000 004C | 0x400C B04C
MASK4B89 | WO | 32 | 0x0000 0000 | 0x0000 0050 | 0x400C B050
MASK4B1011 | WO | 32 | 0x0000 0000 | 0x0000 0054 | 0x400C B054
MASK4B1213 | WO | 32 | 0x0000 0000 | 0x0000 0058 | 0x400C B058
MASK4B1415 | WO | 32 | 0x0000 0000 | 0x0000 005C | 0x400C B05C
MASK8B01 | WO | 32 | 0x0000 0000 | 0x0000 0060 | 0x400C B060
MASK8B23 | WO | 32 | 0x0000 0000 | 0x0000 0064 | 0x400C B064
MASK8B45 | WO | 32 | 0x0000 0000 | 0x0000 0068 | 0x400C B068
MASK8B67 | WO | 32 | 0x0000 0000 | 0x0000 006C | 0x400C B06C
MASK8B89 | WO | 32 | 0x0000 0000 | 0x0000 0070 | 0x400C B070
MASK8B1011 | WO | 32 | 0x0000 0000 | 0x0000 0074 | 0x400C B074
MASK8B1213 | WO | 32 | 0x0000 0000 | 0x0000 0078 | 0x400C B078
MASK8B1415 | WO | 32 | 0x0000 0000 | 0x0000 007C | 0x400C B07C
MASK16B01 | WO | 32 | 0x0000 0000 | 0x0000 0080 | 0x400C B080
MASK16B23 | WO | 32 | 0x0000 0000 | 0x0000 0084 | 0x400C B084
MASK16B45 | WO | 32 | 0x0000 0000 | 0x0000 0088 | 0x400C B088
MASK16B67 | WO | 32 | 0x0000 0000 | 0x0000 008C | 0x400C B08C
MASK16B89 | WO | 32 | 0x0000 0000 | 0x0000 0090 | 0x400C B090
MASK16B1011 | WO | 32 | 0x0000 0000 | 0x0000 0094 | 0x400C B094
MASK16B1213 | WO | 32 | 0x0000 0000 | 0x0000 0098 | 0x400C B098
MASK16B1415 | WO | 32 | 0x0000 0000 | 0x0000 009C | 0x400C B09C

### TOP:AUX_ADI4 Register Descriptions

### TOP:ADI:DIR03

Address offset | 0x0000 0000
Physical address | 0x400C B000 | Instance | AUX_ADI4
Description | Direct access for adi byte offsets 0 to 3
Type | RW

Bits | Field Name | Description | Type | Reset
31:24 | B3 | Direct access to ADI register 3 | RW | 0x00
23:16 | B2 | Direct access to ADI register 2 | RW | 0x00
15:8 | B1 | Direct access to ADI register 1 | RW | 0x00
7:0 | B0 | Direct access to ADI register 0 | RW | 0x00

### TOP:ADI:DIR47

Address offset | 0x0000 0004
Physical address | 0x400C B004 | Instance | AUX_ADI4
Description | Direct access for adi byte offsets 4 to 7
Type | RW

Bits | Field Name | Description | Type | Reset
31:24 | B3 | Direct access to ADI register 7 | RW | 0x00
23:16 | B2 | Direct access to ADI register 6 | RW | 0x00
15:8 | B1 | Direct access to ADI register 5 | RW | 0x00
7:0 | B0 | Direct access to ADI register 4 | RW | 0x00

### TOP:ADI:DIR811

Address offset | 0x0000 0008
Physical address | 0x400C B008 | Instance | AUX_ADI4
Description | Direct access for adi byte offsets 8 to 11
Type | RW

Bits | Field Name | Description | Type | Reset
31:24 | B3 | Direct access to ADI register 11 | RW | 0x00
23:16 | B2 | Direct access to ADI register 10 | RW | 0x00
15:8 | B1 | Direct access to ADI register 9 | RW | 0x00
7:0 | B0 | Direct access to ADI register 8 | RW | 0x00

### TOP:ADI:DIR1215

Address offset | 0x0000 000C
Physical address | 0x400C B00C | Instance | AUX_ADI4
Description | Direct access for adi byte offsets 12 to 15
Type | RW

Bits | Field Name | Description | Type | Reset
31:24 | B3 | Direct access to ADI register 15 | RW | 0x00
23:16 | B2 | Direct access to ADI register 14 | RW | 0x00
15:8 | B1 | Direct access to ADI register 13 | RW | 0x00
7:0 | B0 | Direct access to ADI register 12 | RW | 0x00

### TOP:ADI:SET03

Address offset | 0x0000 0010
Physical address | 0x400C B010 | Instance | AUX_ADI4
Description | Set register for ADI byte offsets 0 to 3
Type | WO

Bits | Field Name | Description | Type | Reset
31:24 | S3 | A high bit value will set the corresponding bit in ADI register 3. Read returns 0. | WO | 0x00
23:16 | S2 | A high bit value will set the corresponding bit in ADI register 2. Read returns 0. | WO | 0x00
15:8 | S1 | A high bit value will set the corresponding bit in ADI register 1. Read returns 0. | WO | 0x00
7:0 | S0 | A high bit value will set the corresponding bit in ADI register 0. Read returns 0. | WO | 0x00

### TOP:ADI:SET47

Address offset | 0x0000 0014
Physical address | 0x400C B014 | Instance | AUX_ADI4
Description | Set register for ADI byte offsets 4 to 7
Type | WO

Bits | Field Name | Description | Type | Reset
31:24 | S3 | A high bit value will set the corresponding bit in ADI register 7. Read returns 0. | WO | 0x00
23:16 | S2 | A high bit value will set the corresponding bit in ADI register 6. Read returns 0. | WO | 0x00
15:8 | S1 | A high bit value will set the corresponding bit in ADI register 5. Read returns 0. | WO | 0x00
7:0 | S0 | A high bit value will set the corresponding bit in ADI register 4. Read returns 0. | WO | 0x00

### TOP:ADI:SET811

Address offset | 0x0000 0018
Physical address | 0x400C B018 | Instance | AUX_ADI4
Description | Set register for ADI byte offsets 8 to 11
Type | WO

Bits | Field Name | Description | Type | Reset
31:24 | S3 | A high bit value will set the corresponding bit in ADI register 11. Read returns 0. | WO | 0x00
23:16 | S2 | A high bit value will set the corresponding bit in ADI register 10. Read returns 0. | WO | 0x00
15:8 | S1 | A high bit value will set the corresponding bit in ADI register 9. Read returns 0. | WO | 0x00
7:0 | S0 | A high bit value will set the corresponding bit in ADI register 8. Read returns 0. | WO | 0x00

### TOP:ADI:SET1215

Address offset | 0x0000 001C
Physical address | 0x400C B01C | Instance | AUX_ADI4
Description | Set register for ADI byte offsets 12 to 15
Type | WO

Bits | Field Name | Description | Type | Reset
31:24 | S3 | A high bit value will set the corresponding bit in ADI register 15. Read returns 0. | WO | 0x00
23:16 | S2 | A high bit value will set the corresponding bit in ADI register 14. Read returns 0. | WO | 0x00
15:8 | S1 | A high bit value will set the corresponding bit in ADI register 13. Read returns 0. | WO | 0x00
7:0 | S0 | A high bit value will set the corresponding bit in ADI register 12. Read returns 0. | WO | 0x00

### TOP:ADI:CLR03

Address offset | 0x0000 0020
Physical address | 0x400C B020 | Instance | AUX_ADI4
Description | Clear register for ADI byte offsets 0 to 3
Type | WO

Bits | Field Name | Description | Type | Reset
31:24 | S3 | A high bit value will clear the corresponding bit in ADI register 3 | WO | 0x00
23:16 | S2 | A high bit value will clear the corresponding bit in ADI register 2 | WO | 0x00
15:8 | S1 | A high bit value will clear the corresponding bit in ADI register 1 | WO | 0x00
7:0 | S0 | A high bit value will clear the corresponding bit in ADI register 0 | WO | 0x00

### TOP:ADI:CLR47

Address offset | 0x0000 0024
Physical address | 0x400C B024 | Instance | AUX_ADI4
Description | Clear register for ADI byte offsets 4 to 7
Type | WO

Bits | Field Name | Description | Type | Reset
31:24 | S3 | A high bit value will clear the corresponding bit in ADI register 7 | WO | 0x00
23:16 | S2 | A high bit value will clear the corresponding bit in ADI register 6 | WO | 0x00
15:8 | S1 | A high bit value will clear the corresponding bit in ADI register 5 | WO | 0x00
7:0 | S0 | A high bit value will clear the corresponding bit in ADI register 4 | WO | 0x00

### TOP:ADI:CLR811

Address offset | 0x0000 0028
Physical address | 0x400C B028 | Instance | AUX_ADI4
Description | Clear register for ADI byte offsets 8 to 11
Type | WO

Bits | Field Name | Description | Type | Reset
31:24 | S3 | A high bit value will clear the corresponding bit in ADI register 11 | WO | 0x00
23:16 | S2 | A high bit value will clear the corresponding bit in ADI register 10 | WO | 0x00
15:8 | S1 | A high bit value will clear the corresponding bit in ADI register 9 | WO | 0x00
7:0 | S0 | A high bit value will clear the corresponding bit in ADI register 8 | WO | 0x00

### TOP:ADI:CLR1215

Address offset | 0x0000 002C
Physical address | 0x400C B02C | Instance | AUX_ADI4
Description | Clear register for ADI byte offsets 12 to 15
Type | WO

Bits | Field Name | Description | Type | Reset
31:24 | S3 | A high bit value will clear the corresponding bit in ADI register 15 | WO | 0x00
23:16 | S2 | A high bit value will clear the corresponding bit in ADI register 14 | WO | 0x00
15:8 | S1 | A high bit value will clear the corresponding bit in ADI register 13 | WO | 0x00
7:0 | S0 | A high bit value will clear the corresponding bit in ADI register 12 | WO | 0x00

### TOP:ADI:SLAVESTAT

Address offset | 0x0000 0030
Physical address | 0x400C B030 | Instance | AUX_ADI4
Description | ADI Slave status register
Type | RW

Bits | Field Name | Description | Type | Reset
31:2 | RESERVED2 | Software should not rely on the value of a reserved. Writing any other value than the reset value may result in undefined behavior. | RO | 0x0000 0000
1 | DI_REQ | Read current value of DI_REQ signal. Writing 0 to this bit forces a sync with slave, ensuring that req will be 0. It is recommended to write 0 to this register before power down of the master. | RW | 0
0 | DI_ACK | Read current value of DI_ACK signal | RO | 0

### TOP:ADI:SLAVECONF

Address offset | 0x0000 0038
Physical address | 0x400C B038 | Instance | AUX_ADI4
Description | ADI Master configuration register
Type | RW

Bits | Field Name | Description | Type | Reset
31:8 | RESERVED8 | Software should not rely on the value of a reserved. Writing any other value than the reset value may result in undefined behavior. | RO | 0x00 0000
7 | CONFLOCK | This register is no longer accessible when this bit is set. (unless sticky_bit_overwrite is asserted on top module) | RW | 0
6:3 | RESERVED3 | Software should not rely on the value of a reserved. Writing any other value than the reset value may result in undefined behavior. | RO | 0x0
2 | WAITFORACK | A transaction on the ADI interface does not end until ack has been received from the slave when this bit is set. | RW | 1
1:0 | ADICLKSPEED | Sets the period of an ADI transactions. ADI clock rising edge occurs in the middle of the period. Data and ctrl to slave is set up in beginning of cycle, and data from slave is read in after the transaction 00: One ADI transaction takes 2 master clock cycles 01: One ADI transaction takes 4 master clock cycles 10: One ADI Transaction takes 8 master clock cycles 11: One ADI transaction takes 16 master clock cycles | RW | 0x0

### TOP:ADI:MASK4B01

Address offset | 0x0000 0040
Physical address | 0x400C B040 | Instance | AUX_ADI4
Description | Masked access (4m/4d) for ADI Registers at byte offsets 0 and 1
Type | WO

Bits | Field Name | Description | Type | Reset
31:28 | M1H | Mask for bits [7:4] in ADI register 1 | WO | 0x0
27:24 | D1H | Data for bits [7:4] in ADI register 1, only bits selected by mask M1H will be affected by access | WO | 0x0
23:20 | M1L | Mask for bits [3:0] in ADI register 1 | WO | 0x0
19:16 | D1L | Data for bits [3:0] in ADI register 1, only bits selected by mask M1L will be affected by access | WO | 0x0
15:12 | M0H | Mask for bits [7:4] in ADI register 0 | WO | 0x0
11:8 | D0H | Data for bits [7:4] in ADI register 0, only bits selected by mask M0H will be affected by access | WO | 0x0
7:4 | M0L | Mask for bits [3:0] in ADI register 0 | WO | 0x0
3:0 | D0L | Data for bits [3:0] in ADI register 0, only bits selected by mask M0L will be affected by access | WO | 0x0

### TOP:ADI:MASK4B23

Address offset | 0x0000 0044
Physical address | 0x400C B044 | Instance | AUX_ADI4
Description | Masked access (4m/4d) for ADI Registers at byte offsets 2 and 3
Type | WO

Bits | Field Name | Description | Type | Reset
31:28 | M1H | Mask for bits [7:4] in ADI register 3 | WO | 0x0
27:24 | D1H | Data for bits [7:4] in ADI register 3, only bits selected by mask M1H will be affected by access | WO | 0x0
23:20 | M1L | Mask for bits [3:0] in ADI register 3 | WO | 0x0
19:16 | D1L | Data for bits [3:0] in ADI register 3, only bits selected by mask M1L will be affected by access | WO | 0x0
15:12 | M0H | Mask for bits [7:4] in ADI register 2 | WO | 0x0
11:8 | D0H | Data for bits [7:4] in ADI register 2, only bits selected by mask M0H will be affected by access | WO | 0x0
7:4 | M0L | Mask for bits [3:0] in ADI register 2 | WO | 0x0
3:0 | D0L | Data for bits [3:0] in ADI register 2, only bits selected by mask M0L will be affected by access | WO | 0x0

### TOP:ADI:MASK4B45

Address offset | 0x0000 0048
Physical address | 0x400C B048 | Instance | AUX_ADI4
Description | Masked access (4m/4d) for ADI Registers at byte offsets 4 and 5
Type | WO

Bits | Field Name | Description | Type | Reset
31:28 | M1H | Mask for bits [7:4] in ADI register 5 | WO | 0x0
27:24 | D1H | Data for bits [7:4] in ADI register 5, only bits selected by mask M1H will be affected by access | WO | 0x0
23:20 | M1L | Mask for bits [3:0] in ADI register 5 | WO | 0x0
19:16 | D1L | Data for bits [3:0] in ADI register 5, only bits selected by mask M1L will be affected by access | WO | 0x0
15:12 | M0H | Mask for bits [7:4] in ADI register 4 | WO | 0x0
11:8 | D0H | Data for bits [7:4] in ADI register 4, only bits selected by mask M0H will be affected by access | WO | 0x0
7:4 | M0L | Mask for bits [3:0] in ADI register 4 | WO | 0x0
3:0 | D0L | Data for bits [3:0] in ADI register 4, only bits selected by mask M0L will be affected by access | WO | 0x0

### TOP:ADI:MASK4B67

Address offset | 0x0000 004C
Physical address | 0x400C B04C | Instance | AUX_ADI4
Description | Masked access (4m/4d) for ADI Registers at byte offsets 6 and 7
Type | WO

Bits | Field Name | Description | Type | Reset
31:28 | M1H | Mask for bits [7:4] in ADI register 7 | WO | 0x0
27:24 | D1H | Data for bits [7:4] in ADI register 7, only bits selected by mask M1H will be affected by access | WO | 0x0
23:20 | M1L | Mask for bits [3:0] in ADI register 7 | WO | 0x0
19:16 | D1L | Data for bits [3:0] in ADI register 7, only bits selected by mask M1L will be affected by access | WO | 0x0
15:12 | M0H | Mask for bits [7:4] in ADI register 6 | WO | 0x0
11:8 | D0H | Data for bits [7:4] in ADI register 6, only bits selected by mask M0H will be affected by access | WO | 0x0
7:4 | M0L | Mask for bits [3:0] in ADI register 6 | WO | 0x0
3:0 | D0L | Data for bits [3:0] in ADI register 6, only bits selected by mask M0L will be affected by access | WO | 0x0

### TOP:ADI:MASK4B89

Address offset | 0x0000 0050
Physical address | 0x400C B050 | Instance | AUX_ADI4
Description | Masked access (4m/4d) for ADI Registers at byte offsets 8 and 9
Type | WO

Bits | Field Name | Description | Type | Reset
31:28 | M1H | Mask for bits [7:4] in ADI register 9 | WO | 0x0
27:24 | D1H | Data for bits [7:4] in ADI register 9, only bits selected by mask M1H will be affected by access | WO | 0x0
23:20 | M1L | Mask for bits [3:0] in ADI register 9 | WO | 0x0
19:16 | D1L | Data for bits [3:0] in ADI register 9, only bits selected by mask M1L will be affected by access | WO | 0x0
15:12 | M0H | Mask for bits [7:4] in ADI register 8 | WO | 0x0
11:8 | D0H | Data for bits [7:4] in ADI register 8, only bits selected by mask M0H will be affected by access | WO | 0x0
7:4 | M0L | Mask for bits [3:0] in ADI register 8 | WO | 0x0
3:0 | D0L | Data for bits [3:0] in ADI register 8, only bits selected by mask M0L will be affected by access | WO | 0x0

### TOP:ADI:MASK4B1011

Address offset | 0x0000 0054
Physical address | 0x400C B054 | Instance | AUX_ADI4
Description | Masked access (4m/4d) for ADI Registers at byte offsets 10 and 11
Type | WO

Bits | Field Name | Description | Type | Reset
31:28 | M1H | Mask for bits [7:4] in ADI register 11 | WO | 0x0
27:24 | D1H | Data for bits [7:4] in ADI register 11, only bits selected by mask M1H will be affected by access | WO | 0x0
23:20 | M1L | Mask for bits [3:0] in ADI register 11 | WO | 0x0
19:16 | D1L | Data for bits [3:0] in ADI register 11, only bits selected by mask M1L will be affected by access | WO | 0x0
15:12 | M0H | Mask for bits [7:4] in ADI register 10 | WO | 0x0
11:8 | D0H | Data for bits [7:4] in ADI register 10, only bits selected by mask M0H will be affected by access | WO | 0x0
7:4 | M0L | Mask for bits [3:0] in ADI register 10 | WO | 0x0
3:0 | D0L | Data for bits [3:0] in ADI register 10, only bits selected by mask M0L will be affected by access | WO | 0x0

### TOP:ADI:MASK4B1213

Address offset | 0x0000 0058
Physical address | 0x400C B058 | Instance | AUX_ADI4
Description | Masked access (4m/4d) for ADI Registers at byte offsets 12 and 13
Type | WO

Bits | Field Name | Description | Type | Reset
31:28 | M1H | Mask for bits [7:4] in ADI register 13 | WO | 0x0
27:24 | D1H | Data for bits [7:4] in ADI register 13, only bits selected by mask M1H will be affected by access | WO | 0x0
23:20 | M1L | Mask for bits [3:0] in ADI register 13 | WO | 0x0
19:16 | D1L | Data for bits [3:0] in ADI register 13, only bits selected by mask M1L will be affected by access | WO | 0x0
15:12 | M0H | Mask for bits [7:4] in ADI register 12 | WO | 0x0
11:8 | D0H | Data for bits [7:4] in ADI register 12, only bits selected by mask M0H will be affected by access | WO | 0x0
7:4 | M0L | Mask for bits [3:0] in ADI register 12 | WO | 0x0
3:0 | D0L | Data for bits [3:0] in ADI register 12, only bits selected by mask M0L will be affected by access | WO | 0x0

### TOP:ADI:MASK4B1415

Address offset | 0x0000 005C
Physical address | 0x400C B05C | Instance | AUX_ADI4
Description | Masked access (4m/4d) for ADI Registers at byte offsets 14 and 15
Type | WO

Bits | Field Name | Description | Type | Reset
31:28 | M1H | Mask for bits [7:4] in ADI register 15 | WO | 0x0
27:24 | D1H | Data for bits [7:4] in ADI register 15, only bits selected by mask M1H will be affected by access | WO | 0x0
23:20 | M1L | Mask for bits [3:0] in ADI register 15 | WO | 0x0
19:16 | D1L | Data for bits [3:0] in ADI register 15, only bits selected by mask M1L will be affected by access | WO | 0x0
15:12 | M0H | Mask for bits [7:4] in ADI register 14 | WO | 0x0
11:8 | D0H | Data for bits [7:4] in ADI register 14, only bits selected by mask M0H will be affected by access | WO | 0x0
7:4 | M0L | Mask for bits [3:0] in ADI register 14 | WO | 0x0
3:0 | D0L | Data for bits [3:0] in ADI register 14, only bits selected by mask M0L will be affected by access | WO | 0x0

### TOP:ADI:MASK8B01

Address offset | 0x0000 0060
Physical address | 0x400C B060 | Instance | AUX_ADI4
Description | Masked access (8m/8d) for ADI Registers at byte offsets 0 and 1
Type | WO

Bits | Field Name | Description | Type | Reset
31:24 | M1 | Mask for ADI register 1 | WO | 0x00
23:16 | D1 | Data for ADI register 1, only bits selected by mask M1 will be affected by access | WO | 0x00
15:8 | M0 | Mask for ADI register 0 | WO | 0x00
7:0 | D0 | Data for ADI register 0, only bits selected by mask M0 will be affected by access | WO | 0x00

### TOP:ADI:MASK8B23

Address offset | 0x0000 0064
Physical address | 0x400C B064 | Instance | AUX_ADI4
Description | Masked access (8m/8d) for ADI Registers at byte offsets 2 and 3
Type | WO

Bits | Field Name | Description | Type | Reset
31:24 | M1 | Mask for ADI register 3 | WO | 0x00
23:16 | D1 | Data for ADI register 3, only bits selected by mask M1 will be affected by access | WO | 0x00
15:8 | M0 | Mask for ADI register 2 | WO | 0x00
7:0 | D0 | Data for ADI register 2, only bits selected by mask M0 will be affected by access | WO | 0x00

### TOP:ADI:MASK8B45

Address offset | 0x0000 0068
Physical address | 0x400C B068 | Instance | AUX_ADI4
Description | Masked access (8m/8d) for ADI Registers at byte offsets 4 and 5
Type | WO

Bits | Field Name | Description | Type | Reset
31:24 | M1 | Mask for ADI register 5 | WO | 0x00
23:16 | D1 | Data for ADI register 5, only bits selected by mask M1 will be affected by access | WO | 0x00
15:8 | M0 | Mask for ADI register 4 | WO | 0x00
7:0 | D0 | Data for ADI register 4, only bits selected by mask M0 will be affected by access | WO | 0x00

### TOP:ADI:MASK8B67

Address offset | 0x0000 006C
Physical address | 0x400C B06C | Instance | AUX_ADI4
Description | Masked access (8m/8d) for ADI Registers at byte offsets 6 and 7
Type | WO

Bits | Field Name | Description | Type | Reset
31:24 | M1 | Mask for ADI register 7 | WO | 0x00
23:16 | D1 | Data for ADI register 7, only bits selected by mask M1 will be affected by access | WO | 0x00
15:8 | M0 | Mask for ADI register 6 | WO | 0x00
7:0 | D0 | Data for ADI register 6, only bits selected by mask M0 will be affected by access | WO | 0x00

### TOP:ADI:MASK8B89

Address offset | 0x0000 0070
Physical address | 0x400C B070 | Instance | AUX_ADI4
Description | Masked access (8m/8d) for ADI Registers at byte offsets 8 and 9
Type | WO

Bits | Field Name | Description | Type | Reset
31:24 | M1 | Mask for ADI register 9 | WO | 0x00
23:16 | D1 | Data for ADI register 9, only bits selected by mask M1 will be affected by access | WO | 0x00
15:8 | M0 | Mask for ADI register 8 | WO | 0x00
7:0 | D0 | Data for ADI register 8, only bits selected by mask M0 will be affected by access | WO | 0x00

### TOP:ADI:MASK8B1011

Address offset | 0x0000 0074
Physical address | 0x400C B074 | Instance | AUX_ADI4
Description | Masked access (8m/8d) for ADI Registers at byte offsets 10 and 11
Type | WO

Bits | Field Name | Description | Type | Reset
31:24 | M1 | Mask for ADI register 11 | WO | 0x00
23:16 | D1 | Data for ADI register 11, only bits selected by mask M1 will be affected by access | WO | 0x00
15:8 | M0 | Mask for ADI register 10 | WO | 0x00
7:0 | D0 | Data for ADI register 10, only bits selected by mask M0 will be affected by access | WO | 0x00

### TOP:ADI:MASK8B1213

Address offset | 0x0000 0078
Physical address | 0x400C B078 | Instance | AUX_ADI4
Description | Masked access (8m/8d) for ADI Registers at byte offsets 12 and 13
Type | WO

Bits | Field Name | Description | Type | Reset
31:24 | M1 | Mask for ADI register 13 | WO | 0x00
23:16 | D1 | Data for ADI register 13, only bits selected by mask M1 will be affected by access | WO | 0x00
15:8 | M0 | Mask for ADI register 12 | WO | 0x00
7:0 | D0 | Data for ADI register 12, only bits selected by mask M0 will be affected by access | WO | 0x00

### TOP:ADI:MASK8B1415

Address offset | 0x0000 007C
Physical address | 0x400C B07C | Instance | AUX_ADI4
Description | Masked access (8m/8d) for ADI Registers at byte offsets 14 and 15
Type | WO

Bits | Field Name | Description | Type | Reset
31:24 | M1 | Mask for ADI register 15 | WO | 0x00
23:16 | D1 | Data for ADI register 15, only bits selected by mask M1 will be affected by access | WO | 0x00
15:8 | M0 | Mask for ADI register 14 | WO | 0x00
7:0 | D0 | Data for ADI register 14, only bits selected by mask M0 will be affected by access | WO | 0x00

### TOP:ADI:MASK16B01

Address offset | 0x0000 0080
Physical address | 0x400C B080 | Instance | AUX_ADI4
Description | Masked access (16m/16d) for ADI Registers at byte offsets 0 and 1
Type | WO

Bits | Field Name | Description | Type | Reset
31:16 | M | Mask for ADI register 0 and 1 | WO | 0x0000
15:0 | D | Data for ADI register at offsets 0 and 1, only bits selected by mask M will be affected by access | WO | 0x0000

### TOP:ADI:MASK16B23

Address offset | 0x0000 0084
Physical address | 0x400C B084 | Instance | AUX_ADI4
Description | Masked access (16m/16d) for ADI Registers at byte offsets 2 and 3
Type | WO

Bits | Field Name | Description | Type | Reset
31:16 | M | Mask for ADI register 2 and 3 | WO | 0x0000
15:0 | D | Data for ADI register at offsets 2 and 3, only bits selected by mask M will be affected by access | WO | 0x0000

### TOP:ADI:MASK16B45

Address offset | 0x0000 0088
Physical address | 0x400C B088 | Instance | AUX_ADI4
Description | Masked access (16m/16d) for ADI Registers at byte offsets 4 and 5
Type | WO

Bits | Field Name | Description | Type | Reset
31:16 | M | Mask for ADI register 4 and 5 | WO | 0x0000
15:0 | D | Data for ADI register at offsets 4 and 5, only bits selected by mask M will be affected by access | WO | 0x0000

### TOP:ADI:MASK16B67

Address offset | 0x0000 008C
Physical address | 0x400C B08C | Instance | AUX_ADI4
Description | Masked access (16m/16d) for ADI Registers at byte offsets 6 and 7
Type | WO

Bits | Field Name | Description | Type | Reset
31:16 | M | Mask for ADI register 6 and 7 | WO | 0x0000
15:0 | D | Data for ADI register at offsets 6 and 7, only bits selected by mask M will be affected by access | WO | 0x0000

### TOP:ADI:MASK16B89

Address offset | 0x0000 0090
Physical address | 0x400C B090 | Instance | AUX_ADI4
Description | Masked access (16m/16d) for ADI Registers at byte offsets 8 and 9
Type | WO

Bits | Field Name | Description | Type | Reset
31:16 | M | Mask for ADI register 8 and 9 | WO | 0x0000
15:0 | D | Data for ADI register at offsets 8 and 9, only bits selected by mask M will be affected by access | WO | 0x0000

### TOP:ADI:MASK16B1011

Address offset | 0x0000 0094
Physical address | 0x400C B094 | Instance | AUX_ADI4
Description | Masked access (16m/16d) for ADI Registers at byte offsets 10 and 11
Type | WO

Bits | Field Name | Description | Type | Reset
31:16 | M | Mask for ADI register 10 and 11 | WO | 0x0000
15:0 | D | Data for ADI register at offsets 10 and 11, only bits selected by mask M will be affected by access | WO | 0x0000

### TOP:ADI:MASK16B1213

Address offset | 0x0000 0098
Physical address | 0x400C B098 | Instance | AUX_ADI4
Description | Masked access (16m/16d) for ADI Registers at byte offsets 12 and 13
Type | WO

Bits | Field Name | Description | Type | Reset
31:16 | M | Mask for ADI register 12 and 13 | WO | 0x0000
15:0 | D | Data for ADI register at offsets 12 and 13, only bits selected by mask M will be affected by access | WO | 0x0000

### TOP:ADI:MASK16B1415

Address offset | 0x0000 009C
Physical address | 0x400C B09C | Instance | AUX_ADI4
Description | Masked access (16m/16d) for ADI Registers at byte offsets 14 and 15
Type | WO

Bits | Field Name | Description | Type | Reset
31:16 | M | Mask for ADI register 14 and 15 | WO | 0x0000
15:0 | D | Data for ADI register at offsets 14 and 15, only bits selected by mask M will be affected by access | WO | 0x0000