XXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXxxxxxxxxxxxxX
X   	Artwork and documentation done by: 			            X
X								            X
X	TEXAS INSTRUMENTS NORWAY LPRF              		            X
X  								            X
X	Address: Hoffsveien 70C    0377 OSLO	              	            X
X 	web: http://www.ti.com/lsds/ti/wireless-connectivity/overview.page  x
X                                                           	            X
XXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXxxxxxxxxxxxx

PCB NAME : CC1352-P7EM-XD7793-XD24-PA24
REVISION: B0
DATE: 2020-10-09

FILE:  PACKED WITH 7Zip 

PCB DESCRIPTION:4 LAYER PCB 
Design Cross Section
TOP,CONDUCTOR,COPPER,0.035mm
DIELECTRIC,FR-4,0.175mm
L2,CONDUCTOR, COPPER,0.018mm
DIELECTRIC,FR-4,1.14mm
L3,CONDUCTOR,COPPER,0.018mm
DIELECTRIC,FR-4,0.175mm
BOTTOM,CONDUCTOR,COPPER,0.035mm

Total Thickness: 0.8mm (Tolerance +/- 0.08mm)

 
Via L1-L4

Soldermask color: GREEN

  IPC 4101/126 or equivalent substrate (Resin contents around 45%, which gives Er=4.4@2.4GHz, TanD=0.016)
  Dimensions in mm
  DOUBLE SIDE SOLDER MASK,
  DOUBLE SIDE SILKSCREEN,
  0.15 MM MIN TRACE WIDTH AND 0.15 MM MIN ISOLATION.

                 
FILE NAME            		DESCRIPTION                               	FILE TYPE
-------------------------------------------------------------------------------------------
***PCB MANUFACTURING FILES: (Folder Gerber)
Top.art                 	LAYER 1 TOP SIDE/POSITIV              		EXT. GERBER
L2.art				LAYER 2 SIDE/POSITIV				EXT. GERBER
L3.art				LAYER 3 SIDE/POSITIV				EXT. GERBER
Bottom.art                  	LAYER 4 SOLDER SIDE/POSITIV                 	EXT. GERBER
soldmask_top.art            	SOLDER MASK COMPONENT SIDE/NEGATIVE             EXT. GERBER
soldmask_bottom.art             SOLDER MASK SOLDER SIDE/NEGATIVE            	EXT. GERBER
silk_top.art	            	SILKSCREEN COMPONENT SIDE/POSITIVE              EXT. GERBER
silk_bottom.art		        SILKSCREEN SOLDER SIDE/POSITIVE             	EXT. GERBER
drill.art		        DRILL/MECHANICAL DRAWING                    	EXT. GERBER
art_param.txt                   Gerber report 				        ASCII
photoplot.log                   Gerber report					ASCII


***PCB DRILL FILES: (Folder Drill)
NCdrill-1-4.drl                 NC DRILL Plated		                       	EXCELLON
NCdrill-1-4-np.drl		NC DRILL non-Plated		 	        EXCELLON
ncdrill.log		        DRILL/NC DRILL REPORT                           ASCII
nc_pararm.txt		        PCB PHOTOPLOTTER DEFINITION FILE	        ASCII
nc_tools_auto.txt               Drill diameters				        ASCII


*** ASSEMBLY FILES: (Folder Assembly)
assembly_top.art	        ASSEMBLY DRAWING COMPONENT SIDE/NEGATIVE        EXT. GERBER
assembly_bot_mirror.art        	ASSEMBLY DRAWING SOLDER SIDE/NEGATIVE, MIRROR   EXT. GERBER
paste_top.art	             	SOLDER PAST COMPONENT SIDE/POSITIVE             EXT. GERBER
paste_bottom.art	        SOLDER PAST SOLDER SIDE/POSITIVE                EXT. GERBER
pick_and_place.txt            	PICK AND PLACE FILE 			        ASCII
CC1352-P7EM-XD7793-XD24-PA24_partlist.xls 	BOM						Excel


*** Document files: (Folder docs)
CC1352-P7EM-XD7793-XD24-PA24_schematic.pdf		Circuit Diagram			PDF
CC1352-P7EM-XD7793-XD24-PA24_layout.pdf      		Layout Diagram			PDF
CC1352-P7EM-XD7793-XD24-PA24_mechanical.pdf		Mechanical drawing		PDF
CC1352-P7EM-XD7793-XD24-PA24_assembly.pdf		Assembly drawing               	PDF


README.TXT           			THIS FILE                     	        ASCII


Revision history:

A.0
---------------------------------------------------------------------------------------------
- Based on CC1352PEM-XD7793-XD24-PA24 revision C1.
- Changed C1 from GRM188R60J226MEA0D to GRM188C80J226ME15D
- Changed C11,C15,C51,C81,C91 from GRM1555C1H120JA01D to GJM1555C1H120JB01D
- Changed C12,C21 from GRM1555C1H1R1BA01D to GJM1555C1H1R1BB01D
- Changed C13,C14 from GRM1555C1H1R0BA01D to GJM1555C1H1R0BB01D
- Changed C16,C32,C36 from GRM1555C1H101JA01D to GRT1555C1H101JA02D
- Changed C31,C53,C61 from GRM1555C1H1R2BA01D to GJM1555C1H1R2BB01D
- Changed C33,C41 from GRM1555C1H3R0CA01D to GJM1555C1H3R0CB01D
- Changed C34 from GRM1555C1H2R7CA01D to GJM1555C1H2R7CB01D
- Changed C35 from GRM1555C1H5R6CA01D to GJM1555C1H5R6CB01D
- Changed C52 from GRM155R71E103KA01D to GRM155R71H103MA88D
- Changed C54 from GRM1555C1HR80BA01D to GJM1555C1HR80BB01D
- Changed C55,C56 from GRM1555C1H1R6BA01D to GJM1555C1H1R6BB01D
- Changed C57 from GRM1555C1H6R8CA01D to GJM1555C1H6R8BB01D
- Changed C231 from GRM155R61E105KA12D to GRM155C81C105KE11D
- Changed C331,C341 from GRM188R60J226MEA0D to GRM188C80J226ME15D
- Changed C461,C471 from GRM1555C1H7R5CA01D to GJM1555C1H7R5CB01D
- Changed U1 from CC1352P1F3RGZR to CC1352P1F64TRGZE
- Changed Y1 from FC-135 32.7680KA-AG0 to TZ1166C
- Changed Y2 from NX2016SA 48.000MHz EXS00A-CS05517 to TZ2365C

B.0
---------------------------------------------------------------------------------------------
- Changed design name from CC1352P1F64EM-XD7793-XD24-PA24 to CC1352-P7EM-XD7793-XD24-PA24
- Updated CC1352P1F64TRGZE to CC1352P74T0RGZR