XXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXxxxxxxxxxxxxX
X   	Artwork and documentation done by: a0132638			            X
X								            X
X	TEXAS INSTRUMENTS NORWAY LPRF              		            X
X  								            X
X	Address: Hoffsveien 70C    0377 OSLO	              	            X
X 	web: http://www.ti.com/lsds/ti/wireless-connectivity/overview.page  x
X                                                           	            X
XXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXxxxxxxxxxxxx

PCB NAME : CC1352P1F64EM-XD7793-XD24-PA24_10dBm
REVISION: B0
DATE: 2020-11-24

FILE:  PACKED WITH WinZIP 

PCB DESCRIPTION:4 LAYER PCB 
Design Cross Section
TOP,CONDUCTOR,COPPER,0.035mm
DIELECTRIC,FR-4,0.175mm
L2,PLANE,COPPER,0.018mm
DIELECTRIC,FR-4,1.140000mm
L3,PLANE,COPPER,0.018mm
DIELECTRIC,FR-4,0.175mm
BOTTOM,CONDUCTOR,COPPER,0.035mm


Total Thickness: 1.60 MM (Tollerance +/- 0.16MM)
PCB description are measurements after PCB press

Via L1-L4

Soldermask color: GREEN

  IPC 4101/126 or equivalent substrate
  Dimensions in mm
  DOUBLE SIDE SOLDER MASK,
  DOUBLE SIDE SILKSCREEN,
  0.15 MM MIN TRACE WIDTH AND 0.15 MM MIN ISOLATION.
  Line widths should not be altered unless permission granted from TI

                 
FILE NAME            		DESCRIPTION                               	FILE TYPE
-------------------------------------------------------------------------------------------
***PCB MANUFACTURING FILES: (Folder Gerber)
Top.art                 	LAYER 1 TOP SIDE/POSITIV              		EXT. GERBER
Bottom.art                  	LAYER 4 SOLDER SIDE/POSITIV                 	EXT. GERBER
soldmask_top.art            	SOLDER MASK COMPONENT SIDE/NEGATIVE             EXT. GERBER
soldmask_bottom.art             SOLDER MASK SOLDER SIDE/NEGATIVE            	EXT. GERBER
silk_top.art	            	SILKSCREEN COMPONENT SIDE/POSITIVE              EXT. GERBER
silk_bottom.art		        SILKSCREEN SOLDER SIDE/POSITIVE             	EXT. GERBER
drill.art		        DRILL/MECHANICAL DRAWING                    	EXT. GERBER
art_param.txt                   Gerber report 				        ASCII
photoplot.log                   Gerber report					ASCII


***PCB DRILL FILES: (Folder Drill)
NCdrill-1-4.drl                 NC DRILL Plated		                       	EXCELLON
NCdrill-1-4-np.drl		NC DRILL non-Plated		 	        EXCELLON
ncdrill.log		        DRILL/NC DRILL REPORT                           ASCII
nc_pararm.txt		        PCB PHOTOPLOTTER DEFINITION FILE	        ASCII
nc_tools_auto.txt               Drill diameters				        ASCII


*** ASSEMBLY FILES: (Folder Assembly)
assembly_top.art	        ASSEMBLY DRAWING COMPONENT SIDE/NEGATIVE        EXT. GERBER
assembly_bot_mirror.art        	ASSEMBLY DRAWING SOLDER SIDE/NEGATIVE, MIRROR   EXT. GERBER
paste_top.art	             	SOLDER PAST COMPONENT SIDE/POSITIVE             EXT. GERBER
paste_bottom.art	        SOLDER PAST SOLDER SIDE/POSITIVE                EXT. GERBER
pick_and_place.txt            	PICK AND PLACE FILE 			        ASCII
CC1352PEM-XD7793-XD24-PA24_partlist.xls 	BOM					Excel


*** Document files: (Folder docs)
CC1352P1F64EM-XD7793-XD24-PA24_10dBm_schematic.pdf	Circuit Diagram			PDF
CC1352P1F64EM-XD7793-XD24-PA24_10dBm_layout.pdf      	Layout Diagram			PDF
CC1352P1F64EM-XD7793-XD24-PA24_10dBm_mechanical.pdf	Mechanical drawing		PDF
CC1352P1F64EM-XD7793-XD24-PA24_10dBm_assembly.pdf	Assembly drawing       		PDF


README.TXT           			THIS FILE                     	        ASCII


Revision history:
A0
--------------------------------------------------------------------------------------------
-Based on CC1352PM-XD7793-XD24-PA24_10dBm Rev: 1.0.0
- Changed C1 C331 C341 from GRM188R60J226MEA0D to GRM188C80J226ME15D
- Changed C11 C15 C51 C81 C91 from GRM1555C1H120JA01D to GJM1555C1H120JB01D
- Changed C12 C21 from GRM1555C1H1R1BA01D to GJM1555C1H1R1BB01D
- Changed C13 C14 from GRM1555C1H1R0BA01D to GJM1555C1H1R0BB01D
- Changed C31 C53 C54 C61 from GRM1555C1H1R2BA01D to GJM1555C1H1R2BB01D
- Changed C32 C36 from GRM1555C1H101JA01D to GRT1555C1H101JA02D
- Changed C33 C41 from GRM1555C1H3R0CA01D to GJM1555C1H3R0CB01D
- Changed C34 from GRM1555C1H2R7CA01D to GJM1555C1H2R7CB01D
- Changed C35 from GRM1555C1H5R6CA01D to GJM1555C1H5R6CB01D
- Changed C52 from GRM155R71E103KA01D to GRM155R71H103MA88D
- Changed C55 from GRM1555C1H1R4BA01D to GJM1555C1H1R4BB01
- Changed C56 from GRM1555C1H1R6BA01D to GJM1555C1H1R6BB01D
- Changed C57 from GRM1555C1H6R8CA01D to GJM1555C1H6R8BB01D
- Changed C231 from GRM155R61C105KA12D to GRM155C81C105KE15D
- Changed U1 from CC1352P1F3RGZR to CC1352P1F64TRGZE
- Changed Y1 from FC-135 32.7680KA-AG0 to TZ1166C
- Changed Y2 from NX2016SA 48.000MHz EXS00A-CS05517 to TZ2365C

B0
---------------------------------------------------------------------------------------------
- Changed design name to CC1352-P7EM-XD7793-XD24-PA24_10dBm

END.
