                                                                   June 30, 2011
 TEXAS INSTRUMENTS
   3535 40th Ave. NW, Suite 103
   ValleyHigh Business Center
   ROCHESTER, MN 55901


   Texas Instruments	
   PART NO. RF4CE_4MOD
   REV. C


 PCB DESCRIPTION: 2 LAYER PCB, .047" NOMINAL THICKNESS FR4 WITH 1OZ COPPER PER LAYER.

 This board has 2 plated thru slots - please see RF4CE_4MOD.GM3 for dimensioning.
  
 Please note this board requires a low resistance (10 ohm) carbon overlay (see RF4CE_4MOD.GM6).

 
  
 THIS ARCHIVED (WINZIP) FILE "RF4CE_4MOD RevC.ZIP" CONTAINS 25 FILES.

   RF4CE_4MOD.GTO = TOP SILKSCREEN GERBER FILE
   RF4CE_4MOD.GTS = TOP SOLDER MASK GERBER FILE
   RF4CE_4MOD.GTL = LAYER 1 TOP SIGNAL GERBER FILE
   RF4CE_4MOD.GBL = LAYER 2 BOTTOM SIGNAL GERBER FILE
   RF4CE_4MOD.GBS = BOTTOM SOLDER MASK GERBER FILE
   RF4CE_4MOD.GBO = BOTTOM SILKSCREEN GERBER FILE
   RF4CE_4MOD.GBP = BOTTOM SOLDER PASTE STENCIL GERBER FILE
   RF4CE_4MOD.GG1 = DRILL GUIDE GERBER FILE
   RF4CE_4MOD.GD1 = DRILL DRAWING GERBER FILE
   RF4CE_4MOD.GM4 = BOARD OUTLINE GERBER FILE
   RF4CE_4MOD.GM3 = FAB DIMENSION GERBER FILE (SLOT CALLOUT)
   RF4CE_4MOD.GM8 = BOARD PANELIZATION DIMENSION GERBER FILE
   RF4CE_4MOD.GM6 = CARBON OVERLAY GERBER FILE
   RF4CE_4MOD.DRR = DRILL SIZE REPORT
   RF4CE_4MOD.DRL = NC DRILL BINARY FILE
   RF4CE_4MOD.TXT = NC DRILL FILE
   RF4CE_4MOD.GM5 = BOTTOM ASSEMBLY DRAWING GERBER FILE
   RF4CE_4MOD.APR = APERTURE FILE
   RF4CE_4MOD ASCII.PCB = BOARD DESIGN IN PROTEL PCB V2.8 ASCII FORMAT
   RF4CE_4MOD.DDB = PROTEL DESIGN EXPLORER 99SE DESIGN DATABASE 
   RF4CE_4MOD BOM RevC.XLS = BILL OF MATERIALS
   PICK PLACE FOR RF4CE_4MOD.XLS = PICK AND PLACE SPREADSHEET
   RF4CE_4MOD Schematic RevC.pdf = SCHEMATIC PDF FILE
   RF4CE_4MOD Artwork RevC.pdf = BOARD ARTWORK PDF FILE
   README.TXT = THIS FILE


  

READ.ME
