Functions

# UsbIsr.h File Reference

For more information on this file please refer to Programmer’s Guide: MSP430 USB API Stack for CDC/HID http://focus.ti.com/docs/prod/folders/print/msp430f5529.html#toolssoftware. More...

Go to the source code of this file.

## Functions
BYTE | SetupPacketInterruptHandler (VOID)
VOID | PWRVBUSonHandler (VOID)
VOID | PWRVBUSoffHandler (VOID)
VOID | IEP0InterruptHandler (VOID)
VOID | OEP0InterruptHandler (VOID)

## Detailed Description

For more information on this file please refer to Programmer’s Guide: MSP430 USB API Stack for CDC/HID http://focus.ti.com/docs/prod/folders/print/msp430f5529.html#toolssoftware.

Author:
  Texas Instruments, Inc

Date:
  2009/06/11

Version:
  1.18 Initial Release

Note:
  Built with IAR Embedded Workbench for MSP430 Version: 5.10.1

Definition in file UsbIsr.h.

## Function Documentation

VOID IEP0InterruptHandler | ( | VOID |  | ) |

Handle In-requests from control pipe.

Definition at line 351 of file UsbIsr.c.

VOID OEP0InterruptHandler | ( | VOID |  | ) |

Handle Out-requests from control pipe.

Definition at line 367 of file UsbIsr.c.

VOID PWRVBUSoffHandler | ( | VOID |  | ) |

Handle VBuss off signal.

Definition at line 321 of file UsbIsr.c.

VOID PWRVBUSonHandler | ( | VOID |  | ) |

Handle VBuss on signal.

Definition at line 339 of file UsbIsr.c.

BYTE SetupPacketInterruptHandler | ( | VOID |  | ) |

Handle incoming setup packet. returns TRUE to keep CPU awake

Definition at line 280 of file UsbIsr.c.