Functions | Variables

# dma.c File Reference

For more information on this file please refer to Programmer’s Guide: MSP430 USB API Stack for CDC/HID http://focus.ti.com/docs/prod/folders/print/msp430f5529.html#toolssoftware. More...

`#include "MSP430.h"`
`#include "..\Common\types.h"`
`#include "..\USB_Common\defMSP430USB.h"`
`#include "..\USB_Common\descriptors.h"`
`#include <string.h>`

Go to the source code of this file.

## Functions
VOID * | memcpyDMA0 (VOID *dest, const VOID *source, size_t count)
VOID * | memcpyDMA1 (VOID *dest, const VOID *source, size_t count)
VOID * | memcpyDMA2 (VOID *dest, const VOID *source, size_t count)
VOID * | memcpyV (VOID *dest, const VOID *source, size_t count)
VOID | USB_initMemcpy (VOID)
## Variables
VOID *(* | USB_TX_memcpy )(VOID *dest, const VOID *source, size_t count)
VOID *(* | USB_RX_memcpy )(VOID *dest, const VOID *source, size_t count)

## Detailed Description

For more information on this file please refer to Programmer’s Guide: MSP430 USB API Stack for CDC/HID http://focus.ti.com/docs/prod/folders/print/msp430f5529.html#toolssoftware.

Author:
  Texas Instruments, Inc

Date:
  2009/06/11

Version:
  1.18 Initial Release

Note:
  Built with IAR Embedded Workbench for MSP430 Version: 5.10.1

Definition in file dma.c.