This demo requires the MSP430FR2355 EVM. Connect P5.3 to P3.5 and P5.2 to P3.1 on your Launchpad for evaluation.

To start, please plug the EVM board into your computer's USB port and close this README.md file.

The GUI should automatically connect with your EVM.  
* You can click the ![](images/disconnected.gif) button in the status bar at the bottom of the GUI to connect to the EVM.
* 
Once connected, clicking on the ![](images/connected.gif) button in the status bar will disconnect from the EVM.

To see this readme again once it has been closed, please select Help / View README.md