# Readme

## Example Summary

Toggles three GPIO pins using HW toggle register.

## Peripherals & Pin Assignments

Peripheral | Pin | Function
--- | --- | ---
GPIOA | PA27 | Standard Output
GPIOA | PA26 | Standard Output
GPIOA | PA13 | Standard Output
SYSCTL |  |
EVENT |  |
DEBUGSS | PA20 | Debug Clock
DEBUGSS | PA19 | Debug Data In Out

## BoosterPacks, Board Resources & Jumper Settings

Visit LP_MSPM0L1306 for LaunchPad information, including user guide and hardware files.

Pin | Peripheral | Function | LaunchPad Pin | LaunchPad Settings
--- | --- | --- | --- | ---
PA27 | GPIOA | PA27 | J4_37 | J13 ON/OFF: Connect/Disconnect LED2 Blue
PA26 | GPIOA | PA26 | J4_38 | J12 ON/OFF: Connect/Disconnect LED2 Red
PA13 | GPIOA | PA13 | J4_39 | J3 ON/OFF: Connect/Disconnect LED2 Green
PA20 | DEBUGSS | SWCLK | J2_13 | J101 15:16 ON: Connect to XDS-110 SWCLK (debug)
PA19 | DEBUGSS | SWDIO | J2_17 | J101 13:14 ON: Connect to XDS-110 SWDIO (debug)

### Low-Power Recommendations

TI recommends to terminate unused pins by setting the corresponding functions to GPIO and configure the pins to output low or input with internal pullup/pulldown resistor.

SysConfig allows developers to easily configure unused pins by selecting Board→Configure Unused Pins.

For more information about jumper configuration to achieve low-power using the MSPM0 LaunchPad, please visit the LP-MSPM0L1306 User’s Guide.

## Example Usage

Compile, load and run the example. RGB LEDs will toggle with red being opposite of blue and green.