ACMDOC CONTENT :

A829-PCB-001-1.cad		: Cadence allegro ASCII file to be used by CircuitCAM.
A829-PCB-001-1.ipc		: IPC356 netlist file, as alternative to A829-PCB-001-1.CAD 
art_param.txt					:	File telling sys setup for gerbers.
ASSY_BOT_DRAWING.art	:	Assambly drawing of Bottom layer in gerber. Not allways present.
ASSY_BOT_DRAWING.pdf	:	Assambly drawing of Bottom layer in PDF. Not allways present.
ASSY_TOP_DRAWING.art	:	Assambly drawing of Top layer in gerber.
ASSY_TOP_DRAWING.pdf	:	Assambly drawing of Top layer in PDF.
BMSK.art							:	Bottom Solder Mask in gerber.
BPST.art							:	Bottom Paste Mask in gerber.
BSLK.art							:	Bottom SiLK print in gerber. Not allways present.
comp_X-Y_list.htm			: HTM file telling position and rotation of components.
comp_X-Y_list.rpt			:	Same as above, but in RTF.
FAB1_DRAWING.art			:	Fabrication drawing of outline, drill and milling holes. In gerber.
FAB1_DRAWING.pdf			:	Fabrication drawing of outline, drill and milling holes. In pdf.
FAB2_DRAWING.art			: Same as above, number of files is depending on driffent number of drilling
FAB2_DRAWING.pdf			:		and / or milling.
Legend.txt						:	This file.
odbjob.tgz						:	Tarzipped files containing ODB++ files.
OUTLINE.art						:	Gerber of the board outline.
photoplot.log					:	Log file on every gerber file made.
TMSK.art							:	Top Solder Mask in gerber.
TPST.art							:	Top Paste Mask in gerber.
TSLK.art							:	Top SiLK print in gerber. Not allways present.

