Design Name C:/CADENCE_DESIGNS/PCB/TSW1418_E2/DESIGN_DATA/allegro/TSW1418_E2_7-13_NOON.brd
Date Fri Jul 13 12:04:41 2018
Drawing Statistics:
Drawing Extents XL(-9295.000) YL(-9759.000) XU(26705.000) YU(14241.000)
Dimensions in mils with 3 decimal places
Package Symbols: Total(267) Mirrored(92) Embedded(0) Pins(1494)
Mechanical Symbols: Total(3) Mirrored(3) Pins(0)
Format Symbols: Total(3)
DRC State: UP TO DATE
DRC Errors: 1
Short DRC: 0
Waived DRC: 5
Padstack Definitions: 403
Dynamic shapes: Total(48) Out_of_date(0)
Functions: Assigned(269) Unassigned(0) Total(269)

Connection Statistics:
Connections: W/Rats(959) No/Rats(0) Total(959)
Already Connected: W/Rats(959) No/Rats(0) Total(959)
Missing Connections: W/Rats(0) No/Rats(0) Total(0)
Dangling Connections (See logfile): 0
Connection Completion: W/Rats(100.00%) No/Rats(0.00%) Total(100.00%)
Manh Distance (inches): 315.226
Etch Length (inches): W/Rats(323.06) No/Rats(0.00) Total(323.06)
Number of Vias: W/Rats(1111) No/Rats(0) Total(1111)
Vias per Connection: W/Rats(1.16) No/Rats(0.00)Total(1.16)
SMD pins with attached clines: 840

Layout Statistics:
Components: Placed(257) Unplaced(0) Total(257)
Nets: W/Rats(216) No/Rats(0) Total(216)
Pins: W/Rats(1175) No/Rats(0) Unused(299) Unplaced(0) Total(1474)
Equivalent ICs (1 pin = 1/14 EIC): 105
RatTs: 0
Router Keepin (in): (0.0000,0.0000) by (0.0000,0.0000)
Layout area (sq in): 0.00
Average ratlength (in): 0.3
Rat density (in/sq in): 0.000
Double-sided rat density (in/sq in): 0.000

Layout/Pin Density Statistics
Layer | Layout Area (sq in) | Components | Pins | Layout Density (sq in/EIC) | Pin Density (pins/sq in)
External(Double-Sided) | 0.00 | 267 | 1494 | 0.000 | 0.000
Embedded(0) | 0.00 | 0 | 0 | 0.000 | 0.000
Design | 0.00 | 267 | 1494 | 0.000 | 0.000

Etch Layer Statistics:

Layer | Clines/Carcs | Shapes(voids) | Rectangles | Lines/Arcs | Text | Components(Pins)
TOP | 769 | 20(13) | 0 | 0 | 1 | 175(1317)
LY2-GND | 208 | 1(628) | 0 | 0 | 1 | 0(0)
LY3-SIGNAL | 39 | 1(48) | 0 | 0 | 1 | 0(0)
LY4-GND | 208 | 1(628) | 0 | 0 | 1 | 0(0)
LY5-SIGNAL | 84 | 1(6) | 0 | 0 | 1 | 0(0)
LY6-GND | 208 | 1(628) | 0 | 0 | 1 | 0(0)
LY7-PWR | 71 | 10(235) | 0 | 0 | 1 | 0(0)
LYR8-GND | 208 | 1(628) | 0 | 0 | 1 | 0(0)
LYR9-PWR | 56 | 6(799) | 0 | 0 | 1 | 0(0)
BOTTOM | 206 | 7(10) | 0 | 0 | 1 | 92(177)