Error Report for  - Users\a0864280\AppData\Local\Temp\QjzCCB1.tmp
4/9/2025 4:50:58 AM

Warning arcs were not exported.

Net FMC_C\S\_DUT_LVLS with allias 1 too long.
Net FMC_SCLK_DUT_LVLS with allias 2 too long.
Net FMC_SDO_DUT_LVLS with allias 3 too long.
Net FTDI_C\S\_DUT_LVLS with allias 4 too long.
Net FTDI_SCLK_DUT_LVLS with allias 5 too long.
Net FTDI_SCLK_SHIFT with allias 6 too long.
Net FTDI_SDIO_DUT_LVLS with allias 7 too long.
Warning pad shape change for U17-7 from  to rectangular 0.2mm,0.35mm
Warning pad shape change for U17-4 from  to rectangular 0.25mm,0.3mm
Warning pad shape change for U17-2 from  to rectangular 0.2mm,0.35mm
Warning pad shape change for U11-33 from  to rectangular 1.35mm,0.3mm
Warning pad shape change for U11-34 from  to rectangular 1.35mm,0.3mm
Warning pad shape change for U11-36 from  to rectangular 1.35mm,0.3mm
Warning pad shape change for U11-38 from  to rectangular 1.35mm,0.3mm
Warning pad shape change for U11-39 from  to rectangular 1.35mm,0.3mm
Warning pad shape change for U11-40 from  to rectangular 1.35mm,0.3mm
Warning pad shape change for U11-41 from  to rectangular 1.35mm,0.3mm
Warning pad shape change for U11-43 from  to rectangular 1.35mm,0.3mm
Warning pad shape change for U11-44 from  to rectangular 1.35mm,0.3mm
Warning pad shape change for U11-45 from  to rectangular 1.35mm,0.3mm
Warning pad shape change for U11-46 from  to rectangular 1.35mm,0.3mm
Warning pad shape change for U11-48 from  to rectangular 1.35mm,0.3mm
Warning pad shape change for U11-21 from  to rectangular 0.3mm,1.35mm
Warning pad shape change for U11-22 from  to rectangular 0.3mm,1.35mm
Warning pad shape change for U11-23 from  to rectangular 0.3mm,1.35mm
Warning pad shape change for U11-24 from  to rectangular 0.3mm,1.35mm
Warning pad shape change for U11-29 from  to rectangular 0.3mm,1.35mm
Warning pad shape change for U11-30 from  to rectangular 0.3mm,1.35mm
Warning pad shape change for U11-32 from  to rectangular 0.3mm,1.35mm
Warning pad shape change for U11-52 from  to rectangular 0.3mm,1.35mm
Warning pad shape change for U11-53 from  to rectangular 0.3mm,1.35mm
Warning pad shape change for U11-54 from  to rectangular 0.3mm,1.35mm
Warning pad shape change for U11-55 from  to rectangular 0.3mm,1.35mm
Warning pad shape change for U11-57 from  to rectangular 0.3mm,1.35mm
Warning pad shape change for U11-58 from  to rectangular 0.3mm,1.35mm
Warning pad shape change for U11-59 from  to rectangular 0.3mm,1.35mm
Warning pad shape change for U11-60 from  to rectangular 0.3mm,1.35mm
Warning pad shape change for J3-B5 from  to rectangular 0.3mm,0.85mm
Warning pad shape change for J3-A8 from  to rectangular 0.3mm,0.85mm
Warning pad shape change for J3-A5 from  to rectangular 0.3mm,0.85mm
Warning pad shape change for J3-B8 from  to rectangular 0.3mm,0.85mm
Warning pad shape change for R109-2 from  to rounded 1.1mm,1.1mm
Warning pad shape change for R109-1 from  to rounded 1.1mm,1.1mm
Warning pad shape change for R107-1 from  to rounded 1.1mm,1.1mm
Warning pad shape change for R107-2 from  to rounded 1.1mm,1.1mm
Warning pad shape change for R108-1 from  to rounded 1.1mm,1.1mm
Warning pad shape change for R108-2 from  to rounded 1.1mm,1.1mm
Warning pad shape change for U12-7 from  to rectangular 0.35mm,1.35mm
Warning pad shape change for U12-6 from  to rectangular 0.35mm,1.35mm
Warning pad shape change for U15-10 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for U15-11 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for U15-12 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for U4-4 from  to rectangular 0.45mm,0.25mm
Warning pad shape change for U22-8 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for U20-5 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U2-9 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U1-36 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for U1-15 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for U1-5 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for C21-2 from  to rounded 0.8mm,0.8mm
Warning pad shape change for FB2-2 from  to rounded 1.1mm,1.1mm
Warning pad shape change for U9-8 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for C73-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C74-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C75-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C92-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C89-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C90-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C91-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R151-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C93-2 from  to rounded 0.8mm,0.8mm
Warning pad shape change for FC1-3 from  to rounded 0.95mm,0.95mm
Warning pad shape change for U22-42 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for U22-31 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for U22-18 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for U22-7 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for U1-30 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for U1-21 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for C27-2 from  to rounded 0.8mm,0.8mm
Warning pad shape change for FB3-2 from  to rounded 1.1mm,1.1mm
Warning pad shape change for U9-4 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for C76-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C77-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U8-9 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U8-10 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for R27-1 from  to rounded 0.92mm,0.92mm
Warning pad shape change for C26-2 from  to rounded 1.1mm,1.1mm
Warning pad shape change for C46-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R70-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R28-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U16-5 from  to rectangular 0.3mm,0.37mm
Warning pad shape change for R61-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U23-5 from  to rectangular 0.3mm,0.37mm
Warning pad shape change for R148-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R110-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for FC1-1 from  to rounded 0.95mm,0.95mm
Warning pad shape change for U19-5 from  to rectangular 0.4mm,0.5mm
Warning pad shape change for U7-1 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U14-15 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for C81-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R122-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R120-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U18-5 from  to rounded 0.6mm,0.6mm
Warning pad shape change for R56-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R59-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R60-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R130-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U8-1 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U8-2 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U6-1 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U6-2 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for C19-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C18-2 from  to rounded 1.1mm,1.1mm
Warning pad shape change for C25-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C24-2 from  to rounded 1.1mm,1.1mm
Warning pad shape change for R16-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for FB1-2 from  to rounded 0.8mm,0.8mm
Warning pad shape change for C15-2 from  to rounded 1.1mm,1.1mm
Warning pad shape change for C14-2 from  to rounded 1.1mm,1.1mm
Warning pad shape change for R12-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R26-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U21-8 from  to rectangular 0.45mm,0.3mm
Warning pad shape change for C88-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C44-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C45-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U17-10 from  to rounded 0.3mm,0.3mm
Warning pad shape change for U11-42 from  to rectangular 1.35mm,0.3mm
Warning pad shape change for U11-20 from  to rectangular 0.3mm,1.35mm
Warning pad shape change for U11-31 from  to rectangular 0.3mm,1.35mm
Warning pad shape change for U11-50 from  to rectangular 0.3mm,1.35mm
Warning pad shape change for U11-56 from  to rectangular 0.3mm,1.35mm
Warning pad shape change for R41-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C47-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R15-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C17-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R24-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C55-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C23-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R51-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C29-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R131-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U20-4 from  to rounded 0.6mm,0.6mm
Warning pad shape change for C85-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U12-8 from  to rectangular 0.35mm,1.35mm
Warning pad shape change for U3-5 from  to rounded 0.4mm,0.4mm
Warning pad shape change for U3-4 from  to rounded 0.4mm,0.4mm
Warning pad shape change for U9-7 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U9-10 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U9-11 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U15-14 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for U13-8 from  to rounded 0.4mm,0.4mm
Warning pad shape change for U10-8 from  to rectangular 0.3mm,0.5mm
Warning pad shape change for U7-5 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U14-1 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U14-16 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U14-2 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U14-8 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for C38-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C40-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C36-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R48-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R34-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R47-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R52-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C37-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R35-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R37-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R38-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C39-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C41-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C30-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R49-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R53-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R54-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C7-2 from  to rounded 1.1mm,1.1mm
Warning pad shape change for R7-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R5-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R10-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U5-5 from  to rounded 0.6mm,0.6mm
Warning pad shape change for R33-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R32-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R73-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R9-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U3-7 from  to rounded 0.4mm,0.4mm
Warning pad shape change for R5-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for D3-1 from  to rounded 0.915mm,0.915mm
Warning pad shape change for U3-2 from  to rounded 0.4mm,0.4mm
Warning pad shape change for U4-18 from  to rounded 0.7mm,0.7mm
Warning pad shape change for U2-6 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U2-7 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U2-8 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for C3-2 from  to rounded 1.1mm,1.1mm
Warning pad shape change for C2-2 from  to rounded 1.1mm,1.1mm
Warning pad shape change for C6-2 from  to rounded 1.1mm,1.1mm
Warning pad shape change for R6-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R11-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C9-2 from  to rounded 1.1mm,1.1mm
Warning pad shape change for C10-2 from  to rounded 1.1mm,1.1mm
Warning pad shape change for U1-13 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for R85-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U1-12 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for R77-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U6-4 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for R15-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for Q2-1 from  to rounded 0.15mm,0.15mm
Warning pad shape change for U1-38 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for R89-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U1-39 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for R97-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U1-7 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for C54-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R66-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U1-6 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for C48-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R66-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for SW5-3 from  to rectangular 0.76mm,0.84mm
Warning pad shape change for SW5-4 from  to rectangular 0.76mm,0.84mm
Warning pad shape change for U1-4 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for C87-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C86-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R153-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U22-19 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for R155-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U22-20 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for R159-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U22-23 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for R157-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U22-22 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for R161-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U22-17 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for R163-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U22-16 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for R165-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U22-14 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for R169-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U22-2 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for R171-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U22-3 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for R175-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U22-6 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for R173-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U22-5 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for R177-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U22-9 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for R179-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U22-11 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for R181-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U22-12 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for R23-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R10-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R167-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U22-13 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for U17-8 from  to rectangular 0.2mm,0.35mm
Warning pad shape change for R127-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R99-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R152-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U22-30 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for R100-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R154-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U22-29 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for R158-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R102-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U22-26 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for R103-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R156-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U22-27 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for R104-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R160-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U22-32 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for R105-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R162-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U22-33 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for R106-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R164-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U22-35 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for R111-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R168-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U22-47 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for R123-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R170-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U22-46 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for R113-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R174-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U22-43 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for R114-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R172-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U22-44 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for R115-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R176-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U22-40 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for R116-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R178-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U22-38 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for R117-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R180-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U22-37 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for R98-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R166-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U22-36 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for R142-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U15-4 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for R60-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R139-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U13-4 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for R140-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U13-2 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for R143-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U15-1 from  to rectangular 0.2mm,0.5mm
Warning pad shape change for R59-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R146-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U23-1 from  to rectangular 0.3mm,0.37mm
Warning pad shape change for R147-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R144-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R61-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R149-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R62-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R148-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U15-8 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for U17-3 from  to rectangular 0.2mm,0.35mm
Warning pad shape change for U15-3 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for U14-13 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U11-17 from  to rectangular 0.3mm,1.35mm
Warning pad shape change for U14-4 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for R53-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U13-7 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U10-3 from  to rectangular 0.3mm,0.5mm
Warning pad shape change for R35-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U15-16 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for U14-14 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for R36-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U14-3 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for R52-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U11-19 from  to rectangular 0.3mm,1.35mm
Warning pad shape change for U14-6 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for R54-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R57-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U15-9 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for U14-12 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for R56-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R58-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U11-18 from  to rectangular 0.3mm,1.35mm
Warning pad shape change for U14-5 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U21-1 from  to rectangular 0.45mm,0.3mm
Warning pad shape change for R134-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U21-2 from  to rectangular 0.45mm,0.3mm
Warning pad shape change for R135-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R55-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C44-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C45-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U21-4 from  to rectangular 0.45mm,0.3mm
Warning pad shape change for U21-7 from  to rectangular 0.45mm,0.3mm
Warning pad shape change for U21-9 from  to rounded 1.36mm,1.36mm
Warning pad shape change for U17-5 from  to rounded 0.3mm,0.3mm
Warning pad shape change for U17-6 from  to rectangular 0.25mm,0.3mm
Warning pad shape change for U1-40 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for U1-37 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for U1-26 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for U1-14 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for U1-11 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for U1-3 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for U11-47 from  to rectangular 1.35mm,0.3mm
Warning pad shape change for U11-51 from  to rectangular 0.3mm,1.35mm
Warning pad shape change for U11-35 from  to rectangular 1.35mm,0.3mm
Warning pad shape change for U11-25 from  to rectangular 0.3mm,1.35mm
Warning pad shape change for U11-1 from  to rectangular 1.35mm,0.3mm
Warning pad shape change for U11-5 from  to rectangular 1.35mm,0.3mm
Warning pad shape change for U11-11 from  to rectangular 1.35mm,0.3mm
Warning pad shape change for U11-10 from  to rectangular 1.35mm,0.3mm
Warning pad shape change for U11-13 from  to rectangular 1.35mm,0.3mm
Warning pad shape change for U11-15 from  to rectangular 1.35mm,0.3mm
Warning pad shape change for SW4-2 from  to rounded 1.6mm,1.6mm
Warning pad shape change for J3-A1 from  to rounded 0.6mm,0.6mm
Warning pad shape change for J3-B1 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U8-6 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U8-11 from  to rectangular 1.65mm,1.75mm
Warning pad shape change for T3-2 from  to rounded 1.651mm,1.651mm
Warning pad shape change for T3-3 from  to rounded 1.651mm,1.651mm
Warning pad shape change for T1-5 from  to rounded 1.651mm,1.651mm
Warning pad shape change for T1-1 from  to rounded 1.651mm,1.651mm
Warning pad shape change for C26-1 from  to rounded 1.1mm,1.1mm
Warning pad shape change for C27-1 from  to rounded 0.8mm,0.8mm
Warning pad shape change for C92-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C84-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C88-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R134-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R150-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R136-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R135-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R145-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C31-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C32-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C34-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C33-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C42-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C43-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C47-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C46-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C61-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C60-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C68-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C69-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C50-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C51-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R71-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R72-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for T2-2 from  to rounded 1.651mm,1.651mm
Warning pad shape change for T2-3 from  to rounded 1.651mm,1.651mm
Warning pad shape change for U6-6 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U6-11 from  to rectangular 1.65mm,1.75mm
Warning pad shape change for C19-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C18-1 from  to rounded 1.1mm,1.1mm
Warning pad shape change for R22-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C20-1 from  to rounded 1.1mm,1.1mm
Warning pad shape change for R20-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C17-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C21-1 from  to rounded 0.8mm,0.8mm
Warning pad shape change for C25-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C24-1 from  to rounded 1.1mm,1.1mm
Warning pad shape change for C55-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R31-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R29-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C23-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C89-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C90-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C91-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R182-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C93-1 from  to rounded 0.8mm,0.8mm
Warning pad shape change for U16-3 from  to rectangular 0.3mm,0.37mm
Warning pad shape change for U16-2 from  to rectangular 0.3mm,0.37mm
Warning pad shape change for C29-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U23-2 from  to rectangular 0.3mm,0.37mm
Warning pad shape change for U23-3 from  to rectangular 0.3mm,0.37mm
Warning pad shape change for R62-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R147-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U20-2 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U20-1 from  to rounded 0.6mm,0.6mm
Warning pad shape change for C85-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R101-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for Q3-2 from  to rounded 0.15mm,0.15mm
Warning pad shape change for U12-5 from  to rectangular 0.35mm,1.35mm
Warning pad shape change for D3-2 from  to rounded 0.915mm,0.915mm
Warning pad shape change for U3-9 from  to rounded 1.1mm,1.1mm
Warning pad shape change for U3-3 from  to rounded 0.4mm,0.4mm
Warning pad shape change for U9-2 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U9-3 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U9-6 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U9-15 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U9-16 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U15-13 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for U15-6 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for U4-5 from  to rectangular 0.45mm,0.25mm
Warning pad shape change for U4-3 from  to rectangular 0.45mm,0.25mm
Warning pad shape change for U4-16 from  to rectangular 0.45mm,0.25mm
Warning pad shape change for U4-17 from  to rectangular 0.45mm,0.25mm
Warning pad shape change for U4-8 from  to rectangular 0.25mm,0.45mm
Warning pad shape change for U4-9 from  to rectangular 0.25mm,0.45mm
Warning pad shape change for U4-20 from  to rectangular 0.25mm,0.45mm
Warning pad shape change for U4-26 from  to rounded 1.15mm,1.15mm
Warning pad shape change for U4-6 from  to rounded 0.7mm,0.7mm
Warning pad shape change for U4-2 from  to rounded 0.7mm,0.7mm
Warning pad shape change for Q1-4 from  to rounded 0.3mm,0.3mm
Warning pad shape change for Q1-7 from  to rectangular 0.45mm,0.3mm
Warning pad shape change for U13-3 from  to rounded 0.4mm,0.4mm
Warning pad shape change for U22-45 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for U22-39 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for U22-34 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for U22-28 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for U22-21 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for U22-15 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for U22-10 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for U22-4 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for U10-5 from  to rectangular 0.3mm,0.5mm
Warning pad shape change for U10-4 from  to rectangular 0.3mm,0.5mm
Warning pad shape change for U10-2 from  to rectangular 0.3mm,0.5mm
Warning pad shape change for U19-3 from  to rectangular 0.4mm,0.5mm
Warning pad shape change for U7-2 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U14-7 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U14-10 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U14-9 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U14-17 from  to rounded 1mm,1mm
Warning pad shape change for C38-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C40-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C36-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C37-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R46-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C39-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C41-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C35-1 from  to rounded 0.8mm,0.8mm
Warning pad shape change for C30-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R45-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C81-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U18-2 from  to rounded 0.6mm,0.6mm
Warning pad shape change for C80-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R58-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U2-11 from  to rectangular 1.65mm,1.75mm
Warning pad shape change for R3-1 from  to rounded 1.1mm,1.1mm
Warning pad shape change for R8-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C7-1 from  to rounded 1.1mm,1.1mm
Warning pad shape change for C8-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C4-1 from  to rounded 0.8mm,0.8mm
Warning pad shape change for C3-1 from  to rounded 1.1mm,1.1mm
Warning pad shape change for R2-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C5-1 from  to rounded 0.8mm,0.8mm
Warning pad shape change for R4-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C2-1 from  to rounded 1.1mm,1.1mm
Warning pad shape change for C6-1 from  to rounded 1.1mm,1.1mm
Warning pad shape change for R13-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C12-1 from  to rounded 1.1mm,1.1mm
Warning pad shape change for C13-1 from  to rounded 1.1mm,1.1mm
Warning pad shape change for C15-1 from  to rounded 1.1mm,1.1mm
Warning pad shape change for C9-1 from  to rounded 1.1mm,1.1mm
Warning pad shape change for C10-1 from  to rounded 1.1mm,1.1mm
Warning pad shape change for R14-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C14-1 from  to rounded 1.1mm,1.1mm
Warning pad shape change for C11-1 from  to rounded 1.1mm,1.1mm
Warning pad shape change for C16-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C73-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C74-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C75-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C76-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C77-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C78-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C79-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C87-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C86-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C82-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C83-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R133-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R132-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U5-2 from  to rounded 0.6mm,0.6mm
Warning pad shape change for Q2-2 from  to rounded 0.15mm,0.15mm
Warning pad shape change for R124-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U8-4 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for R24-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for Q3-1 from  to rounded 0.15mm,0.15mm
Warning pad shape change for U19-1 from  to rectangular 0.4mm,0.5mm
Warning pad shape change for U9-9 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U5-4 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U9-5 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U7-4 from  to rounded 0.6mm,0.6mm
Warning pad shape change for D2-2 from  to rounded 2.159mm,2.159mm
Warning pad shape change for Q1-3 from  to rounded 0.3mm,0.3mm
Warning pad shape change for C1-1 from  to rounded 1.1mm,1.1mm
Warning pad shape change for D2-1 from  to rounded 2.159mm,2.159mm
Warning pad shape change for Q1-1 from  to rounded 0.3mm,0.3mm
Warning pad shape change for Q1-2 from  to rounded 0.3mm,0.3mm
Warning pad shape change for Q1-5 from  to rounded 0.3mm,0.3mm
Warning pad shape change for Q1-6 from  to rounded 0.3mm,0.3mm
Warning pad shape change for Q1-8 from  to rounded 0.95mm,0.95mm
Warning pad shape change for C1-2 from  to rounded 1.1mm,1.1mm
Warning pad shape change for U2-2 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for C4-2 from  to rounded 0.8mm,0.8mm
Warning pad shape change for R1-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R4-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U2-1 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for C5-2 from  to rounded 0.8mm,0.8mm
Warning pad shape change for U3-8 from  to rounded 0.4mm,0.4mm
Warning pad shape change for C8-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U4-15 from  to rectangular 0.45mm,0.25mm
Warning pad shape change for U4-10 from  to rectangular 0.25mm,0.45mm
Warning pad shape change for U4-11 from  to rectangular 0.25mm,0.45mm
Warning pad shape change for U4-12 from  to rectangular 0.25mm,0.45mm
Warning pad shape change for U4-27 from  to rounded 1.15mm,1.15mm
Warning pad shape change for U4-14 from  to rounded 0.7mm,0.7mm
Warning pad shape change for U4-13 from  to rounded 0.925mm,0.925mm
Warning pad shape change for FB1-1 from  to rounded 0.8mm,0.8mm
Warning pad shape change for C12-2 from  to rounded 1.1mm,1.1mm
Warning pad shape change for C13-2 from  to rounded 1.1mm,1.1mm
Warning pad shape change for C11-2 from  to rounded 1.1mm,1.1mm
Warning pad shape change for U4-21 from  to rectangular 0.25mm,0.45mm
Warning pad shape change for C16-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U6-9 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U6-10 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for R19-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C20-2 from  to rounded 1.1mm,1.1mm
Warning pad shape change for R17-1 from  to rounded 0.92mm,0.92mm
Warning pad shape change for U5-1 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U6-7 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U8-7 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U11-9 from  to rectangular 1.35mm,0.3mm
Warning pad shape change for C31-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C32-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U11-4 from  to rectangular 1.35mm,0.3mm
Warning pad shape change for C34-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C33-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for Y1-1 from  to rounded 1.9mm,1.9mm
Warning pad shape change for U11-2 from  to rectangular 1.35mm,0.3mm
Warning pad shape change for C42-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for Y1-2 from  to rounded 1.9mm,1.9mm
Warning pad shape change for U11-3 from  to rectangular 1.35mm,0.3mm
Warning pad shape change for C43-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C48-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C49-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R63-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R65-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for T1-6 from  to rounded 1.651mm,1.651mm
Warning pad shape change for C49-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for T1-2 from  to rounded 1.651mm,1.651mm
Warning pad shape change for C50-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C51-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R65-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R67-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for T1-3 from  to rounded 1.651mm,1.651mm
Warning pad shape change for C52-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C53-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C54-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R67-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R69-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for T1-4 from  to rounded 1.651mm,1.651mm
Warning pad shape change for C53-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U17-1 from  to rectangular 0.25mm,0.3mm
Warning pad shape change for C56-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R70-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R72-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C56-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R71-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C57-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C58-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C57-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R74-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C58-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for T2-1 from  to rounded 1.651mm,1.651mm
Warning pad shape change for C59-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for T2-6 from  to rounded 1.651mm,1.651mm
Warning pad shape change for C59-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R74-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R75-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C60-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for T2-5 from  to rounded 1.651mm,1.651mm
Warning pad shape change for C62-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for L2-1 from  to rounded 0.55mm,0.55mm
Warning pad shape change for R83-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R84-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C62-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for L1-1 from  to rounded 0.55mm,0.55mm
Warning pad shape change for R75-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R76-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C63-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R82-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R83-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C63-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for T2-4 from  to rounded 1.651mm,1.651mm
Warning pad shape change for C64-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C64-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R82-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C65-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C66-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C65-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R86-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for T3-1 from  to rounded 1.651mm,1.651mm
Warning pad shape change for C66-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for T3-6 from  to rounded 1.651mm,1.651mm
Warning pad shape change for C67-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C67-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R86-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R87-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for T3-5 from  to rounded 1.651mm,1.651mm
Warning pad shape change for C69-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for L4-1 from  to rounded 0.55mm,0.55mm
Warning pad shape change for C70-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R95-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R96-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C70-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for L3-1 from  to rounded 0.55mm,0.55mm
Warning pad shape change for R87-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R88-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C71-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R94-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R95-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for T3-4 from  to rounded 1.651mm,1.651mm
Warning pad shape change for C71-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C72-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C72-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R94-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R3-2 from  to rounded 1.1mm,1.1mm
Warning pad shape change for R18-2 from  to rounded 1.1mm,1.1mm
Warning pad shape change for R25-2 from  to rounded 1.1mm,1.1mm
Warning pad shape change for R45-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U6-8 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for R17-2 from  to rounded 0.92mm,0.92mm
Warning pad shape change for FB2-1 from  to rounded 1.1mm,1.1mm
Warning pad shape change for U5-3 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U8-8 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for R27-2 from  to rounded 0.92mm,0.92mm
Warning pad shape change for FB3-1 from  to rounded 1.1mm,1.1mm
Warning pad shape change for U7-3 from  to rounded 0.6mm,0.6mm
Warning pad shape change for R145-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R141-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R142-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R143-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R144-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R146-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for J3-A4 from  to rounded 0.6mm,0.6mm
Warning pad shape change for J3-B4 from  to rounded 0.6mm,0.6mm
Warning pad shape change for R42-1 from  to rounded 1.1mm,1.1mm
Warning pad shape change for J3-A6 from  to rectangular 0.3mm,0.85mm
Warning pad shape change for J3-B6 from  to rectangular 0.3mm,0.85mm
Warning pad shape change for R44-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for J3-B7 from  to rectangular 0.3mm,0.85mm
Warning pad shape change for J3-A7 from  to rectangular 0.3mm,0.85mm
Warning pad shape change for R43-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R101-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R118-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R110-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U20-6 from  to rounded 0.6mm,0.6mm
Warning pad shape change for L1-2 from  to rounded 0.55mm,0.55mm
Warning pad shape change for R78-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for L2-2 from  to rounded 0.55mm,0.55mm
Warning pad shape change for R81-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for L3-2 from  to rounded 0.55mm,0.55mm
Warning pad shape change for R90-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for L4-2 from  to rounded 0.55mm,0.55mm
Warning pad shape change for R93-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for Q2-3 from  to rectangular 0.15mm,0.35mm
Warning pad shape change for R18-1 from  to rounded 1.1mm,1.1mm
Warning pad shape change for Q3-3 from  to rectangular 0.15mm,0.35mm
Warning pad shape change for R25-1 from  to rounded 1.1mm,1.1mm
Warning pad shape change for U2-3 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U2-4 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U2-5 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for R1-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U2-10 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for R2-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U3-1 from  to rounded 0.4mm,0.4mm
Warning pad shape change for R6-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U3-6 from  to rounded 0.4mm,0.4mm
Warning pad shape change for R8-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R7-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R9-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U4-24 from  to rectangular 0.25mm,0.45mm
Warning pad shape change for R11-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U4-22 from  to rectangular 0.25mm,0.45mm
Warning pad shape change for R14-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R12-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U4-23 from  to rectangular 0.25mm,0.45mm
Warning pad shape change for R13-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U8-3 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U6-3 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for R23-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R16-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R26-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U6-5 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for R19-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R20-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R22-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U8-5 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for R28-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R29-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R31-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U9-12 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for R32-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U9-1 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for R33-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U11-16 from  to rectangular 1.35mm,0.3mm
Warning pad shape change for R36-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U11-26 from  to rectangular 0.3mm,1.35mm
Warning pad shape change for R39-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U10-6 from  to rectangular 0.3mm,0.5mm
Warning pad shape change for R40-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U11-14 from  to rectangular 1.35mm,0.3mm
Warning pad shape change for R41-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U11-7 from  to rectangular 1.35mm,0.3mm
Warning pad shape change for R43-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U11-8 from  to rectangular 1.35mm,0.3mm
Warning pad shape change for R44-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U11-6 from  to rectangular 1.35mm,0.3mm
Warning pad shape change for R46-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U11-62 from  to rectangular 0.3mm,1.35mm
Warning pad shape change for U12-2 from  to rectangular 0.35mm,1.35mm
Warning pad shape change for R47-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U12-4 from  to rectangular 0.35mm,1.35mm
Warning pad shape change for R48-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R50-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U11-63 from  to rectangular 0.3mm,1.35mm
Warning pad shape change for U12-1 from  to rectangular 0.35mm,1.35mm
Warning pad shape change for R49-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U11-61 from  to rectangular 0.3mm,1.35mm
Warning pad shape change for U12-3 from  to rectangular 0.35mm,1.35mm
Warning pad shape change for R50-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R51-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R55-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U16-1 from  to rectangular 0.3mm,0.37mm
Warning pad shape change for U14-11 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U16-4 from  to rectangular 0.3mm,0.37mm
Warning pad shape change for R57-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R63-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R64-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R68-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R69-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R73-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R76-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R77-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R78-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R79-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R80-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R81-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R84-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R85-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R88-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R89-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R90-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R91-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R92-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R93-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R96-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R97-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U1-25 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for R98-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U1-17 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for R99-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U1-18 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for R100-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U1-19 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for R102-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U1-20 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for R103-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U1-22 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for R104-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U1-23 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for R105-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U1-24 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for R106-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U1-34 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for R111-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U1-33 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for R112-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R127-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R123-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R112-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U1-32 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for R113-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U1-31 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for R114-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U1-29 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for R115-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U1-28 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for R116-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U1-27 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for R117-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U1-1 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for R118-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U1-9 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for R119-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R121-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U18-1 from  to rounded 0.6mm,0.6mm
Warning pad shape change for SW4-1 from  to rounded 1.6mm,1.6mm
Warning pad shape change for U19-2 from  to rectangular 0.4mm,0.5mm
Warning pad shape change for R122-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U1-35 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for R125-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U1-10 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for R126-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R128-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U18-3 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U1-16 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for R129-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for SW5-1 from  to rectangular 0.76mm,0.84mm
Warning pad shape change for R130-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R131-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U20-3 from  to rounded 0.6mm,0.6mm
Warning pad shape change for SW5-2 from  to rectangular 0.76mm,0.84mm
Warning pad shape change for R133-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U21-3 from  to rectangular 0.45mm,0.3mm
Warning pad shape change for R136-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U23-4 from  to rectangular 0.3mm,0.37mm
Warning pad shape change for R149-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R151-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R182-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U22-48 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for U22-41 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for U22-25 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for U22-24 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for U22-1 from  to rectangular 1.2mm,0.3mm
Warning pad shape change for R152-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R153-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R154-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R155-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R156-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R157-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R158-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R159-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R160-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R161-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R162-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R163-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R164-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R165-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R166-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R167-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R168-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R169-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R170-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R171-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R172-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R173-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R174-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R175-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R176-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R177-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R178-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R179-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R180-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R181-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U15-15 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for U13-5 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U13-1 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U17-9 from  to rectangular 0.25mm,0.3mm
Warning pad shape change for U19-4 from  to rectangular 0.4mm,0.5mm
Warning pad shape change for U18-4 from  to rounded 0.6mm,0.6mm
Warning pad shape change for R141-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R137-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R137-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R150-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R128-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R120-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R121-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C80-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R119-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R124-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U21-6 from  to rectangular 0.45mm,0.3mm
Warning pad shape change for U9-14 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U13-6 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for R139-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R125-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U15-2 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for U21-5 from  to rectangular 0.45mm,0.3mm
Warning pad shape change for U9-13 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U13-10 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for R140-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U15-7 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for R126-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R129-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U15-5 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for C52-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R68-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R64-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R138-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R138-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R42-2 from  to rounded 1.1mm,1.1mm
Warning pad shape change for U10-7 from  to rectangular 0.3mm,0.5mm
Warning pad shape change for R39-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R34-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U11-28 from  to rectangular 0.3mm,1.35mm
Warning pad shape change for U13-9 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for R38-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for R40-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U11-27 from  to rectangular 0.3mm,1.35mm
Warning pad shape change for U10-1 from  to rectangular 0.3mm,0.5mm
Warning pad shape change for R37-1 from  to rounded 0.5mm,0.5mm
Warning pad shape change for U1-8 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for C61-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C68-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R79-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R80-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R91-1 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R92-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C78-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C79-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for U11-64 from  to rectangular 0.3mm,1.35mm
Warning pad shape change for U11-49 from  to rectangular 0.3mm,1.35mm
Warning pad shape change for U11-37 from  to rectangular 1.35mm,0.3mm
Warning pad shape change for U11-12 from  to rectangular 1.35mm,0.3mm
Warning pad shape change for C35-2 from  to rounded 0.8mm,0.8mm
Warning pad shape change for U1-2 from  to rectangular 0.2mm,0.4mm
Warning pad shape change for C84-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for C82-2 from  to rounded 0.5mm,0.5mm
Warning pad shape change for C83-2 from  to rounded 0.32mm,0.32mm
Warning pad shape change for R132-2 from  to rounded 0.32mm,0.32mm
