UNITS=INCH
#
#Component attribute names
#
@0 .comp_mount_type
@1 .comp_height
@2 .no_pop
@3 .comp_ignore
@4 .comp_variant_list

#
#Component attribute text strings
#

# CMP 0
CMP 7 0.9664828 1.0359905 270 N C93 GRM188R61E106KA73J ;0=1,1=0.0394
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet '-'
PRP Manufacturer 'Murata'
PRP Operating_Temperature '-55°C ~ 85°C'
PRP PackageReference '0603'
PRP PartNumber 'GRM188R61E106KA73J'
PRP Ratings '-'
PRP Series '-'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-key'
PRP Supplier_Part_Number_1 '490-GRM188R61E106KA73JCT-ND'
PRP Temperature_Coefficient 'X5R'
PRP Tolerance '±10%'
PRP UniqueID 'capcc09400'
PRP Value '10 uF'
PRP Voltage_-_Rated '25V'
TOP 0 0.9664828 1.0084314 0 N 248 332 1
TOP 1 0.9664828 1.0635495 0 N 33 7 2
#
# CMP 1
CMP 26 1.0640493 2.4198001 0 N U23 SN74LVC1G125DRL ;0=1,1=0.0236
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color '-'
PRP CompType 'Buffer'
PRP Current_Rating_(Amps) '-'
PRP datasheet '-'
PRP Length_(in) '-'
PRP Manufacturer 'Texas Instruments'
PRP Mount_Type 'SMD'
PRP PackageReference 'SOT-5'
PRP PartNumber 'SN74LVC1G125DRL'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Supplier_1 'Digi-Key'
PRP Text1 '-'
PRP UniqueID 'SN74LVC1G125DRL'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 1.0931832 2.4394852 270 N 199 1 1
TOP 1 1.0931832 2.4198002 270 N 248 328 2
TOP 2 1.0931832 2.4001151 270 N 248 327 3
TOP 3 1.0349154 2.4001151 270 N 4 1 4
TOP 4 1.0349154 2.4394852 270 N 170 18 5
#
# CMP 2
CMP 2 1.0546004 2.290745 180 N R62 ERA-2AEB103X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thin Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDM0000/AOA0000C307.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERA-2AEB103X'
PRP Power_(Watts) '0.063W, 1/16W'
PRP Ratings 'AEC-Q200'
PRP Resistance '10 kO'
PRP Series 'ERA-2A'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P10KDCCT-ND'
PRP Temperature_Coefficient '±25ppm/°C'
PRP Tolerance '±0.1%'
PRP UniqueID 'RSMD040200315'
PRP Value '10 kO'
TOP 0 1.0349154 2.290745 90 N 198 2 1
TOP 1 1.0742855 2.290745 90 N 248 326 2
#
# CMP 3
CMP 2 1.0349154 2.3454301 90 N R149 ERJ-2RKF1000X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1000X'
PRP Power_(Watts) '0.1W, 1/10W'
PRP Ratings 'AEC-Q200'
PRP Resistance '100 O'
PRP Series 'ERJ-2RK'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P100LCT-ND'
PRP Temperature_Coefficient '±100ppm/°C'
PRP Tolerance '±1%'
PRP UniqueID 'RSMD040200375'
PRP Value '100 O'
TOP 0 1.0349154 2.3651151 180 N 4 0 1
TOP 1 1.0349154 2.325745 180 N 198 3 2
#
# CMP 4
CMP 2 1.0152303 2.290745 180 N R148 ERA-2AEB103X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thin Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDM0000/AOA0000C307.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERA-2AEB103X'
PRP Power_(Watts) '0.063W, 1/16W'
PRP Ratings 'AEC-Q200'
PRP Resistance '10 kO'
PRP Series 'ERA-2A'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P10KDCCT-ND'
PRP Temperature_Coefficient '±25ppm/°C'
PRP Tolerance '±0.1%'
PRP UniqueID 'RSMD040200315'
PRP Value '10 kO'
TOP 0 0.9955453 2.290745 90 N 170 17 1
TOP 1 1.0349154 2.290745 90 N 198 1 2
#
# CMP 5
CMP 2 1.1331832 2.4198001 270 N R147 ERA-2AEB103X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thin Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDM0000/AOA0000C307.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERA-2AEB103X'
PRP Power_(Watts) '0.063W, 1/16W'
PRP Ratings 'AEC-Q200'
PRP Resistance '10 kO'
PRP Series 'ERA-2A'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P10KDCCT-ND'
PRP Temperature_Coefficient '±25ppm/°C'
PRP Tolerance '±0.1%'
PRP UniqueID 'RSMD040200315'
PRP Value '10 kO'
TOP 0 1.1331832 2.4001151 0 N 248 325 1
TOP 1 1.1331832 2.4394852 0 N 199 0 2
#
# CMP 6
CMP 2 0.3417938 0.836122 0 N R23 ERJ-U020R00X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDP0000/AOA0000C334.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-U020R00X'
PRP Power_(Watts) '0.1W, 1/10W'
PRP Ratings 'AEC-Q200'
PRP Resistance '0 O'
PRP Series 'ERJ-U02'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '10-ERJ-U020R00XCT-ND'
PRP Temperature_Coefficient '-100/ +600ppm/°C'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD040200004'
PRP Value '0 O'
TOP 0 0.3614788 0.836122 270 N 8 2 1
TOP 1 0.3221087 0.836122 270 N 177 3 2
#
# CMP 7
CMP 2 1.1217169 0.7598291 0 N R9 ERJ-U020R00X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDP0000/AOA0000C334.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-U020R00X'
PRP Power_(Watts) '0.1W, 1/10W'
PRP Ratings 'AEC-Q200'
PRP Resistance '0 O'
PRP Series 'ERJ-U02'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '10-ERJ-U020R00XCT-ND'
PRP Temperature_Coefficient '-100/ +600ppm/°C'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD040200004'
PRP Value '0 O'
TOP 0 1.1414019 0.7598291 270 N 9 2 1
TOP 1 1.1020318 0.7598291 270 N 168 2 2
#
# CMP 8
CMP 2 1.6384108 0.6910239 270 N R124 ERJ-2GEJ104X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://b2b-api.panasonic.eu/file_stream/pids/fileversion/1242'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GEJ104X'
PRP Power_(Watts) '0.1W, 1/10W'
PRP Ratings 'AEC-Q200'
PRP Resistance '100 kO'
PRP Series 'ERJ-2G'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P100KJCT-ND'
PRP Temperature_Coefficient '±200ppm/°C'
PRP Tolerance '±5%'
PRP UniqueID 'RSMD040200354'
PRP Value '100 kO'
TOP 0 1.6384108 0.6713389 0 N 248 61 1
TOP 1 1.6384108 0.710709 0 N 203 0 2
#
# CMP 9
CMP 39 0.8505379 1.0610495 180 N FC1 dcp00001 ;0=1,1=0.3300
PRP CompType 'Feed Thru Cap'
PRP Current '6A'
PRP datasheet 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/NFM31PC276B0J3-01.pdf'
PRP DCR '5 mO'
PRP Impedance '-'
PRP Manufacturer 'Murata'
PRP Operating_Temperature '-40°C ~ 85°C'
PRP PackageReference '1206'
PRP PartNumber 'NFM31PC276B0J3L'
PRP SizeX_mm '3.2'
PRP SizeY_mm '1.6'
PRP SizeZ_mm '1.5'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '490-6984-1-ND'
PRP Temperature_Coefficient '-'
PRP Tolerance '±20%'
PRP UniqueID 'dcp00001'
PRP Value '27uF'
PRP Voltage_-_Rated '6.3V'
TOP 0 0.784593 1.0610495 0 N 170 15 1
TOP 1 0.8505379 1.0925456 0 N 248 133 2
TOP 2 0.8505379 1.0295534 0 N 248 134 2
TOP 3 0.8625379 1.1045456 180 N 248 468 2
TOP 4 0.8385379 1.1045456 180 N 248 469 2
TOP 5 0.8385379 1.0175534 0 N 248 470 2
TOP 6 0.8625379 1.0175534 0 N 248 471 2
TOP 7 0.9164828 1.0610495 0 N 33 6 3
#
# CMP 10
CMP 22 2.7576378 1.2586396 0 N U22 SN74AUCH16244DGG ;0=1,1=0.4400
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.ti.com/lit/ds/symlink/sn74auch16244.pdf?ts=1739109321738&ref_url=https%253A%252F%252Fwww.ti.com%252Fproduct%252FSN74AUCH16244%252Fpart-details%252FSN74AUCH16244DGGR'
PRP CompType 'Buffer'
PRP Manufacturer 'Texas Instruments'
PRP PartNumber 'SN74AUCH16244DGG'
PRP Supplier_1 '-'
PRP Supplier_Part_Number_1 '-'
TOP 0 2.9052756 1.4850176 180 N 32 0 1
TOP 1 2.9052756 1.4653325 180 N 75 0 2
TOP 2 2.9052756 1.4456475 180 N 53 0 3
TOP 3 2.9052756 1.4259624 180 N 248 122 4
TOP 4 2.9052756 1.4062774 180 N 73 0 5
TOP 5 2.9052756 1.3865924 180 N 74 0 6
TOP 6 2.9052756 1.3669073 180 N 33 2 7
TOP 7 2.9052756 1.3472223 180 N 0 2 8
TOP 8 2.9052756 1.3275372 180 N 72 0 9
TOP 9 2.9052756 1.3078522 180 N 248 123 10
TOP 10 2.9052756 1.2881672 180 N 71 0 11
TOP 11 2.9052756 1.2684821 180 N 70 0 12
TOP 12 2.9052756 1.2487971 180 N 69 0 13
TOP 13 2.9052756 1.229112 180 N 76 0 14
TOP 14 2.9052756 1.209427 180 N 248 124 15
TOP 15 2.9052756 1.189742 180 N 77 0 16
TOP 16 2.9052756 1.1700569 180 N 78 0 17
TOP 17 2.9052756 1.1503719 180 N 33 3 18
TOP 18 2.9052756 1.1306868 180 N 82 0 19
TOP 19 2.9052756 1.1110018 180 N 81 0 20
TOP 20 2.9052756 1.0913168 180 N 248 125 21
TOP 21 2.9052756 1.0716317 180 N 79 0 22
TOP 22 2.9052756 1.0519467 180 N 80 0 23
TOP 23 2.9052756 1.0322616 180 N 32 1 24
TOP 24 2.61 1.0322616 180 N 32 2 25
TOP 25 2.61 1.0519467 180 N 43 0 26
TOP 26 2.61 1.0716317 180 N 42 0 27
TOP 27 2.61 1.0913168 180 N 248 126 28
TOP 28 2.61 1.1110018 180 N 44 0 29
TOP 29 2.61 1.1306868 180 N 45 0 30
TOP 30 2.61 1.1503719 180 N 33 4 31
TOP 31 2.61 1.1700569 180 N 41 0 32
TOP 32 2.61 1.189742 180 N 40 0 33
TOP 33 2.61 1.209427 180 N 248 127 34
TOP 34 2.61 1.229112 180 N 39 0 35
TOP 35 2.61 1.2487971 180 N 34 0 36
TOP 36 2.61 1.2684821 180 N 35 0 37
TOP 37 2.61 1.2881672 180 N 36 0 38
TOP 38 2.61 1.3078522 180 N 248 128 39
TOP 39 2.61 1.3275372 180 N 37 0 40
TOP 40 2.61 1.3472223 180 N 32 3 41
TOP 41 2.61 1.3669073 180 N 33 5 42
TOP 42 2.61 1.3865924 180 N 46 0 43
TOP 43 2.61 1.4062774 180 N 38 0 44
TOP 44 2.61 1.4259624 180 N 248 129 45
TOP 45 2.61 1.4456475 180 N 48 0 46
TOP 46 2.61 1.4653325 180 N 47 0 47
TOP 47 2.61 1.4850176 180 N 32 4 48
#
# CMP 11
CMP 2 3.0234467 0.0790345 90 N R73 ERA-2AEB103X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thin Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDM0000/AOA0000C307.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERA-2AEB103X'
PRP Power_(Watts) '0.063W, 1/16W'
PRP Ratings 'AEC-Q200'
PRP Resistance '10 kO'
PRP Series 'ERA-2A'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P10KDCCT-ND'
PRP Temperature_Coefficient '±25ppm/°C'
PRP Tolerance '±0.1%'
PRP UniqueID 'RSMD040200315'
PRP Value '10 kO'
TOP 0 3.0234467 0.0987195 180 N 14 0 1
TOP 1 3.0234467 0.0593494 180 N 238 6 2
#
# CMP 12
CMP 55 1.1968898 2.6531102 180 N Q3 CSD13380F3 ;0=1,1=0.0138
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/csd13380f3.pdf'
PRP CompType 'NMOS'
PRP Manufacturer 'Texas Instruments'
PRP PartNumber 'CSD13380F3'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'CSD13380F3-ND'
PRP Supplier_Part_Number_2 '02AC9628'
PRP Supplier_Part_Number_3 '595-CSD13380F3'
TOP 0 1.19 2.6462204 0 N 204 1 1
TOP 1 1.19 2.66 0 N 248 320 2
TOP 2 1.2057481 2.6531102 0 N 15 1 3
#
# CMP 13
CMP 8 1.1600001 2.5445276 270 N R25 ERJ-HP6F1002V ;0=1,1=0.0571
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDQ0000/ast-ind-151033.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 175°C'
PRP PackageReference '0805'
PRP PartNumber 'ERJ-HP6F1002V'
PRP Power_(Watts) '0.5W, 1/2W'
PRP Ratings 'AEC-Q200'
PRP Resistance '10 kO'
PRP Series 'ERJ-HP6'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '10-ERJ-HP6F1002VCT-ND'
PRP Temperature_Coefficient '±100ppm/°C'
PRP Tolerance '±1%'
PRP UniqueID 'RSMD080502076'
PRP Value '10 kO'
TOP 0 1.1600001 2.515 0 N 15 0 1
TOP 1 1.1600001 2.5740551 0 N 91 0 2
#
# CMP 14
CMP 8 1.0650001 2.5445276 270 N R18 ERJ-HP6F1002V ;0=1,1=0.0571
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDQ0000/ast-ind-151033.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 175°C'
PRP PackageReference '0805'
PRP PartNumber 'ERJ-HP6F1002V'
PRP Power_(Watts) '0.5W, 1/2W'
PRP Ratings 'AEC-Q200'
PRP Resistance '10 kO'
PRP Series 'ERJ-HP6'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '10-ERJ-HP6F1002VCT-ND'
PRP Temperature_Coefficient '±100ppm/°C'
PRP Tolerance '±1%'
PRP UniqueID 'RSMD080502076'
PRP Value '10 kO'
TOP 0 1.0650001 2.515 0 N 16 0 1
TOP 1 1.0650001 2.5740551 0 N 92 0 2
#
# CMP 15
CMP 55 1.1018898 2.6531102 180 N Q2 CSD13380F3 ;0=1,1=0.0138
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/csd13380f3.pdf'
PRP CompType 'NMOS'
PRP Manufacturer 'Texas Instruments'
PRP PartNumber 'CSD13380F3'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'CSD13380F3-ND'
PRP Supplier_Part_Number_2 '02AC9628'
PRP Supplier_Part_Number_3 '595-CSD13380F3'
TOP 0 1.095 2.6462204 0 N 95 0 1
TOP 1 1.095 2.66 0 N 248 62 2
TOP 2 1.1107481 2.6531102 0 N 16 1 3
#
# CMP 16
CMP 20 1.5636083 0.4086393 180 N U19 SN74AUP1G08DCKT ;0=1,1=0.0433
PRP Color '-'
PRP CompType 'AND Gate'
PRP Current_Rating_(Amps) '-'
PRP datasheet '-'
PRP Length_(in) '-'
PRP Manufacturer 'Texas Instruments'
PRP Mount_Type 'SMD'
PRP PackageReference 'SC70'
PRP PartNumber 'SN74AUP1G08DCKT'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '296-19075-1-ND'
PRP Text1 '-'
PRP UniqueID 'cmp00268'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 1.5203011 0.3830487 90 N 204 0 1
TOP 1 1.5203012 0.4086392 90 N 202 1 2
TOP 2 1.5203012 0.4342297 90 N 248 118 3
TOP 3 1.6069155 0.4342298 90 N 94 1 4
TOP 4 1.6069155 0.3830487 90 N 170 14 5
#
# CMP 17
CMP 4 1.1540918 1.9482942 180 N C29 GRT155R71E104KE01J ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet '-'
PRP Manufacturer 'Murata'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0402'
PRP PartNumber 'GRT155R71E104KE01J'
PRP Ratings '-'
PRP Series '-'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Digi-key'
PRP Supplier_Part_Number_1 '490-GRT155R71E104KE01JCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±10%'
PRP UniqueID 'capcc09401'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '25V'
TOP 0 1.1344068 1.9482942 90 N 248 329 1
TOP 1 1.1737769 1.9482942 90 N 238 48 2
#
# CMP 18
CMP 2 1.2040919 2.0278218 0 N R32 ERA-2AEB103X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thin Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDM0000/AOA0000C307.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERA-2AEB103X'
PRP Power_(Watts) '0.063W, 1/16W'
PRP Ratings 'AEC-Q200'
PRP Resistance '10 kO'
PRP Series 'ERA-2A'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P10KDCCT-ND'
PRP Temperature_Coefficient '±25ppm/°C'
PRP Tolerance '±0.1%'
PRP UniqueID 'RSMD040200315'
PRP Value '10 kO'
TOP 0 1.2237769 2.0278218 270 N 96 0 1
TOP 1 1.1844068 2.0278218 270 N 238 7 2
#
# CMP 19
CMP 2 1.3536981 2.0278218 180 N R33 ERA-2AEB103X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thin Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDM0000/AOA0000C307.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERA-2AEB103X'
PRP Power_(Watts) '0.063W, 1/16W'
PRP Ratings 'AEC-Q200'
PRP Resistance '10 kO'
PRP Series 'ERA-2A'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P10KDCCT-ND'
PRP Temperature_Coefficient '±25ppm/°C'
PRP Tolerance '±0.1%'
PRP UniqueID 'RSMD040200315'
PRP Value '10 kO'
TOP 0 1.3340131 2.0278218 90 N 97 0 1
TOP 1 1.3733832 2.0278218 90 N 238 8 2
#
# CMP 20
CMP 47 1.278895 1.9482942 0 N U9 ADS1119IRTER ;0=1,1=0.0000
PRP Addresss '0x40'
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber 'ADS1119IRTET'
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/ads1119.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/ads1119'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/ads1119/datasheet'
PRP CompType 'ADC'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP Operating_Temperature_Range '-40 to 125 C'
PRP PackageDescription 'WQFN-16'
PRP PackageReference 'RTE0016D'
PRP PartNumber 'ADS1119IRTER'
PRP Rating ''
PRP RoHS ''
PRP SizeArea_mm2 '9'
PRP SizeAreaWB_mm2 '16'
PRP SizeX_mm '3'
PRP SizeY_mm '3'
PRP SizeZ_mm '0.8'
TOP 0 1.3340131 1.9778218 180 N 97 1 1
TOP 1 1.3340131 1.9581367 180 N 248 156 2
TOP 2 1.3340131 1.9384517 180 N 248 155 3
TOP 3 1.3340131 1.9187666 180 N 102 4 4
TOP 4 1.3084226 1.8931761 180 N 169 1 5
TOP 5 1.2887375 1.8931761 180 N 248 154 6
TOP 6 1.2690525 1.8931761 180 N 238 41 7
TOP 7 1.2493674 1.8931761 180 N 171 5 8
TOP 8 1.2237769 1.9187666 180 N 108 1 9
TOP 9 1.2237769 1.9384517 180 N 238 40 10
TOP 10 1.2237769 1.9581367 180 N 238 39 11
TOP 11 1.2237769 1.9778218 180 N 96 1 12
TOP 12 1.2493674 2.0034123 180 N 194 1 13
TOP 13 1.2690525 2.0034123 180 N 196 1 14
TOP 14 1.2887375 2.0034123 180 N 248 153 15
TOP 15 1.3084226 2.0034123 180 N 248 152 16
TOP 16 1.278895 1.9482942 180 N 248 151 17
TOP 17 1.2788982 1.948291 180 N 248 489 17
#
# CMP 21
CMP 18 0.9096454 1.1881502 180 N U7 INA180B1IDBVR ;0=1,1=0.0571
PRP Alt_Manufacturer 'Texas Instruments'
PRP Alt_PartNumber 'INA180B1IDBVT'
PRP CompType 'Current Amplifier'
PRP Manufacturer 'Texas Instruments'
PRP PartNumber 'INA180B1IDBVR'
PRP Supplier_1 ''
PRP Supplier_Part_Number_1 ''
PRP Text1 'Text1'
TOP 0 0.8584642 1.1507486 90 N 170 13 1
TOP 1 0.8584642 1.1881502 90 N 248 117 2
TOP 2 0.8584642 1.2255517 90 N 100 1 3
TOP 3 0.9608265 1.2255517 90 N 169 0 4
TOP 4 0.9608265 1.1507486 90 N 238 35 5
#
# CMP 22
CMP 2 0.5196105 1.132048 0 N R26 ERJ-2RKF1002X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_(Watts) '0.1W, 1/10W'
PRP Ratings 'AEC-Q200'
PRP Resistance '10 kO'
PRP Series 'ERJ-2RK'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Temperature_Coefficient '±100ppm/°C'
PRP Tolerance '±1%'
PRP UniqueID 'RSMD040200314'
PRP Value '10 kO'
TOP 0 0.5392955 1.132048 270 N 8 0 1
TOP 1 0.4999254 1.132048 270 N 176 4 2
#
# CMP 23
CMP 18 0.9096455 1.5881505 180 N U5 INA180B1IDBVR ;0=1,1=0.0571
PRP Alt_Manufacturer 'Texas Instruments'
PRP Alt_PartNumber 'INA180B1IDBVT'
PRP CompType 'Current Amplifier'
PRP Manufacturer 'Texas Instruments'
PRP PartNumber 'INA180B1IDBVR'
PRP Supplier_1 ''
PRP Supplier_Part_Number_1 ''
PRP Text1 'Text1'
TOP 0 0.8584643 1.5507489 90 N 107 1 1
TOP 1 0.8584643 1.5881505 90 N 248 63 2
TOP 2 0.8584643 1.625552 90 N 105 1 3
TOP 3 0.9608266 1.625552 90 N 108 0 4
TOP 4 0.9608266 1.5507489 90 N 238 9 5
#
# CMP 24
CMP 2 0.5196106 1.5320483 0 N R16 ERJ-2RKF1002X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_(Watts) '0.1W, 1/10W'
PRP Ratings 'AEC-Q200'
PRP Resistance '10 kO'
PRP Series 'ERJ-2RK'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Temperature_Coefficient '±100ppm/°C'
PRP Tolerance '±1%'
PRP UniqueID 'RSMD040200314'
PRP Value '10 kO'
TOP 0 0.5392956 1.5320483 270 N 8 1 1
TOP 1 0.4999255 1.5320483 270 N 176 9 2
#
# CMP 25
CMP 19 1.926239 1.5545201 135 N U20 REF35160QDBV ;0=1,1=0.0571
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color '-'
PRP CompType 'Reference'
PRP Current_Rating_(Amps) '-'
PRP datasheet 'https://www.ti.com/lit/ds/symlink/ref35.pdf?ts=1667837850745&ref_url=https%253A%252F%252Fwww.ti.com%252Fsitesearch%252Fen-us%252Fdocs%252Funiversalsearch.tsp%253FlangPref%253Den-US%2526searchTerm%253DREF35160%2526nr%253D1'
PRP Length_(in) '-'
PRP Manufacturer 'Texas Instruments'
PRP Mount_Type 'SMD'
PRP PackageReference 'SOT-23-6'
PRP PartNumber 'REF35160QDBV'
PRP Pitch_(mm) '1.27'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Supplier_1 '-'
PRP Supplier_Part_Number_1 '-'
PRP Text1 '-'
PRP UniqueID 'cmp00301'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 1.8636015 1.5642637 135 N 248 323 1
TOP 1 1.8900484 1.5907107 135 N 248 324 2
TOP 2 1.9164953 1.6171575 135 N 116 0 3
TOP 3 1.9888764 1.5447765 135 N 238 46 4
TOP 4 1.9624295 1.5183296 135 N 0 1 5
TOP 5 1.9359826 1.4918827 135 N 10 0 6
#
# CMP 26
CMP 0 2.0837454 1.3741547 0 N R132 ERJ-1GNF3001C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GNF3001C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '3 kO'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P122912CT-ND'
PRP Temperature_Coefficient '±200ppm/°C'
PRP Tolerance '±1%'
PRP UniqueID 'RSMD020100769'
PRP Value '3 kO'
TOP 0 2.094769 1.3741547 270 N 248 64 1
TOP 1 2.0727218 1.3741547 270 N 109 1 2
#
# CMP 27
CMP 0 1.8787004 1.6549524 315 N R131 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 1.8864953 1.6471575 315 N 116 1 1
TOP 1 1.8709055 1.6627473 315 N 238 47 2
#
# CMP 28
CMP 2 2.6129298 1.9085608 90 N R101 ERA-2AEB103X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thin Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDM0000/AOA0000C307.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERA-2AEB103X'
PRP Power_(Watts) '0.063W, 1/16W'
PRP Ratings 'AEC-Q200'
PRP Resistance '10 kO'
PRP Series 'ERA-2A'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P10KDCCT-ND'
PRP Temperature_Coefficient '±25ppm/°C'
PRP Tolerance '±0.1%'
PRP UniqueID 'RSMD040200315'
PRP Value '10 kO'
TOP 0 2.6129298 1.9282458 180 N 248 321 1
TOP 1 2.6129298 1.8888757 180 N 11 1 2
#
# CMP 29
CMP 0 1.7272774 1.7410857 315 N R133 ERJ-1GNF4991C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GNF4991C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '4.99 kO'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P123046CT-ND'
PRP Temperature_Coefficient '±200ppm/°C'
PRP Tolerance '±1%'
PRP UniqueID 'RSMD020100641'
PRP Value '4.99 kO'
TOP 0 1.7350723 1.7332908 315 N 248 65 1
TOP 1 1.7194825 1.7488806 315 N 5 0 2
#
# CMP 30
CMP 0 2.0301789 1.3196638 180 N R118 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.0191553 1.3196638 90 N 11 0 1
TOP 1 2.0412025 1.3196638 90 N 119 0 2
#
# CMP 31
CMP 2 2.7224623 2.0085607 270 N R110 ERA-2AEB103X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thin Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDM0000/AOA0000C307.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERA-2AEB103X'
PRP Power_(Watts) '0.063W, 1/16W'
PRP Ratings 'AEC-Q200'
PRP Resistance '10 kO'
PRP Series 'ERA-2A'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P10KDCCT-ND'
PRP Temperature_Coefficient '±25ppm/°C'
PRP Tolerance '±0.1%'
PRP UniqueID 'RSMD040200315'
PRP Value '10 kO'
TOP 0 2.7224623 1.9888757 0 N 12 0 1
TOP 1 2.7224623 2.0282458 0 N 170 16 2
#
# CMP 32
CMP 0 2.0212025 1.1259079 270 N R119 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.0212025 1.1148843 0 N 203 1 1
TOP 1 2.0212025 1.1369315 0 N 84 0 2
#
# CMP 33
CMP 0 2.0712025 1.1559079 270 N R126 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.0712025 1.1448843 0 N 192 0 1
TOP 1 2.0712025 1.1669315 0 N 117 0 2
#
# CMP 34
CMP 0 1.6919221 1.7057303 135 N R130 ERJ-1GNF2491C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GNF2491C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '2.49 kO'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P122865CT-ND'
PRP Temperature_Coefficient '±200ppm/°C'
PRP Tolerance '±1%'
PRP UniqueID 'RSMD020100692'
PRP Value '2.49 kO'
TOP 0 1.6841272 1.7135252 135 N 6 0 1
TOP 1 1.699717 1.6979354 135 N 170 4 2
#
# CMP 35
CMP 4 2.0327959 1.500857 315 N C85 GRT155R71E104KE01J ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet '-'
PRP Manufacturer 'Murata'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0402'
PRP PartNumber 'GRT155R71E104KE01J'
PRP Ratings '-'
PRP Series '-'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Digi-key'
PRP Supplier_Part_Number_1 '490-GRT155R71E104KE01JCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±10%'
PRP UniqueID 'capcc09401'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '25V'
TOP 0 2.0467153 1.4869376 315 N 248 322 1
TOP 1 2.0188764 1.5147765 315 N 238 45 2
#
# CMP 36
CMP 1 2.0822261 1.3269158 0 N C83 GRM033Z71C104ME14D ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033Z71C104ME14-01.pdf'
PRP Manufacturer 'Murata Electronics'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'GRM033Z71C104ME14D'
PRP Ratings '-'
PRP Series 'GRM'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.33'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '490-GRM033Z71C104ME14DCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±20%'
PRP UniqueID 'capcc09270'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '16V'
TOP 0 2.0932497 1.3269158 270 N 248 66 1
TOP 1 2.0712025 1.3269158 270 N 109 2 2
#
# CMP 37
CMP 4 2.0908876 1.2989158 0 N C82 0402ZD106MAT2A ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://datasheets.kyocera-avx.com/cx5r.pdf'
PRP Manufacturer 'KYOCERA AVX'
PRP Operating_Temperature '-55°C ~ 85°C'
PRP PackageReference '0402'
PRP PartNumber '0402ZD106MAT2A'
PRP Ratings '-'
PRP Series '-'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Digi-key'
PRP Supplier_Part_Number_1 '478-10052-1-ND'
PRP Temperature_Coefficient 'X5R'
PRP Tolerance '±20%'
PRP UniqueID 'capcc09406'
PRP Value '10 uF'
PRP Voltage_-_Rated '10V'
TOP 0 2.1105726 1.2989158 270 N 248 67 1
TOP 1 2.0712025 1.2989158 270 N 109 3 2
#
# CMP 38
CMP 4 2.0215174 1.2724197 180 N C86 0402ZD106MAT2A ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://datasheets.kyocera-avx.com/cx5r.pdf'
PRP Manufacturer 'KYOCERA AVX'
PRP Operating_Temperature '-55°C ~ 85°C'
PRP PackageReference '0402'
PRP PartNumber '0402ZD106MAT2A'
PRP Ratings '-'
PRP Series '-'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Digi-key'
PRP Supplier_Part_Number_1 '478-10052-1-ND'
PRP Temperature_Coefficient 'X5R'
PRP Tolerance '±20%'
PRP UniqueID 'capcc09406'
PRP Value '10 uF'
PRP Voltage_-_Rated '10V'
TOP 0 2.0018324 1.2724197 90 N 248 68 1
TOP 1 2.0412025 1.2724197 90 N 114 0 2
#
# CMP 39
CMP 1 2.0251789 1.2484197 180 N C87 GRM033Z71C104ME14D ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033Z71C104ME14-01.pdf'
PRP Manufacturer 'Murata Electronics'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'GRM033Z71C104ME14D'
PRP Ratings '-'
PRP Series 'GRM'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.33'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '490-GRM033Z71C104ME14DCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±20%'
PRP UniqueID 'capcc09270'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '16V'
TOP 0 2.0141553 1.2484197 90 N 248 69 1
TOP 1 2.0362025 1.2484197 90 N 114 1 2
#
# CMP 40
CMP 1 2.0935092 1.2104276 0 N C79 GRM033Z71C104ME14D ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033Z71C104ME14-01.pdf'
PRP Manufacturer 'Murata Electronics'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'GRM033Z71C104ME14D'
PRP Ratings '-'
PRP Series 'GRM'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.33'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '490-GRM033Z71C104ME14DCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±20%'
PRP UniqueID 'capcc09270'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '16V'
TOP 0 2.1045328 1.2104276 270 N 248 70 1
TOP 1 2.0824856 1.2104276 270 N 110 3 2
#
# CMP 41
CMP 1 2.0497465 1.2104276 180 N C78 GRM033R61A105ME44D ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033R61A105ME44-04A.pdf'
PRP Manufacturer 'Murata Electronics'
PRP Operating_Temperature '-55°C ~ 85°C'
PRP PackageReference '0201'
PRP PartNumber 'GRM033R61A105ME44D'
PRP Ratings '-'
PRP Series 'GRM'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.33'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '490-GRM033R61A105ME44DCT-ND'
PRP Temperature_Coefficient 'X5R'
PRP Tolerance '±20%'
PRP UniqueID 'capcc09264'
PRP Value '1 uF'
PRP Voltage_-_Rated '10V'
TOP 0 2.0387229 1.2104276 90 N 248 71 1
TOP 1 2.0607701 1.2104276 90 N 110 4 2
#
# CMP 42
CMP 1 2.2879738 1.3324587 45 N C77 GRM033Z71C104ME14D ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033Z71C104ME14-01.pdf'
PRP Manufacturer 'Murata Electronics'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'GRM033Z71C104ME14D'
PRP Ratings '-'
PRP Series 'GRM'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.33'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '490-GRM033Z71C104ME14DCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±20%'
PRP UniqueID 'capcc09270'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '16V'
TOP 0 2.2957686 1.3402535 225 N 248 72 1
TOP 1 2.2801789 1.3246638 225 N 102 2 2
#
# CMP 43
CMP 1 2.2879738 1.1651366 315 N C76 GRM033R61A105ME44D ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033R61A105ME44-04A.pdf'
PRP Manufacturer 'Murata Electronics'
PRP Operating_Temperature '-55°C ~ 85°C'
PRP PackageReference '0201'
PRP PartNumber 'GRM033R61A105ME44D'
PRP Ratings '-'
PRP Series 'GRM'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.33'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '490-GRM033R61A105ME44DCT-ND'
PRP Temperature_Coefficient 'X5R'
PRP Tolerance '±20%'
PRP UniqueID 'capcc09264'
PRP Value '1 uF'
PRP Voltage_-_Rated '10V'
TOP 0 2.2957686 1.1573418 315 N 248 73 1
TOP 1 2.2801789 1.1729315 315 N 102 3 2
#
# CMP 44
CMP 1 2.17 1.38 90 N C75 GRM033Z71C104ME14D ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033Z71C104ME14-01.pdf'
PRP Manufacturer 'Murata Electronics'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'GRM033Z71C104ME14D'
PRP Ratings '-'
PRP Series 'GRM'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.33'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '490-GRM033Z71C104ME14DCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±20%'
PRP UniqueID 'capcc09270'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '16V'
TOP 0 2.17 1.3910236 180 N 248 74 1
TOP 1 2.17 1.3689764 180 N 171 2 2
#
# CMP 45
CMP 1 2.0935092 1.2566717 0 N C74 GRM033Z71C104ME14D ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033Z71C104ME14-01.pdf'
PRP Manufacturer 'Murata Electronics'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'GRM033Z71C104ME14D'
PRP Ratings '-'
PRP Series 'GRM'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.33'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '490-GRM033Z71C104ME14DCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±20%'
PRP UniqueID 'capcc09270'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '16V'
TOP 0 2.1045328 1.2566717 270 N 248 75 1
TOP 1 2.0824856 1.2566717 270 N 171 3 2
#
# CMP 46
CMP 1 2.1778167 1.1559079 90 N C73 GRM033R61A105ME44D ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033R61A105ME44-04A.pdf'
PRP Manufacturer 'Murata Electronics'
PRP Operating_Temperature '-55°C ~ 85°C'
PRP PackageReference '0201'
PRP PartNumber 'GRM033R61A105ME44D'
PRP Ratings '-'
PRP Series 'GRM'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.33'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '490-GRM033R61A105ME44DCT-ND'
PRP Temperature_Coefficient 'X5R'
PRP Tolerance '±20%'
PRP UniqueID 'capcc09264'
PRP Value '1 uF'
PRP Voltage_-_Rated '10V'
TOP 0 2.1778167 1.1669315 180 N 248 76 1
TOP 1 2.1778167 1.1448843 180 N 171 4 2
#
# CMP 47
CMP 4 0.2178892 0.816437 90 N C16 CGA2B1X5R1C224M050BC ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://product.tdk.com/system/files/dam/doc/product/capacitor/ceramic/mlcc/catalog/mlcc_automotive_general_en.pdf'
PRP Manufacturer 'TDK Corporation'
PRP Operating_Temperature '-55°C ~ 85°C'
PRP PackageReference '0402'
PRP PartNumber 'CGA2B1X5R1C224M050BC'
PRP Ratings 'AEC-Q200'
PRP Series 'CGA'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.55'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '445-12172-1-ND'
PRP Temperature_Coefficient 'X5R'
PRP Tolerance '±20%'
PRP UniqueID 'capcc01693'
PRP Value '0.22 uF'
PRP Voltage_-_Rated '16V'
TOP 0 0.2178892 0.836122 180 N 174 0 1
TOP 1 0.2178892 0.7967519 180 N 248 77 2
#
# CMP 48
CMP 2 0.2518892 0.816437 90 N R10 ERA-2AEB103X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thin Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDM0000/AOA0000C307.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERA-2AEB103X'
PRP Power_(Watts) '0.063W, 1/16W'
PRP Ratings 'AEC-Q200'
PRP Resistance '10 kO'
PRP Series 'ERA-2A'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P10KDCCT-ND'
PRP Temperature_Coefficient '±25ppm/°C'
PRP Tolerance '±0.1%'
PRP UniqueID 'RSMD040200315'
PRP Value '10 kO'
TOP 0 0.2518892 0.836122 180 N 177 1 1
TOP 1 0.2518892 0.7967519 180 N 238 10 2
#
# CMP 49
CMP 2 0.1838892 0.816437 90 N R12 ERA-2AEB9311X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thin Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDM0000/AOA0000C307.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERA-2AEB9311X'
PRP Power_(Watts) '0.063W, 1/16W'
PRP Ratings 'AEC-Q200'
PRP Resistance '9.31 kO'
PRP Series 'ERA-2A'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P9.31KDCCT-ND'
PRP Temperature_Coefficient '±25ppm/°C'
PRP Tolerance '±0.1%'
PRP UniqueID 'RSMD040203923'
PRP Value '9.31 kO'
TOP 0 0.1838892 0.836122 180 N 173 0 1
TOP 1 0.1838892 0.7967519 180 N 176 5 2
#
# CMP 50
CMP 9 0.1567871 1.155 180 N C11 C2012X7S1A226M125AC ;0=1,1=0.0571
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet '-'
PRP Manufacturer 'TDK Corporation'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0805'
PRP PartNumber 'C2012X7S1A226M125AC'
PRP Ratings '-'
PRP Series '-'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-key'
PRP Supplier_Part_Number_1 '445-14560-1-ND'
PRP Temperature_Coefficient 'X7S'
PRP Tolerance '±20%'
PRP UniqueID 'capcc09395'
PRP Value '22 uF'
PRP Voltage_-_Rated '10V'
TOP 0 0.1272595 1.155 90 N 248 78 1
TOP 1 0.1863146 1.155 90 N 175 1 2
#
# CMP 51
CMP 9 0.2207954 1.33849 180 N C14 C2012X7S1A226M125AC ;0=1,1=0.0571
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet '-'
PRP Manufacturer 'TDK Corporation'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0805'
PRP PartNumber 'C2012X7S1A226M125AC'
PRP Ratings '-'
PRP Series '-'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-key'
PRP Supplier_Part_Number_1 '445-14560-1-ND'
PRP Temperature_Coefficient 'X7S'
PRP Tolerance '±20%'
PRP UniqueID 'capcc09395'
PRP Value '22 uF'
PRP Voltage_-_Rated '10V'
TOP 0 0.1912678 1.33849 90 N 248 79 1
TOP 1 0.2503229 1.33849 90 N 176 6 2
#
# CMP 52
CMP 6 0.2555819 1.257625 270 N FB1 BLE18PS080SN1D ;0=1,1=0.0394
PRP CompType 'FerriteBead'
PRP Current '8A'
PRP datasheet 'https://www.murata.com/products/productdata/8800169525278/ENFA0080.pdf'
PRP DCR '4 mO'
PRP Impedance '8.5 O'
PRP Manufacturer 'Murata'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0603'
PRP PartNumber 'BLE18PS080SN1D'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '-'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '490-BLE18PS080SN1DCT-ND'
PRP Temperature_Coefficient '-'
PRP Tolerance '-'
PRP UniqueID 'dcp00004'
PRP Value '-'
PRP Voltage_-_Rated '-'
TOP 0 0.2555819 1.2300659 0 N 175 4 1
TOP 1 0.2555819 1.285184 0 N 176 8 2
#
# CMP 53
CMP 2 0.1498892 0.8164369 270 N R14 ERA-2AEB4871X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thin Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDM0000/AOA0000C307.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERA-2AEB4871X'
PRP Power_(Watts) '0.063W, 1/16W'
PRP Ratings 'AEC-Q200'
PRP Resistance '4.87 kO'
PRP Series 'ERA-2A'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P4.87KDCCT-ND'
PRP Temperature_Coefficient '±25ppm/°C'
PRP Tolerance '±0.1%'
PRP UniqueID 'RSMD040202615'
PRP Value '4.87 kO'
TOP 0 0.1498892 0.7967519 0 N 248 80 1
TOP 1 0.1498892 0.836122 0 N 173 1 2
#
# CMP 54
CMP 9 0.3222606 0.9647229 90 N C10 C2012X7S1E106K125AC ;0=1,1=0.0571
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://product.tdk.com/system/files/dam/doc/product/capacitor/ceramic/mlcc/catalog/mlcc_commercial_general_en.pdf'
PRP Manufacturer 'TDK Corporation'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0805'
PRP PartNumber 'C2012X7S1E106K125AC'
PRP Ratings '-'
PRP Series 'C'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.5'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '445-181600-1-ND'
PRP Temperature_Coefficient 'X7S'
PRP Tolerance '±10%'
PRP UniqueID 'capcc03511'
PRP Value '10 uF'
PRP Voltage_-_Rated '25V'
TOP 0 0.3222606 0.9942505 180 N 248 81 1
TOP 1 0.3222606 0.9351954 180 N 237 3 2
#
# CMP 55
CMP 9 0.3922606 0.9647229 90 N C9 C2012X7S1E106K125AC ;0=1,1=0.0571
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://product.tdk.com/system/files/dam/doc/product/capacitor/ceramic/mlcc/catalog/mlcc_commercial_general_en.pdf'
PRP Manufacturer 'TDK Corporation'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0805'
PRP PartNumber 'C2012X7S1E106K125AC'
PRP Ratings '-'
PRP Series 'C'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.5'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '445-181600-1-ND'
PRP Temperature_Coefficient 'X7S'
PRP Tolerance '±10%'
PRP UniqueID 'capcc03511'
PRP Value '10 uF'
PRP Voltage_-_Rated '25V'
TOP 0 0.3922606 0.9942505 180 N 248 82 1
TOP 1 0.3922606 0.9351954 180 N 237 4 2
#
# CMP 56
CMP 9 0.3448094 1.33849 0 N C15 C2012X7S1A226M125AC ;0=1,1=0.0571
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet '-'
PRP Manufacturer 'TDK Corporation'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0805'
PRP PartNumber 'C2012X7S1A226M125AC'
PRP Ratings '-'
PRP Series '-'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-key'
PRP Supplier_Part_Number_1 '445-14560-1-ND'
PRP Temperature_Coefficient 'X7S'
PRP Tolerance '±20%'
PRP UniqueID 'capcc09395'
PRP Value '22 uF'
PRP Voltage_-_Rated '10V'
TOP 0 0.374337 1.33849 270 N 248 83 1
TOP 1 0.3152819 1.33849 270 N 176 7 2
#
# CMP 57
CMP 2 0.0818892 0.816437 90 N R11 ERJ-2RKF1002X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_(Watts) '0.1W, 1/10W'
PRP Ratings 'AEC-Q200'
PRP Resistance '10 kO'
PRP Series 'ERJ-2RK'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Temperature_Coefficient '±100ppm/°C'
PRP Tolerance '±1%'
PRP UniqueID 'RSMD040200314'
PRP Value '10 kO'
TOP 0 0.0818892 0.836122 180 N 9 0 1
TOP 1 0.0818892 0.7967519 180 N 237 5 2
#
# CMP 58
CMP 9 0.2808014 1.155 0 N C13 C2012X7S1A226M125AC ;0=1,1=0.0571
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet '-'
PRP Manufacturer 'TDK Corporation'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0805'
PRP PartNumber 'C2012X7S1A226M125AC'
PRP Ratings '-'
PRP Series '-'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-key'
PRP Supplier_Part_Number_1 '445-14560-1-ND'
PRP Temperature_Coefficient 'X7S'
PRP Tolerance '±20%'
PRP UniqueID 'capcc09395'
PRP Value '22 uF'
PRP Voltage_-_Rated '10V'
TOP 0 0.310329 1.155 270 N 248 84 1
TOP 1 0.2512739 1.155 270 N 175 2 2
#
# CMP 59
CMP 9 0.1567868 1.2250599 180 N C12 C2012X7S1A226M125AC ;0=1,1=0.0571
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet '-'
PRP Manufacturer 'TDK Corporation'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0805'
PRP PartNumber 'C2012X7S1A226M125AC'
PRP Ratings '-'
PRP Series '-'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-key'
PRP Supplier_Part_Number_1 '445-14560-1-ND'
PRP Temperature_Coefficient 'X7S'
PRP Tolerance '±20%'
PRP UniqueID 'capcc09395'
PRP Value '22 uF'
PRP Voltage_-_Rated '10V'
TOP 0 0.1272592 1.2250599 90 N 248 85 1
TOP 1 0.1863143 1.2250599 90 N 175 3 2
#
# CMP 60
CMP 2 0.1158892 0.8164369 270 N R13 ERJ-2RKF8062X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF8062X'
PRP Power_(Watts) '0.1W, 1/10W'
PRP Ratings 'AEC-Q200'
PRP Resistance '80.6 kO'
PRP Series 'ERJ-2RK'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P80.6KLCT-ND'
PRP Temperature_Coefficient '±100ppm/°C'
PRP Tolerance '±1%'
PRP UniqueID 'RSMD040203748'
PRP Value '80.6 kO'
TOP 0 0.1158892 0.7967519 0 N 248 86 1
TOP 1 0.1158892 0.836122 0 N 172 0 2
#
# CMP 61
CMP 41 0.3181394 1.2450659 270 N PP2 Probe_Point ;0=2,1=0.1570
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color '-'
PRP CompType 'Probe Point'
PRP Current_Rating_(Amps) '-'
PRP datasheet '-'
PRP Length_(in) '-'
PRP Manufacturer '-'
PRP Mount_Type '-'
PRP PackageReference '-'
PRP PartNumber '-'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Text1 '2p3V'
PRP UniqueID 'cmp00025'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 0.3181394 1.2450659 270 N 176 18 1
#
# CMP 62
CMP 43 0.1695822 0.9912992 180 N U4 TPSM82913RDU ;0=1,1=0.0000
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'No'
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Color '-'
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/GPN.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/GPN'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/GPN/datasheet'
PRP CompType 'Switcher'
PRP Current_Rating_(Amps) '-'
PRP datasheet '-'
PRP Datasheet_Path 'datasheets/IC-TPSM82913RDUR.pdf'
PRP Discharge 'On'
PRP FSW '1MHz'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP helpURL 'https://upverter.com/upn/revision/fdaa521e769c8694/'
PRP Length_(in) '-'
PRP Manufacturer 'Texas Instruments'
PRP Max_Duty_Cycle '100%'
PRP Max_Supply_Voltage '17V'
PRP Min_Supply_Voltage '3V'
PRP Mount_Type 'SMD'
PRP MountType ''
PRP Nominal_Supply_Current '5mA'
PRP Number_Of_Outputs '1'
PRP Operating_Temperature_Range '-55°C to +125°C'
PRP Output_Type 'AdjustableProgrammable'
PRP Output_Voltage '0.8-5.5V'
PRP PackageDescription ''
PRP PackageReference 'Module'
PRP Part_Number 'TPSM82913RDUR'
PRP PartNumber 'TPSM82913RDU'
PRP Pitch_(mm) '-'
PRP Rating ''
PRP RoHS 'UNKNOWN'
PRP Series '-'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP SSpec 'Random'
PRP Standoff_Height '0mm'
PRP Supplier_1 'Digi-Key'
PRP Switching_Frequency '1/2.2MHz'
PRP Switching_Topology 'Buck'
PRP Sync 'Off'
PRP Text1 '3A, Vin = 3V ? 17V'
PRP TJmax_C '+125°C'
PRP UniqueID 'cmp00201'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 0.0913342 0.8933662 0 N 248 138 1
TOP 1 0.086905 0.9420866 0 N 248 135 2
TOP 2 0.086905 0.9716142 0 N 248 147 3
TOP 3 0.086905 0.9912992 0 N 0 3 4
TOP 4 0.086905 1.0109842 0 N 248 148 5
TOP 5 0.0869063 1.0405105 0 N 248 136 6
TOP 6 0.0913342 1.0892335 0 N 248 137 7
TOP 7 0.1302121 1.0936614 0 N 248 144 8
TOP 8 0.1498972 1.0936614 0 N 248 143 9
TOP 9 0.1695822 1.0936614 0 N 175 10 10
TOP 10 0.1892672 1.0936614 0 N 175 9 11
TOP 11 0.2089523 1.0936614 0 N 175 8 12
TOP 12 0.2478289 1.0892336 0 N 175 5 13
TOP 13 0.2522606 1.0405105 0 N 175 6 14
TOP 14 0.2522594 1.0109842 0 N 175 11 15
TOP 15 0.2522594 0.9912992 0 N 248 146 16
TOP 16 0.2522594 0.9716142 0 N 248 145 17
TOP 17 0.2522606 0.9420854 0 N 237 13 18
TOP 18 0.2478314 0.8933649 0 N 177 2 19
TOP 19 0.2089523 0.888937 0 N 248 142 20
TOP 20 0.1892672 0.888937 0 N 174 1 21
TOP 21 0.1695822 0.888937 0 N 173 2 22
TOP 22 0.1498972 0.888937 0 N 172 1 23
TOP 23 0.1302121 0.888937 0 N 9 1 24
TOP 24 0.1410389 0.9627559 0 N 248 141 25
TOP 25 0.1518657 0.9735827 180 N 248 480 25
TOP 26 0.1302122 0.9735827 180 N 248 481 25
TOP 27 0.1302121 0.9519291 0 N 248 482 25
TOP 28 0.1518656 0.9519291 0 N 248 483 25
TOP 29 0.1410389 1.029685 0 N 248 139 26
TOP 30 0.1518657 1.01 180 N 248 472 26
TOP 31 0.1518657 1.0493701 180 N 248 473 26
TOP 32 0.1302121 1.0493701 0 N 248 474 26
TOP 33 0.1302121 1.01 0 N 248 475 26
TOP 34 0.1981255 1.029685 0 N 175 7 27
TOP 35 0.2089523 1.01 180 N 175 12 27
TOP 36 0.2089523 1.0493701 180 N 175 13 27
TOP 37 0.1872987 1.0493701 0 N 175 14 27
TOP 38 0.1872987 1.01 0 N 175 15 27
TOP 39 0.1981255 0.9627559 0 N 248 140 28
TOP 40 0.2089523 0.9735827 180 N 248 476 28
TOP 41 0.1872988 0.9735827 180 N 248 477 28
TOP 42 0.1872987 0.9519291 0 N 248 478 28
TOP 43 0.2089522 0.9519291 0 N 248 479 28
#
# CMP 63
CMP 48 3.5864179 1.359267 270 N J1 ASP-134488-01 ;0=1,1=0.0602
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color '-'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://suddendocs.samtec.com/prints/asp-184330-01-mkt.pdf'
PRP CompType 'FMC'
PRP Current_Rating_(Amps) '-'
PRP datasheet '-'
PRP Length_(in) '-'
PRP Manufacturer 'Samtec'
PRP Mount_Type 'SMD'
PRP PackageReference '-'
PRP PartNumber 'ASP-134488-01'
PRP Pitch_(mm) '1.27'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'SAM8730-ND'
PRP Text1 '-'
PRP UniqueID 'cmp00010'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 3.8114179 2.3332674 270 N 248 168 A1
TOP 1 3.8114179 2.2832674 270 N 0 198 A2
TOP 2 3.8114179 2.2332674 270 N 0 199 A3
TOP 3 3.8114179 2.1832674 270 N 248 186 A4
TOP 4 3.8114179 2.1332674 270 N 248 187 A5
TOP 5 3.8114179 2.0832674 270 N 0 181 A6
TOP 6 3.8114179 2.0332674 270 N 0 180 A7
TOP 7 3.8114179 1.9832674 270 N 248 204 A8
TOP 8 3.8114179 1.9332674 270 N 248 205 A9
TOP 9 3.8114179 1.8832674 270 N 0 158 A10
TOP 10 3.8114179 1.8332674 270 N 0 157 A11
TOP 11 3.8114179 1.7832674 270 N 248 206 A12
TOP 12 3.8114179 1.7332674 270 N 248 218 A13
TOP 13 3.8114179 1.6832674 270 N 0 141 A14
TOP 14 3.8114179 1.6332674 270 N 0 120 A15
TOP 15 3.8114179 1.5832674 270 N 248 231 A16
TOP 16 3.8114179 1.5332674 270 N 248 235 A17
TOP 17 3.8114179 1.4832674 270 N 0 115 A18
TOP 18 3.8114179 1.4332674 270 N 0 112 A19
TOP 19 3.8114179 1.3832674 270 N 248 240 A20
TOP 20 3.8114179 1.3332674 270 N 248 242 A21
TOP 21 3.8114179 1.2832674 270 N 0 83 A22
TOP 22 3.8114179 1.2332674 270 N 0 79 A23
TOP 23 3.8114179 1.1832674 270 N 248 259 A24
TOP 24 3.8114179 1.1332674 270 N 248 261 A25
TOP 25 3.8114179 1.0832674 270 N 0 71 A26
TOP 26 3.8114179 1.0332674 270 N 0 67 A27
TOP 27 3.8114179 0.9832674 270 N 248 266 A28
TOP 28 3.8114179 0.9332674 270 N 248 281 A29
TOP 29 3.8114179 0.8832674 270 N 0 44 A30
TOP 30 3.8114179 0.8332674 270 N 0 42 A31
TOP 31 3.8114179 0.7832674 270 N 248 285 A32
TOP 32 3.8114179 0.7332674 270 N 248 287 A33
TOP 33 3.8114179 0.6832674 270 N 0 35 A34
TOP 34 3.8114179 0.6332674 270 N 0 18 A35
TOP 35 3.8114179 0.5832674 270 N 248 305 A36
TOP 36 3.8114179 0.5332674 270 N 248 307 A37
TOP 37 3.8114179 0.4832674 270 N 0 10 A38
TOP 38 3.8114179 0.4332674 270 N 0 8 A39
TOP 39 3.8114179 0.3832674 270 N 248 315 A40
TOP 40 3.7614179 2.3332674 270 N 0 195 B1
TOP 41 3.7614179 2.2832674 270 N 248 169 B2
TOP 42 3.7614179 2.2332674 270 N 248 166 B3
TOP 43 3.7614179 2.1832674 270 N 0 197 B4
TOP 44 3.7614179 2.1332674 270 N 0 182 B5
TOP 45 3.7614179 2.0832674 270 N 248 184 B6
TOP 46 3.7614179 2.0332674 270 N 248 185 B7
TOP 47 3.7614179 1.9832674 270 N 0 160 B8
TOP 48 3.7614179 1.9332674 270 N 0 159 B9
TOP 49 3.7614179 1.8832674 270 N 248 202 B10
TOP 50 3.7614179 1.8332674 270 N 248 203 B11
TOP 51 3.7614179 1.7832674 270 N 0 143 B12
TOP 52 3.7614179 1.7332674 270 N 0 142 B13
TOP 53 3.7614179 1.6832674 270 N 248 216 B14
TOP 54 3.7614179 1.6332674 270 N 248 217 B15
TOP 55 3.7614179 1.5832674 270 N 0 119 B16
TOP 56 3.7614179 1.5332674 270 N 0 118 B17
TOP 57 3.7614179 1.4832674 270 N 248 236 B18
TOP 58 3.7614179 1.4332674 270 N 248 238 B19
TOP 59 3.7614179 1.3832674 270 N 0 110 B20
TOP 60 3.7614179 1.3332674 270 N 0 107 B21
TOP 61 3.7614179 1.2832674 270 N 248 254 B22
TOP 62 3.7614179 1.2332674 270 N 248 257 B23
TOP 63 3.7614179 1.1832674 270 N 0 77 B24
TOP 64 3.7614179 1.1332674 270 N 0 74 B25
TOP 65 3.7614179 1.0832674 270 N 248 264 B26
TOP 66 3.7614179 1.0332674 270 N 248 265 B27
TOP 67 3.7614179 0.9832674 270 N 0 66 B28
TOP 68 3.7614179 0.9332674 270 N 0 46 B29
TOP 69 3.7614179 0.8832674 270 N 248 282 B30
TOP 70 3.7614179 0.8332674 270 N 248 283 B31
TOP 71 3.7614179 0.7832674 270 N 0 41 B32
TOP 72 3.7614179 0.7332674 270 N 0 39 B33
TOP 73 3.7614179 0.6832674 270 N 248 289 B34
TOP 74 3.7614179 0.6332674 270 N 248 302 B35
TOP 75 3.7614179 0.5832674 270 N 0 15 B36
TOP 76 3.7614179 0.5332674 270 N 0 13 B37
TOP 77 3.7614179 0.4832674 270 N 248 310 B38
TOP 78 3.7614179 0.4332674 270 N 248 312 B39
TOP 79 3.7614179 0.3832674 270 N 246 0 B40
TOP 80 3.7114179 2.3332674 270 N 248 170 C1
TOP 81 3.7114179 2.2832674 270 N 0 201 C2
TOP 82 3.7114179 2.2332674 270 N 0 200 C3
TOP 83 3.7114179 2.1832674 270 N 248 172 C4
TOP 84 3.7114179 2.1332674 270 N 248 183 C5
TOP 85 3.7114179 2.0832674 270 N 0 184 C6
TOP 86 3.7114179 2.0332674 270 N 0 183 C7
TOP 87 3.7114179 1.9832674 270 N 248 200 C8
TOP 88 3.7114179 1.9332674 270 N 248 201 C9
TOP 89 3.7114179 1.8832674 270 N 74 1 C10
TOP 90 3.7114179 1.8332674 270 N 0 161 C11
TOP 91 3.7114179 1.7832674 270 N 248 214 C12
TOP 92 3.7114179 1.7332674 270 N 248 215 C13
TOP 93 3.7114179 1.6832674 270 N 0 144 C14
TOP 94 3.7114179 1.6332674 270 N 0 121 C15
TOP 95 3.7114179 1.5832674 270 N 248 232 C16
TOP 96 3.7114179 1.5332674 270 N 248 234 C17
TOP 97 3.7114179 1.4832674 270 N 79 1 C18
TOP 98 3.7114179 1.4332674 270 N 0 113 C19
TOP 99 3.7114179 1.3832674 270 N 248 241 C20
TOP 100 3.7114179 1.3332674 270 N 248 243 C21
TOP 101 3.7114179 1.2832674 270 N 0 82 C22
TOP 102 3.7114179 1.2332674 270 N 0 81 C23
TOP 103 3.7114179 1.1832674 270 N 248 258 C24
TOP 104 3.7114179 1.1332674 270 N 248 260 C25
TOP 105 3.7114179 1.0832674 270 N 0 73 C26
TOP 106 3.7114179 1.0332674 270 N 0 69 C27
TOP 107 3.7114179 0.9832674 270 N 248 277 C28
TOP 108 3.7114179 0.9332674 270 N 248 280 C29
TOP 109 3.7114179 0.8832674 270 N 215 0 C30
TOP 110 3.7114179 0.8332674 270 N 214 0 C31
TOP 111 3.7114179 0.7832674 270 N 248 286 C32
TOP 112 3.7114179 0.7332674 270 N 248 288 C33
TOP 113 3.7114179 0.6832674 270 N 250 0 C34
TOP 114 3.7114179 0.6332674 270 N 251 1 C35
TOP 115 3.7114179 0.5832674 270 N 248 304 C36
TOP 116 3.7114179 0.5332674 270 N 251 2 C37
TOP 117 3.7114179 0.4832674 270 N 248 309 C38
TOP 118 3.7114179 0.4332674 270 N 0 9 C39
TOP 119 3.7114179 0.3832674 270 N 248 314 C40
TOP 120 3.6614179 2.3332674 270 N 245 0 D1
TOP 121 3.6614179 2.2832674 270 N 248 171 D2
TOP 122 3.6614179 2.2332674 270 N 248 167 D3
TOP 123 3.6614179 2.1832674 270 N 0 196 D4
TOP 124 3.6614179 2.1332674 270 N 0 185 D5
TOP 125 3.6614179 2.0832674 270 N 248 181 D6
TOP 126 3.6614179 2.0332674 270 N 248 182 D7
TOP 127 3.6614179 1.9832674 270 N 81 1 D8
TOP 128 3.6614179 1.9332674 270 N 0 162 D9
TOP 129 3.6614179 1.8832674 270 N 248 194 D10
TOP 130 3.6614179 1.8332674 270 N 72 1 D11
TOP 131 3.6614179 1.7832674 270 N 0 145 D12
TOP 132 3.6614179 1.7332674 270 N 248 213 D13
TOP 133 3.6614179 1.6832674 270 N 76 1 D14
TOP 134 3.6614179 1.6332674 270 N 0 122 D15
TOP 135 3.6614179 1.5832674 270 N 248 230 D16
TOP 136 3.6614179 1.5332674 270 N 82 1 D17
TOP 137 3.6614179 1.4832674 270 N 0 116 D18
TOP 138 3.6614179 1.4332674 270 N 248 237 D19
TOP 139 3.6614179 1.3832674 270 N 0 111 D20
TOP 140 3.6614179 1.3332674 270 N 0 108 D21
TOP 141 3.6614179 1.2832674 270 N 248 255 D22
TOP 142 3.6614179 1.2332674 270 N 0 80 D23
TOP 143 3.6614179 1.1832674 270 N 0 76 D24
TOP 144 3.6614179 1.1332674 270 N 248 262 D25
TOP 145 3.6614179 1.0832674 270 N 0 72 D26
TOP 146 3.6614179 1.0332674 270 N 0 68 D27
TOP 147 3.6614179 0.9832674 270 N 248 278 D28
TOP 148 3.6614179 0.9332674 270 N 0 47 D29
TOP 149 3.6614179 0.8832674 270 N 242 0 D30
TOP 150 3.6614179 0.8332674 270 N 241 0 D31
TOP 151 3.6614179 0.7832674 270 N 252 1 D32
TOP 152 3.6614179 0.7332674 270 N 0 38 D33
TOP 153 3.6614179 0.6832674 270 N 0 36 D34
TOP 154 3.6614179 0.6332674 270 N 249 0 D35
TOP 155 3.6614179 0.5832674 270 N 0 16 D36
TOP 156 3.6614179 0.5332674 270 N 248 306 D37
TOP 157 3.6614179 0.4832674 270 N 0 11 D38
TOP 158 3.6614179 0.4332674 270 N 248 311 D39
TOP 159 3.6614179 0.3832674 270 N 0 7 D40
TOP 160 3.6114179 2.3332674 270 N 248 159 E1
TOP 161 3.6114179 2.2832674 270 N 0 202 E2
TOP 162 3.6114179 2.2332674 270 N 0 203 E3
TOP 163 3.6114179 2.1832674 270 N 248 165 E4
TOP 164 3.6114179 2.1332674 270 N 248 180 E5
TOP 165 3.6114179 2.0832674 270 N 0 187 E6
TOP 166 3.6114179 2.0332674 270 N 0 186 E7
TOP 167 3.6114179 1.9832674 270 N 248 190 E8
TOP 168 3.6114179 1.9332674 270 N 0 172 E9
TOP 169 3.6114179 1.8832674 270 N 0 167 E10
TOP 170 3.6114179 1.8332674 270 N 248 197 E11
TOP 171 3.6114179 1.7832674 270 N 0 163 E12
TOP 172 3.6114179 1.7332674 270 N 0 147 E13
TOP 173 3.6114179 1.6832674 270 N 248 212 E14
TOP 174 3.6114179 1.6332674 270 N 0 146 E15
TOP 175 3.6114179 1.5832674 270 N 0 136 E16
TOP 176 3.6114179 1.5332674 270 N 248 233 E17
TOP 177 3.6114179 1.4832674 270 N 0 117 E18
TOP 178 3.6114179 1.4332674 270 N 0 114 E19
TOP 179 3.6114179 1.3832674 270 N 248 239 E20
TOP 180 3.6114179 1.3332674 270 N 0 109 E21
TOP 181 3.6114179 1.2832674 270 N 0 84 E22
TOP 182 3.6114179 1.2332674 270 N 248 256 E23
TOP 183 3.6114179 1.1832674 270 N 0 78 E24
TOP 184 3.6114179 1.1332674 270 N 0 75 E25
TOP 185 3.6114179 1.0832674 270 N 248 263 E26
TOP 186 3.6114179 1.0332674 270 N 0 70 E27
TOP 187 3.6114179 0.9832674 270 N 0 63 E28
TOP 188 3.6114179 0.9332674 270 N 248 279 E29
TOP 189 3.6114179 0.8832674 270 N 0 45 E30
TOP 190 3.6114179 0.8332674 270 N 0 43 E31
TOP 191 3.6114179 0.7832674 270 N 248 284 E32
TOP 192 3.6114179 0.7332674 270 N 0 40 E33
TOP 193 3.6114179 0.6832674 270 N 0 37 E34
TOP 194 3.6114179 0.6332674 270 N 248 301 E35
TOP 195 3.6114179 0.5832674 270 N 0 17 E36
TOP 196 3.6114179 0.5332674 270 N 0 14 E37
TOP 197 3.6114179 0.4832674 270 N 248 308 E38
TOP 198 3.6114179 0.4332674 270 N 247 3 E39
TOP 199 3.6114179 0.3832674 270 N 248 313 E40
TOP 200 3.5074179 0.1182672 90 N 0 259 empty-1
TOP 201 3.5074179 2.5982672 90 N 0 260 empty-2
TOP 202 3.4663392 0.2877556 270 N 0 261 empty-3
TOP 203 3.5864179 2.4287792 270 N 0 262 empty-4
TOP 204 3.5614179 2.3332674 270 N 244 0 F1
TOP 205 3.5614179 2.2832674 270 N 248 161 F2
TOP 206 3.5614179 2.2332674 270 N 248 162 F3
TOP 207 3.5614179 2.1832674 270 N 0 190 F4
TOP 208 3.5614179 2.1332674 270 N 0 189 F5
TOP 209 3.5614179 2.0832674 270 N 248 179 F6
TOP 210 3.5614179 2.0332674 270 N 0 188 F7
TOP 211 3.5614179 1.9832674 270 N 0 174 F8
TOP 212 3.5614179 1.9332674 270 N 248 193 F9
TOP 213 3.5614179 1.8832674 270 N 0 168 F10
TOP 214 3.5614179 1.8332674 270 N 0 164 F11
TOP 215 3.5614179 1.7832674 270 N 248 199 F12
TOP 216 3.5614179 1.7332674 270 N 0 149 F13
TOP 217 3.5614179 1.6832674 270 N 0 148 F14
TOP 218 3.5614179 1.6332674 270 N 248 211 F15
TOP 219 3.5614179 1.5832674 270 N 0 137 F16
TOP 220 3.5614179 1.5332674 270 N 0 133 F17
TOP 221 3.5614179 1.4832674 270 N 248 224 F18
TOP 222 3.5614179 1.4332674 270 N 0 127 F19
TOP 223 3.5614179 1.3832674 270 N 0 124 F20
TOP 224 3.5614179 1.3332674 270 N 248 229 F21
TOP 225 3.5614179 1.2832674 270 N 0 102 F22
TOP 226 3.5614179 1.2332674 270 N 0 99 F23
TOP 227 3.5614179 1.1832674 270 N 248 248 F24
TOP 228 3.5614179 1.1332674 270 N 0 92 F25
TOP 229 3.5614179 1.0832674 270 N 0 90 F26
TOP 230 3.5614179 1.0332674 270 N 248 253 F27
TOP 231 3.5614179 0.9832674 270 N 0 64 F28
TOP 232 3.5614179 0.9332674 270 N 0 60 F29
TOP 233 3.5614179 0.8832674 270 N 248 271 F30
TOP 234 3.5614179 0.8332674 270 N 0 55 F31
TOP 235 3.5614179 0.7832674 270 N 0 52 F32
TOP 236 3.5614179 0.7332674 270 N 248 276 F33
TOP 237 3.5614179 0.6832674 270 N 0 48 F34
TOP 238 3.5614179 0.6332674 270 N 0 30 F35
TOP 239 3.5614179 0.5832674 270 N 248 303 F36
TOP 240 3.5614179 0.5332674 270 N 0 23 F37
TOP 241 3.5614179 0.4832674 270 N 0 12 F38
TOP 242 3.5614179 0.4332674 270 N 248 298 F39
TOP 243 3.5614179 0.3832674 270 N 247 2 F40
TOP 244 3.5114179 2.3332674 270 N 248 157 G1
TOP 245 3.5114179 2.2832674 270 N 0 207 G2
TOP 246 3.5114179 2.2332674 270 N 0 205 G3
TOP 247 3.5114179 2.1832674 270 N 248 177 G4
TOP 248 3.5114179 2.1332674 270 N 248 178 G5
TOP 249 3.5114179 2.0832674 270 N 69 1 G6
TOP 250 3.5114179 2.0332674 270 N 0 177 G7
TOP 251 3.5114179 1.9832674 270 N 248 189 G8
TOP 252 3.5114179 1.9332674 270 N 53 1 G9
TOP 253 3.5114179 1.8832674 270 N 0 169 G10
TOP 254 3.5114179 1.8332674 270 N 248 196 G11
TOP 255 3.5114179 1.7832674 270 N 71 1 G12
TOP 256 3.5114179 1.7332674 270 N 0 150 G13
TOP 257 3.5114179 1.6832674 270 N 248 210 G14
TOP 258 3.5114179 1.6332674 270 N 77 1 G15
TOP 259 3.5114179 1.5832674 270 N 0 138 G16
TOP 260 3.5114179 1.5332674 270 N 248 221 G17
TOP 261 3.5114179 1.4832674 270 N 0 131 G18
TOP 262 3.5114179 1.4332674 270 N 0 128 G19
TOP 263 3.5114179 1.3832674 270 N 248 226 G20
TOP 264 3.5114179 1.3332674 270 N 51 0 G21
TOP 265 3.5114179 1.2832674 270 N 0 103 G22
TOP 266 3.5114179 1.2332674 270 N 248 245 G23
TOP 267 3.5114179 1.1832674 270 N 0 97 G24
TOP 268 3.5114179 1.1332674 270 N 0 93 G25
TOP 269 3.5114179 1.0832674 270 N 248 251 G26
TOP 270 3.5114179 1.0332674 270 N 0 87 G27
TOP 271 3.5114179 0.9832674 270 N 90 0 G28
TOP 272 3.5114179 0.9332674 270 N 248 268 G29
TOP 273 3.5114179 0.8832674 270 N 89 0 G30
TOP 274 3.5114179 0.8332674 270 N 88 0 G31
TOP 275 3.5114179 0.7832674 270 N 248 273 G32
TOP 276 3.5114179 0.7332674 270 N 3 0 G33
TOP 277 3.5114179 0.6832674 270 N 0 49 G34
TOP 278 3.5114179 0.6332674 270 N 248 291 G35
TOP 279 3.5114179 0.5832674 270 N 0 28 G36
TOP 280 3.5114179 0.5332674 270 N 0 24 G37
TOP 281 3.5114179 0.4832674 270 N 248 295 G38
TOP 282 3.5114179 0.4332674 270 N 247 0 G39
TOP 283 3.5114179 0.3832674 270 N 248 300 G40
TOP 284 3.4614179 2.3332674 270 N 0 209 H1
TOP 285 3.4614179 2.2832674 270 N 243 0 H2
TOP 286 3.4614179 2.2332674 270 N 248 164 H3
TOP 287 3.4614179 2.1832674 270 N 49 0 H4
TOP 288 3.4614179 2.1332674 270 N 0 191 H5
TOP 289 3.4614179 2.0832674 270 N 248 176 H6
TOP 290 3.4614179 2.0332674 270 N 75 1 H7
TOP 291 3.4614179 1.9832674 270 N 0 176 H8
TOP 292 3.4614179 1.9332674 270 N 248 192 H9
TOP 293 3.4614179 1.8832674 270 N 73 1 H10
TOP 294 3.4614179 1.8332674 270 N 0 166 H11
TOP 295 3.4614179 1.7832674 270 N 248 208 H12
TOP 296 3.4614179 1.7332674 270 N 70 1 H13
TOP 297 3.4614179 1.6832674 270 N 0 151 H14
TOP 298 3.4614179 1.6332674 270 N 248 209 H15
TOP 299 3.4614179 1.5832674 270 N 78 1 H16
TOP 300 3.4614179 1.5332674 270 N 0 134 H17
TOP 301 3.4614179 1.4832674 270 N 248 223 H18
TOP 302 3.4614179 1.4332674 270 N 80 1 H19
TOP 303 3.4614179 1.3832674 270 N 0 125 H20
TOP 304 3.4614179 1.3332674 270 N 248 228 H21
TOP 305 3.4614179 1.2832674 270 N 0 104 H22
TOP 306 3.4614179 1.2332674 270 N 0 100 H23
TOP 307 3.4614179 1.1832674 270 N 248 247 H24
TOP 308 3.4614179 1.1332674 270 N 0 94 H25
TOP 309 3.4614179 1.0832674 270 N 0 91 H26
TOP 310 3.4614179 1.0332674 270 N 248 252 H27
TOP 311 3.4614179 0.9832674 270 N 0 65 H28
TOP 312 3.4614179 0.9332674 270 N 0 61 H29
TOP 313 3.4614179 0.8832674 270 N 248 270 H30
TOP 314 3.4614179 0.8332674 270 N 0 56 H31
TOP 315 3.4614179 0.7832674 270 N 0 53 H32
TOP 316 3.4614179 0.7332674 270 N 248 275 H33
TOP 317 3.4614179 0.6832674 270 N 0 50 H34
TOP 318 3.4614179 0.6332674 270 N 0 31 H35
TOP 319 3.4614179 0.5832674 270 N 248 292 H36
TOP 320 3.4614179 0.5332674 270 N 0 25 H37
TOP 321 3.4614179 0.4832674 270 N 0 22 H38
TOP 322 3.4614179 0.4332674 270 N 248 297 H39
TOP 323 3.4614179 0.3832674 270 N 247 1 H40
TOP 324 3.4114179 2.3332674 270 N 248 158 J1
TOP 325 3.4114179 2.2832674 270 N 0 206 J2
TOP 326 3.4114179 2.2332674 270 N 0 204 J3
TOP 327 3.4114179 2.1832674 270 N 248 174 J4
TOP 328 3.4114179 2.1332674 270 N 248 175 J5
TOP 329 3.4114179 2.0832674 270 N 0 192 J6
TOP 330 3.4114179 2.0332674 270 N 0 179 J7
TOP 331 3.4114179 1.9832674 270 N 248 188 J8
TOP 332 3.4114179 1.9332674 270 N 0 173 J9
TOP 333 3.4114179 1.8832674 270 N 0 170 J10
TOP 334 3.4114179 1.8332674 270 N 248 195 J11
TOP 335 3.4114179 1.7832674 270 N 0 154 J12
TOP 336 3.4114179 1.7332674 270 N 0 153 J13
TOP 337 3.4114179 1.6832674 270 N 248 207 J14
TOP 338 3.4114179 1.6332674 270 N 0 152 J15
TOP 339 3.4114179 1.5832674 270 N 0 139 J16
TOP 340 3.4114179 1.5332674 270 N 248 220 J17
TOP 341 3.4114179 1.4832674 270 N 0 132 J18
TOP 342 3.4114179 1.4332674 270 N 0 129 J19
TOP 343 3.4114179 1.3832674 270 N 248 225 J20
TOP 344 3.4114179 1.3332674 270 N 0 123 J21
TOP 345 3.4114179 1.2832674 270 N 0 105 J22
TOP 346 3.4114179 1.2332674 270 N 248 244 J23
TOP 347 3.4114179 1.1832674 270 N 0 98 J24
TOP 348 3.4114179 1.1332674 270 N 0 95 J25
TOP 349 3.4114179 1.0832674 270 N 248 250 J26
TOP 350 3.4114179 1.0332674 270 N 0 88 J27
TOP 351 3.4114179 0.9832674 270 N 0 85 J28
TOP 352 3.4114179 0.9332674 270 N 248 267 J29
TOP 353 3.4114179 0.8832674 270 N 0 59 J30
TOP 354 3.4114179 0.8332674 270 N 0 58 J31
TOP 355 3.4114179 0.7832674 270 N 248 272 J32
TOP 356 3.4114179 0.7332674 270 N 0 51 J33
TOP 357 3.4114179 0.6832674 270 N 0 33 J34
TOP 358 3.4114179 0.6332674 270 N 248 290 J35
TOP 359 3.4114179 0.5832674 270 N 0 29 J36
TOP 360 3.4114179 0.5332674 270 N 0 26 J37
TOP 361 3.4114179 0.4832674 270 N 248 294 J38
TOP 362 3.4114179 0.4332674 270 N 0 20 J39
TOP 363 3.4114179 0.3832674 270 N 248 299 J40
TOP 364 3.3614179 2.3332674 270 N 0 208 K1
TOP 365 3.3614179 2.2832674 270 N 248 160 K2
TOP 366 3.3614179 2.2332674 270 N 248 163 K3
TOP 367 3.3614179 2.1832674 270 N 0 194 K4
TOP 368 3.3614179 2.1332674 270 N 0 193 K5
TOP 369 3.3614179 2.0832674 270 N 248 173 K6
TOP 370 3.3614179 2.0332674 270 N 0 178 K7
TOP 371 3.3614179 1.9832674 270 N 0 175 K8
TOP 372 3.3614179 1.9332674 270 N 248 191 K9
TOP 373 3.3614179 1.8832674 270 N 0 171 K10
TOP 374 3.3614179 1.8332674 270 N 0 165 K11
TOP 375 3.3614179 1.7832674 270 N 248 198 K12
TOP 376 3.3614179 1.7332674 270 N 0 156 K13
TOP 377 3.3614179 1.6832674 270 N 0 155 K14
TOP 378 3.3614179 1.6332674 270 N 248 219 K15
TOP 379 3.3614179 1.5832674 270 N 0 140 K16
TOP 380 3.3614179 1.5332674 270 N 0 135 K17
TOP 381 3.3614179 1.4832674 270 N 248 222 K18
TOP 382 3.3614179 1.4332674 270 N 0 130 K19
TOP 383 3.3614179 1.3832674 270 N 0 126 K20
TOP 384 3.3614179 1.3332674 270 N 248 227 K21
TOP 385 3.3614179 1.2832674 270 N 0 106 K22
TOP 386 3.3614179 1.2332674 270 N 0 101 K23
TOP 387 3.3614179 1.1832674 270 N 248 246 K24
TOP 388 3.3614179 1.1332674 270 N 0 96 K25
TOP 389 3.3614179 1.0832674 270 N 248 249 K26
TOP 390 3.3614179 1.0332674 270 N 0 89 K27
TOP 391 3.3614179 0.9832674 270 N 0 86 K28
TOP 392 3.3614179 0.9332674 270 N 0 62 K29
TOP 393 3.3614179 0.8832674 270 N 248 269 K30
TOP 394 3.3614179 0.8332674 270 N 0 57 K31
TOP 395 3.3614179 0.7832674 270 N 0 54 K32
TOP 396 3.3614179 0.7332674 270 N 248 274 K33
TOP 397 3.3614179 0.6832674 270 N 0 34 K34
TOP 398 3.3614179 0.6332674 270 N 0 32 K35
TOP 399 3.3614179 0.5832674 270 N 248 293 K36
TOP 400 3.3614179 0.5332674 270 N 0 27 K37
TOP 401 3.3614179 0.4832674 270 N 0 21 K38
TOP 402 3.3614179 0.4332674 270 N 248 296 K39
TOP 403 3.3614179 0.3832674 270 N 0 19 K40
#
# CMP 64
CMP 2 1.069292 0.7795141 270 N R5 ERA-2AEB103X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thin Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDM0000/AOA0000C307.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERA-2AEB103X'
PRP Power_(Watts) '0.063W, 1/16W'
PRP Ratings 'AEC-Q200'
PRP Resistance '10 kO'
PRP Series 'ERA-2A'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P10KDCCT-ND'
PRP Temperature_Coefficient '±25ppm/°C'
PRP Tolerance '±0.1%'
PRP UniqueID 'RSMD040200315'
PRP Value '10 kO'
TOP 0 1.069292 0.7598291 0 N 168 0 1
TOP 1 1.069292 0.7991992 0 N 238 11 2
#
# CMP 65
CMP 2 1.0357014 0.7795141 270 N R7 ERA-2AEB3742X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thin Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDM0000/AOA0000C307.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERA-2AEB3742X'
PRP Power_(Watts) '0.063W, 1/16W'
PRP Ratings 'AEC-Q200'
PRP Resistance '37.4 kO'
PRP Series 'ERA-2A'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P37.4KDCCT-ND'
PRP Temperature_Coefficient '±25ppm/°C'
PRP Tolerance '±0.1%'
PRP UniqueID 'RSMD040202418'
PRP Value '37.4 kO'
TOP 0 1.0357014 0.7598291 0 N 178 0 1
TOP 1 1.0357014 0.7991992 0 N 238 12 2
#
# CMP 66
CMP 9 0.8329002 0.5164264 270 N C1 C2012X7R1H105K125AB ;0=1,1=0.0571
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://product.tdk.com/system/files/dam/doc/product/capacitor/ceramic/mlcc/catalog/mlcc_commercial_general_en.pdf'
PRP Manufacturer 'TDK Corporation'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0805'
PRP PartNumber 'C2012X7R1H105K125AB'
PRP Ratings '-'
PRP Series 'C'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '445-7547-1-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±10%'
PRP UniqueID 'capcc02687'
PRP Value '1 uF'
PRP Voltage_-_Rated '50V'
TOP 0 0.8329002 0.4868988 0 N 189 1 1
TOP 1 0.8329002 0.5459539 0 N 188 1 2
#
# CMP 67
CMP 2 1.1338825 0.621467 90 N R6 ERA-2AEB103X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thin Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDM0000/AOA0000C307.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERA-2AEB103X'
PRP Power_(Watts) '0.063W, 1/16W'
PRP Ratings 'AEC-Q200'
PRP Resistance '10 kO'
PRP Series 'ERA-2A'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P10KDCCT-ND'
PRP Temperature_Coefficient '±25ppm/°C'
PRP Tolerance '±0.1%'
PRP UniqueID 'RSMD040200315'
PRP Value '10 kO'
TOP 0 1.1338825 0.641152 180 N 179 0 1
TOP 1 1.1338825 0.6017819 180 N 237 6 2
#
# CMP 68
CMP 9 1.1981261 0.6288894 90 N C6 C2012X7S1E106K125AC ;0=1,1=0.0571
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://product.tdk.com/system/files/dam/doc/product/capacitor/ceramic/mlcc/catalog/mlcc_commercial_general_en.pdf'
PRP Manufacturer 'TDK Corporation'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0805'
PRP PartNumber 'C2012X7S1E106K125AC'
PRP Ratings '-'
PRP Series 'C'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.5'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '445-181600-1-ND'
PRP Temperature_Coefficient 'X7S'
PRP Tolerance '±10%'
PRP UniqueID 'capcc03511'
PRP Value '10 uF'
PRP Voltage_-_Rated '25V'
TOP 0 1.1981261 0.658417 180 N 248 87 1
TOP 1 1.1981261 0.5993619 180 N 237 7 2
#
# CMP 69
CMP 51 1.0617706 0.5393619 0 N D3 MBR130T1G ;0=1,1=0.0531
PRP Alt_Manufacturer 'Rohm Semiconductor'
PRP Alt_PartNumber 'RB160M-30TR'
PRP Color '-'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.onsemi.com/pub_link/Collateral/MBR130T1-D.PDF'
PRP CompType 'Diode'
PRP Current_Rating_(Amps) '-'
PRP datasheet 'https://www.onsemi.com/pdf/datasheet/mbr130t1-d.pdf'
PRP Length_(in) '-'
PRP Manufacturer 'Onsemi'
PRP Mount_Type 'SMD'
PRP PackageReference '-'
PRP PartNumber 'MBR130T1G'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'MBR130T1GOSCT-ND'
PRP Text1 '-'
PRP UniqueID 'cmp00438'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 1.1262391 0.5393619 0 N 237 15 1
TOP 1 0.9973021 0.5393619 0 N 248 318 2
#
# CMP 70
CMP 9 1.2335591 0.5336393 0 N C2 C2012X7R1H105K125AB ;0=1,1=0.0571
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://product.tdk.com/system/files/dam/doc/product/capacitor/ceramic/mlcc/catalog/mlcc_commercial_general_en.pdf'
PRP Manufacturer 'TDK Corporation'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0805'
PRP PartNumber 'C2012X7R1H105K125AB'
PRP Ratings '-'
PRP Series 'C'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '445-7547-1-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±10%'
PRP UniqueID 'capcc02687'
PRP Value '1 uF'
PRP Voltage_-_Rated '50V'
TOP 0 1.2630867 0.5336393 270 N 248 88 1
TOP 1 1.2040316 0.5336393 270 N 237 8 2
#
# CMP 71
CMP 2 1.2966248 0.2056218 0 N R4 ERA-2AEB1622X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thin Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDM0000/AOA0000C307.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERA-2AEB1622X'
PRP Power_(Watts) '0.063W, 1/16W'
PRP Ratings 'AEC-Q200'
PRP Resistance '16.2 kO'
PRP Series 'ERA-2A'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P16.2KDCCT-ND'
PRP Temperature_Coefficient '±25ppm/°C'
PRP Tolerance '±0.1%'
PRP UniqueID 'RSMD040200899'
PRP Value '16.2 kO'
TOP 0 1.3163098 0.2056218 270 N 248 89 1
TOP 1 1.2769397 0.2056218 270 N 187 1 2
#
# CMP 72
CMP 7 1.3228701 0.2984031 0 N C5 CGA3E2X7R1H102K080AA ;0=1,1=0.0394
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://product.tdk.com/system/files/dam/doc/product/capacitor/ceramic/mlcc/catalog/mlcc_automotive_general_en.pdf'
PRP Manufacturer 'TDK Corporation'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0603'
PRP PartNumber 'CGA3E2X7R1H102K080AA'
PRP Ratings 'AEC-Q200'
PRP Series 'CGA'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '0.9'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '445-5659-1-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±10%'
PRP UniqueID 'capcc03751'
PRP Value '0.001 uF'
PRP Voltage_-_Rated '50V'
TOP 0 1.3504292 0.2984031 270 N 248 90 1
TOP 1 1.2953111 0.2984031 270 N 186 1 2
#
# CMP 73
CMP 2 1.3102718 0.4086393 0 N R2 ERJ-2RKF4532X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF4532X'
PRP Power_(Watts) '0.1W, 1/10W'
PRP Ratings 'AEC-Q200'
PRP Resistance '45.3 kO'
PRP Series 'ERJ-2RK'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P45.3KLCT-ND'
PRP Temperature_Coefficient '±100ppm/°C'
PRP Tolerance '±1%'
PRP UniqueID 'RSMD040202774'
PRP Value '45.3 kO'
TOP 0 1.3299568 0.4086393 270 N 248 91 1
TOP 1 1.2905867 0.4086393 270 N 180 0 2
#
# CMP 74
CMP 9 1.2335591 0.4636393 0 N C3 C2012X7R1H105K125AB ;0=1,1=0.0571
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://product.tdk.com/system/files/dam/doc/product/capacitor/ceramic/mlcc/catalog/mlcc_commercial_general_en.pdf'
PRP Manufacturer 'TDK Corporation'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0805'
PRP PartNumber 'C2012X7R1H105K125AB'
PRP Ratings '-'
PRP Series 'C'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '445-7547-1-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±10%'
PRP UniqueID 'capcc02687'
PRP Value '1 uF'
PRP Voltage_-_Rated '50V'
TOP 0 1.2630867 0.4636393 270 N 248 92 1
TOP 1 1.2040316 0.4636393 270 N 237 9 2
#
# CMP 75
CMP 2 1.2167585 0.2584031 0 N R1 ERA-2AED104X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thin Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDM0000/AOA0000C307.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERA-2AED104X'
PRP Power_(Watts) '0.063W, 1/16W'
PRP Ratings 'AEC-Q200'
PRP Resistance '100 kO'
PRP Series 'ERA-2A'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P100KDECT-ND'
PRP Temperature_Coefficient '±25ppm/°C'
PRP Tolerance '±0.5%'
PRP UniqueID 'RSMD040200361'
PRP Value '100 kO'
TOP 0 1.2364435 0.2584031 270 N 187 2 1
TOP 1 1.1970734 0.2584031 270 N 181 1 2
#
# CMP 76
CMP 7 1.3040911 0.2484031 0 N C4 CGA3E2X7R1H102K080AA ;0=1,1=0.0394
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://product.tdk.com/system/files/dam/doc/product/capacitor/ceramic/mlcc/catalog/mlcc_automotive_general_en.pdf'
PRP Manufacturer 'TDK Corporation'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0603'
PRP PartNumber 'CGA3E2X7R1H102K080AA'
PRP Ratings 'AEC-Q200'
PRP Series 'CGA'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '0.9'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '445-5659-1-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±10%'
PRP UniqueID 'capcc03751'
PRP Value '0.001 uF'
PRP Voltage_-_Rated '50V'
TOP 0 1.3316502 0.2484031 270 N 248 93 1
TOP 1 1.2765321 0.2484031 270 N 187 3 2
#
# CMP 77
CMP 4 1.1338825 0.704144 270 N C8 CGA2B2X7R1H332K050BA ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://product.tdk.com/system/files/dam/doc/product/capacitor/ceramic/mlcc/catalog/mlcc_automotive_general_en.pdf'
PRP Manufacturer 'TDK Corporation'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0402'
PRP PartNumber 'CGA2B2X7R1H332K050BA'
PRP Ratings 'AEC-Q200'
PRP Series 'CGA'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.55'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '445-6891-1-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±10%'
PRP UniqueID 'capcc04738'
PRP Value '3300 pF'
PRP Voltage_-_Rated '50V'
TOP 0 1.1338825 0.684459 0 N 248 94 1
TOP 1 1.1338825 0.7238291 0 N 185 0 2
#
# CMP 78
CMP 9 0.9524967 0.621467 270 N C7 C2012X7S1A226M125AC ;0=1,1=0.0571
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet '-'
PRP Manufacturer 'TDK Corporation'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0805'
PRP PartNumber 'C2012X7S1A226M125AC'
PRP Ratings '-'
PRP Series '-'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-key'
PRP Supplier_Part_Number_1 '445-14560-1-ND'
PRP Temperature_Coefficient 'X7S'
PRP Tolerance '±20%'
PRP UniqueID 'capcc09395'
PRP Value '22 uF'
PRP Voltage_-_Rated '10V'
TOP 0 0.9524967 0.5919394 0 N 248 95 1
TOP 1 0.9524967 0.6509945 0 N 238 13 2
#
# CMP 79
CMP 2 1.0021014 0.7795142 90 N R8 ERJ-2RKF1202X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1202X'
PRP Power_(Watts) '0.1W, 1/10W'
PRP Ratings 'AEC-Q200'
PRP Resistance '12 kO'
PRP Series 'ERJ-2RK'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P12.0KLCT-ND'
PRP Temperature_Coefficient '±100ppm/°C'
PRP Tolerance '±1%'
PRP UniqueID 'RSMD040200519'
PRP Value '12 kO'
TOP 0 1.0021014 0.7991992 180 N 248 96 1
TOP 1 1.0021014 0.7598291 180 N 178 1 2
#
# CMP 80
CMP 50 0.9610104 0.3031772 270 N D2 SMBJ15CA ;0=1,1=0.1043
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color '-'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://www.fairchildsemi.com/datasheets/SM/SMBJ100A.pdf'
PRP CompType 'Diode TVS'
PRP Current_Rating_(Amps) '-'
PRP datasheet 'https://www.littelfuse.com/~/media/electronics/datasheets/tvs_diodes/littelfuse_tvs_diode_smbj_datasheet.pdf.pdf'
PRP Length_(in) '-'
PRP Manufacturer 'Littlefuse'
PRP Mount_Type 'SMD'
PRP PackageReference '-'
PRP PartNumber 'SMBJ15CA'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'SMBJ15CALFCT-ND'
PRP Text1 '-'
PRP UniqueID 'cmp00440'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 0.9610104 0.2161693 180 N 188 7 1
TOP 1 0.9610104 0.3901851 180 N 189 3 2
#
# CMP 81
CMP 24 0.8372312 0.3181581 90 N Q1 CSD15571Q2 ;0=1,1=0.0315
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color '-'
PRP CompType 'FET'
PRP Current_Rating_(Amps) '-'
PRP datasheet '-'
PRP Length_(in) '-'
PRP Manufacturer 'Texas Instruments'
PRP Mount_Type 'SMD'
PRP PackageReference 'WSON-8'
PRP PartNumber 'CSD15571Q2'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '296-39992-1-ND'
PRP Text1 '-'
PRP UniqueID 'cmp00159'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 0.8116406 0.3565439 90 N 188 6 1
TOP 1 0.8372312 0.3565439 90 N 188 5 2
TOP 2 0.8628217 0.3565439 90 N 189 2 3
TOP 3 0.8628217 0.2797722 90 N 248 132 4
TOP 4 0.8372312 0.2797722 90 N 188 4 5
TOP 5 0.8116406 0.2797722 90 N 188 3 6
TOP 6 0.8628218 0.3144179 90 N 248 131 7
TOP 7 0.8244359 0.3181581 90 N 188 2 8
#
# CMP 82
CMP 8 0.6841993 0.1198529 0 N R3 ERJ-HP6F1002V ;0=1,1=0.0571
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDQ0000/ast-ind-151033.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 175°C'
PRP PackageReference '0805'
PRP PartNumber 'ERJ-HP6F1002V'
PRP Power_(Watts) '0.5W, 1/2W'
PRP Ratings 'AEC-Q200'
PRP Resistance '10 kO'
PRP Series 'ERJ-HP6'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '10-ERJ-HP6F1002VCT-ND'
PRP Temperature_Coefficient '±100ppm/°C'
PRP Tolerance '±1%'
PRP UniqueID 'RSMD080502076'
PRP Value '10 kO'
TOP 0 0.7137269 0.1198529 270 N 248 97 1
TOP 1 0.6546718 0.1198529 270 N 184 0 2
#
# CMP 83
CMP 49 1.0524967 0.6824905 270 N U3 TPS82140SILR ;0=1,1=0.0602
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber 'TPS82140SILT'
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/tps82140.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/tps82140'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/tps82140/datasheet'
PRP CompType 'Switcher'
PRP Manufacturer 'Texas Instruments'
PRP PartNumber 'TPS82140SILR'
PRP Text1 '2A, Vin = 3V ? 17V'
TOP 0 1.0908825 0.6411519 270 N 179 1 1
TOP 1 1.065292 0.6411519 270 N 237 14 2
TOP 2 1.0397014 0.6411519 270 N 248 316 3
TOP 3 1.0141109 0.6411519 270 N 238 42 4
TOP 4 1.0141109 0.7238291 270 N 238 43 5
TOP 5 1.0397014 0.7238291 270 N 178 2 6
TOP 6 1.065292 0.7238291 270 N 168 1 7
TOP 7 1.0908825 0.7238291 270 N 185 1 8
TOP 8 1.0524967 0.6824905 270 N 248 317 9
TOP 9 1.0820243 0.6824905 270 N 248 490 9
TOP 10 1.0524967 0.6824905 270 N 248 491 9
TOP 11 1.0229691 0.6824905 270 N 248 492 9
#
# CMP 84
CMP 25 1.2012166 0.3535212 270 N U2 TPS259261DRC ;0=1,1=0.0394
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color '-'
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/tps25926.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/tps25926'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/tps25926/datasheet'
PRP CompType 'eFuse'
PRP Current_Rating_(Amps) '-'
PRP datasheet 'http://www.ti.com/lit/ds/symlink/tps25926.pdf'
PRP Length_(in) '-'
PRP Manufacturer 'Texas Instruments'
PRP Mount_Type 'SMD'
PRP PackageReference 'VSON-10'
PRP PartNumber 'TPS259261DRC'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Supplier_1 'Digi-Key'
PRP Text1 '-'
PRP UniqueID 'cmp00157'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 1.2405867 0.2984031 270 N 186 2 1
TOP 1 1.2209017 0.2984031 270 N 187 4 2
TOP 2 1.2012166 0.2984031 270 N 181 4 3
TOP 3 1.1815316 0.2984031 270 N 181 3 4
TOP 4 1.1618465 0.2984031 270 N 181 2 5
TOP 5 1.1618465 0.4086393 270 N 237 12 6
TOP 6 1.1815315 0.4086393 270 N 237 11 7
TOP 7 1.2012166 0.4086393 270 N 237 10 8
TOP 8 1.2209016 0.4086393 270 N 0 0 9
TOP 9 1.2405867 0.4086393 270 N 180 1 10
TOP 10 1.2012166 0.3535211 270 N 248 98 11
TOP 11 1.2012166 0.376159 270 N 248 448 11
TOP 12 1.163815 0.3535212 270 N 248 449 11
TOP 13 1.2012166 0.3308834 270 N 248 450 11
TOP 14 1.2386182 0.3535212 270 N 248 451 11
#
# CMP 85
CMP 26 1.3303149 2.0950989 270 N U16 SN74LVC1G125DRL ;0=1,1=0.0236
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color '-'
PRP CompType 'Buffer'
PRP Current_Rating_(Amps) '-'
PRP datasheet '-'
PRP Length_(in) '-'
PRP Manufacturer 'Texas Instruments'
PRP Mount_Type 'SMD'
PRP PackageReference 'SOT-5'
PRP PartNumber 'SN74LVC1G125DRL'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Supplier_1 'Digi-Key'
PRP Text1 '-'
PRP UniqueID 'SN74LVC1G125DRL'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 1.35 2.065965 0 N 7 1 1
TOP 1 1.330315 2.065965 0 N 248 330 2
TOP 2 1.3106299 2.065965 0 N 248 331 3
TOP 3 1.3106299 2.1242328 0 N 2 1 4
TOP 4 1.35 2.1242328 0 N 170 20 5
#
# CMP 86
CMP 2 1.4121265 2.3189514 270 N R61 ERA-2AEB103X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thin Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDM0000/AOA0000C307.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERA-2AEB103X'
PRP Power_(Watts) '0.063W, 1/16W'
PRP Ratings 'AEC-Q200'
PRP Resistance '10 kO'
PRP Series 'ERA-2A'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P10KDCCT-ND'
PRP Temperature_Coefficient '±25ppm/°C'
PRP Tolerance '±0.1%'
PRP UniqueID 'RSMD040200315'
PRP Value '10 kO'
TOP 0 1.4121265 2.2992664 0 N 198 4 1
TOP 1 1.4121265 2.3386365 0 N 170 19 2
#
# CMP 87
CMP 2 1.478895 2.3004698 270 N R60 ERA-2AEB103X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thin Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDM0000/AOA0000C307.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERA-2AEB103X'
PRP Power_(Watts) '0.063W, 1/16W'
PRP Ratings 'AEC-Q200'
PRP Resistance '10 kO'
PRP Series 'ERA-2A'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P10KDCCT-ND'
PRP Temperature_Coefficient '±25ppm/°C'
PRP Tolerance '±0.1%'
PRP UniqueID 'RSMD040200315'
PRP Value '10 kO'
TOP 0 1.478895 2.2807848 0 N 191 0 1
TOP 1 1.478895 2.3201549 0 N 170 5 2
#
# CMP 88
CMP 2 1.4442099 2.3054698 270 N R59 ERA-2AEB103X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thin Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDM0000/AOA0000C307.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERA-2AEB103X'
PRP Power_(Watts) '0.063W, 1/16W'
PRP Ratings 'AEC-Q200'
PRP Resistance '10 kO'
PRP Series 'ERA-2A'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P10KDCCT-ND'
PRP Temperature_Coefficient '±25ppm/°C'
PRP Tolerance '±0.1%'
PRP UniqueID 'RSMD040200315'
PRP Value '10 kO'
TOP 0 1.4442099 2.2857848 0 N 190 0 1
TOP 1 1.4442099 2.3251549 0 N 170 6 2
#
# CMP 89
CMP 2 1.1199709 2.2430212 0 N R58 ERA-2AEB103X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thin Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDM0000/AOA0000C307.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERA-2AEB103X'
PRP Power_(Watts) '0.063W, 1/16W'
PRP Ratings 'AEC-Q200'
PRP Resistance '10 kO'
PRP Series 'ERA-2A'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P10KDCCT-ND'
PRP Temperature_Coefficient '±25ppm/°C'
PRP Tolerance '±0.1%'
PRP UniqueID 'RSMD040200315'
PRP Value '10 kO'
TOP 0 1.1396559 2.2430212 270 N 206 0 1
TOP 1 1.1002858 2.2430212 270 N 248 99 2
#
# CMP 90
CMP 2 1.3379501 2.1793243 270 N R57 ERJ-2RKF1000X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1000X'
PRP Power_(Watts) '0.1W, 1/10W'
PRP Ratings 'AEC-Q200'
PRP Resistance '100 O'
PRP Series 'ERJ-2RK'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P100LCT-ND'
PRP Temperature_Coefficient '±100ppm/°C'
PRP Tolerance '±1%'
PRP UniqueID 'RSMD040200375'
PRP Value '100 O'
TOP 0 1.3379501 2.1596393 0 N 2 0 1
TOP 1 1.3379501 2.1990094 0 N 206 4 2
#
# CMP 91
CMP 2 1.3094069 2.247336 0 N R56 ERA-2AEB103X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thin Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDM0000/AOA0000C307.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERA-2AEB103X'
PRP Power_(Watts) '0.063W, 1/16W'
PRP Ratings 'AEC-Q200'
PRP Resistance '10 kO'
PRP Series 'ERA-2A'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P10KDCCT-ND'
PRP Temperature_Coefficient '±25ppm/°C'
PRP Tolerance '±0.1%'
PRP UniqueID 'RSMD040200315'
PRP Value '10 kO'
TOP 0 1.3290919 2.247336 270 N 170 7 1
TOP 1 1.2897218 2.247336 270 N 206 1 2
#
# CMP 92
CMP 2 0.581221 1.9780052 270 N R54 ERA-2AEB103X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thin Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDM0000/AOA0000C307.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERA-2AEB103X'
PRP Power_(Watts) '0.063W, 1/16W'
PRP Ratings 'AEC-Q200'
PRP Resistance '10 kO'
PRP Series 'ERA-2A'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P10KDCCT-ND'
PRP Temperature_Coefficient '±25ppm/°C'
PRP Tolerance '±0.1%'
PRP UniqueID 'RSMD040200315'
PRP Value '10 kO'
TOP 0 0.581221 1.9583202 0 N 208 0 1
TOP 1 0.581221 1.9976903 0 N 238 14 2
#
# CMP 93
CMP 2 0.5418509 1.9780052 270 N R53 ERA-2AEB103X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thin Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDM0000/AOA0000C307.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERA-2AEB103X'
PRP Power_(Watts) '0.063W, 1/16W'
PRP Ratings 'AEC-Q200'
PRP Resistance '10 kO'
PRP Series 'ERA-2A'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P10KDCCT-ND'
PRP Temperature_Coefficient '±25ppm/°C'
PRP Tolerance '±0.1%'
PRP UniqueID 'RSMD040200315'
PRP Value '10 kO'
TOP 0 0.5418509 1.9583202 0 N 211 0 1
TOP 1 0.5418509 1.9976903 0 N 238 15 2
#
# CMP 94
CMP 2 0.6256013 2.3874972 0 N R50 ERJ-2GEJ222X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://b2b-api.panasonic.eu/file_stream/pids/fileversion/1242'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GEJ222X'
PRP Power_(Watts) '0.1W, 1/10W'
PRP Ratings 'AEC-Q200'
PRP Resistance '2.2 kO'
PRP Series 'ERJ-2G'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P2.2KJCT-ND'
PRP Temperature_Coefficient '±200ppm/°C'
PRP Tolerance '±5%'
PRP UniqueID 'RSMD040201206'
PRP Value '2.2 kO'
TOP 0 0.6452863 2.3874972 270 N 225 0 1
TOP 1 0.6059162 2.3874972 270 N 223 0 2
#
# CMP 95
CMP 2 0.7583864 2.0805651 90 N R40 ERJ-2RKF1000X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1000X'
PRP Power_(Watts) '0.1W, 1/10W'
PRP Ratings 'AEC-Q200'
PRP Resistance '100 O'
PRP Series 'ERJ-2RK'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P100LCT-ND'
PRP Temperature_Coefficient '±100ppm/°C'
PRP Tolerance '±1%'
PRP UniqueID 'RSMD040200375'
PRP Value '100 O'
TOP 0 0.7583864 2.1002501 180 N 193 0 1
TOP 1 0.7583864 2.06088 180 N 219 0 2
#
# CMP 96
CMP 23 1.245414 2.323596 180 N U13 TMUX1136DGS ;0=1,1=0.0217
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color '-'
PRP CompType 'MUX'
PRP Current_Rating_(Amps) '-'
PRP datasheet '-'
PRP Length_(in) '-'
PRP Manufacturer 'Texas Instruments'
PRP Mount_Type 'SMD'
PRP PackageReference 'USON-10'
PRP PartNumber 'TMUX1136DQA'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '296-TMUX1136DQARCT-ND'
PRP Text1 'SEL: Low = B?D, High = A?D'
PRP UniqueID 'cmp00307'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 1.228977 2.2842259 90 N 205 0 1
TOP 1 1.228977 2.3039109 90 N 239 0 2
TOP 2 1.228977 2.3235959 90 N 248 130 3
TOP 3 1.228977 2.343281 90 N 240 0 4
TOP 4 1.228977 2.362966 90 N 205 1 5
TOP 5 1.261851 2.362966 90 N 196 0 6
TOP 6 1.261851 2.343281 90 N 222 2 7
TOP 7 1.261851 2.3235959 90 N 238 37 8
TOP 8 1.261851 2.3039109 90 N 219 2 9
TOP 9 1.261851 2.2842259 90 N 194 0 10
#
# CMP 97
CMP 46 1.2267722 2.1625133 270 N U15 SN74CBTLV3257RSV ;0=1,1=0.0217
PRP Color '-'
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/sn74cbtlv3257.pdf'
PRP CompType 'MUX'
PRP Current_Rating_(Amps) '-'
PRP datasheet 'https://www.ti.com/lit/ds/symlink/sn74cbtlv3257.pdf?ts=1653214641522&ref_url=https%253A%252F%252Fwww.ti.com%252Fproduct%252FSN74CBTLV3257%253FkeyMatch%253DSN74CBTLV3257DGVR%2526tisearch%253Dsearch-everything%2526usecase%253DOPN'
PRP Length_(in) '-'
PRP Manufacturer 'Texas Instruments'
PRP Mount_Type 'SMD'
PRP PackageReference 'UQFN'
PRP PartNumber 'SN74CBTLV3257RSVR'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '296-35586-1-ND'
PRP Text1 'S: LOW = B1, HIGH = B2'
PRP UniqueID 'cmp00269'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 1.2503943 2.1329857 0 N 190 1 1
TOP 1 1.2346463 2.1310172 0 N 195 0 2
TOP 2 1.2188982 2.1310172 0 N 197 1 3
TOP 3 1.2031502 2.1310172 0 N 191 1 4
TOP 4 1.1795281 2.1388913 270 N 113 0 5
TOP 5 1.1795281 2.1546393 270 N 248 149 6
TOP 6 1.1795281 2.1703873 270 N 192 1 7
TOP 7 1.1795281 2.1861354 270 N 198 0 8
TOP 8 1.2031502 2.1940094 0 N 206 3 9
TOP 9 1.2188982 2.1940094 0 N 0 6 10
TOP 10 1.2346463 2.1940094 0 N 0 5 11
TOP 11 1.2503943 2.1940094 0 N 0 4 12
TOP 12 1.2740163 2.1861354 270 N 248 150 13
TOP 13 1.2740163 2.1703873 270 N 238 38 14
TOP 14 1.2740163 2.1546393 270 N 205 2 15
TOP 15 1.2740163 2.1388913 270 N 209 1 16
#
# CMP 98
CMP 4 1.5636087 0.6910239 270 N C80 GRT155R71E104KE01J ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet '-'
PRP Manufacturer 'Murata'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0402'
PRP PartNumber 'GRT155R71E104KE01J'
PRP Ratings '-'
PRP Series '-'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Digi-key'
PRP Supplier_Part_Number_1 '490-GRT155R71E104KE01JCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±10%'
PRP UniqueID 'capcc09401'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '25V'
TOP 0 1.5636087 0.6713389 0 N 248 100 1
TOP 1 1.5636087 0.710709 0 N 203 2 2
#
# CMP 99
CMP 18 1.5636083 0.5766927 90 N U18 TPS3125J18DBVR ;0=1,1=0.0571
PRP Alt_Manufacturer 'Texas Instruments'
PRP Alt_PartNumber 'TPS3125J18DBVT'
PRP Color '-'
PRP CompType 'Voltage Detector'
PRP Current_Rating_(Amps) '-'
PRP datasheet '-'
PRP Length_(in) '-'
PRP Manufacturer 'Texas Instruments'
PRP Mount_Type 'SMD'
PRP PackageReference 'SOT-23'
PRP PartNumber 'TPS3125J18DBVR'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Supplier_1 'Digi-Key'
PRP Text1 'VIT- = 1.68V (max)'
PRP UniqueID 'cmp00229'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 1.5262067 0.6278739 180 N 201 0 1
TOP 1 1.5636083 0.6278739 180 N 248 101 2
TOP 2 1.6010098 0.6278739 180 N 200 0 3
TOP 3 1.6010098 0.5255116 180 N 94 0 4
TOP 4 1.5262067 0.5255116 180 N 170 8 5
#
# CMP 100
CMP 2 1.5262067 0.691024 90 N R121 ERJ-U020R00X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDP0000/AOA0000C334.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-U020R00X'
PRP Power_(Watts) '0.1W, 1/10W'
PRP Ratings 'AEC-Q200'
PRP Resistance '0 O'
PRP Series 'ERJ-U02'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '10-ERJ-U020R00XCT-ND'
PRP Temperature_Coefficient '-100/ +600ppm/°C'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD040200004'
PRP Value '0 O'
TOP 0 1.5262067 0.710709 180 N 203 3 1
TOP 1 1.5262067 0.6713389 180 N 201 1 2
#
# CMP 101
CMP 2 0.5615359 2.5069816 270 N R49 ERA-2AEB103X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thin Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDM0000/AOA0000C307.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERA-2AEB103X'
PRP Power_(Watts) '0.063W, 1/16W'
PRP Ratings 'AEC-Q200'
PRP Resistance '10 kO'
PRP Series 'ERA-2A'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P10KDCCT-ND'
PRP Temperature_Coefficient '±25ppm/°C'
PRP Tolerance '±0.1%'
PRP UniqueID 'RSMD040200315'
PRP Value '10 kO'
TOP 0 0.5615359 2.4872966 0 N 224 0 1
TOP 1 0.5615359 2.5266667 0 N 238 16 2
#
# CMP 102
CMP 2 1.4962067 0.691024 90 N R120 ERJ-2GEJ104X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://b2b-api.panasonic.eu/file_stream/pids/fileversion/1242'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GEJ104X'
PRP Power_(Watts) '0.1W, 1/10W'
PRP Ratings 'AEC-Q200'
PRP Resistance '100 kO'
PRP Series 'ERJ-2G'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P100KJCT-ND'
PRP Temperature_Coefficient '±200ppm/°C'
PRP Tolerance '±5%'
PRP UniqueID 'RSMD040200354'
PRP Value '100 kO'
TOP 0 1.4962067 0.710709 180 N 203 4 1
TOP 1 1.4962067 0.6713389 180 N 170 9 2
#
# CMP 103
CMP 2 1.6010098 0.691024 90 N R128 ERJ-U020R00X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDP0000/AOA0000C334.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-U020R00X'
PRP Power_(Watts) '0.1W, 1/10W'
PRP Ratings 'AEC-Q200'
PRP Resistance '0 O'
PRP Series 'ERJ-U02'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '10-ERJ-U020R00XCT-ND'
PRP Temperature_Coefficient '-100/ +600ppm/°C'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD040200004'
PRP Value '0 O'
TOP 0 1.6010098 0.710709 180 N 203 5 1
TOP 1 1.6010098 0.6713389 180 N 200 1 2
#
# CMP 104
CMP 2 1.5867751 0.3347818 0 N R122 ERA-2AEB103X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thin Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDM0000/AOA0000C307.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERA-2AEB103X'
PRP Power_(Watts) '0.063W, 1/16W'
PRP Ratings 'AEC-Q200'
PRP Resistance '10 kO'
PRP Series 'ERA-2A'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P10KDCCT-ND'
PRP Temperature_Coefficient '±25ppm/°C'
PRP Tolerance '±0.1%'
PRP UniqueID 'RSMD040200315'
PRP Value '10 kO'
TOP 0 1.6064601 0.3347818 270 N 170 10 1
TOP 1 1.56709 0.3347818 270 N 202 0 2
#
# CMP 105
CMP 4 1.506576 0.4836491 180 N C81 GRT155R71E104KE01J ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet '-'
PRP Manufacturer 'Murata'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0402'
PRP PartNumber 'GRT155R71E104KE01J'
PRP Ratings '-'
PRP Series '-'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Digi-key'
PRP Supplier_Part_Number_1 '490-GRT155R71E104KE01JCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±10%'
PRP UniqueID 'capcc09401'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '25V'
TOP 0 1.486891 0.4836491 90 N 248 102 1
TOP 1 1.5262611 0.4836491 90 N 170 11 2
#
# CMP 106
CMP 12 1.0542525 2.1625133 180 N U14 SN74AVC4T774BQB ;0=1,1=0.2500
PRP Alt_Manufacturer 'Texas Instruments'
PRP Alt_PartNumber 'SN74AXC4T774BQB'
PRP Color '-'
PRP CompType 'Level Shifter'
PRP Current_Rating_(Amps) '-'
PRP datasheet 'https://www.ti.com/lit/ds/symlink/sn74avc4t774.pdf?ts=1653168494556&ref_url=https%253A%252F%252Fwww.ti.com%252Fproduct%252FSN74AVC4T774%253FkeyMatch%253DSN74AVC4T774%2526tisearch%253Dsearch-everything%2526usecase%253DGPN'
PRP Length_(in) '-'
PRP Manufacturer 'Texas Instruments'
PRP Mount_Type 'SMD'
PRP PackageReference 'WQFN-16'
PRP PartNumber 'SN74AVC4T774BQB'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Supplier_1 'Digi-Key'
PRP Text1 'DIR: Low = B?A, High = A?B'
PRP UniqueID 'cmp00170'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 1.04441 2.0975527 0 N 238 34 1
TOP 1 1.0089769 2.1133007 0 N 238 32 2
TOP 2 1.0089769 2.1329857 0 N 210 1 3
TOP 3 1.0089769 2.1526708 0 N 211 1 4
TOP 4 1.0089769 2.1723558 0 N 207 0 5
TOP 5 1.0089769 2.1920409 0 N 208 1 6
TOP 6 1.0089769 2.2117259 0 N 248 116 7
TOP 7 1.04441 2.2274739 0 N 238 31 8
TOP 8 1.064095 2.2274739 0 N 248 114 9
TOP 9 1.0995281 2.2117259 0 N 248 115 10
TOP 10 1.0995281 2.1920409 0 N 7 0 11
TOP 11 1.0995281 2.1723558 0 N 206 2 12
TOP 12 1.0995281 2.1526708 0 N 197 0 13
TOP 13 1.0995281 2.1329857 0 N 209 0 14
TOP 14 1.0995281 2.1133007 0 N 170 12 15
TOP 15 1.064095 2.0975527 0 N 238 33 16
TOP 16 1.0542525 2.1625133 0 N 248 113 17
TOP 17 1.0542525 2.1920409 0 N 248 454 17
TOP 18 1.0542525 2.1329857 0 N 248 455 17
#
# CMP 107
CMP 2 0.34 2.0303149 270 N R45 ERJ-2GEJ222X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://b2b-api.panasonic.eu/file_stream/pids/fileversion/1242'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GEJ222X'
PRP Power_(Watts) '0.1W, 1/10W'
PRP Ratings 'AEC-Q200'
PRP Resistance '2.2 kO'
PRP Series 'ERJ-2G'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P2.2KJCT-ND'
PRP Temperature_Coefficient '±200ppm/°C'
PRP Tolerance '±5%'
PRP UniqueID 'RSMD040201206'
PRP Value '2.2 kO'
TOP 0 0.34 2.0106299 0 N 248 103 1
TOP 1 0.34 2.05 0 N 213 0 2
#
# CMP 108
CMP 4 0.6702863 2.1685959 90 N C30 GRT155R71E104KE01J ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet '-'
PRP Manufacturer 'Murata'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0402'
PRP PartNumber 'GRT155R71E104KE01J'
PRP Ratings '-'
PRP Series '-'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Digi-key'
PRP Supplier_Part_Number_1 '490-GRT155R71E104KE01JCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±10%'
PRP UniqueID 'capcc09401'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '25V'
TOP 0 0.6702863 2.1882809 180 N 248 104 1
TOP 1 0.6702863 2.1489108 180 N 238 17 2
#
# CMP 109
CMP 7 0.8464179 2.1489108 180 N C35 CGA3E1X5R1A335K080AC ;0=1,1=0.0394
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://product.tdk.com/system/files/dam/doc/product/capacitor/ceramic/mlcc/catalog/mlcc_automotive_general_en.pdf'
PRP Manufacturer 'TDK Corporation'
PRP Operating_Temperature '-55°C ~ 85°C'
PRP PackageReference '0603'
PRP PartNumber 'CGA3E1X5R1A335K080AC'
PRP Ratings 'AEC-Q200'
PRP Series 'CGA'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '0.9'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '445-7879-1-ND'
PRP Temperature_Coefficient 'X5R'
PRP Tolerance '±10%'
PRP UniqueID 'capcc03130'
PRP Value '3.3 uF'
PRP Voltage_-_Rated '10V'
TOP 0 0.8188588 2.1489108 90 N 248 105 1
TOP 1 0.8739769 2.1489108 90 N 217 3 2
#
# CMP 110
CMP 4 0.8174415 2.3626115 270 N C41 GRT155R71E104KE01J ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet '-'
PRP Manufacturer 'Murata'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0402'
PRP PartNumber 'GRT155R71E104KE01J'
PRP Ratings '-'
PRP Series '-'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Digi-key'
PRP Supplier_Part_Number_1 '490-GRT155R71E104KE01JCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±10%'
PRP UniqueID 'capcc09401'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '25V'
TOP 0 0.8174415 2.3429265 0 N 248 106 1
TOP 1 0.8174415 2.3822966 0 N 238 18 2
#
# CMP 111
CMP 4 0.6993312 2.5119817 90 N C39 GRT155R71E104KE01J ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet '-'
PRP Manufacturer 'Murata'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0402'
PRP PartNumber 'GRT155R71E104KE01J'
PRP Ratings '-'
PRP Series '-'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Digi-key'
PRP Supplier_Part_Number_1 '490-GRT155R71E104KE01JCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±10%'
PRP UniqueID 'capcc09401'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '25V'
TOP 0 0.6993312 2.5316667 180 N 248 107 1
TOP 1 0.6993312 2.4922966 180 N 238 19 2
#
# CMP 112
CMP 2 0.8076043 2.06088 0 N R38 ERJ-2RKF4701X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF4701X'
PRP Power_(Watts) '0.1W, 1/10W'
PRP Ratings 'AEC-Q200'
PRP Resistance '4.7 kO'
PRP Series 'ERJ-2RK'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P4.70KLCT-ND'
PRP Temperature_Coefficient '±100ppm/°C'
PRP Tolerance '±1%'
PRP UniqueID 'RSMD040202594'
PRP Value '4.7 kO'
TOP 0 0.8272893 2.06088 270 N 238 20 1
TOP 1 0.7879192 2.06088 270 N 219 1 2
#
# CMP 113
CMP 2 0.6993313 2.3219501 270 N R37 ERA-2AEB103X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thin Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDM0000/AOA0000C307.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERA-2AEB103X'
PRP Power_(Watts) '0.063W, 1/16W'
PRP Ratings 'AEC-Q200'
PRP Resistance '10 kO'
PRP Series 'ERA-2A'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P10KDCCT-ND'
PRP Temperature_Coefficient '±25ppm/°C'
PRP Tolerance '±0.1%'
PRP UniqueID 'RSMD040200315'
PRP Value '10 kO'
TOP 0 0.6993313 2.3022651 0 N 218 0 1
TOP 1 0.6993313 2.3416352 0 N 238 21 2
#
# CMP 114
CMP 2 0.7387014 2.3219501 90 N R35 ERJ-2RKF4701X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF4701X'
PRP Power_(Watts) '0.1W, 1/10W'
PRP Ratings 'AEC-Q200'
PRP Resistance '4.7 kO'
PRP Series 'ERJ-2RK'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P4.70KLCT-ND'
PRP Temperature_Coefficient '±100ppm/°C'
PRP Tolerance '±1%'
PRP UniqueID 'RSMD040202594'
PRP Value '4.7 kO'
TOP 0 0.7387014 2.3416351 180 N 238 22 1
TOP 1 0.7387014 2.302265 180 N 222 0 2
#
# CMP 115
CMP 2 0.5120005 2.2382982 270 N R46 ERJ-2RKF1202X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1202X'
PRP Power_(Watts) '0.1W, 1/10W'
PRP Ratings 'AEC-Q200'
PRP Resistance '12 kO'
PRP Series 'ERJ-2RK'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P12.0KLCT-ND'
PRP Temperature_Coefficient '±100ppm/°C'
PRP Tolerance '±1%'
PRP UniqueID 'RSMD040200519'
PRP Value '12 kO'
TOP 0 0.5120005 2.2186132 0 N 248 108 1
TOP 1 0.5120005 2.2579833 0 N 227 0 2
#
# CMP 116
CMP 8 0.1891149 2.0245897 180 N R42 ERJ-6GEY0R00V ;0=1,1=0.0571
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ6GEY0R00V'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0805'
PRP PartNumber 'ERJ-6GEY0R00V'
PRP Power_(Watts) '0.125W, 1/8W'
PRP Ratings 'AEC-Q200'
PRP Resistance '0 O'
PRP Series 'ERJ-6G'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P0.0ACT-ND'
PRP Temperature_Coefficient '-'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD080510615'
PRP Value '0 O'
TOP 0 0.1595873 2.0245897 90 N 87 1 1
TOP 1 0.2186424 2.0245897 90 N 221 0 2
#
# CMP 117
CMP 4 0.5099296 2.1095407 180 N C37 GRT155R71E104KE01J ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet '-'
PRP Manufacturer 'Murata'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0402'
PRP PartNumber 'GRT155R71E104KE01J'
PRP Ratings '-'
PRP Series '-'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Digi-key'
PRP Supplier_Part_Number_1 '490-GRT155R71E104KE01JCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±10%'
PRP UniqueID 'capcc09401'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '25V'
TOP 0 0.4902446 2.1095407 90 N 248 109 1
TOP 1 0.5296147 2.1095407 90 N 238 23 2
#
# CMP 118
CMP 2 0.3929533 2.0256323 270 N R52 ERA-2AEB103X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thin Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDM0000/AOA0000C307.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERA-2AEB103X'
PRP Power_(Watts) '0.063W, 1/16W'
PRP Ratings 'AEC-Q200'
PRP Resistance '10 kO'
PRP Series 'ERA-2A'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P10KDCCT-ND'
PRP Temperature_Coefficient '±25ppm/°C'
PRP Tolerance '±0.1%'
PRP UniqueID 'RSMD040200315'
PRP Value '10 kO'
TOP 0 0.3929533 2.0059473 0 N 210 0 1
TOP 1 0.3929533 2.0453174 0 N 238 24 2
#
# CMP 119
CMP 2 0.596221 2.5069816 270 N R47 ERA-2AEB103X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thin Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDM0000/AOA0000C307.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERA-2AEB103X'
PRP Power_(Watts) '0.063W, 1/16W'
PRP Ratings 'AEC-Q200'
PRP Resistance '10 kO'
PRP Series 'ERA-2A'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P10KDCCT-ND'
PRP Temperature_Coefficient '±25ppm/°C'
PRP Tolerance '±0.1%'
PRP UniqueID 'RSMD040200315'
PRP Value '10 kO'
TOP 0 0.596221 2.4872966 0 N 226 0 1
TOP 1 0.596221 2.5266667 0 N 238 25 2
#
# CMP 120
CMP 2 0.187165 1.915 180 N R51 ERA-2AEB103X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thin Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDM0000/AOA0000C307.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERA-2AEB103X'
PRP Power_(Watts) '0.063W, 1/16W'
PRP Ratings 'AEC-Q200'
PRP Resistance '10 kO'
PRP Series 'ERA-2A'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P10KDCCT-ND'
PRP Temperature_Coefficient '±25ppm/°C'
PRP Tolerance '±0.1%'
PRP UniqueID 'RSMD040200315'
PRP Value '10 kO'
TOP 0 0.16748 1.915 90 N 1 0 1
TOP 1 0.2068501 1.915 90 N 238 49 2
#
# CMP 121
CMP 2 0.6993312 2.1062178 0 N R34 ERA-2AEB103X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thin Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDM0000/AOA0000C307.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERA-2AEB103X'
PRP Power_(Watts) '0.063W, 1/16W'
PRP Ratings 'AEC-Q200'
PRP Resistance '10 kO'
PRP Series 'ERA-2A'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P10KDCCT-ND'
PRP Temperature_Coefficient '±25ppm/°C'
PRP Tolerance '±0.1%'
PRP UniqueID 'RSMD040200315'
PRP Value '10 kO'
TOP 0 0.7190162 2.1062178 270 N 220 0 1
TOP 1 0.6796461 2.1062178 270 N 238 26 2
#
# CMP 122
CMP 2 0.6899713 2.3874972 180 N R48 ERA-2AEB103X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thin Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDM0000/AOA0000C307.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERA-2AEB103X'
PRP Power_(Watts) '0.063W, 1/16W'
PRP Ratings 'AEC-Q200'
PRP Resistance '10 kO'
PRP Series 'ERA-2A'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P10KDCCT-ND'
PRP Temperature_Coefficient '±25ppm/°C'
PRP Tolerance '±0.1%'
PRP UniqueID 'RSMD040200315'
PRP Value '10 kO'
TOP 0 0.6702863 2.3874972 90 N 225 1 1
TOP 1 0.7096564 2.3874972 90 N 238 27 2
#
# CMP 123
CMP 21 0.7288589 2.2032414 90 N U10 SN74LVC2G125DCUT ;0=1,1=0.0354
PRP 3-State_Output 'Yes'
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Bits(#) '2'
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/sn74lvc2g125.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/sn74lvc2g125'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/sn74lvc2g125/datasheet'
PRP CompType 'IC'
PRP F_@_Nom_Voltage(Max)(Mhz) '150'
PRP Generic_Part_Number 'SN74LVC2G125'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP ICC_@_Nom_Voltage(Max)(mA) '0.01'
PRP Input_Type 'CMOS/TTL'
PRP Logic 'True'
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP Operating_Temperature_Range '-40 to 125 C'
PRP Output_Drive_(IOL/IOH)(Max)(mA) '32/-32'
PRP Output_Type 'CMOS'
PRP PackageDescription 'VSSOP-8'
PRP PackageReference 'DCU0008A'
PRP PartNumber 'SN74LVC2G125DCUT'
PRP Rating 'Catalog'
PRP RoHS ''
PRP Schmitt_Trigger 'No'
PRP SizeArea_mm2 '6.4'
PRP SizeAreaWB_mm2 '12.6'
PRP SizeX_mm '3.2'
PRP SizeY_mm '2.0'
PRP SizeZ_mm '0.9'
PRP Technology_Family 'LVC'
PRP tpd_@_Nom_Voltage(Max)(ns) '9.1,4.8,4.3,3.7'
PRP VCC(Max)(V) '5.5'
PRP VCC(Min)(V) '1.65'
PRP Voltage(Nom)(V) '1.8,2.5,3.3,5'
TOP 0 0.6993313 2.264265 180 N 218 1 1
TOP 1 0.7190163 2.264265 180 N 248 119 2
TOP 2 0.7387014 2.264265 180 N 222 1 3
TOP 3 0.7583864 2.264265 180 N 248 120 4
TOP 4 0.7583864 2.1422178 180 N 248 121 5
TOP 5 0.7387014 2.1422178 180 N 193 1 6
TOP 6 0.7190163 2.1422178 180 N 220 2 7
TOP 7 0.6993313 2.1422178 180 N 238 36 8
#
# CMP 124
CMP 0 0.7190163 2.0751942 270 N R39 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 0.7190163 2.0641706 0 N 231 0 1
TOP 1 0.7190163 2.0862178 0 N 220 1 2
#
# CMP 125
CMP 53 0.5950005 2.2217454 90 N U12 93LC46B-I/ST ;0=1,1=0.0472
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Color '-'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://ww1.microchip.com/downloads/en/DeviceDoc/20001749K.pdf'
PRP CompType 'EEPROM'
PRP Current_Rating_(Amps) '-'
PRP datasheet 'https://www.mouser.com/datasheet/2/268/20001749K-277859.pdf'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Length_(in) '-'
PRP Manufacturer 'Microchip Technology'
PRP Mount_Type 'SMD'
PRP MountType 'SMT'
PRP PackageReference 'TSSOP-8'
PRP PartNumber '93LC46B-I/ST'
PRP Pitch_(mm) '-'
PRP RoHS 'Y'
PRP Series '-'
PRP SizeArea_mm2 '19.2'
PRP SizeAreaWB_mm2 '42'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '93LC46B-I/ST-ND'
PRP Supplier_Part_Number_2 '92C7658'
PRP Supplier_Part_Number_3 '579-93LC46B-I/ST'
PRP SymbolCreator 'Altium'
PRP SymbolVersion '2016-2-18'
PRP Text1 '-'
PRP UniqueID 'cmp00156'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 0.5566147 2.3339501 180 N 224 1 1
TOP 1 0.5822052 2.3339501 180 N 226 1 2
TOP 2 0.6077958 2.3339501 180 N 223 1 3
TOP 3 0.6333863 2.3339501 180 N 225 2 4
TOP 4 0.6333863 2.1095407 180 N 248 319 5
TOP 5 0.6077958 2.1095407 180 N 0 210 6
TOP 6 0.5822052 2.1095407 180 N 0 211 7
TOP 7 0.5566147 2.1095407 180 N 238 44 8
#
# CMP 126
CMP 4 0.8479769 2.2670211 90 N C36 GRT155R71E104KE01J ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet '-'
PRP Manufacturer 'Murata'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0402'
PRP PartNumber 'GRT155R71E104KE01J'
PRP Ratings '-'
PRP Series '-'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Digi-key'
PRP Supplier_Part_Number_1 '490-GRT155R71E104KE01JCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±10%'
PRP UniqueID 'capcc09401'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '25V'
TOP 0 0.8479769 2.2867061 180 N 248 110 1
TOP 1 0.8479769 2.247336 180 N 238 28 2
#
# CMP 127
CMP 4 0.8371266 2.0333202 0 N C40 GRT155R71E104KE01J ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet '-'
PRP Manufacturer 'Murata'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0402'
PRP PartNumber 'GRT155R71E104KE01J'
PRP Ratings '-'
PRP Series '-'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Digi-key'
PRP Supplier_Part_Number_1 '490-GRT155R71E104KE01JCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±10%'
PRP UniqueID 'capcc09401'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '25V'
TOP 0 0.8568116 2.0333202 270 N 248 111 1
TOP 1 0.8174415 2.0333202 270 N 238 29 2
#
# CMP 128
CMP 4 0.6205911 2.0483202 0 N C38 GRT155R71E104KE01J ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet '-'
PRP Manufacturer 'Murata'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0402'
PRP PartNumber 'GRT155R71E104KE01J'
PRP Ratings '-'
PRP Series '-'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Digi-key'
PRP Supplier_Part_Number_1 '490-GRT155R71E104KE01JCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±10%'
PRP UniqueID 'capcc09401'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '25V'
TOP 0 0.6402761 2.0483202 270 N 248 112 1
TOP 1 0.600906 2.0483202 270 N 238 30 2
#
