                                                                   Jan 2, 2008
 TEXAS INSTRUMENTS


   PART NO. Wireless 2Way 2510
   REV. C
   Artworks were created using Protel Design Explorer 99SE.

   PCB DESCRIPTION: 4 LAYER PCB, .062" NOMINAL THICKNESS FR4 WITH 1OZ COPPER PER LAYER.
  
   Board layer stack-up: 
   Layer 1 - layer 2 .0122" nominal
   Layer 2 - layer 3 .028" nominal core
   Layer 3 - layer 4 .0122" nominal

  
 THIS ARCHIVED (WINZIP) FILE "Wireless 2Way 2510.ZIP" CONTAINS 27 FILES.

   Wireless 2Way.GTO = TOP SILKSCREEN GERBER FILE
   Wireless 2Way.GTS = TOP SOLDER MASK GERBER FILE
   Wireless 2Way.GTL = LAYER 1 TOP SIGNAL GERBER FILE
   Wireless 2Way.GP1 = LAYER 2 INTERNAL GROUND PLANE GERBER FILE
   Wireless 2Way.GP2 = LAYER 3 INTERNAL POWER PLANE GERBER FILE
   Wireless 2Way.GBL = LAYER 4 BOTTOM SIGNAL GERBER FILE
   Wireless 2Way.GBS = BOTTOM SOLDER MASK GERBER FILE
   Wireless 2Way.GBO = BOTTOM SILKSCREEN GERBER FILE
   Wireless 2Way.GTP = TOP PASTE STENCIL GERBER FILE
   Wireless 2Way.GBP = BOTTOM PASTE STENCIL GERBER FILE
   Wireless 2Way.GG1 = DRILL GUIDE GERBER FILE
   Wireless 2Way.GD1 = DRILL DRAWIING GERBER FILE
   Wireless 2Way.GM3 = FAB DIMENSION GERBER FILE
   Wireless 2Way.GM4 = BOARD OUTLINE GERBER FILE
   Wireless 2Way.GM1 = TOP ASSEMBLY DRAWING GERBER FILE
   Wireless 2Way.GM5 = BOTTOM ASSEMBLY DRAWING GERBER FILE
   Wireless 2Way.DRR = ASCII DRILL SIZE REPORT
   Wireless 2Way.TXT = ASCII DRILL FILE
   Wireless 2Way.DRL = BINARY DRILL FILE
   Wireless 2Way.APR = APERTURE FILE
   README.TXT = THIS FILE
   PICK PLACE FOR Wireless 2Way.XLS = PICK AND PLACE SPREADSHEET
   Wireless 2Way RevC BOM.XLS = BILL OF MATERIALS
   Wireless 2Way ASCII.PCB = BOARD DESIGN IN PROTEL PCB V2.8 ASCII FORMAT
   Wireless 2Way 2510 Schematics RevC.PDF = Schematic in PDF form
   Wireless 2Way 2510 Artwork RevC.PDF = Artworks in PDF form	
   Wireless 2Way.DDB = Protel Design Database (Protel Design Explorer 99SE)



READ.ME
