Cross Section Report
C:/srf04/Agama/Agama_EM_Designs/CC26x2RBEM-7ID/Cadence/Allegro/CC26x2RBEM-7ID.brd
Thu Dec 12 07:57:19 2019

Design Cross Section
Subclass Name,Type,Material,Thickness (MM),Tol +,Tol -,Conductivity (mho/cm),Dielectric Constant,Loss Tangent,Negative Artwork,Shield,Width (MM),Unused Pin Pad Suppression,Unused Via Pad Suppression
,SURFACE,AIR,,,,0,1,0,,,,,
TOP,CONDUCTOR,COPPER,0.035,0,0,595900,4.2,0,,,0.127,,
,DIELECTRIC,FR-4,0.73,0,0,0,4.2,0.035,,,,,
BOTTOM,CONDUCTOR,COPPER,0.035,0,0,595900,4.2,0,,,0.127,,
,SURFACE,AIR,,,,0,1,0,,,,,

Total Thickness: 0.8 MM
