Design Name C:/Users/a0274226/Documents/MyDocs/Projects/LAUNCHXL-CC1312R1/Rev-D/Cadence/LAUNCHXL-CC1312R1.brd
Date Wed Oct 10 11:07:41 2018

Design Cross Section
Subclass Name | Type | Material | Thickness (MM) | Tol + | Tol - | Conductivity (mho/cm) | Dielectric Constant | Loss Tangent | Negative Artwork | Shield | Width (MM) | Unused Pin Pad Suppression | Unused Via Pad Suppression
| SURFACE | AIR |  |  |  | 0 | 1 | 0 |  |  |  |  |
TOP | CONDUCTOR | COPPER | 0.035 | 0 | 0 | 595900 | 4.5 | 0 |  |  | 0.1270 |  |
| DIELECTRIC | FR-4 | 0.175 | 0 | 0 | 0 | 4.5 | 0.035 |  |  |  |  |
L2 | PLANE | COPPER | 0.035 | 0 | 0 | 595900 | 4.5 | 0.035 |  | Yes |  |  | Yes
| DIELECTRIC | FR-4 | 1.110000 | 0 | 0 | 0 | 4.5 | 0.035 |  |  |  |  |
L3 | PLANE | COPPER | 0.035 | 0 | 0 | 595900 | 4.5 | 0.035 |  | Yes |  |  | Yes
| DIELECTRIC | FR-4 | 0.175 | 0 | 0 | 0 | 4.5 | 0.035 |  |  |  |  |
BOTTOM | CONDUCTOR | COPPER | 0.035 | 0 | 0 | 595900 | 4.5 | 0 |  |  | 0.1270 |  |
| SURFACE | AIR |  |  |  | 0 | 1 | 0 |  |  |  |  |

Total Thickness: 1.6 MM