Revision history of Board changes:

|  |  |  |
| --- | --- | --- |
| Board Revision | Details of changes | Device version |
| xWRL6432BOOST Rev A | Baseline | ES1.0 |
| xWRL6432BOOST Rev B | * CANH/CANL Text swap on CAN header * Moved the I2C headers that are close to mounting holes * Moving the SOP lines before the Analog mux * I2C resistor connecting to DCA1000 board by default made DNI * Introduced switch on the I2C lines between XDS110 and mmWave device * Moved the crystal to the bottom side of the board. | ES1.0 |
|  | * **ASSY REV A1**   + INA226 were updated to INA228 for enabling Deep sleep power measurements   + Series resistances on the power rails updated to enhance the dynamic rage of the measurements | ES1.0 |
|  | * **ASSY REV A1**   + Serial number for ES2.0 silicon is updated to xWRL6432REVB\_ES2.0SOC\_XXX | ES2.0 |