PMP8740 Rev\_C Enclosure details

Housing profile 2: GL GP 20 21 – 290

1. Side panels: refer to front and rear panel, described in the „Front Panel Designer“ Files (PMP8740 Rev\_A Front panel.fpd and PMP8740 Rev\_A Back panel.fpd files).
2. Cover panel Pair A:
3. Case 1 (F1)
4. Dimension G = 290mm
5. Dimension M = 2.5mm
6. Dimension F = 150mm
7. Cover panel Pair B:
8. Dimension B = 125mm
9. Dimension G = 290mm
10. Dimension M = 2.5mm
11. Dimension K = 10mm
12. Dimension K1 = K2 = K3 = 90mm
13. Assembly kit Screws: GG MS 1612
14. Assembly kit Screws: twice GG MS 1742

Front Panel Designer Software:

<http://www.schaeffer-ag.de/en/front_panel_designer/look_inside_the_software/>