customize

# Variant Report

Date: |  | 5/13/2022
Time: |  | 12:00:32 PM
Elapsed Time: |  | 00:00:01

## Variations

Physical | Document | Parameter Name | Original Value | 001
--- | --- | --- | --- | ---
!PCB1 | HVP053B_Hardware.SchDoc |  | Fitted | Fitted
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | ClassName |  |
|  | Comment | Printed Circuit Board | Printed Circuit Board
|  | ComponentLink1Description |  |
|  | ComponentLink1URL |  |
|  | CompType | PCB | PCB
|  | Description | Printed Circuit Board | Printed Circuit Board
|  | Footprint |  |
|  | Key | PCB | PCB
|  | LatestRevisionDate | 2017-03-09 | 2017-03-09
|  | Manufacturer | Any | Any
|  | MountType | N/A | N/A
|  | Note |  |
|  | PackageReference |  |
|  | PartNumber | HVP053 | HVP053
|  | Publisher | Texas Instruments | Texas Instruments
|  | RoHS | O | O
|  | Supplier 1 |  |
|  | Supplier 2 |  |
|  | Supplier 3 |  |
|  | Supplier Part Number 1 |  |
|  | Supplier Part Number 2 |  |
|  | Supplier Part Number 3 |  |
|  | Value |  |
C1 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AC_Derating |  |
|  | AEC Category | Q200 | Q200
|  | AEC Grade | 2 | 2
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Cap_Case | 10x16 | 10x16
|  | Cap_F | 15µF | 15µF
|  | Comment | UVC2G150MPD | UVC2G150MPD
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | https://www.nichicon.co.jp/english/products/pdfs/e-ucy.pdf | https://www.nichicon.co.jp/english/products/pdfs/e-ucy.pdf
|  | CompType | Capacitor | Capacitor
|  | Description | CAP, AL, 15 µF, 400 V, +/- 20%, AEC-Q200 Grade 2, TH | CAP, AL, 15 µF, 400 V, +/- 20%, AEC-Q200 Grade 2, TH
|  | ESR_ohm |  |
|  | Footprint | UVC_1000x1600 | UVC_1000x1600
|  | IRMS_A | 180mA | 180mA
|  | LatestRevisionDate |  |
|  | Manufacturer | Nichicon | Nichicon
|  | MountType | TH | TH
|  | PackageReference | 10x16mm | 10x16mm
|  | PartNumber | UVC2G150MPD | UVC2G150MPD
|  | Polarized | Y | Y
|  | Publisher |  |
|  | RoHS | Y | Y
|  | Series | UVC | UVC
|  | SizeArea_mm2 | 100 | 100
|  | SizeAreaWB_mm2 | 144 | 144
|  | SizeX_mm | 10 | 10
|  | SizeY_mm | 10 | 10
|  | SizeZ_mm | 18 | 18
|  | Supplier 1 |  |
|  | Supplier 2 |  |
|  | Supplier 3 |  |
|  | Supplier Part Number 1 |  |
|  | Supplier Part Number 2 |  |
|  | Supplier Part Number 3 |  |
|  | TaMax_C | 105°C | 105°C
|  | TaMin_C | -40°C | -40°C
|  | Technology | AL | AL
|  | Tolerance_% | 20% | 20%
|  | U/M | EA | EA
|  | Value | 15uF | 15uF
|  | Value1 |  |
|  | Value2 | 400V | 400V
|  | ValueDisplayed | 15µF | 15µF
|  | VDC_V | 400V | 400V
C2 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AC_Derating |  |
|  | AEC Category | Q200 | Q200
|  | AEC Grade | N/A | N/A
|  | AEC Qualified | N | N
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Cap_Case | 18x25mm | 18x25mm
|  | Cap_F | 82µF | 82µF
|  | Comment | 400BXW82MEFR18X25 | 400BXW82MEFR18X25
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.rubycon.co.jp/en/catalog/e_pdfs/aluminum/e_BXW.pdf | http://www.rubycon.co.jp/en/catalog/e_pdfs/aluminum/e_BXW.pdf
|  | CompType | Capacitor | Capacitor
|  | Description | CAP, AL, 82 µF, 400 V, +/- 20%, TH | CAP, AL, 82 µF, 400 V, +/- 20%, TH
|  | ESR_ohm |  |
|  | Footprint | Rubycon_1800x2500_HD | Rubycon_1800x2500_HD
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | IRMS_A |  |
|  | LatestRevisionDate |  |
|  | Manufacturer | Rubycon | Rubycon
|  | MountType | TH | TH
|  | PackageReference | Dia 18mm | Dia 18mm
|  | PartNumber | 400BXW82MEFR18X25 | 400BXW82MEFR18X25
|  | Polarized | Y | Y
|  | Publisher |  |
|  | RoHS | Y | Y
|  | Series | BXW | BXW
|  | SizeArea_mm2 | 324 | 324
|  | SizeAreaWB_mm2 | 400 | 400
|  | SizeX_mm | 18 | 18
|  | SizeY_mm | 18 | 18
|  | SizeZ_mm | 27 | 27
|  | Supplier 1 |  |
|  | Supplier 2 |  |
|  | Supplier 3 |  |
|  | Supplier Part Number 1 |  |
|  | Supplier Part Number 2 |  |
|  | Supplier Part Number 3 |  |
|  | TaMax_C | 105°C | 105°C
|  | TaMin_C | -40°C | -40°C
|  | Technology | AL | AL
|  | Tolerance_% | 20% | 20%
|  | U/M | EA | EA
|  | Value | 82uF | 82uF
|  | Value1 |  |
|  | Value2 | 400V | 400V
|  | ValueDisplayed | 82µF | 82µF
|  | VDC_V | 400V | 400V
C3 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AC_Derating |  |
|  | AC_Safety | X2 | X2
|  | AEC Category | Q200 | Q200
|  | AEC Grade | N/A | N/A
|  | AEC Qualified | N | N
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Cap_Case | 15x8.5mm | 15x8.5mm
|  | Cap_F | 330nF | 330nF
|  | Comment | 890324024003 | 890324024003
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | https://katalog.we-online.de/pbs/datasheet/890324024003.pdf | https://katalog.we-online.de/pbs/datasheet/890324024003.pdf
|  | CompType | Capacitor | Capacitor
|  | Description | CAP, Film, 0.33 µF, X2 275 VAC, +/- 10%, TH | CAP, Film, 0.33 µF, X2 275 VAC, +/- 10%, TH
|  | ESR_ohm |  |
|  | Footprint | WCAP-FTX2_1500x850 | WCAP-FTX2_1500x850
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | IRMS_A |  |
|  | Manufacturer | Wurth Elektronik | Wurth Elektronik
|  | MountType | TH | TH
|  | PackageReference | 15x8.5mm | 15x8.5mm
|  | PartNumber | 890324024003 | 890324024003
|  | Polarized | N | N
|  | RoHS | Y | Y
|  | Series | WCAP-FTX2 | WCAP-FTX2
|  | SizeArea_mm2 | 127.5 | 127.5
|  | SizeAreaWB_mm2 | 178.5 | 178.5
|  | SizeX_mm | 15 | 15
|  | SizeY_mm | 8.5 | 8.5
|  | SizeZ_mm | 14.5 | 14.5
|  | Supplier 1 |  |
|  | Supplier 2 |  |
|  | Supplier 3 |  |
|  | Supplier Part Number 1 |  |
|  | Supplier Part Number 2 |  |
|  | Supplier Part Number 3 |  |
|  | TaMax_C | 105°C | 105°C
|  | TaMin_C | -40°C | -40°C
|  | Technology | Film | Film
|  | Tolerance_% | 10% | 10%
|  | VAC |  |
|  | VAC_X | 275 | 275
|  | VAC_Y |  |
|  | Value | 0.33uF | 0.33uF
|  | Value1 |  |
|  | Value2 |  |
|  | ValueDisplayed | 0.33µF | 0.33µF
|  | VDC_V |  |
C4 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | N/A | N/A
|  | AEC Qualified | N | N
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Cap_Case | 1210 | 1210
|  | Cap_F | 100nF | 100nF
|  | Comment | C1210C104KBRAC7800 | C1210C104KBRAC7800
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.kemet.com/docfinder?Partnumber=C1210C104KBRAC7800 | http://www.kemet.com/docfinder?Partnumber=C1210C104KBRAC7800
|  | CompType | Capacitor | Capacitor
|  | Description | CAP, CERM, 0.1 uF, 630 V, +/- 10%, X7R, 1210 | CAP, CERM, 0.1 uF, 630 V, +/- 10%, X7R, 1210
|  | ESR_ohm |  |
|  | Footprint | 1210_280 | 1210_280
|  | IRMS_A |  |
|  | LatestRevisionDate | 2017-03-09 | 2017-03-09
|  | Manufacturer | Kemet | Kemet
|  | MountType | SMT | SMT
|  | PackageReference | 1210 | 1210
|  | PartNumber | C1210C104KBRAC7800 | C1210C104KBRAC7800
|  | Polarized | N | N
|  | Published | 2008-06-19 | 2008-06-19
|  | Publisher | Texas Instruments | Texas Instruments
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 8 | 8
|  | SizeAreaWB_mm2 | 14.7 | 14.7
|  | SizeX_mm | 3.2 | 3.2
|  | SizeY_mm | 2.5 | 2.5
|  | SizeZ_mm | 2.8 | 2.8
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Mouser | Mouser
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | 399-13490-1-ND | 399-13490-1-ND
|  | Supplier Part Number 2 | 80-C1210C104KBR | 80-C1210C104KBR
|  | Supplier Part Number 3 |  |
|  | TaMax_C | 125°C | 125°C
|  | TaMin_C | -55°C | -55°C
|  | Technology | Ceramic | Ceramic
|  | TempCo | X7R | X7R
|  | Tolerance_% | 10% | 10%
|  | U/M | EA | EA
|  | Value | 0.1uF | 0.1uF
|  | Value1 | Unknown | Unknown
|  | Value2 | 630V | 630V
|  | ValueDisplayed | 0.1uF | 0.1uF
|  | VDC_V | 630V | 630V
C5 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | N/A | N/A
|  | AEC Qualified | N | N
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Cap_Case | 1210 | 1210
|  | Cap_F | 100nF | 100nF
|  | Comment | C1210C104KBRAC7800 | C1210C104KBRAC7800
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.kemet.com/docfinder?Partnumber=C1210C104KBRAC7800 | http://www.kemet.com/docfinder?Partnumber=C1210C104KBRAC7800
|  | CompType | Capacitor | Capacitor
|  | Description | CAP, CERM, 0.1 uF, 630 V, +/- 10%, X7R, 1210 | CAP, CERM, 0.1 uF, 630 V, +/- 10%, X7R, 1210
|  | ESR_ohm |  |
|  | Footprint | 1210_280 | 1210_280
|  | IRMS_A |  |
|  | LatestRevisionDate | 2017-03-09 | 2017-03-09
|  | Manufacturer | Kemet | Kemet
|  | MountType | SMT | SMT
|  | PackageReference | 1210 | 1210
|  | PartNumber | C1210C104KBRAC7800 | C1210C104KBRAC7800
|  | Polarized | N | N
|  | Published | 2008-06-19 | 2008-06-19
|  | Publisher | Texas Instruments | Texas Instruments
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 8 | 8
|  | SizeAreaWB_mm2 | 14.7 | 14.7
|  | SizeX_mm | 3.2 | 3.2
|  | SizeY_mm | 2.5 | 2.5
|  | SizeZ_mm | 2.8 | 2.8
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Mouser | Mouser
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | 399-13490-1-ND | 399-13490-1-ND
|  | Supplier Part Number 2 | 80-C1210C104KBR | 80-C1210C104KBR
|  | Supplier Part Number 3 |  |
|  | TaMax_C | 125°C | 125°C
|  | TaMin_C | -55°C | -55°C
|  | Technology | Ceramic | Ceramic
|  | TempCo | X7R | X7R
|  | Tolerance_% | 10% | 10%
|  | U/M | EA | EA
|  | Value | 0.1uF | 0.1uF
|  | Value1 | Unknown | Unknown
|  | Value2 | 630V | 630V
|  | ValueDisplayed | 0.1uF | 0.1uF
|  | VDC_V | 630V | 630V
C6 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade |  |
|  | AEC Qualified | ? | ?
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Cap_Case | 1206 | 1206
|  | Cap_F | 1nF | 1nF
|  | Comment | GRM31BR72J102KW01L | GRM31BR72J102KW01L
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM31BR72J102KW01L&x=9&y=9&search=startwith | http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM31BR72J102KW01L&x=9&y=9&search=startwith
|  | CompType | Capacitor | Capacitor
|  | Description | CAP, CERM, 1000 pF, 630 V, +/- 10%, X7R, 1206 | CAP, CERM, 1000 pF, 630 V, +/- 10%, X7R, 1206
|  | ESR_ohm |  |
|  | Footprint | 1206L | 1206L
|  | IRMS_A |  |
|  | LatestRevisionDate | 2017-03-09 | 2017-03-09
|  | Manufacturer | MuRata | MuRata
|  | MountType | SMT | SMT
|  | PackageReference | 1206 | 1206
|  | PartNumber | GRM31BR72J102KW01L | GRM31BR72J102KW01L
|  | Polarized | N | N
|  | Published | 2008-06-19 | 2008-06-19
|  | Publisher | Texas Instruments | Texas Instruments
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 5.12 | 5.12
|  | SizeAreaWB_mm2 | 10.92 | 10.92
|  | SizeX_mm | 3.2 | 3.2
|  | SizeY_mm | 1.6 | 1.6
|  | SizeZ_mm | 1.35 | 1.35
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Mouser | Mouser
|  | Supplier 3 | Farnell | Farnell
|  | Supplier Part Number 1 | 490-3506-1-ND | 490-3506-1-ND
|  | Supplier Part Number 2 | 81-GRM31BR72J102KW01 | 81-GRM31BR72J102KW01
|  | Supplier Part Number 3 | 2057302 | 2057302
|  | TaMax_C | 125°C | 125°C
|  | TaMin_C | -55°C | -55°C
|  | Technology | Ceramic | Ceramic
|  | TempCo | X7R | X7R
|  | Tolerance_% | 10% | 10%
|  | U/M | EA | EA
|  | Value | 1000pF | 1000pF
|  | Value1 | Unknown | Unknown
|  | Value2 | 630V | 630V
|  | ValueDisplayed | 1000pF | 1000pF
|  | VDC_V | 630V | 630V
C7 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AC_Derating |  |
|  | AC_Safety |  |
|  | AEC Category | Q200 | Q200
|  | AEC Grade | N/A | N/A
|  | AEC Qualified | N | N
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Cap_Case | 10x11.5 | 10x11.5
|  | Cap_F | 680µF | 680µF
|  | Comment | APSG200ELL681MJB5S | APSG200ELL681MJB5S
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.chemi-con.co.jp/cgi-bin/CAT_DB/SEARCH/cat_db_al.cgi?e=e&j=p&pdfname=psg | http://www.chemi-con.co.jp/cgi-bin/CAT_DB/SEARCH/cat_db_al.cgi?e=e&j=p&pdfname=psg
|  | CompType | Capacitor | Capacitor
|  | Description | CAP, Aluminum Polymer, 680 uF, 20 V, +/- 20%, 0.012 ohm, TH | CAP, Aluminum Polymer, 680 uF, 20 V, +/- 20%, 0.012 ohm, TH
|  | ESR_ohm | 0.012 | 0.012
|  | Footprint | PSG_1000x1150 | PSG_1000x1150
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | IRMS_A | 5.4A | 5.4A
|  | Manufacturer | Chemi-Con | Chemi-Con
|  | MountType | TH | TH
|  | PackageReference | 10x11.5mm | 10x11.5mm
|  | PartNumber | APSG200ELL681MJB5S | APSG200ELL681MJB5S
|  | Polarized | Y | Y
|  | RoHS | Y | Y
|  | Series | PSG | PSG
|  | SizeArea_mm2 | 100 | 100
|  | SizeAreaWB_mm2 | 144 | 144
|  | SizeX_mm | 10 | 10
|  | SizeY_mm | 10 | 10
|  | SizeZ_mm | 13 | 13
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Mouser | Mouser
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | 565-3623-ND | 565-3623-ND
|  | Supplier Part Number 2 | 661-APSG200E681MJB5S | 661-APSG200E681MJB5S
|  | Supplier Part Number 3 |  |
|  | TaMax_C | 105°C | 105°C
|  | TaMin_C | -55°C | -55°C
|  | Technology | Aluminum Polymer | Aluminum Polymer
|  | Tolerance_% | 20% | 20%
|  | VAC |  |
|  | VAC_X |  |
|  | VAC_Y |  |
|  | Value | 680uF | 680uF
|  | Value1 | 0.012 ohm | 0.012 ohm
|  | Value2 | 20V | 20V
|  | ValueDisplayed | 680uF | 680uF
|  | VDC_V | 20V | 20V
C8 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AC_Safety |  |
|  | AEC Category | Q200 | Q200
|  | AEC Grade | 1 | 1
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Cap_Case | 1206_180 | 1206_180
|  | Cap_F | 10µF | 10µF
|  | Comment | C1206C106J3RACAUTO | C1206C106J3RACAUTO
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | https://content.kemet.com/datasheets/KEM_C1023_X7R_AUTO_SMD.pdf | https://content.kemet.com/datasheets/KEM_C1023_X7R_AUTO_SMD.pdf
|  | CompType | Capacitor | Capacitor
|  | Description | CAP, CERM, 10 µF, 25 V,+/- 5%, X7R, AEC-Q200 Grade 1, 1206 | CAP, CERM, 10 µF, 25 V,+/- 5%, X7R, AEC-Q200 Grade 1, 1206
|  | ESR_ohm |  |
|  | Footprint | 1206_180L | 1206_180L
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | IRMS_A |  |
|  | Manufacturer | Kemet | Kemet
|  | MountType | SMT | SMT
|  | PackageReference | 1206 | 1206
|  | PartNumber | C1206C106J3RACAUTO | C1206C106J3RACAUTO
|  | Polarized | N | N
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 5.12 | 5.12
|  | SizeAreaWB_mm2 | 10.92 | 10.92
|  | SizeX_mm | 3.2 | 3.2
|  | SizeY_mm | 1.6 | 1.6
|  | SizeZ_mm | 1.8 | 1.8
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Mouser | Mouser
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | 399-15734-1-ND | 399-15734-1-ND
|  | Supplier Part Number 2 | 80-C1206C106J3RAUTO | 80-C1206C106J3RAUTO
|  | Supplier Part Number 3 |  |
|  | TaMax_C | 125°C | 125°C
|  | TaMin_C | -55°C | -55°C
|  | Technology | Ceramic | Ceramic
|  | TempCo | X7R | X7R
|  | Tolerance_% | 5% | 5%
|  | U/M | EA | EA
|  | VAC |  |
|  | VAC_X |  |
|  | VAC_Y |  |
|  | Value | 10uF | 10uF
|  | Value1 |  |
|  | Value2 | 25V | 25V
|  | ValueDisplayed | 10µF | 10µF
|  | VDC_V | 25V | 25V
C9 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade |  |
|  | AEC Qualified | ? | ?
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Cap_Case | 1210 | 1210
|  | Cap_F | 22µF | 22µF
|  | Comment | GRM32ER71E226KE15L | GRM32ER71E226KE15L
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM32ER71E226KE15L&x=9&y=9&search=startwith | http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM32ER71E226KE15L&x=9&y=9&search=startwith
|  | CompType | Capacitor | Capacitor
|  | Description | CAP, CERM, 22 uF, 25 V, +/- 10%, X7R, 1210 | CAP, CERM, 22 uF, 25 V, +/- 10%, X7R, 1210
|  | ESR_ohm |  |
|  | Footprint | 1210_270L | 1210_270L
|  | IRMS_A |  |
|  | LatestRevisionDate | 2017-03-09 | 2017-03-09
|  | Manufacturer | MuRata | MuRata
|  | MountType | SMT | SMT
|  | PackageReference | 1210 | 1210
|  | PartNumber | GRM32ER71E226KE15L | GRM32ER71E226KE15L
|  | Polarized | N | N
|  | Published | 2008-06-19 | 2008-06-19
|  | Publisher | Texas Instruments | Texas Instruments
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 8 | 8
|  | SizeAreaWB_mm2 | 14.7 | 14.7
|  | SizeX_mm | 3.2 | 3.2
|  | SizeY_mm | 2.5 | 2.5
|  | SizeZ_mm | 2.7 | 2.7
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Mouser | Mouser
|  | Supplier 3 | Farnell | Farnell
|  | Supplier Part Number 1 | 490-5313-1-ND | 490-5313-1-ND
|  | Supplier Part Number 2 | 81-GRM32ER71E226KE5L | 81-GRM32ER71E226KE5L
|  | Supplier Part Number 3 | 1797019 | 1797019
|  | TaMax_C | 125°C | 125°C
|  | TaMin_C | -55°C | -55°C
|  | Technology | Ceramic | Ceramic
|  | TempCo | X7R | X7R
|  | Tolerance_% | 10% | 10%
|  | U/M | EA | EA
|  | Value | 22uF | 22uF
|  | Value1 | Unknown | Unknown
|  | Value2 | 25V | 25V
|  | ValueDisplayed | 22uF | 22uF
|  | VDC_V | 25V | 25V
C10 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | N/A | N/A
|  | AEC Qualified | N | N
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Cap_Case | 1206_180 | 1206_180
|  | Cap_F | 10µF | 10µF
|  | Comment | C3216X5R1H106K160AB | C3216X5R1H106K160AB
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=C3216X5R1H106K160AB | https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=C3216X5R1H106K160AB
|  | CompType | Capacitor | Capacitor
|  | Description | CAP, CERM, 10 uF, 50 V, +/- 10%, X5R, 1206 | CAP, CERM, 10 uF, 50 V, +/- 10%, X5R, 1206
|  | ESR_ohm | 2.229m | 2.229m
|  | Footprint | 1206_180L | 1206_180L
|  | IRMS_A | 4.85932A | 4.85932A
|  | LatestRevisionDate | 2017-03-09 | 2017-03-09
|  | Manufacturer | TDK | TDK
|  | MountType | SMT | SMT
|  | PackageReference | 1206 | 1206
|  | PartNumber | C3216X5R1H106K160AB | C3216X5R1H106K160AB
|  | Polarized | N | N
|  | Published | 2008-06-19 | 2008-06-19
|  | Publisher | Texas Instruments | Texas Instruments
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 5.12 | 5.12
|  | SizeAreaWB_mm2 | 10.92 | 10.92
|  | SizeX_mm | 3.2 | 3.2
|  | SizeY_mm | 1.6 | 1.6
|  | SizeZ_mm | 1.8 | 1.8
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Mouser | Mouser
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | 445-5998-1-ND | 445-5998-1-ND
|  | Supplier Part Number 2 | 810-C3216X5R1H106K160AB | 810-C3216X5R1H106K160AB
|  | Supplier Part Number 3 |  |
|  | TaMax_C | 85°C | 85°C
|  | TaMin_C | -55°C | -55°C
|  | Technology | Ceramic | Ceramic
|  | TempCo | X5R | X5R
|  | Tolerance_% | 10% | 10%
|  | U/M | EA | EA
|  | Value | 10uF | 10uF
|  | Value1 | 0.002229 ohm | 0.002229 ohm
|  | Value2 | 50V | 50V
|  | ValueDisplayed | 10uF | 10uF
|  | VDC_V | 50V | 50V
C11 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | N/A | N/A
|  | AEC Qualified | N | N
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Cap_Case | 0402 | 0402
|  | Cap_F | 100nF | 100nF
|  | Comment | GRM155R71H104ME14D | GRM155R71H104ME14D
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71H104ME14-01.pdf | http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71H104ME14-01.pdf
|  | CompType | Capacitor | Capacitor
|  | Description | CAP, CERM, 0.1 uF, 50 V, +/- 20%, X7R, 0402 | CAP, CERM, 0.1 uF, 50 V, +/- 20%, X7R, 0402
|  | ESR_ohm |  |
|  | Footprint | 0402S | 0402S
|  | IRMS_A |  |
|  | LatestRevisionDate | 2017-03-09 | 2017-03-09
|  | Manufacturer | MuRata | MuRata
|  | MountType | SMT | SMT
|  | PackageReference | 0402 | 0402
|  | PartNumber | GRM155R71H104ME14D | GRM155R71H104ME14D
|  | Polarized | N | N
|  | Published | 2008-06-19 | 2008-06-19
|  | Publisher | Texas Instruments | Texas Instruments
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 0.5 | 0.5
|  | SizeAreaWB_mm2 | 3 | 3
|  | SizeX_mm | 1 | 1
|  | SizeY_mm | 0.5 | 0.5
|  | SizeZ_mm | 0.6 | 0.6
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Mouser | Mouser
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | 490-10701-1-ND | 490-10701-1-ND
|  | Supplier Part Number 2 | 81-GRM155R71H104ME4D | 81-GRM155R71H104ME4D
|  | Supplier Part Number 3 |  |
|  | TaMax_C | 125°C | 125°C
|  | TaMin_C | -55°C | -55°C
|  | Technology | Ceramic | Ceramic
|  | TempCo | X7R | X7R
|  | Tolerance_% | 20% | 20%
|  | U/M | EA | EA
|  | Value | 0.1uF | 0.1uF
|  | Value1 | Unknown | Unknown
|  | Value2 | 50V | 50V
|  | ValueDisplayed | 0.1uF | 0.1uF
|  | VDC_V | 50V | 50V
C12 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade |  |
|  | AEC Qualified | ? | ?
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Cap_Case | 0402 | 0402
|  | Cap_F | 220nF | 220nF
|  | Comment | GRM155R71C224KA12D | GRM155R71C224KA12D
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R71C224KA12D&x=9&y=9&search=startwith | http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R71C224KA12D&x=9&y=9&search=startwith
|  | CompType | Capacitor | Capacitor
|  | Description | CAP, CERM, 0.22 uF, 16 V, +/- 10%, X7R, 0402 | CAP, CERM, 0.22 uF, 16 V, +/- 10%, X7R, 0402
|  | ESR_ohm |  |
|  | Footprint | 0402S | 0402S
|  | IRMS_A |  |
|  | LatestRevisionDate | 2017-03-09 | 2017-03-09
|  | Manufacturer | MuRata | MuRata
|  | MountType | SMT | SMT
|  | PackageReference | 0402 | 0402
|  | PartNumber | GRM155R71C224KA12D | GRM155R71C224KA12D
|  | Polarized | N | N
|  | Published | 2008-06-19 | 2008-06-19
|  | Publisher | Texas Instruments | Texas Instruments
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 0.5 | 0.5
|  | SizeAreaWB_mm2 | 3 | 3
|  | SizeX_mm | 1 | 1
|  | SizeY_mm | 0.5 | 0.5
|  | SizeZ_mm | 0.6 | 0.6
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Mouser | Mouser
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | 490-5418-1-ND | 490-5418-1-ND
|  | Supplier Part Number 2 | 81-GRM155R71C224KA2D | 81-GRM155R71C224KA2D
|  | Supplier Part Number 3 |  |
|  | TaMax_C | 125°C | 125°C
|  | TaMin_C | -55°C | -55°C
|  | Technology | Ceramic | Ceramic
|  | TempCo | X7R | X7R
|  | Tolerance_% | 10% | 10%
|  | U/M | EA | EA
|  | Value | 0.22uF | 0.22uF
|  | Value1 | Unknown | Unknown
|  | Value2 | 16V | 16V
|  | ValueDisplayed | 0.22uF | 0.22uF
|  | VDC_V | 16V | 16V
C13 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade |  |
|  | AEC Qualified | ? | ?
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Cap_Case | 0402 | 0402
|  | Cap_F | 330pF | 330pF
|  | Comment | GRM155R71H331KA01D | GRM155R71H331KA01D
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R71H331KA01D&x=9&y=9&search=startwith | http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R71H331KA01D&x=9&y=9&search=startwith
|  | CompType | Capacitor | Capacitor
|  | Description | CAP, CERM, 330 pF, 50 V, +/- 10%, X7R, 0402 | CAP, CERM, 330 pF, 50 V, +/- 10%, X7R, 0402
|  | ESR_ohm |  |
|  | Footprint | 0402S | 0402S
|  | IRMS_A |  |
|  | LatestRevisionDate | 2017-03-09 | 2017-03-09
|  | Manufacturer | MuRata | MuRata
|  | MountType | SMT | SMT
|  | PackageReference | 0402 | 0402
|  | PartNumber | GRM155R71H331KA01D | GRM155R71H331KA01D
|  | Polarized | N | N
|  | Published | 2008-06-19 | 2008-06-19
|  | Publisher | Texas Instruments | Texas Instruments
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 0.5 | 0.5
|  | SizeAreaWB_mm2 | 3 | 3
|  | SizeX_mm | 1 | 1
|  | SizeY_mm | 0.5 | 0.5
|  | SizeZ_mm | 0.6 | 0.6
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Mouser | Mouser
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | 490-3247-1-ND | 490-3247-1-ND
|  | Supplier Part Number 2 | 81-GRM36X331K50 | 81-GRM36X331K50
|  | Supplier Part Number 3 |  |
|  | TaMax_C | 125°C | 125°C
|  | TaMin_C | -55°C | -55°C
|  | Technology | Ceramic | Ceramic
|  | TempCo | X7R | X7R
|  | Tolerance_% | 10% | 10%
|  | U/M | EA | EA
|  | Value | 330pF | 330pF
|  | Value1 | Unknown | Unknown
|  | Value2 | 50V | 50V
|  | ValueDisplayed | 330pF | 330pF
|  | VDC_V | 50V | 50V
C14 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade |  |
|  | AEC Qualified | ? | ?
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Cap_Case | 0402 | 0402
|  | Cap_F | 330pF | 330pF
|  | Comment | GRM155R71H331KA01D | GRM155R71H331KA01D
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R71H331KA01D&x=9&y=9&search=startwith | http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R71H331KA01D&x=9&y=9&search=startwith
|  | CompType | Capacitor | Capacitor
|  | Description | CAP, CERM, 330 pF, 50 V, +/- 10%, X7R, 0402 | CAP, CERM, 330 pF, 50 V, +/- 10%, X7R, 0402
|  | ESR_ohm |  |
|  | Footprint | 0402S | 0402S
|  | IRMS_A |  |
|  | LatestRevisionDate | 2017-03-09 | 2017-03-09
|  | Manufacturer | MuRata | MuRata
|  | MountType | SMT | SMT
|  | PackageReference | 0402 | 0402
|  | PartNumber | GRM155R71H331KA01D | GRM155R71H331KA01D
|  | Polarized | N | N
|  | Published | 2008-06-19 | 2008-06-19
|  | Publisher | Texas Instruments | Texas Instruments
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 0.5 | 0.5
|  | SizeAreaWB_mm2 | 3 | 3
|  | SizeX_mm | 1 | 1
|  | SizeY_mm | 0.5 | 0.5
|  | SizeZ_mm | 0.6 | 0.6
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Mouser | Mouser
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | 490-3247-1-ND | 490-3247-1-ND
|  | Supplier Part Number 2 | 81-GRM36X331K50 | 81-GRM36X331K50
|  | Supplier Part Number 3 |  |
|  | TaMax_C | 125°C | 125°C
|  | TaMin_C | -55°C | -55°C
|  | Technology | Ceramic | Ceramic
|  | TempCo | X7R | X7R
|  | Tolerance_% | 10% | 10%
|  | U/M | EA | EA
|  | Value | 330pF | 330pF
|  | Value1 | Unknown | Unknown
|  | Value2 | 50V | 50V
|  | ValueDisplayed | 330pF | 330pF
|  | VDC_V | 50V | 50V
C15 | HVP053B_sheet1.schdoc |  | Fitted | Not Fitted
|  | AEC Category | Q200 |
|  | AEC Grade |  |
|  | AEC Qualified | ? |
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Cap_Case | 0805 |
|  | Cap_F | 1nF |
|  | Comment | GRM21AR72E102KW01D |
|  | ComponentLink1Description | Datasheet link |
|  | ComponentLink1URL | http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM21AR72E102KW01D&x=9&y=9&search=startwith |
|  | CompType | Capacitor |
|  | Description | CAP, CERM, 1000 pF, 250 V, +/- 10%, X7R, 0805 |
|  | ESR_ohm |  |
|  | Footprint | 0805L |
|  | IRMS_A |  |
|  | LatestRevisionDate | 2017-03-09 |
|  | Manufacturer | MuRata |
|  | MountType | SMT |
|  | PackageReference | 0805 |
|  | PartNumber | GRM21AR72E102KW01D |
|  | Polarized | N |
|  | Published | 2008-06-19 |
|  | Publisher | Texas Instruments |
|  | RoHS | Y |
|  | SizeArea_mm2 | 2.5 |
|  | SizeAreaWB_mm2 | 6.75 |
|  | SizeX_mm | 2 |
|  | SizeY_mm | 1.25 |
|  | SizeZ_mm | 1.45 |
|  | Supplier 1 | Digi-Key |
|  | Supplier 2 | Mouser |
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | 490-3525-1-ND |
|  | Supplier Part Number 2 | 81-GRM21AR72E102KW01 |
|  | Supplier Part Number 3 |  |
|  | TaMax_C | 125°C |
|  | TaMin_C | -55°C |
|  | Technology | Ceramic |
|  | TempCo | X7R |
|  | Tolerance_% | 10% |
|  | U/M | EA |
|  | Value | 1000pF |
|  | Value1 | Unknown |
|  | Value2 | 250V |
|  | ValueDisplayed | 1000pF |
|  | VDC_V | 250V |
C16 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade |  |
|  | AEC Qualified | ? | ?
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Cap_Case | 0805 | 0805
|  | Cap_F | 1.5nF | 1.5nF
|  | Comment | GRM21AR72E152KW01D | GRM21AR72E152KW01D
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM21AR72E152KW01D&x=9&y=9&search=startwith | http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM21AR72E152KW01D&x=9&y=9&search=startwith
|  | CompType | Capacitor | Capacitor
|  | Description | CAP, CERM, 1500 pF, 250 V, +/- 10%, X7R, 0805 | CAP, CERM, 1500 pF, 250 V, +/- 10%, X7R, 0805
|  | ESR_ohm |  |
|  | Footprint | 0805_HV1 | 0805_HV1
|  | IRMS_A |  |
|  | LatestRevisionDate | 2017-03-09 | 2017-03-09
|  | Manufacturer | MuRata | MuRata
|  | MountType | SMT | SMT
|  | PackageReference | 0805 | 0805
|  | PartNumber | GRM21AR72E152KW01D | GRM21AR72E152KW01D
|  | Polarized | N | N
|  | Published | 2008-06-19 | 2008-06-19
|  | Publisher | Texas Instruments | Texas Instruments
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 2.5 | 2.5
|  | SizeAreaWB_mm2 | 6.75 | 6.75
|  | SizeX_mm | 2 | 2
|  | SizeY_mm | 1.25 | 1.25
|  | SizeZ_mm | 1.45 | 1.45
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Mouser | Mouser
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | 490-3527-1-ND | 490-3527-1-ND
|  | Supplier Part Number 2 | 81-GRM21AR72E152KW01 | 81-GRM21AR72E152KW01
|  | Supplier Part Number 3 |  |
|  | TaMax_C | 125°C | 125°C
|  | TaMin_C | -55°C | -55°C
|  | Technology | Ceramic | Ceramic
|  | TempCo | X7R | X7R
|  | Tolerance_% | 10% | 10%
|  | U/M | EA | EA
|  | Value | 1500pF | 1500pF
|  | Value1 | Unknown | Unknown
|  | Value2 | 250V | 250V
|  | ValueDisplayed | 1500pF | 1500pF
|  | VDC_V | 250V | 250V
C17 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | N/A | N/A
|  | AEC Qualified | N | N
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Cap_Case | 0402 | 0402
|  | Cap_F | 100nF | 100nF
|  | Comment | GRM155R71H104ME14D | GRM155R71H104ME14D
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71H104ME14-01.pdf | http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71H104ME14-01.pdf
|  | CompType | Capacitor | Capacitor
|  | Description | CAP, CERM, 0.1 uF, 50 V, +/- 20%, X7R, 0402 | CAP, CERM, 0.1 uF, 50 V, +/- 20%, X7R, 0402
|  | ESR_ohm |  |
|  | Footprint | 0402S | 0402S
|  | IRMS_A |  |
|  | LatestRevisionDate | 2017-03-09 | 2017-03-09
|  | Manufacturer | MuRata | MuRata
|  | MountType | SMT | SMT
|  | PackageReference | 0402 | 0402
|  | PartNumber | GRM155R71H104ME14D | GRM155R71H104ME14D
|  | Polarized | N | N
|  | Published | 2008-06-19 | 2008-06-19
|  | Publisher | Texas Instruments | Texas Instruments
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 0.5 | 0.5
|  | SizeAreaWB_mm2 | 3 | 3
|  | SizeX_mm | 1 | 1
|  | SizeY_mm | 0.5 | 0.5
|  | SizeZ_mm | 0.6 | 0.6
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Mouser | Mouser
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | 490-10701-1-ND | 490-10701-1-ND
|  | Supplier Part Number 2 | 81-GRM155R71H104ME4D | 81-GRM155R71H104ME4D
|  | Supplier Part Number 3 |  |
|  | TaMax_C | 125°C | 125°C
|  | TaMin_C | -55°C | -55°C
|  | Technology | Ceramic | Ceramic
|  | TempCo | X7R | X7R
|  | Tolerance_% | 20% | 20%
|  | U/M | EA | EA
|  | Value | 0.1uF | 0.1uF
|  | Value1 | Unknown | Unknown
|  | Value2 | 50V | 50V
|  | ValueDisplayed | 0.1uF | 0.1uF
|  | VDC_V | 50V | 50V
C18 | HVP053B_sheet1.schdoc |  | Fitted | Not Fitted
|  | AC_Safety |  |
|  | AEC Category | Q200 |
|  | AEC Grade | N/A |
|  | AEC Qualified | N |
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Cap_Case | 1210 |
|  | Cap_F | 22µF |
|  | Comment | GMK325BJ226MM-P |
|  | ComponentLink1Description | Datasheet link |
|  | ComponentLink1URL | http://ds.yuden.co.jp/TYCOMPAS/ut/detail.do?productNo=GMK325BJ226MM-P&fileName=GMK325BJ226MM-P_SS&mode=specSheetDownload |
|  | CompType | Capacitor |
|  | Description | CAP, CERM, 22 µF, 35 V,+/- 20%, X5R, 1210 |
|  | ESR_ohm |  |
|  | Footprint | 1210L |
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | IRMS_A |  |
|  | Manufacturer | Taiyo Yuden |
|  | MountType | SMT |
|  | PackageReference | 1210 |
|  | PartNumber | GMK325BJ226MM-P |
|  | Polarized | N |
|  | RoHS | Y |
|  | SizeArea_mm2 | 8 |
|  | SizeAreaWB_mm2 | 14.7 |
|  | SizeX_mm | 3.2 |
|  | SizeY_mm | 2.5 |
|  | SizeZ_mm | 1.35 |
|  | Supplier 1 |  |
|  | Supplier 2 |  |
|  | Supplier 3 |  |
|  | Supplier Part Number 1 |  |
|  | Supplier Part Number 2 |  |
|  | Supplier Part Number 3 |  |
|  | TaMax_C | 85°C |
|  | TaMin_C | -55°C |
|  | Technology | Ceramic |
|  | TempCo | X5R |
|  | Tolerance_% | 20% |
|  | U/M | EA |
|  | VAC |  |
|  | VAC_X |  |
|  | VAC_Y |  |
|  | Value | 22uF |
|  | Value1 |  |
|  | Value2 | 35V |
|  | ValueDisplayed | 22µF |
|  | VDC_V | 35V |
C19 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade |  |
|  | AEC Qualified | ? | ?
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Cap_Case | 0402 | 0402
|  | Cap_F | 100pF | 100pF
|  | Comment | GRM1555C1H101JA01D | GRM1555C1H101JA01D
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM1555C1H101JA01D&x=9&y=9&search=startwith | http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM1555C1H101JA01D&x=9&y=9&search=startwith
|  | CompType | Capacitor | Capacitor
|  | Description | CAP, CERM, 100 pF, 50 V, +/- 5%, C0G/NP0, 0402 | CAP, CERM, 100 pF, 50 V, +/- 5%, C0G/NP0, 0402
|  | ESR_ohm |  |
|  | Footprint | 0402S | 0402S
|  | IRMS_A |  |
|  | LatestRevisionDate | 2017-03-09 | 2017-03-09
|  | Manufacturer | MuRata | MuRata
|  | MountType | SMT | SMT
|  | PackageReference | 0402 | 0402
|  | PartNumber | GRM1555C1H101JA01D | GRM1555C1H101JA01D
|  | Polarized | N | N
|  | Published | 2008-06-19 | 2008-06-19
|  | Publisher | Texas Instruments | Texas Instruments
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 0.5 | 0.5
|  | SizeAreaWB_mm2 | 3 | 3
|  | SizeX_mm | 1 | 1
|  | SizeY_mm | 0.5 | 0.5
|  | SizeZ_mm | 0.6 | 0.6
|  | Supplier 1 | Mouser | Mouser
|  | Supplier 2 |  |
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | 81-GRM1555C1H101JA1D | 81-GRM1555C1H101JA1D
|  | Supplier Part Number 2 |  |
|  | Supplier Part Number 3 |  |
|  | TaMax_C | 125°C | 125°C
|  | TaMin_C | -55°C | -55°C
|  | Technology | Ceramic | Ceramic
|  | TempCo | C0G/NP0 | C0G/NP0
|  | Tolerance_% | 5% | 5%
|  | U/M | EA | EA
|  | Value | 100pF | 100pF
|  | Value1 | Unknown | Unknown
|  | Value2 | 50V | 50V
|  | ValueDisplayed | 100pF | 100pF
|  | VDC_V | 50V | 50V
C20 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AC_Safety | X1Y1 | X1Y1
|  | AEC Category | Q200 | Q200
|  | AEC Grade | N/A | N/A
|  | AEC Qualified | N | N
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Cap_Case | 9x13mm | 9x13mm
|  | Cap_F | 2.2nF | 2.2nF
|  | Comment | C921U222MVVDBA7317 | C921U222MVVDBA7317
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | https://content.kemet.com/datasheets/KEM_C1068_X1_400_VAC_Y1_400_VAC.pdf | https://content.kemet.com/datasheets/KEM_C1068_X1_400_VAC_Y1_400_VAC.pdf
|  | CompType | Capacitor | Capacitor
|  | Description | CAP, CERM, 2200 pF, X1 400 VAC/Y1 400 VAC, +/- 20%, Y5V, D9xL13mm | CAP, CERM, 2200 pF, X1 400 VAC/Y1 400 VAC, +/- 20%, Y5V, D9xL13mm
|  | ESR_ohm |  |
|  | Footprint | C900_9x13 | C900_9x13
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | IRMS_A |  |
|  | Manufacturer | Kemet | Kemet
|  | MountType | TH | TH
|  | PackageReference | D9xL13mm | D9xL13mm
|  | PartNumber | C921U222MVVDBA7317 | C921U222MVVDBA7317
|  | Polarized | N | N
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 81 | 81
|  | SizeAreaWB_mm2 | 121 | 121
|  | SizeX_mm | 9 | 9
|  | SizeY_mm | 9 | 9
|  | SizeZ_mm | 13 | 13
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Newark | Newark
|  | Supplier 3 | Mouser | Mouser
|  | Supplier Part Number 1 | 399-9487-1-ND | 399-9487-1-ND
|  | Supplier Part Number 2 | 31Y0991 | 31Y0991
|  | Supplier Part Number 3 | 80-C921U222MVVDBAP | 80-C921U222MVVDBAP
|  | TaMax_C | 125°C | 125°C
|  | TaMin_C | -40°C | -40°C
|  | Technology | Ceramic | Ceramic
|  | TempCo | Y5V | Y5V
|  | Tolerance_% | 20% | 20%
|  | U/M | EA | EA
|  | VAC |  |
|  | VAC_X | 400V | 400V
|  | VAC_Y | 400V | 400V
|  | Value | 2200pF | 2200pF
|  | Value1 |  |
|  | Value2 |  |
|  | ValueDisplayed | 2200pF | 2200pF
|  | VDC_V |  |
C21 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade |  |
|  | AEC Qualified | ? | ?
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Cap_Case | 0402 | 0402
|  | Cap_F | 100pF | 100pF
|  | Comment | GRM1555C1H101JA01D | GRM1555C1H101JA01D
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM1555C1H101JA01D&x=9&y=9&search=startwith | http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM1555C1H101JA01D&x=9&y=9&search=startwith
|  | CompType | Capacitor | Capacitor
|  | Description | CAP, CERM, 100 pF, 50 V, +/- 5%, C0G/NP0, 0402 | CAP, CERM, 100 pF, 50 V, +/- 5%, C0G/NP0, 0402
|  | ESR_ohm |  |
|  | Footprint | 0402S | 0402S
|  | IRMS_A |  |
|  | LatestRevisionDate | 2017-03-09 | 2017-03-09
|  | Manufacturer | MuRata | MuRata
|  | MountType | SMT | SMT
|  | PackageReference | 0402 | 0402
|  | PartNumber | GRM1555C1H101JA01D | GRM1555C1H101JA01D
|  | Polarized | N | N
|  | Published | 2008-06-19 | 2008-06-19
|  | Publisher | Texas Instruments | Texas Instruments
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 0.5 | 0.5
|  | SizeAreaWB_mm2 | 3 | 3
|  | SizeX_mm | 1 | 1
|  | SizeY_mm | 0.5 | 0.5
|  | SizeZ_mm | 0.6 | 0.6
|  | Supplier 1 | Mouser | Mouser
|  | Supplier 2 |  |
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | 81-GRM1555C1H101JA1D | 81-GRM1555C1H101JA1D
|  | Supplier Part Number 2 |  |
|  | Supplier Part Number 3 |  |
|  | TaMax_C | 125°C | 125°C
|  | TaMin_C | -55°C | -55°C
|  | Technology | Ceramic | Ceramic
|  | TempCo | C0G/NP0 | C0G/NP0
|  | Tolerance_% | 5% | 5%
|  | U/M | EA | EA
|  | Value | 100pF | 100pF
|  | Value1 | Unknown | Unknown
|  | Value2 | 50V | 50V
|  | ValueDisplayed | 100pF | 100pF
|  | VDC_V | 50V | 50V
C22 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AC_Safety |  |
|  | AEC Category | Q200 | Q200
|  | AEC Grade | N/A | N/A
|  | AEC Qualified | N | N
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Cap_Case | 1210 | 1210
|  | Cap_F | 22µF | 22µF
|  | Comment | GMK325BJ226MM-P | GMK325BJ226MM-P
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://ds.yuden.co.jp/TYCOMPAS/ut/detail.do?productNo=GMK325BJ226MM-P&fileName=GMK325BJ226MM-P_SS&mode=specSheetDownload | http://ds.yuden.co.jp/TYCOMPAS/ut/detail.do?productNo=GMK325BJ226MM-P&fileName=GMK325BJ226MM-P_SS&mode=specSheetDownload
|  | CompType | Capacitor | Capacitor
|  | Description | CAP, CERM, 22 µF, 35 V,+/- 20%, X5R, 1210 | CAP, CERM, 22 µF, 35 V,+/- 20%, X5R, 1210
|  | ESR_ohm |  |
|  | Footprint | 1210L | 1210L
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | IRMS_A |  |
|  | Manufacturer | Taiyo Yuden | Taiyo Yuden
|  | MountType | SMT | SMT
|  | PackageReference | 1210 | 1210
|  | PartNumber | GMK325BJ226MM-P | GMK325BJ226MM-P
|  | Polarized | N | N
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 8 | 8
|  | SizeAreaWB_mm2 | 14.7 | 14.7
|  | SizeX_mm | 3.2 | 3.2
|  | SizeY_mm | 2.5 | 2.5
|  | SizeZ_mm | 1.35 | 1.35
|  | Supplier 1 |  |
|  | Supplier 2 |  |
|  | Supplier 3 |  |
|  | Supplier Part Number 1 |  |
|  | Supplier Part Number 2 |  |
|  | Supplier Part Number 3 |  |
|  | TaMax_C | 85°C | 85°C
|  | TaMin_C | -55°C | -55°C
|  | Technology | Ceramic | Ceramic
|  | TempCo | X5R | X5R
|  | Tolerance_% | 20% | 20%
|  | U/M | EA | EA
|  | VAC |  |
|  | VAC_X |  |
|  | VAC_Y |  |
|  | Value | 22uF | 22uF
|  | Value1 |  |
|  | Value2 | 35V | 35V
|  | ValueDisplayed | 22µF | 22µF
|  | VDC_V | 35V | 35V
C23 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | 1 | 1
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Cap_Case | 0603 | 0603
|  | Cap_F | 1µF | 1µF
|  | Comment | CGA3E1X7R1V105K080AC | CGA3E1X7R1V105K080AC
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=CGA3E1X7R1V105K080AC | https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=CGA3E1X7R1V105K080AC
|  | CompType | Capacitor | Capacitor
|  | Description | CAP, CERM, 1 uF, 35 V, +/- 10%, X7R, AEC-Q200 Grade 1, 0603 | CAP, CERM, 1 uF, 35 V, +/- 10%, X7R, AEC-Q200 Grade 1, 0603
|  | ESR_ohm | 5.522m | 5.522m
|  | Footprint | 0603S | 0603S
|  | IRMS_A | 2.21617A | 2.21617A
|  | LatestRevisionDate | 2017-03-09 | 2017-03-09
|  | Manufacturer | TDK | TDK
|  | MountType | SMT | SMT
|  | PackageReference | 0603 | 0603
|  | PartNumber | CGA3E1X7R1V105K080AC | CGA3E1X7R1V105K080AC
|  | Polarized | N | N
|  | Published | 2008-06-19 | 2008-06-19
|  | Publisher | Texas Instruments | Texas Instruments
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 1.28 | 1.28
|  | SizeAreaWB_mm2 | 4.68 | 4.68
|  | SizeX_mm | 1.6 | 1.6
|  | SizeY_mm | 0.8 | 0.8
|  | SizeZ_mm | 1 | 1
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Mouser | Mouser
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | 445-174215-1-ND | 445-174215-1-ND
|  | Supplier Part Number 2 | 810-CGA3E1X7R1V105K080AC | 810-CGA3E1X7R1V105K080AC
|  | Supplier Part Number 3 |  |
|  | TaMax_C | 125°C | 125°C
|  | TaMin_C | -55°C | -55°C
|  | Technology | Ceramic | Ceramic
|  | TempCo | X7R | X7R
|  | Tolerance_% | 10% | 10%
|  | U/M | EA | EA
|  | Value | 1uF | 1uF
|  | Value1 | 0.005522 ohm | 0.005522 ohm
|  | Value2 | 35V | 35V
|  | ValueDisplayed | 1uF | 1uF
|  | VDC_V | 35V | 35V
C24 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | 1 | 1
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Cap_Case | 0402 | 0402
|  | Cap_F | 22pF | 22pF
|  | Comment | GCM1555C1H220JA16D | GCM1555C1H220JA16D
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://psearch.murata.com/capacitor/product/GCM1555C1H220JA16%23.pdf | http://psearch.murata.com/capacitor/product/GCM1555C1H220JA16%23.pdf
|  | CompType | Capacitor | Capacitor
|  | Description | CAP, CERM, 22 pF, 50 V, +/- 5%, C0G/NP0, AEC-Q200 Grade 1, 0402 | CAP, CERM, 22 pF, 50 V, +/- 5%, C0G/NP0, AEC-Q200 Grade 1, 0402
|  | ESR_ohm |  |
|  | Footprint | 0402S | 0402S
|  | IRMS_A |  |
|  | LatestRevisionDate | 2017-03-09 | 2017-03-09
|  | Manufacturer | MuRata | MuRata
|  | MountType | SMT | SMT
|  | PackageReference | 0402 | 0402
|  | PartNumber | GCM1555C1H220JA16D | GCM1555C1H220JA16D
|  | Polarized | N | N
|  | Published | 2008-06-19 | 2008-06-19
|  | Publisher | Texas Instruments | Texas Instruments
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 0.5 | 0.5
|  | SizeAreaWB_mm2 | 3 | 3
|  | SizeX_mm | 1 | 1
|  | SizeY_mm | 0.5 | 0.5
|  | SizeZ_mm | 0.6 | 0.6
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Mouser | Mouser
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | 490-9648-1-ND | 490-9648-1-ND
|  | Supplier Part Number 2 | 81-GCM1555C1H220JA6D | 81-GCM1555C1H220JA6D
|  | Supplier Part Number 3 |  |
|  | TaMax_C | 125°C | 125°C
|  | TaMin_C | -55°C | -55°C
|  | Technology | Ceramic | Ceramic
|  | TempCo | C0G/NP0 | C0G/NP0
|  | Tolerance_% | 5% | 5%
|  | U/M | EA | EA
|  | Value | 22pF | 22pF
|  | Value1 | Unknown | Unknown
|  | Value2 | 50V | 50V
|  | ValueDisplayed | 22pF | 22pF
|  | VDC_V | 50V | 50V
C25 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade |  |
|  | AEC Qualified | ? | ?
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Cap_Case | 0402 | 0402
|  | Cap_F | 15nF | 15nF
|  | Comment | GRM155R71H153KA12D | GRM155R71H153KA12D
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R71H153KA12D&x=9&y=9&search=startwith | http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R71H153KA12D&x=9&y=9&search=startwith
|  | CompType | Capacitor | Capacitor
|  | Description | CAP, CERM, 0.015 uF, 50 V, +/- 10%, X7R, 0402 | CAP, CERM, 0.015 uF, 50 V, +/- 10%, X7R, 0402
|  | ESR_ohm |  |
|  | Footprint | 0402S | 0402S
|  | IRMS_A |  |
|  | LatestRevisionDate | 2017-03-09 | 2017-03-09
|  | Manufacturer | MuRata | MuRata
|  | MountType | SMT | SMT
|  | PackageReference | 0402 | 0402
|  | PartNumber | GRM155R71H153KA12D | GRM155R71H153KA12D
|  | Polarized | N | N
|  | Published | 2008-06-19 | 2008-06-19
|  | Publisher | Texas Instruments | Texas Instruments
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 0.5 | 0.5
|  | SizeAreaWB_mm2 | 3 | 3
|  | SizeX_mm | 1 | 1
|  | SizeY_mm | 0.5 | 0.5
|  | SizeZ_mm | 0.6 | 0.6
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Mouser | Mouser
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | 490-4517-1-ND | 490-4517-1-ND
|  | Supplier Part Number 2 | 81-GRM155R71H153KA2D | 81-GRM155R71H153KA2D
|  | Supplier Part Number 3 |  |
|  | TaMax_C | 125°C | 125°C
|  | TaMin_C | -55°C | -55°C
|  | Technology | Ceramic | Ceramic
|  | TempCo | X7R | X7R
|  | Tolerance_% | 10% | 10%
|  | U/M | EA | EA
|  | Value | 0.015uF | 0.015uF
|  | Value1 | Unknown | Unknown
|  | Value2 | 50V | 50V
|  | ValueDisplayed | 0.015uF | 0.015uF
|  | VDC_V | 50V | 50V
C26 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade |  |
|  | AEC Qualified | ? | ?
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Cap_Case | 1210 | 1210
|  | Cap_F | 22µF | 22µF
|  | Comment | GRM32ER71E226KE15L | GRM32ER71E226KE15L
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM32ER71E226KE15L&x=9&y=9&search=startwith | http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM32ER71E226KE15L&x=9&y=9&search=startwith
|  | CompType | Capacitor | Capacitor
|  | Description | CAP, CERM, 22 uF, 25 V, +/- 10%, X7R, 1210 | CAP, CERM, 22 uF, 25 V, +/- 10%, X7R, 1210
|  | ESR_ohm |  |
|  | Footprint | 1210_270L | 1210_270L
|  | IRMS_A |  |
|  | LatestRevisionDate | 2017-03-09 | 2017-03-09
|  | Manufacturer | MuRata | MuRata
|  | MountType | SMT | SMT
|  | PackageReference | 1210 | 1210
|  | PartNumber | GRM32ER71E226KE15L | GRM32ER71E226KE15L
|  | Polarized | N | N
|  | Published | 2008-06-19 | 2008-06-19
|  | Publisher | Texas Instruments | Texas Instruments
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 8 | 8
|  | SizeAreaWB_mm2 | 14.7 | 14.7
|  | SizeX_mm | 3.2 | 3.2
|  | SizeY_mm | 2.5 | 2.5
|  | SizeZ_mm | 2.7 | 2.7
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Mouser | Mouser
|  | Supplier 3 | Farnell | Farnell
|  | Supplier Part Number 1 | 490-5313-1-ND | 490-5313-1-ND
|  | Supplier Part Number 2 | 81-GRM32ER71E226KE5L | 81-GRM32ER71E226KE5L
|  | Supplier Part Number 3 | 1797019 | 1797019
|  | TaMax_C | 125°C | 125°C
|  | TaMin_C | -55°C | -55°C
|  | Technology | Ceramic | Ceramic
|  | TempCo | X7R | X7R
|  | Tolerance_% | 10% | 10%
|  | U/M | EA | EA
|  | Value | 22uF | 22uF
|  | Value1 | Unknown | Unknown
|  | Value2 | 25V | 25V
|  | ValueDisplayed | 22uF | 22uF
|  | VDC_V | 25V | 25V
C27 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade |  |
|  | AEC Qualified | ? | ?
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Cap_Case | 0402 | 0402
|  | Cap_F | 10nF | 10nF
|  | Comment | GRM155R71H103KA88D | GRM155R71H103KA88D
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R71H103KA88D&x=9&y=9&search=startwith | http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R71H103KA88D&x=9&y=9&search=startwith
|  | CompType | Capacitor | Capacitor
|  | Description | CAP, CERM, 0.01 uF, 50 V, +/- 10%, X7R, 0402 | CAP, CERM, 0.01 uF, 50 V, +/- 10%, X7R, 0402
|  | ESR_ohm |  |
|  | Footprint | 0402S | 0402S
|  | IRMS_A |  |
|  | LatestRevisionDate | 2017-03-09 | 2017-03-09
|  | Manufacturer | MuRata | MuRata
|  | MountType | SMT | SMT
|  | PackageReference | 0402 | 0402
|  | PartNumber | GRM155R71H103KA88D | GRM155R71H103KA88D
|  | Polarized | N | N
|  | Published | 2008-06-19 | 2008-06-19
|  | Publisher | Texas Instruments | Texas Instruments
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 0.5 | 0.5
|  | SizeAreaWB_mm2 | 3 | 3
|  | SizeX_mm | 1 | 1
|  | SizeY_mm | 0.5 | 0.5
|  | SizeZ_mm | 0.6 | 0.6
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Newark | Newark
|  | Supplier 3 | Mouser | Mouser
|  | Supplier Part Number 1 | 490-4516-1-ND | 490-4516-1-ND
|  | Supplier Part Number 2 | 14T3284 | 14T3284
|  | Supplier Part Number 3 | 81-GRM155R71H103KA8D | 81-GRM155R71H103KA8D
|  | TaMax_C | 125°C | 125°C
|  | TaMin_C | -55°C | -55°C
|  | Technology | Ceramic | Ceramic
|  | TempCo | X7R | X7R
|  | Tolerance_% | 10% | 10%
|  | U/M | EA | EA
|  | Value | 0.01uF | 0.01uF
|  | Value1 | Unknown | Unknown
|  | Value2 | 50V | 50V
|  | ValueDisplayed | 0.01uF | 0.01uF
|  | VDC_V | 50V | 50V
C28 | HVP053B_sheet1.schdoc |  | Fitted | Not Fitted
|  | AEC Category | Q200 |
|  | AEC Grade | 1 |
|  | AEC Qualified | Y |
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Cap_Case | 0402 |
|  | Cap_F | 22pF |
|  | Comment | GCM1555C1H220JA16D |
|  | ComponentLink1Description | Datasheet link |
|  | ComponentLink1URL | http://psearch.murata.com/capacitor/product/GCM1555C1H220JA16%23.pdf |
|  | CompType | Capacitor |
|  | Description | CAP, CERM, 22 pF, 50 V, +/- 5%, C0G/NP0, AEC-Q200 Grade 1, 0402 |
|  | ESR_ohm |  |
|  | Footprint | 0402S |
|  | IRMS_A |  |
|  | LatestRevisionDate | 2017-03-09 |
|  | Manufacturer | MuRata |
|  | MountType | SMT |
|  | PackageReference | 0402 |
|  | PartNumber | GCM1555C1H220JA16D |
|  | Polarized | N |
|  | Published | 2008-06-19 |
|  | Publisher | Texas Instruments |
|  | RoHS | Y |
|  | SizeArea_mm2 | 0.5 |
|  | SizeAreaWB_mm2 | 3 |
|  | SizeX_mm | 1 |
|  | SizeY_mm | 0.5 |
|  | SizeZ_mm | 0.6 |
|  | Supplier 1 | Digi-Key |
|  | Supplier 2 | Mouser |
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | 490-9648-1-ND |
|  | Supplier Part Number 2 | 81-GCM1555C1H220JA6D |
|  | Supplier Part Number 3 |  |
|  | TaMax_C | 125°C |
|  | TaMin_C | -55°C |
|  | Technology | Ceramic |
|  | TempCo | C0G/NP0 |
|  | Tolerance_% | 5% |
|  | U/M | EA |
|  | Value | 22pF |
|  | Value1 | Unknown |
|  | Value2 | 50V |
|  | ValueDisplayed | 22pF |
|  | VDC_V | 50V |
D1 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q101 | Q101
|  | AEC Qualified | N | N
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | RFU02VSM6STR | RFU02VSM6STR
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://rohmfs.rohm.com/en/products/databook/datasheet/discrete/diode/fast_recovery/rfu02vsm6s.pdf | http://rohmfs.rohm.com/en/products/databook/datasheet/discrete/diode/fast_recovery/rfu02vsm6s.pdf
|  | CompType | Diode | Diode
|  | Description | Diode, Standard Recovery Rectifier, 600 V, 0.2 A, 2x1.4mm | Diode, Standard Recovery Rectifier, 600 V, 0.2 A, 2x1.4mm
|  | Footprint | TUMD2SM | TUMD2SM
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Io_A | 200mA | 200mA
|  | Manufacturer | Rohm | Rohm
|  | MountType | SMT | SMT
|  | PackageReference | 2x1.4mm | 2x1.4mm
|  | PartNumber | RFU02VSM6STR | RFU02VSM6STR
|  | RJC_CperW |  |
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 3.5 | 3.5
|  | SizeAreaWB_mm2 | 8.4 | 8.4
|  | SizeX_mm | 2.5 | 2.5
|  | SizeY_mm | 1.4 | 1.4
|  | SizeZ_mm | 0.8 | 0.8
|  | TJmax_C | 150°C | 150°C
|  | Type | Standard Recovery Rectifier | Standard Recovery Rectifier
|  | Value | 600V | 600V
|  | Value1 | 0.2A | 0.2A
|  | Value2 | 2.2V | 2.2V
|  | Vf_V | 2.2V | 2.2V
|  | Vr_V | 600V | 600V
D2 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q101 | Q101
|  | AEC Qualified | N | N
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | RFU02VSM6STR | RFU02VSM6STR
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://rohmfs.rohm.com/en/products/databook/datasheet/discrete/diode/fast_recovery/rfu02vsm6s.pdf | http://rohmfs.rohm.com/en/products/databook/datasheet/discrete/diode/fast_recovery/rfu02vsm6s.pdf
|  | CompType | Diode | Diode
|  | Description | Diode, Standard Recovery Rectifier, 600 V, 0.2 A, 2x1.4mm | Diode, Standard Recovery Rectifier, 600 V, 0.2 A, 2x1.4mm
|  | Footprint | TUMD2SM | TUMD2SM
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Io_A | 200mA | 200mA
|  | Manufacturer | Rohm | Rohm
|  | MountType | SMT | SMT
|  | PackageReference | 2x1.4mm | 2x1.4mm
|  | PartNumber | RFU02VSM6STR | RFU02VSM6STR
|  | RJC_CperW |  |
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 3.5 | 3.5
|  | SizeAreaWB_mm2 | 8.4 | 8.4
|  | SizeX_mm | 2.5 | 2.5
|  | SizeY_mm | 1.4 | 1.4
|  | SizeZ_mm | 0.8 | 0.8
|  | TJmax_C | 150°C | 150°C
|  | Type | Standard Recovery Rectifier | Standard Recovery Rectifier
|  | Value | 600V | 600V
|  | Value1 | 0.2A | 0.2A
|  | Value2 | 2.2V | 2.2V
|  | Vf_V | 2.2V | 2.2V
|  | Vr_V | 600V | 600V
D3 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q101 | Q101
|  | AEC Qualified | N | N
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | CSFMT104-HF | CSFMT104-HF
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.comchiptech.com/cms/UserFiles/CSFMT104-HF%20Thru%20CSFMT108-HF%20RevC.pdf | http://www.comchiptech.com/cms/UserFiles/CSFMT104-HF%20Thru%20CSFMT108-HF%20RevC.pdf
|  | CompType | Diode | Diode
|  | Description | Diode, Superfast Rectifier, 200 V, 1 A, 3.5x1.6mm | Diode, Superfast Rectifier, 200 V, 1 A, 3.5x1.6mm
|  | Footprint | SOD-123H | SOD-123H
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Io_A | 1A | 1A
|  | Manufacturer | Comchip Technology | Comchip Technology
|  | MountType | SMT | SMT
|  | PackageReference | 3.5x1.6mm | 3.5x1.6mm
|  | PartNumber | CSFMT104-HF | CSFMT104-HF
|  | RJC_CperW |  |
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 5.6 | 5.6
|  | SizeAreaWB_mm2 | 11.7 | 11.7
|  | SizeX_mm | 3.5 | 3.5
|  | SizeY_mm | 1.6 | 1.6
|  | SizeZ_mm | 1 | 1
|  | TJmax_C | 150°C | 150°C
|  | Type | Superfast Rectifier | Superfast Rectifier
|  | Value | 200V | 200V
|  | Value1 | 1A | 1A
|  | Value2 | 0.95V | 0.95V
|  | Vf_V | 950mV | 950mV
|  | Vr_V | 200V | 200V
D5 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q101 | Q101
|  | AEC Qualified | ? | ?
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | BAS316,115 | BAS316,115
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.nexperia.com/documents/data_sheet/BAS16_SER.pdf | http://www.nexperia.com/documents/data_sheet/BAS16_SER.pdf
|  | CompType | Diode | Diode
|  | Description | Diode, Ultrafast, 100 V, 0.25 A, SOD-323 | Diode, Ultrafast, 100 V, 0.25 A, SOD-323
|  | Footprint | SOD-323 | SOD-323
|  | Green_EU RoHS | Incomplete | Incomplete
|  | Green_EU RoHS-2 | Incomplete | Incomplete
|  | Green_Lifecycle | Not Set | Not Set
|  | Green_REACh | Incomplete | Incomplete
|  | Io_A | 250mA | 250mA
|  | Manufacturer | Nexperia | Nexperia
|  | MountType | SMT | SMT
|  | PackageReference | SOD-323 | SOD-323
|  | PartNumber | BAS316,115 | BAS316,115
|  | RJC_CperW |  |
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 3.645 | 3.645
|  | SizeAreaWB_mm2 | 8.695 | 8.695
|  | SizeX_mm | 2.7 | 2.7
|  | SizeY_mm | 1.35 | 1.35
|  | SizeZ_mm | 1 | 1
|  | TJmax_C | 150°C | 150°C
|  | Type | Ultrafast | Ultrafast
|  | Value | 100V | 100V
|  | Value1 | 0.25A | 0.25A
|  | Value2 | 1.4V | 1.4V
|  | Vf_V | 1.4V | 1.4V
|  | Vr_V | 100V | 100V
D6 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Qualified | No | No
|  | Comment | CDSOD323-T18C | CDSOD323-T18C
|  | ComponentLink1Description | Datasheet | Datasheet
|  | ComponentLink1URL | https://www.bourns.com/docs/product-datasheets/cdsod323-txxc.pdf?sfvrsn=7112114e_8 | https://www.bourns.com/docs/product-datasheets/cdsod323-txxc.pdf?sfvrsn=7112114e_8
|  | Description | Diode, TVS, Bi, 18 V, SOD-323 | Diode, TVS, Bi, 18 V, SOD-323
|  | Footprint | FP-CDSOD323-T18C_SOD323-MFG | FP-CDSOD323-T18C_SOD323-MFG
|  | Manufacturer | Bourns Inc. | Bourns Inc.
|  | PackageReference | SOD323 | SOD323
|  | PartNumber | CDSOD323-T18C | CDSOD323-T18C
|  | RoHS | TRUE | TRUE
|  | SizeZ_mm | 1.14mm | 1.14mm
|  | Symbol Name | SYM-CDSOD323-T18C | SYM-CDSOD323-T18C
|  | Value | 18V | 18V
D7 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q101 | Q101
|  | AEC Qualified | ? | ?
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | BAS40W-05-7-F | BAS40W-05-7-F
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.diodes.com/datasheets/ds30114.pdf | http://www.diodes.com/datasheets/ds30114.pdf
|  | CompType | Diode | Diode
|  | Description | Diode, Schottky, 40 V, 0.2 A, SOT-323 | Diode, Schottky, 40 V, 0.2 A, SOT-323
|  | Footprint | SOT-323 | SOT-323
|  | Green_EU RoHS | Incomplete | Incomplete
|  | Green_EU RoHS-2 | Incomplete | Incomplete
|  | Green_Lifecycle | Not Set | Not Set
|  | Green_REACh | Incomplete | Incomplete
|  | Io_A | 200mA | 200mA
|  | Manufacturer | Diodes Inc. | Diodes Inc.
|  | MountType | SMT | SMT
|  | PackageReference | SOT-323 | SOT-323
|  | PartNumber | BAS40W-05-7-F | BAS40W-05-7-F
|  | RJC_CperW |  |
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 4.84 | 4.84
|  | SizeAreaWB_mm2 | 10.24 | 10.24
|  | SizeX_mm | 2.2 | 2.2
|  | SizeY_mm | 2.2 | 2.2
|  | SizeZ_mm | 1.1 | 1.1
|  | TJmax_C |  |
|  | Type | Schottky | Schottky
|  | Value | 40V | 40V
|  | Value1 | 0.2A | 0.2A
|  | Value2 | 0.8V | 0.8V
|  | Vf_V | 800mV | 800mV
|  | Vr_V | 40V | 40V
D8 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q101 | Q101
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | MRA4007T3G | MRA4007T3G
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.onsemi.com/pub_link/Collateral/MRA4003T3-D.PDF | http://www.onsemi.com/pub_link/Collateral/MRA4003T3-D.PDF
|  | CompType | Diode | Diode
|  | Description | Diode, Standard Recovery Rectifier, 1000 V, 1 A, AEC-Q101, SMA | Diode, Standard Recovery Rectifier, 1000 V, 1 A, AEC-Q101, SMA
|  | Footprint | SMA | SMA
|  | Green_EU RoHS | Passed with Exemption | Passed with Exemption
|  | Green_EU RoHS-2 | Passed | Passed
|  | Green_Lifecycle | Active | Active
|  | Green_REACh | Passed | Passed
|  | Io_A | 1A | 1A
|  | Manufacturer | ON Semiconductor | ON Semiconductor
|  | MountType | SMT | SMT
|  | PackageReference | SMA | SMA
|  | PartNumber | MRA4007T3G | MRA4007T3G
|  | RJC_CperW | 16.2 | 16.2
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 16.3228 | 16.3228
|  | SizeAreaWB_mm2 | 37.3428 | 37.3428
|  | SizeX_mm | 5.59 | 5.59
|  | SizeY_mm | 2.92 | 2.92
|  | SizeZ_mm | 2.87 | 2.87
|  | TJmax_C | 175°C | 175°C
|  | Type | Standard Recovery Rectifier | Standard Recovery Rectifier
|  | Value | 1000V | 1000V
|  | Value1 | 1A | 1A
|  | Value2 | 1.1V | 1.1V
|  | Vf_V | 1.1V | 1.1V
|  | Vr_V | 1kV | 1kV
D9 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q101 | Q101
|  | AEC Qualified | N | N
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | SMAJ150A | SMAJ150A
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | https://www.littelfuse.com/~/media/electronics/datasheets/tvs_diodes/littelfuse_tvs_diode_smaj_datasheet.pdf.pdf | https://www.littelfuse.com/~/media/electronics/datasheets/tvs_diodes/littelfuse_tvs_diode_smaj_datasheet.pdf.pdf
|  | CompType | TVS | TVS
|  | Description | Diode, TVS, Uni, 150 V, 243 Vc, 400 W, 1.6 A, SMA | Diode, TVS, Uni, 150 V, 243 Vc, 400 W, 1.6 A, SMA
|  | Footprint | SMA | SMA
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Ipp | 1.6A | 1.6A
|  | Manufacturer | Littelfuse | Littelfuse
|  | MountType | SMT | SMT
|  | PackageReference | SMA | SMA
|  | PartNumber | SMAJ150A | SMAJ150A
|  | Ppk | 400W | 400W
|  | RJA_CperW | 120 | 120
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 16.3228 | 16.3228
|  | SizeAreaWB_mm2 | 37.3428 | 37.3428
|  | SizeX_mm | 5.59 | 5.59
|  | SizeY_mm | 2.92 | 2.92
|  | SizeZ_mm | 2.87 | 2.87
|  | Value | 150V | 150V
|  | Value1 | 243V | 243V
|  | Vbr_Max | 185V | 185V
|  | Vbr_Min | 167V | 167V
|  | Vc | 243V | 243V
|  | VRWM | 150V | 150V
D10 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q101 | Q101
|  | AEC Qualified | N | N
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | SMAJ120A | SMAJ120A
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | https://www.littelfuse.com/~/media/electronics/datasheets/tvs_diodes/littelfuse_tvs_diode_smaj_datasheet.pdf.pdf | https://www.littelfuse.com/~/media/electronics/datasheets/tvs_diodes/littelfuse_tvs_diode_smaj_datasheet.pdf.pdf
|  | CompType | TVS | TVS
|  | Description | Diode, TVS, Uni, 120 V, 193 Vc, 400 W, 2.1 A, SMA | Diode, TVS, Uni, 120 V, 193 Vc, 400 W, 2.1 A, SMA
|  | Footprint | SMA | SMA
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Ipp | 2.1A | 2.1A
|  | Manufacturer | Littelfuse | Littelfuse
|  | MountType | SMT | SMT
|  | PackageReference | SMA | SMA
|  | PartNumber | SMAJ120A | SMAJ120A
|  | Ppk | 400W | 400W
|  | RJA_CperW | 120 | 120
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 16.3228 | 16.3228
|  | SizeAreaWB_mm2 | 37.3428 | 37.3428
|  | SizeX_mm | 5.59 | 5.59
|  | SizeY_mm | 2.92 | 2.92
|  | SizeZ_mm | 2.87 | 2.87
|  | Value | 120V | 120V
|  | Value1 | 193V | 193V
|  | Vbr_Max | 147V | 147V
|  | Vbr_Min | 133V | 133V
|  | Vc | 193V | 193V
|  | VRWM | 120V | 120V
D11 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q101 | Q101
|  | AEC Qualified | ? | ?
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | 1N4148X-TP | 1N4148X-TP
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.mccsemi.com/up_pdf/1N4148X(SOD-523).PDF | http://www.mccsemi.com/up_pdf/1N4148X(SOD-523).PDF
|  | CompType | Diode | Diode
|  | Description | Diode, Switching, 75 V, 0.3 A, SOD-523 | Diode, Switching, 75 V, 0.3 A, SOD-523
|  | Footprint | SOD-523 | SOD-523
|  | Green_EU RoHS | Incomplete | Incomplete
|  | Green_EU RoHS-2 | Incomplete | Incomplete
|  | Green_Lifecycle | Not Set | Not Set
|  | Green_REACh | Incomplete | Incomplete
|  | Io_A | 300mA | 300mA
|  | Manufacturer | Micro Commercial Components | Micro Commercial Components
|  | MountType | SMT | SMT
|  | PackageReference | SOD-523 | SOD-523
|  | PartNumber | 1N4148X-TP | 1N4148X-TP
|  | RJC_CperW |  |
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 1.53 | 1.53
|  | SizeAreaWB_mm2 | 5.13 | 5.13
|  | SizeX_mm | 1.7 | 1.7
|  | SizeY_mm | 0.9 | 0.9
|  | SizeZ_mm | 0.65 | 0.65
|  | TJmax_C | 150°C | 150°C
|  | Type | Switching | Switching
|  | Value | 75V | 75V
|  | Value1 | 0.3A | 0.3A
|  | Value2 | 1.25V | 1.25V
|  | Vf_V | 1.25V | 1.25V
|  | Vr_V | 75V | 75V
D12 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q101 | Q101
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | SZMM3Z27VST1G | SZMM3Z27VST1G
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | https://www.onsemi.com/pub/Collateral/MM3Z2V4ST1-D.PDF | https://www.onsemi.com/pub/Collateral/MM3Z2V4ST1-D.PDF
|  | CompType | Zener | Zener
|  | Description | Diode, Zener, 27 V, 300 mW, AEC-Q101, SOD-323 | Diode, Zener, 27 V, 300 mW, AEC-Q101, SOD-323
|  | Footprint | SOD-323 | SOD-323
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Manufacturer | ON Semiconductor | ON Semiconductor
|  | MountType | SMT | SMT
|  | PackageReference | SOD-323 | SOD-323
|  | PartNumber | SZMM3Z27VST1G | SZMM3Z27VST1G
|  | Power_W | 300mW | 300mW
|  | RJA_CperW | 416 | 416
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 3.645 | 3.645
|  | SizeAreaWB_mm2 | 8.695 | 8.695
|  | SizeX_mm | 2.7 | 2.7
|  | SizeY_mm | 1.35 | 1.35
|  | SizeZ_mm | 1 | 1
|  | Value | 27V | 27V
|  | Value1 | 0.3W | 0.3W
|  | Vz_V | 27V | 27V
D13 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q101 | Q101
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | BZT585B39T-7 | BZT585B39T-7
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.diodes.com/_files/datasheets/BZT585BxVxT.pdf | http://www.diodes.com/_files/datasheets/BZT585BxVxT.pdf
|  | CompType | Zener | Zener
|  | Description | Diode, Zener, 39 V, 350 mW, AEC-Q101, SOD-523 | Diode, Zener, 39 V, 350 mW, AEC-Q101, SOD-523
|  | Footprint | SOD-523 | SOD-523
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Manufacturer | Diodes Inc. | Diodes Inc.
|  | MountType | SMT | SMT
|  | PackageReference | SOD-523 | SOD-523
|  | PartNumber | BZT585B39T-7 | BZT585B39T-7
|  | Power_W | 350mW | 350mW
|  | RJA_CperW | 357 | 357
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 1.53 | 1.53
|  | SizeAreaWB_mm2 | 5.13 | 5.13
|  | SizeX_mm | 1.7 | 1.7
|  | SizeY_mm | 0.9 | 0.9
|  | SizeZ_mm | 0.65 | 0.65
|  | Value | 39V | 39V
|  | Value1 | 0.35W | 0.35W
|  | Vz_V | 39V | 39V
DB1 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q101 | Q101
|  | AEC Qualified | N | N
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | Z4DGP406L-HF | Z4DGP406L-HF
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.comchiptech.com/cms/UserFiles/Z4DGP406L-HF%20Thru.%20Z4DGP410L-HF%20RevA.pdf | http://www.comchiptech.com/cms/UserFiles/Z4DGP406L-HF%20Thru.%20Z4DGP410L-HF%20RevA.pdf
|  | CompType | Diode | Diode
|  | Description | Diode, P-N-Bridge, 600 V, 4 A, Z4-D | Diode, P-N-Bridge, 600 V, 4 A, Z4-D
|  | Footprint | Z4-D | Z4-D
|  | Green_EU RoHS | Incomplete | Incomplete
|  | Green_EU RoHS-2 | Incomplete | Incomplete
|  | Green_Lifecycle | Not Set | Not Set
|  | Green_REACh | Incomplete | Incomplete
|  | Io_A | 4 | 4
|  | LatestRevisionDate | 2017-06-26 | 2017-06-26
|  | Manufacturer | Comchip Technology | Comchip Technology
|  | MountType | SMT | SMT
|  | PackageReference | Z4-D | Z4-D
|  | PartNumber | Z4DGP406L-HF | Z4DGP406L-HF
|  | Published | 2008-06-26 | 2008-06-26
|  | Publisher | Texas Instruments | Texas Instruments
|  | RJC_CperW |  |
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 85.05 | 85.05
|  | SizeAreaWB_mm2 | 126.25 | 126.25
|  | SizeX_mm | 10.5 | 10.5
|  | SizeY_mm | 8.1 | 8.1
|  | SizeZ_mm | 1.55 | 1.55
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Mouser | Mouser
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | 641-1502-1-ND | 641-1502-1-ND
|  | Supplier Part Number 2 | 750-Z4DGP406L-HF | 750-Z4DGP406L-HF
|  | Supplier Part Number 3 |  |
|  | SymbolVersion | 2009-10-05 | 2009-10-05
|  | TJmax_C | 175 | 175
|  | Type | P-N-Bridge | P-N-Bridge
|  | U/M | EA | EA
|  | Value | 600V | 600V
|  | Value1 | 4A | 4A
|  | Value2 | 0.95V | 0.95V
|  | Vf_V | 0.95 | 0.95
|  | Vr_V | 600 | 600
F1 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | 39213150000 | 39213150000
|  | ComponentLink1Description | Datasheet URL | Datasheet URL
|  | ComponentLink1URL | http://www.littelfuse.com/data/en/Data_Sheets/Ltitelfuse_Fuse_392.pdf | http://www.littelfuse.com/data/en/Data_Sheets/Ltitelfuse_Fuse_392.pdf
|  | CompType | Fuse | Fuse
|  | Description | Fuse, 3.15 A, 250VAC/VDC, TH | Fuse, 3.15 A, 250VAC/VDC, TH
|  | Footprint | FUSE_392 | FUSE_392
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Interrupt_AC |  |
|  | Interrupt_DC |  |
|  | Irating_A | 3.15A | 3.15A
|  | Manufacturer | Littelfuse | Littelfuse
|  | MeltingTyp |  |
|  | MountType | TH | TH
|  | PackageReference | 8x8.5x4mm | 8x8.5x4mm
|  | PartNumber | 39213150000 | 39213150000
|  | RoHS | Y | Y
|  | Rtyp_Ohm |  |
|  | SizeArea_mm2 |  |
|  | SizeAreaWB_mm2 |  |
|  | SizeX_mm |  |
|  | SizeY_mm |  |
|  | SizeZ_mm |  |
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Newark | Newark
|  | Supplier 3 | Mouser | Mouser
|  | Supplier Part Number 1 | F5504CT-ND | F5504CT-ND
|  | Supplier Part Number 2 | 67K2152 | 67K2152
|  | Supplier Part Number 3 | 576-3921315000 | 576-3921315000
|  | VAC_V | 250V | 250V
|  | VDC_V | 250V | 250V
FID1 | HVP053B_Hardware.SchDoc |  | Fitted | Not Fitted
|  | ClassName | FiducialMark |
|  | Comment | Fiducial |
|  | CompType | Fiducial |
|  | Description | Fiducial mark. There is nothing to buy or mount. |
|  | Footprint | Fiducial6.4-20 |
|  | Manufacturer | N/A |
|  | MountType | N/A |
|  | PackageReference | N/A |
|  | PartNumber | N/A |
FID2 | HVP053B_Hardware.SchDoc |  | Fitted | Not Fitted
|  | ClassName | FiducialMark |
|  | Comment | Fiducial |
|  | CompType | Fiducial |
|  | Description | Fiducial mark. There is nothing to buy or mount. |
|  | Footprint | Fiducial6.4-20 |
|  | Manufacturer | N/A |
|  | MountType | N/A |
|  | PackageReference | N/A |
|  | PartNumber | N/A |
FID3 | HVP053B_Hardware.SchDoc |  | Fitted | Not Fitted
|  | ClassName | FiducialMark |
|  | Comment | Fiducial |
|  | CompType | Fiducial |
|  | Description | Fiducial mark. There is nothing to buy or mount. |
|  | Footprint | Fiducial6.4-20 |
|  | Manufacturer | N/A |
|  | MountType | N/A |
|  | PackageReference | N/A |
|  | PartNumber | N/A |
FID4 | HVP053B_Hardware.SchDoc |  | Fitted | Not Fitted
|  | ClassName | FiducialMark |
|  | Comment | Fiducial |
|  | CompType | Fiducial |
|  | Description | Fiducial mark. There is nothing to buy or mount. |
|  | Footprint | Fiducial6.4-20 |
|  | Manufacturer | N/A |
|  | MountType | N/A |
|  | PackageReference | N/A |
|  | PartNumber | N/A |
FID5 | HVP053B_Hardware.SchDoc |  | Fitted | Not Fitted
|  | ClassName | FiducialMark |
|  | Comment | Fiducial |
|  | CompType | Fiducial |
|  | Description | Fiducial mark. There is nothing to buy or mount. |
|  | Footprint | Fiducial6.4-20 |
|  | Manufacturer | N/A |
|  | MountType | N/A |
|  | PackageReference | N/A |
|  | PartNumber | N/A |
FID6 | HVP053B_Hardware.SchDoc |  | Fitted | Not Fitted
|  | ClassName | FiducialMark |
|  | Comment | Fiducial |
|  | CompType | Fiducial |
|  | Description | Fiducial mark. There is nothing to buy or mount. |
|  | Footprint | Fiducial6.4-20 |
|  | Manufacturer | N/A |
|  | MountType | N/A |
|  | PackageReference | N/A |
|  | PartNumber | N/A |
H1 | HVP053B_Hardware.SchDoc |  | Fitted | Fitted
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | ClassName | Mounting Holes | Mounting Holes
|  | Comment | NY PMS 440 0025 PH | NY PMS 440 0025 PH
|  | ComponentLink1Description | Datasheet Link | Datasheet Link
|  | ComponentLink1URL | http://www.fasnetdirect.com/refguide/Nylpanms.pdf | http://www.fasnetdirect.com/refguide/Nylpanms.pdf
|  | CompType | Hardware | Hardware
|  | Description | Machine Screw, Round, #4-40 x 1/4, Nylon, Philips panhead | Machine Screw, Round, #4-40 x 1/4, Nylon, Philips panhead
|  | Footprint | NY PMS 440 0025 PH | NY PMS 440 0025 PH
|  | Key | NY PMS 440 0025 PH | NY PMS 440 0025 PH
|  | LatestRevisionDate | 2017-03-09 | 2017-03-09
|  | Manufacturer | B&F Fastener Supply | B&F Fastener Supply
|  | MountType | N/A | N/A
|  | Note |  |
|  | PackageReference | Screw | Screw
|  | PartNumber | NY PMS 440 0025 PH | NY PMS 440 0025 PH
|  | Publisher | Texas Instruments | Texas Instruments
|  | RoHS | Y | Y
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 |  |
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | H542-ND | H542-ND
|  | Supplier Part Number 2 |  |
|  | Supplier Part Number 3 |  |
|  | Value |  |
H2 | HVP053B_Hardware.SchDoc |  | Fitted | Fitted
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | ClassName | Mounting Holes | Mounting Holes
|  | Comment | NY PMS 440 0025 PH | NY PMS 440 0025 PH
|  | ComponentLink1Description | Datasheet Link | Datasheet Link
|  | ComponentLink1URL | http://www.fasnetdirect.com/refguide/Nylpanms.pdf | http://www.fasnetdirect.com/refguide/Nylpanms.pdf
|  | CompType | Hardware | Hardware
|  | Description | Machine Screw, Round, #4-40 x 1/4, Nylon, Philips panhead | Machine Screw, Round, #4-40 x 1/4, Nylon, Philips panhead
|  | Footprint | NY PMS 440 0025 PH | NY PMS 440 0025 PH
|  | Key | NY PMS 440 0025 PH | NY PMS 440 0025 PH
|  | LatestRevisionDate | 2017-03-09 | 2017-03-09
|  | Manufacturer | B&F Fastener Supply | B&F Fastener Supply
|  | MountType | N/A | N/A
|  | Note |  |
|  | PackageReference | Screw | Screw
|  | PartNumber | NY PMS 440 0025 PH | NY PMS 440 0025 PH
|  | Publisher | Texas Instruments | Texas Instruments
|  | RoHS | Y | Y
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 |  |
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | H542-ND | H542-ND
|  | Supplier Part Number 2 |  |
|  | Supplier Part Number 3 |  |
|  | Value |  |
H3 | HVP053B_Hardware.SchDoc |  | Fitted | Fitted
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | ClassName | Mounting Holes | Mounting Holes
|  | Comment | NY PMS 440 0025 PH | NY PMS 440 0025 PH
|  | ComponentLink1Description | Datasheet Link | Datasheet Link
|  | ComponentLink1URL | http://www.fasnetdirect.com/refguide/Nylpanms.pdf | http://www.fasnetdirect.com/refguide/Nylpanms.pdf
|  | CompType | Hardware | Hardware
|  | Description | Machine Screw, Round, #4-40 x 1/4, Nylon, Philips panhead | Machine Screw, Round, #4-40 x 1/4, Nylon, Philips panhead
|  | Footprint | NY PMS 440 0025 PH | NY PMS 440 0025 PH
|  | Key | NY PMS 440 0025 PH | NY PMS 440 0025 PH
|  | LatestRevisionDate | 2017-03-09 | 2017-03-09
|  | Manufacturer | B&F Fastener Supply | B&F Fastener Supply
|  | MountType | N/A | N/A
|  | Note |  |
|  | PackageReference | Screw | Screw
|  | PartNumber | NY PMS 440 0025 PH | NY PMS 440 0025 PH
|  | Publisher | Texas Instruments | Texas Instruments
|  | RoHS | Y | Y
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 |  |
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | H542-ND | H542-ND
|  | Supplier Part Number 2 |  |
|  | Supplier Part Number 3 |  |
|  | Value |  |
H4 | HVP053B_Hardware.SchDoc |  | Fitted | Fitted
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | ClassName | Mounting Holes | Mounting Holes
|  | Comment | NY PMS 440 0025 PH | NY PMS 440 0025 PH
|  | ComponentLink1Description | Datasheet Link | Datasheet Link
|  | ComponentLink1URL | http://www.fasnetdirect.com/refguide/Nylpanms.pdf | http://www.fasnetdirect.com/refguide/Nylpanms.pdf
|  | CompType | Hardware | Hardware
|  | Description | Machine Screw, Round, #4-40 x 1/4, Nylon, Philips panhead | Machine Screw, Round, #4-40 x 1/4, Nylon, Philips panhead
|  | Footprint | NY PMS 440 0025 PH | NY PMS 440 0025 PH
|  | Key | NY PMS 440 0025 PH | NY PMS 440 0025 PH
|  | LatestRevisionDate | 2017-03-09 | 2017-03-09
|  | Manufacturer | B&F Fastener Supply | B&F Fastener Supply
|  | MountType | N/A | N/A
|  | Note |  |
|  | PackageReference | Screw | Screw
|  | PartNumber | NY PMS 440 0025 PH | NY PMS 440 0025 PH
|  | Publisher | Texas Instruments | Texas Instruments
|  | RoHS | Y | Y
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 |  |
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | H542-ND | H542-ND
|  | Supplier Part Number 2 |  |
|  | Supplier Part Number 3 |  |
|  | Value |  |
H5 | HVP053B_Hardware.SchDoc |  | Fitted | Fitted
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | ClassName |  |
|  | Comment | 1902C | 1902C
|  | ComponentLink1Description | Datasheet Link | Datasheet Link
|  | ComponentLink1URL | http://www.keyelco.com/pdfs/M55-prod31.pdf | http://www.keyelco.com/pdfs/M55-prod31.pdf
|  | CompType | Hardware | Hardware
|  | Description | Standoff, Hex, 0.5"L #4-40 Nylon | Standoff, Hex, 0.5"L #4-40 Nylon
|  | Footprint | Keystone_1902C | Keystone_1902C
|  | Key | 1902C | 1902C
|  | LatestRevisionDate | 2017-03-09 | 2017-03-09
|  | Manufacturer | Keystone | Keystone
|  | MountType | N/A | N/A
|  | Note |  |
|  | PackageReference | Standoff | Standoff
|  | PartNumber | 1902C | 1902C
|  | Publisher | Texas Instruments | Texas Instruments
|  | RoHS | Y | Y
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 |  |
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | 36-1902C-ND | 36-1902C-ND
|  | Supplier Part Number 2 |  |
|  | Supplier Part Number 3 |  |
|  | Value |  |
H6 | HVP053B_Hardware.SchDoc |  | Fitted | Fitted
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | ClassName |  |
|  | Comment | 1902C | 1902C
|  | ComponentLink1Description | Datasheet Link | Datasheet Link
|  | ComponentLink1URL | http://www.keyelco.com/pdfs/M55-prod31.pdf | http://www.keyelco.com/pdfs/M55-prod31.pdf
|  | CompType | Hardware | Hardware
|  | Description | Standoff, Hex, 0.5"L #4-40 Nylon | Standoff, Hex, 0.5"L #4-40 Nylon
|  | Footprint | Keystone_1902C | Keystone_1902C
|  | Key | 1902C | 1902C
|  | LatestRevisionDate | 2017-03-09 | 2017-03-09
|  | Manufacturer | Keystone | Keystone
|  | MountType | N/A | N/A
|  | Note |  |
|  | PackageReference | Standoff | Standoff
|  | PartNumber | 1902C | 1902C
|  | Publisher | Texas Instruments | Texas Instruments
|  | RoHS | Y | Y
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 |  |
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | 36-1902C-ND | 36-1902C-ND
|  | Supplier Part Number 2 |  |
|  | Supplier Part Number 3 |  |
|  | Value |  |
H7 | HVP053B_Hardware.SchDoc |  | Fitted | Fitted
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | ClassName |  |
|  | Comment | 1902C | 1902C
|  | ComponentLink1Description | Datasheet Link | Datasheet Link
|  | ComponentLink1URL | http://www.keyelco.com/pdfs/M55-prod31.pdf | http://www.keyelco.com/pdfs/M55-prod31.pdf
|  | CompType | Hardware | Hardware
|  | Description | Standoff, Hex, 0.5"L #4-40 Nylon | Standoff, Hex, 0.5"L #4-40 Nylon
|  | Footprint | Keystone_1902C | Keystone_1902C
|  | Key | 1902C | 1902C
|  | LatestRevisionDate | 2017-03-09 | 2017-03-09
|  | Manufacturer | Keystone | Keystone
|  | MountType | N/A | N/A
|  | Note |  |
|  | PackageReference | Standoff | Standoff
|  | PartNumber | 1902C | 1902C
|  | Publisher | Texas Instruments | Texas Instruments
|  | RoHS | Y | Y
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 |  |
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | 36-1902C-ND | 36-1902C-ND
|  | Supplier Part Number 2 |  |
|  | Supplier Part Number 3 |  |
|  | Value |  |
H8 | HVP053B_Hardware.SchDoc |  | Fitted | Fitted
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | ClassName |  |
|  | Comment | 1902C | 1902C
|  | ComponentLink1Description | Datasheet Link | Datasheet Link
|  | ComponentLink1URL | http://www.keyelco.com/pdfs/M55-prod31.pdf | http://www.keyelco.com/pdfs/M55-prod31.pdf
|  | CompType | Hardware | Hardware
|  | Description | Standoff, Hex, 0.5"L #4-40 Nylon | Standoff, Hex, 0.5"L #4-40 Nylon
|  | Footprint | Keystone_1902C | Keystone_1902C
|  | Key | 1902C | 1902C
|  | LatestRevisionDate | 2017-03-09 | 2017-03-09
|  | Manufacturer | Keystone | Keystone
|  | MountType | N/A | N/A
|  | Note |  |
|  | PackageReference | Standoff | Standoff
|  | PartNumber | 1902C | 1902C
|  | Publisher | Texas Instruments | Texas Instruments
|  | RoHS | Y | Y
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 |  |
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | 36-1902C-ND | 36-1902C-ND
|  | Supplier Part Number 2 |  |
|  | Supplier Part Number 3 |  |
|  | Value |  |
J1 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Cert_CSA |  |
|  | Cert_CULUS | Y | Y
|  | Cert_UL |  |
|  | Cert_VDE | Y | Y
|  | ClassName |  |
|  | CNHeader | False | False
|  | Color | Blue | Blue
|  | Comment | ED120/2DS | ED120/2DS
|  | ComponentLink1Description | Datasheet URL | Datasheet URL
|  | ComponentLink1URL | http://www.on-shore.com/sites/default/files/manuals/ed120ds.pdf | http://www.on-shore.com/sites/default/files/manuals/ed120ds.pdf
|  | CompType | Terminal Block | Terminal Block
|  | ContactFinish | Brass | Brass
|  | CT | True | True
|  | Current_A | 15A | 15A
|  | Description | Terminal Block, 5.08 mm, 2x1, Brass, TH | Terminal Block, 5.08 mm, 2x1, Brass, TH
|  | Footprint | On-Shore_ED120_2DS | On-Shore_ED120_2DS
|  | Gender | Female | Female
|  | Green_EU RoHS | Incomplete | Incomplete
|  | Green_EU RoHS-2 | Incomplete | Incomplete
|  | Green_Lifecycle | Not Set | Not Set
|  | Green_REACh | Incomplete | Incomplete
|  | LatestRevisionDate | 2017-07-12 | 2017-07-12
|  | Manufacturer | On-Shore Technology | On-Shore Technology
|  | MountType | TH | TH
|  | Note |  |
|  | Orientation | Vertical | Vertical
|  | PackageReference | 2x1 5.08 mm Terminal Block | 2x1 5.08 mm Terminal Block
|  | PartNumber | ED120/2DS | ED120/2DS
|  | PinCount | 2 | 2
|  | Pitch_mm | 5.08 | 5.08
|  | Publisher | Texas Instruments | Texas Instruments
|  | RoHS | Y | Y
|  | Row_Count | 1 | 1
|  | RowSpacing_mm |  |
|  | Shrouded | N | N
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 |  |
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | ED1609-ND | ED1609-ND
|  | Supplier Part Number 2 |  |
|  | Supplier Part Number 3 |  |
|  | Voltage_V | 300V | 300V
J2 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Cert_CSA |  |
|  | Cert_CULUS | Y | Y
|  | Cert_UL |  |
|  | Cert_VDE | Y | Y
|  | ClassName |  |
|  | CNHeader | False | False
|  | Color | Blue | Blue
|  | Comment | ED120/2DS | ED120/2DS
|  | ComponentLink1Description | Datasheet URL | Datasheet URL
|  | ComponentLink1URL | http://www.on-shore.com/sites/default/files/manuals/ed120ds.pdf | http://www.on-shore.com/sites/default/files/manuals/ed120ds.pdf
|  | CompType | Terminal Block | Terminal Block
|  | ContactFinish | Brass | Brass
|  | CT | True | True
|  | Current_A | 15A | 15A
|  | Description | Terminal Block, 5.08 mm, 2x1, Brass, TH | Terminal Block, 5.08 mm, 2x1, Brass, TH
|  | Footprint | On-Shore_ED120_2DS | On-Shore_ED120_2DS
|  | Gender | Female | Female
|  | Green_EU RoHS | Incomplete | Incomplete
|  | Green_EU RoHS-2 | Incomplete | Incomplete
|  | Green_Lifecycle | Not Set | Not Set
|  | Green_REACh | Incomplete | Incomplete
|  | LatestRevisionDate | 2017-07-12 | 2017-07-12
|  | Manufacturer | On-Shore Technology | On-Shore Technology
|  | MountType | TH | TH
|  | Note |  |
|  | Orientation | Vertical | Vertical
|  | PackageReference | 2x1 5.08 mm Terminal Block | 2x1 5.08 mm Terminal Block
|  | PartNumber | ED120/2DS | ED120/2DS
|  | PinCount | 2 | 2
|  | Pitch_mm | 5.08 | 5.08
|  | Publisher | Texas Instruments | Texas Instruments
|  | RoHS | Y | Y
|  | Row_Count | 1 | 1
|  | RowSpacing_mm |  |
|  | Shrouded | N | N
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 |  |
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | ED1609-ND | ED1609-ND
|  | Supplier Part Number 2 |  |
|  | Supplier Part Number 3 |  |
|  | Voltage_V | 300V | 300V
J3 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Cert_CSA |  |
|  | Cert_CULUS | Y | Y
|  | Cert_UL |  |
|  | Cert_VDE | Y | Y
|  | ClassName |  |
|  | CNHeader | False | False
|  | Color | Blue | Blue
|  | Comment | ED120/2DS | ED120/2DS
|  | ComponentLink1Description | Datasheet URL | Datasheet URL
|  | ComponentLink1URL | http://www.on-shore.com/sites/default/files/manuals/ed120ds.pdf | http://www.on-shore.com/sites/default/files/manuals/ed120ds.pdf
|  | CompType | Terminal Block | Terminal Block
|  | ContactFinish | Brass | Brass
|  | CT | True | True
|  | Current_A | 15A | 15A
|  | Description | Terminal Block, 5.08 mm, 2x1, Brass, TH | Terminal Block, 5.08 mm, 2x1, Brass, TH
|  | Footprint | On-Shore_ED120_2DS | On-Shore_ED120_2DS
|  | Gender | Female | Female
|  | Green_EU RoHS | Incomplete | Incomplete
|  | Green_EU RoHS-2 | Incomplete | Incomplete
|  | Green_Lifecycle | Not Set | Not Set
|  | Green_REACh | Incomplete | Incomplete
|  | LatestRevisionDate | 2017-07-12 | 2017-07-12
|  | Manufacturer | On-Shore Technology | On-Shore Technology
|  | MountType | TH | TH
|  | Note |  |
|  | Orientation | Vertical | Vertical
|  | PackageReference | 2x1 5.08 mm Terminal Block | 2x1 5.08 mm Terminal Block
|  | PartNumber | ED120/2DS | ED120/2DS
|  | PinCount | 2 | 2
|  | Pitch_mm | 5.08 | 5.08
|  | Publisher | Texas Instruments | Texas Instruments
|  | RoHS | Y | Y
|  | Row_Count | 1 | 1
|  | RowSpacing_mm |  |
|  | Shrouded | N | N
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 |  |
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | ED1609-ND | ED1609-ND
|  | Supplier Part Number 2 |  |
|  | Supplier Part Number 3 |  |
|  | Voltage_V | 300V | 300V
J4 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Cert_CSA |  |
|  | Cert_CULUS | Y | Y
|  | Cert_UL |  |
|  | Cert_VDE | Y | Y
|  | ClassName |  |
|  | CNHeader | False | False
|  | Color | Blue | Blue
|  | Comment | ED120/2DS | ED120/2DS
|  | ComponentLink1Description | Datasheet URL | Datasheet URL
|  | ComponentLink1URL | http://www.on-shore.com/sites/default/files/manuals/ed120ds.pdf | http://www.on-shore.com/sites/default/files/manuals/ed120ds.pdf
|  | CompType | Terminal Block | Terminal Block
|  | ContactFinish | Brass | Brass
|  | CT | True | True
|  | Current_A | 15A | 15A
|  | Description | Terminal Block, 5.08 mm, 2x1, Brass, TH | Terminal Block, 5.08 mm, 2x1, Brass, TH
|  | Footprint | On-Shore_ED120_2DS | On-Shore_ED120_2DS
|  | Gender | Female | Female
|  | Green_EU RoHS | Incomplete | Incomplete
|  | Green_EU RoHS-2 | Incomplete | Incomplete
|  | Green_Lifecycle | Not Set | Not Set
|  | Green_REACh | Incomplete | Incomplete
|  | LatestRevisionDate | 2017-07-12 | 2017-07-12
|  | Manufacturer | On-Shore Technology | On-Shore Technology
|  | MountType | TH | TH
|  | Note |  |
|  | Orientation | Vertical | Vertical
|  | PackageReference | 2x1 5.08 mm Terminal Block | 2x1 5.08 mm Terminal Block
|  | PartNumber | ED120/2DS | ED120/2DS
|  | PinCount | 2 | 2
|  | Pitch_mm | 5.08 | 5.08
|  | Publisher | Texas Instruments | Texas Instruments
|  | RoHS | Y | Y
|  | Row_Count | 1 | 1
|  | RowSpacing_mm |  |
|  | Shrouded | N | N
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 |  |
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | ED1609-ND | ED1609-ND
|  | Supplier Part Number 2 |  |
|  | Supplier Part Number 3 |  |
|  | Voltage_V | 300V | 300V
J5 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Cert_CSA | Y | Y
|  | Cert_CULUS | N | N
|  | Cert_UL | Y | Y
|  | Cert_VDE | N | N
|  | ClassName | Header | Header
|  | Color | Black | Black
|  | Comment | TSW-103-07-G-S | TSW-103-07-G-S
|  | ComponentLink1Description | Datasheet URL | Datasheet URL
|  | ComponentLink1URL | http://samtec.com/ftppub/pdf/TSW_TH.PDF | http://samtec.com/ftppub/pdf/TSW_TH.PDF
|  | CompType | Header | Header
|  | ContactFinish | Gold | Gold
|  | Current_A | 6.3A | 6.3A
|  | Description | Header, 100mil, 3x1, Gold, TH | Header, 100mil, 3x1, Gold, TH
|  | Footprint | TSW-103-07-G-S | TSW-103-07-G-S
|  | Gender | Male | Male
|  | Green_EU RoHS | Passed | Passed
|  | Green_EU RoHS-2 | Passed | Passed
|  | Green_Lifecycle | Active | Active
|  | Green_REACh | Passed | Passed
|  | Manufacturer | Samtec | Samtec
|  | MountType | TH | TH
|  | Note |  |
|  | Orientation | Vertical | Vertical
|  | PackageReference | 3x1 Header | 3x1 Header
|  | PartNumber | TSW-103-07-G-S | TSW-103-07-G-S
|  | PinCount | 3 | 3
|  | Pitch_mm | 2.54 | 2.54
|  | RoHS | Y | Y
|  | Row_Count | 1 | 1
|  | RowSpacing_mm |  |
|  | Shrouded | N | N
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 |  |
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | SAM1029-03-ND | SAM1029-03-ND
|  | Supplier Part Number 2 |  |
|  | Supplier Part Number 3 |  |
|  | Voltage_V | 550V | 550V
L1 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Qualified | No | No
|  | Comment | RLTI-1387 | RLTI-1387
|  | Datasheet Path | datasheets/Ind-RLTI-1387.pdf | datasheets/Ind-RLTI-1387.pdf
|  | DCR_ohm | 0.03 | 0.03
|  | Description | Common Mode Choke, 2.3mH 35%, 0.6x0.38x0.75 IN | Common Mode Choke, 2.3mH 35%, 0.6x0.38x0.75 IN
|  | Footprint | FP-RLTI-1387_PTH_CMC_0IN38_0IN60-MFG | FP-RLTI-1387_PTH_CMC_0IN38_0IN60-MFG
|  | helpURL | https://upverter.com/upn/revision/6b722364d3a89065/ | https://upverter.com/upn/revision/6b722364d3a89065/
|  | Ind_H | 2.3mH | 2.3mH
|  | Manufacturer | Renco | Renco
|  | Operating Temperature Range | to | to
|  | PackageReference | PTH_CMC_0IN38_0IN60 | PTH_CMC_0IN38_0IN60
|  | Part Number | RLTI-1387 | RLTI-1387
|  | PartNumber | RLTI-1387 | RLTI-1387
|  | RoHS | UNKNOWN | UNKNOWN
|  | SizeZ_mm | 0.75inch | 0.75inch
|  | Technology | Wirewound | Wirewound
|  | Test Frequency | 10kHz | 10kHz
|  | Tolerance_% | 35% | 35%
L2 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Qualified | No | No
|  | Comment | 7447052 | 7447052
|  | ComponentLink1Description | Datasheet | Datasheet
|  | ComponentLink1URL | https://katalog.we-online.com/pbs/datasheet/7447052.pdf | https://katalog.we-online.com/pbs/datasheet/7447052.pdf
|  | DCR_ohm | 0.045 | 0.045
|  | Description | WE-FI Leaded Toroidal Line Choke | WE-FI Leaded Toroidal Line Choke
|  | Footprint | FP-7447052_PTH_D10MM0-MFG | FP-7447052_PTH_D10MM0-MFG
|  | Ind_H | 32µH | 32µH
|  | Irms | 2.6A | 2.6A
|  | Manufacturer | Wurth | Wurth
|  | PackageReference | PTH_D10MM0 | PTH_D10MM0
|  | PartNumber | 7447052 | 7447052
|  | RoHS | TRUE | TRUE
|  | SizeZ_mm | 10mm | 10mm
|  | Symbol Name | SYM-7447052 | SYM-7447052
|  | Technology | Wirewound | Wirewound
LBL1 | HVP053B_Hardware.SchDoc |  | Fitted | Fitted
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | ClassName | Label | Label
|  | Comment | THT-14-423-10 | THT-14-423-10
|  | ComponentLink1Description | Web Page | Web Page
|  | ComponentLink1URL | http://www.bradyid.com/bradyid/pdpv/THT-14-423-10.html | http://www.bradyid.com/bradyid/pdpv/THT-14-423-10.html
|  | CompType | Label | Label
|  | Description | Thermal Transfer Printable Labels, 0.650" W x 0.200" H - 10,000 per roll | Thermal Transfer Printable Labels, 0.650" W x 0.200" H - 10,000 per roll
|  | Footprint | Label_650x200 | Label_650x200
|  | Key | THT-14-423-10 | THT-14-423-10
|  | LatestRevisionDate | 2017-03-09 | 2017-03-09
|  | Manufacturer | Brady | Brady
|  | MountType | N/A | N/A
|  | Note | Size: 0.65" x 0.20 " | Size: 0.65" x 0.20 "
|  | PackageReference | PCB Label 0.650 x 0.200 inch | PCB Label 0.650 x 0.200 inch
|  | PartNumber | THT-14-423-10 | THT-14-423-10
|  | Publisher | Texas Instruments | Texas Instruments
|  | RoHS | Y | Y
|  | Supplier 1 | Newark | Newark
|  | Supplier 2 | Farnell | Farnell
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | 97C5133 | 97C5133
|  | Supplier Part Number 2 | 2065596 | 2065596
|  | Supplier Part Number 3 |  |
|  | Value |  |
Logo1 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | Comment | DANGER HIGH VOLTAGE | DANGER HIGH VOLTAGE
|  | Description | IEC 61010-1 High Voltage Warning | IEC 61010-1 High Voltage Warning
|  | Footprint | IEC_HighVoltage_Small | IEC_HighVoltage_Small
|  | LatestRevisionDate | 2017-07-06 | 2017-07-06
|  | Lib Reference | IEC_HighVoltage | IEC_HighVoltage
|  | PartNumber | DANGER HIGH VOLTAGE | DANGER HIGH VOLTAGE
|  | Published | 2009-03-03 | 2009-03-03
|  | Publisher | Texas Instruments | Texas Instruments
|  | SymbolCreator | a0412235 | a0412235
|  | SymbolVersion | 2011-08-22 | 2011-08-22
Logo2 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | Comment | CAUTION HOT SURFACE | CAUTION HOT SURFACE
|  | Description | IEC 61010-1 Hot Surface Warning | IEC 61010-1 Hot Surface Warning
|  | Footprint | IEC_HotSurface_Small | IEC_HotSurface_Small
|  | LatestRevisionDate | 2017-07-06 | 2017-07-06
|  | Lib Reference | IEC_HotSurface | IEC_HotSurface
|  | PartNumber | CAUTION HOT SURFACE | CAUTION HOT SURFACE
|  | Published | 2009-03-03 | 2009-03-03
|  | Publisher | Texas Instruments | Texas Instruments
|  | SymbolCreator | a0412235 | a0412235
|  | SymbolVersion | 2011-08-22 | 2011-08-22
Logo3 | HVP053B_Hardware.SchDoc |  | Fitted | Fitted
|  | ClassName | Logo | Logo
|  | Comment | Texas Instruments + Symbol | Texas Instruments + Symbol
|  | Description | Texas Instrument Corporate Signature | Texas Instrument Corporate Signature
|  | Footprint | TI_Stacked_Overlay_Small | TI_Stacked_Overlay_Small
|  | LatestRevisionDate | 2017-07-06 | 2017-07-06
|  | Lib Reference | TI_Logo | TI_Logo
|  | PartNumber | Texas Instruments | Texas Instruments
|  | Published | 2009-03-03 | 2009-03-03
|  | Publisher | Texas Instruments | Texas Instruments
|  | SymbolCreator | a0412235 | a0412235
|  | SymbolVersion | 2011-08-22 | 2011-08-22
Logo4 | HVP053B_Hardware.SchDoc |  | Fitted | Fitted
|  | Comment | FCC disclaimer | FCC disclaimer
|  | Description | FCC_disclaimer | FCC_disclaimer
|  | Footprint | FCC_disclaimer | FCC_disclaimer
|  | LatestRevisionDate | 2017-07-06 | 2017-07-06
|  | Lib Reference | FCC_disclaimer | FCC_disclaimer
|  | PartNumber | FCC disclaimer | FCC disclaimer
|  | Published | 2009-03-03 | 2009-03-03
|  | Publisher | Texas Instruments | Texas Instruments
Logo5 | HVP053B_Hardware.SchDoc |  | Fitted | Fitted
|  | Comment | WEEE logo | WEEE logo
|  | Description | WEEE logo | WEEE logo
|  | Footprint | WEEE_Minimum | WEEE_Minimum
|  | Lib Reference | WEEE logo | WEEE logo
|  | PartNumber | WEEE logo | WEEE logo
Logo6 | HVP053B_Hardware.SchDoc |  | Fitted | Fitted
|  | Comment | CE Mark | CE Mark
|  | Description | CE Mark | CE Mark
|  | Footprint | CE_Mark_5mm | CE_Mark_5mm
|  | LatestRevisionDate | 2017-07-06 | 2017-07-06
|  | Lib Reference | CE Mark | CE Mark
|  | PartNumber | CE Mark | CE Mark
|  | Published | 2009-03-03 | 2009-03-03
|  | Publisher | Texas Instruments | Texas Instruments
|  | SymbolCreator | a0412235 | a0412235
Logo7 | HVP053B_Hardware.SchDoc |  | Fitted | Fitted
|  | Comment | DANGER HIGH VOLTAGE | DANGER HIGH VOLTAGE
|  | Description | IEC 61010-1 High Voltage Warning | IEC 61010-1 High Voltage Warning
|  | Footprint | IEC_HighVoltage_Small | IEC_HighVoltage_Small
|  | LatestRevisionDate | 2017-07-06 | 2017-07-06
|  | Lib Reference | IEC_HighVoltage | IEC_HighVoltage
|  | PartNumber | DANGER HIGH VOLTAGE | DANGER HIGH VOLTAGE
|  | Published | 2009-03-03 | 2009-03-03
|  | Publisher | Texas Instruments | Texas Instruments
|  | SymbolCreator | a0412235 | a0412235
|  | SymbolVersion | 2011-08-22 | 2011-08-22
Logo8 | HVP053B_Hardware.SchDoc |  | Fitted | Fitted
|  | Comment | DANGER HIGH VOLTAGE | DANGER HIGH VOLTAGE
|  | Description | IEC 61010-1 High Voltage Warning | IEC 61010-1 High Voltage Warning
|  | Footprint | IEC_HighVoltage_Small | IEC_HighVoltage_Small
|  | LatestRevisionDate | 2017-07-06 | 2017-07-06
|  | Lib Reference | IEC_HighVoltage | IEC_HighVoltage
|  | PartNumber | DANGER HIGH VOLTAGE | DANGER HIGH VOLTAGE
|  | Published | 2009-03-03 | 2009-03-03
|  | Publisher | Texas Instruments | Texas Instruments
|  | SymbolCreator | a0412235 | a0412235
|  | SymbolVersion | 2011-08-22 | 2011-08-22
Logo9 | HVP053B_Hardware.SchDoc |  | Fitted | Fitted
|  | Comment | CAUTION HOT SURFACE | CAUTION HOT SURFACE
|  | Description | IEC 61010-1 Hot Surface Warning | IEC 61010-1 Hot Surface Warning
|  | Footprint | IEC_HotSurface_Small | IEC_HotSurface_Small
|  | LatestRevisionDate | 2017-07-06 | 2017-07-06
|  | Lib Reference | IEC_HotSurface | IEC_HotSurface
|  | PartNumber | CAUTION HOT SURFACE | CAUTION HOT SURFACE
|  | Published | 2009-03-03 | 2009-03-03
|  | Publisher | Texas Instruments | Texas Instruments
|  | SymbolCreator | a0412235 | a0412235
|  | SymbolVersion | 2011-08-22 | 2011-08-22
Logo10 | HVP053B_Hardware.SchDoc |  | Fitted | Fitted
|  | Comment | DANGER HIGH VOLTAGE | DANGER HIGH VOLTAGE
|  | Description | IEC 61010-1 High Voltage Warning | IEC 61010-1 High Voltage Warning
|  | Footprint | IEC_HighVoltage_Small | IEC_HighVoltage_Small
|  | LatestRevisionDate | 2017-07-06 | 2017-07-06
|  | Lib Reference | IEC_HighVoltage | IEC_HighVoltage
|  | PartNumber | DANGER HIGH VOLTAGE | DANGER HIGH VOLTAGE
|  | Published | 2009-03-03 | 2009-03-03
|  | Publisher | Texas Instruments | Texas Instruments
|  | SymbolCreator | a0412235 | a0412235
|  | SymbolVersion | 2011-08-22 | 2011-08-22
Logo11 | HVP053B_Hardware.SchDoc |  | Fitted | Fitted
|  | Comment | CAUTION HOT SURFACE | CAUTION HOT SURFACE
|  | Description | IEC 61010-1 Hot Surface Warning | IEC 61010-1 Hot Surface Warning
|  | Footprint | IEC_HotSurface_Small | IEC_HotSurface_Small
|  | LatestRevisionDate | 2017-07-06 | 2017-07-06
|  | Lib Reference | IEC_HotSurface | IEC_HotSurface
|  | PartNumber | CAUTION HOT SURFACE | CAUTION HOT SURFACE
|  | Published | 2009-03-03 | 2009-03-03
|  | Publisher | Texas Instruments | Texas Instruments
|  | SymbolCreator | a0412235 | a0412235
|  | SymbolVersion | 2011-08-22 | 2011-08-22
Logo12 | HVP053B_Hardware.SchDoc |  | Fitted | Fitted
|  | Comment | DANGER HIGH VOLTAGE | DANGER HIGH VOLTAGE
|  | Description | IEC 61010-1 High Voltage Warning | IEC 61010-1 High Voltage Warning
|  | Footprint | IEC_HighVoltage_Small | IEC_HighVoltage_Small
|  | LatestRevisionDate | 2017-07-06 | 2017-07-06
|  | Lib Reference | IEC_HighVoltage | IEC_HighVoltage
|  | PartNumber | DANGER HIGH VOLTAGE | DANGER HIGH VOLTAGE
|  | Published | 2009-03-03 | 2009-03-03
|  | Publisher | Texas Instruments | Texas Instruments
|  | SymbolCreator | a0412235 | a0412235
|  | SymbolVersion | 2011-08-22 | 2011-08-22
Logo13 | HVP053B_Hardware.SchDoc |  | Fitted | Fitted
|  | Comment | DANGER HIGH VOLTAGE | DANGER HIGH VOLTAGE
|  | Description | IEC 61010-1 High Voltage Warning | IEC 61010-1 High Voltage Warning
|  | Footprint | IEC_HighVoltage_Small | IEC_HighVoltage_Small
|  | LatestRevisionDate | 2017-07-06 | 2017-07-06
|  | Lib Reference | IEC_HighVoltage | IEC_HighVoltage
|  | PartNumber | DANGER HIGH VOLTAGE | DANGER HIGH VOLTAGE
|  | Published | 2009-03-03 | 2009-03-03
|  | Publisher | Texas Instruments | Texas Instruments
|  | SymbolCreator | a0412235 | a0412235
|  | SymbolVersion | 2011-08-22 | 2011-08-22
Logo14 | HVP053B_Hardware.SchDoc |  | Fitted | Fitted
|  | Comment | CAUTION HOT SURFACE | CAUTION HOT SURFACE
|  | Description | IEC 61010-1 Hot Surface Warning | IEC 61010-1 Hot Surface Warning
|  | Footprint | IEC_HotSurface_Small | IEC_HotSurface_Small
|  | LatestRevisionDate | 2017-07-06 | 2017-07-06
|  | Lib Reference | IEC_HotSurface | IEC_HotSurface
|  | PartNumber | CAUTION HOT SURFACE | CAUTION HOT SURFACE
|  | Published | 2009-03-03 | 2009-03-03
|  | Publisher | Texas Instruments | Texas Instruments
|  | SymbolCreator | a0412235 | a0412235
|  | SymbolVersion | 2011-08-22 | 2011-08-22
Logo15 | HVP053B_Hardware.SchDoc |  | Fitted | Fitted
|  | ClassName | Logo | Logo
|  | Comment | Texas Instruments + Symbol | Texas Instruments + Symbol
|  | Description | Texas Instrument Corporate Signature | Texas Instrument Corporate Signature
|  | Footprint | TI_Stacked_Overlay_Small | TI_Stacked_Overlay_Small
|  | LatestRevisionDate | 2017-07-06 | 2017-07-06
|  | Lib Reference | TI_Logo | TI_Logo
|  | PartNumber | Texas Instruments | Texas Instruments
|  | Published | 2009-03-03 | 2009-03-03
|  | Publisher | Texas Instruments | Texas Instruments
|  | SymbolCreator | a0412235 | a0412235
|  | SymbolVersion | 2011-08-22 | 2011-08-22
Logo16 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | Comment | CAUTION. READ USER GUIDE BEFORE USE | CAUTION. READ USER GUIDE BEFORE USE
|  | Description | IEC 61010-1 Caution Warning | IEC 61010-1 Caution Warning
|  | Footprint | IEC_Caution_Small | IEC_Caution_Small
|  | LatestRevisionDate | 2017-07-06 | 2017-07-06
|  | Lib Reference | IEC_Caution | IEC_Caution
|  | PartNumber | CAUTION. READ USER GUIDE BEFORE USE | CAUTION. READ USER GUIDE BEFORE USE
|  | Published | 2009-03-03 | 2009-03-03
|  | Publisher | Texas Instruments | Texas Instruments
|  | SymbolCreator | a0412235 | a0412235
|  | SymbolVersion | 2011-08-22 | 2011-08-22
Logo17 | HVP053B_Hardware.SchDoc |  | Fitted | Fitted
|  | Comment | CAUTION. READ USER GUIDE BEFORE USE | CAUTION. READ USER GUIDE BEFORE USE
|  | Description | IEC 61010-1 Caution Warning | IEC 61010-1 Caution Warning
|  | Footprint | IEC_Caution_Small | IEC_Caution_Small
|  | LatestRevisionDate | 2017-07-06 | 2017-07-06
|  | Lib Reference | IEC_Caution | IEC_Caution
|  | PartNumber | CAUTION. READ USER GUIDE BEFORE USE | CAUTION. READ USER GUIDE BEFORE USE
|  | Published | 2009-03-03 | 2009-03-03
|  | Publisher | Texas Instruments | Texas Instruments
|  | SymbolCreator | a0412235 | a0412235
|  | SymbolVersion | 2011-08-22 | 2011-08-22
Q1 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q101 | Q101
|  | AEC Qualified | N | N
|  | Alternate Manufacturer | None | None
|  | Alternate PartNumber |  |
|  | ChMode | Enhancement | Enhancement
|  | ChType | N | N
|  | Comment | IPD80R600P7ATMA1 | IPD80R600P7ATMA1
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | https://www.infineon.com/dgdl/Infineon-IPD80R600P7-DS-v02_01-EN.pdf?fileId=5546d4625c167129015c1a9c04e36056 | https://www.infineon.com/dgdl/Infineon-IPD80R600P7-DS-v02_01-EN.pdf?fileId=5546d4625c167129015c1a9c04e36056
|  | CompType | MOSFET | MOSFET
|  | Description | MOSFET, N-CH, 800 V, 8 A, DPAK | MOSFET, N-CH, 800 V, 8 A, DPAK
|  | Footprint | DPAK | DPAK
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | IdsMax_A | 8A | 8A
|  | Manufacturer | Infineon Technologies | Infineon Technologies
|  | MountType | SMT | SMT
|  | PackageReference | DPAK | DPAK
|  | PartNumber | IPD80R600P7ATMA1 | IPD80R600P7ATMA1
|  | QgTyp_nC | 20 | 20
|  | Rdson45_ohm |  |
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 64.8114 | 64.8114
|  | SizeAreaWB_mm2 | 101.7114 | 101.7114
|  | SizeX_mm | 9.91 | 9.91
|  | SizeY_mm | 6.54 | 6.54
|  | SizeZ_mm | 2.29 | 2.29
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Mouser | Mouser
|  | Supplier 3 | Farnell | Farnell
|  | Supplier Part Number 1 | IPD80R600P7ATMA1CT-ND | IPD80R600P7ATMA1CT-ND
|  | Supplier Part Number 2 | 726-IPD80R600P7ATMA1 | 726-IPD80R600P7ATMA1
|  | Supplier Part Number 3 | 2771324 | 2771324
|  | Value | 800V | 800V
|  | Value1 | ? ohm | ? ohm
|  | Value2 | 20 nC | 20 nC
|  | VdsMax_V | 800V | 800V
|  | Vgs_V | 20V | 20V
Q2 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q101 | Q101
|  | AEC Qualified | N | N
|  | Alternate Manufacturer | None | None
|  | Alternate PartNumber |  |
|  | ChMode | Depletion | Depletion
|  | ChType | N | N
|  | Comment | CPC3982TTR | CPC3982TTR
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.ixysic.com/home/pdfs.nsf/www/CPC3982_R00D.pdf/$file/CPC3982_R00D.pdf | http://www.ixysic.com/home/pdfs.nsf/www/CPC3982_R00D.pdf/$file/CPC3982_R00D.pdf
|  | CompType | MOSFET | MOSFET
|  | Description | MOSFET, N-CH, Depletion Mode, 800 V, SOT-23 | MOSFET, N-CH, Depletion Mode, 800 V, SOT-23
|  | Footprint | SOT-23L | SOT-23L
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | IdsMax_A |  |
|  | Manufacturer | IXYS | IXYS
|  | MountType | SMT | SMT
|  | PackageReference | SOT-23 | SOT-23
|  | PartNumber | CPC3982TTR | CPC3982TTR
|  | QgTyp_nC |  |
|  | Rdson45_ohm |  |
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 7.5 | 7.5
|  | SizeAreaWB_mm2 | 14 | 14
|  | SizeX_mm | 2.5 | 2.5
|  | SizeY_mm | 3 | 3
|  | SizeZ_mm | 1.1 | 1.1
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Mouser | Mouser
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | CLA4160-1-ND | CLA4160-1-ND
|  | Supplier Part Number 2 | 849-CPC3982TTR | 849-CPC3982TTR
|  | Supplier Part Number 3 |  |
|  | Value | 800V | 800V
|  | Value1 | ? ohm | ? ohm
|  | Value2 | ? nC | ? nC
|  | VdsMax_V | 800V | 800V
|  | Vgs_V | 15V | 15V
Q3 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q101 | Q101
|  | AEC Qualified | N | N
|  | Alternate Manufacturer | None | None
|  | Alternate PartNumber |  |
|  | ChType | N | N
|  | Comment | BSC093N15NS5ATMA1 | BSC093N15NS5ATMA1
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.infineon.com/dgdl/Infineon-BSC093N15NS5-DS-v02_00-EN.pdf?fileId=5546d462503812bb01507033a3fa1175 | http://www.infineon.com/dgdl/Infineon-BSC093N15NS5-DS-v02_00-EN.pdf?fileId=5546d462503812bb01507033a3fa1175
|  | CompType | MOSFET | MOSFET
|  | Description | MOSFET, N-CH, 150 V, 87 A, PG-TDSON-8 | MOSFET, N-CH, 150 V, 87 A, PG-TDSON-8
|  | Footprint | PG-TDSON-8 | PG-TDSON-8
|  | IdsMax_A | 87A | 87A
|  | LatestRevisionDate | 2017-03-09 | 2017-03-09
|  | LatestRevisionNote | Added parts. | Added parts.
|  | Manufacturer | Infineon Technologies | Infineon Technologies
|  | MountType | SMT | SMT
|  | PackageReference | PG-TDSON-8 | PG-TDSON-8
|  | PartNumber | BSC093N15NS5ATMA1 | BSC093N15NS5ATMA1
|  | Published | 2008-06-19 | 2008-06-19
|  | Publisher | Texas Instruments | Texas Instruments
|  | QgTyp_nC | 33 | 33
|  | Rdson45_ohm |  |
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 29.351 | 29.351
|  | SizeAreaWB_mm2 | 55.131 | 55.131
|  | SizeX_mm | 5.99 | 5.99
|  | SizeY_mm | 4.9 | 4.9
|  | SizeZ_mm | 1.12 | 1.12
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Mouser | Mouser
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | BSC093N15NS5ATMA1CT-ND | BSC093N15NS5ATMA1CT-ND
|  | Supplier Part Number 2 | 726-BSC093N15NS5ATMA | 726-BSC093N15NS5ATMA
|  | Supplier Part Number 3 |  |
|  | U/M | EA | EA
|  | Value | 150V | 150V
|  | Value1 |  |
|  | Value2 | 33 nC | 33 nC
|  | Vault Folder |  |
|  | VdsMax_V | 150V | 150V
|  | Vgs_V | 20V | 20V
Q4 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q101 | Q101
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer | None | None
|  | Alternate PartNumber |  |
|  | ChMode | Depletion | Depletion
|  | ChType | N | N
|  | Comment | BSS126H6327XTSA2 | BSS126H6327XTSA2
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.infineon.com/dgdl/Infineon-BSS126-DS-v02_01-en.pdf?fileId=db3a304330f6860601310483af163eba | http://www.infineon.com/dgdl/Infineon-BSS126-DS-v02_01-en.pdf?fileId=db3a304330f6860601310483af163eba
|  | CompType | MOSFET | MOSFET
|  | Description | MOSFET, N-CH, Depletion Mode, 100 V, 0.17 A, AEC-Q101, SOT-23 | MOSFET, N-CH, Depletion Mode, 100 V, 0.17 A, AEC-Q101, SOT-23
|  | Footprint | SOT-23L | SOT-23L
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | IdsMax_A | 21mA | 21mA
|  | Manufacturer | Infineon Technologies | Infineon Technologies
|  | MountType | SMT | SMT
|  | PackageReference | SOT-23 | SOT-23
|  | PartNumber | BSS126H6327XTSA2 | BSS126H6327XTSA2
|  | QgTyp_nC | 1.4 | 1.4
|  | Rdson45_ohm |  |
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 7.5 | 7.5
|  | SizeAreaWB_mm2 | 14.0 | 14.0
|  | SizeX_mm | 2.5 | 2.5
|  | SizeY_mm | 3.0 | 3.0
|  | SizeZ_mm | 1.1 | 1.1
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Newark | Newark
|  | Supplier 3 | Mouser | Mouser
|  | Supplier Part Number 1 | BSS126H6327XTSA2CT-ND | BSS126H6327XTSA2CT-ND
|  | Supplier Part Number 2 | 47W3357 | 47W3357
|  | Supplier Part Number 3 | 726-BSS126H6327XTSA2 | 726-BSS126H6327XTSA2
|  | Value | 600V | 600V
|  | Value1 | ? ohm | ? ohm
|  | Value2 | 1.4 nC | 1.4 nC
|  | VdsMax_V | 600V | 600V
|  | Vgs_V | 20V | 20V
Q5 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q101 | Q101
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | MMST3906-7-F | MMST3906-7-F
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | https://www.diodes.com/assets/Datasheets/ds30079.pdf | https://www.diodes.com/assets/Datasheets/ds30079.pdf
|  | CompType | BJT | BJT
|  | Description | Transistor, PNP, 40 V, 0.2 A, AEC-Q101, SOT-323 | Transistor, PNP, 40 V, 0.2 A, AEC-Q101, SOT-323
|  | Footprint | SOT-323 | SOT-323
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | HfeMax | 300.0 | 300.0
|  | IcRated_A | 200mA | 200mA
|  | Manufacturer | Diodes Inc. | Diodes Inc.
|  | MountType | SMT | SMT
|  | NPN | 0.0 | 0.0
|  | PackageReference | SOT-323 | SOT-323
|  | PartNumber | MMST3906-7-F | MMST3906-7-F
|  | PNP | 1.0 | 1.0
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 4.84 | 4.84
|  | SizeAreaWB_mm2 | 10.24 | 10.24
|  | SizeX_mm | 2.2 | 2.2
|  | SizeY_mm | 2.2 | 2.2
|  | SizeZ_mm | 1.1 | 1.1
|  | TaMax_C | 150°C | 150°C
|  | TaMin_C | -55°C | -55°C
|  | Value | 40 V | 40 V
|  | Value1 | 0.2 A | 0.2 A
|  | Value2 | 300.0 | 300.0
|  | Vceo_V | 40V | 40V
|  | Vcesat1_V | 300mV | 300mV
R1 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | 0 | 0
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | CRCW04023K32FKED | CRCW04023K32FKED
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.vishay.com/docs/20035/dcrcwe3.pdf | http://www.vishay.com/docs/20035/dcrcwe3.pdf
|  | CompType | Resistor | Resistor
|  | Description | RES, 3.32 k, 1%, 0.063 W, AEC-Q200 Grade 0, 0402 | RES, 3.32 k, 1%, 0.063 W, AEC-Q200 Grade 0, 0402
|  | EIA_Code | E96 | E96
|  | Footprint | 0402S | 0402S
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Manufacturer | Vishay-Dale | Vishay-Dale
|  | MountType | SMT | SMT
|  | PackageReference | 0402 | 0402
|  | PartNumber | CRCW04023K32FKED | CRCW04023K32FKED
|  | Power_W | 63mW | 63mW
|  | Res_ohm | 3.32k | 3.32k
|  | RoHS | E | E
|  | SizeArea_mm2 | 0.5 | 0.5
|  | SizeX_mm | 1 | 1
|  | SizeY_mm | 0.5 | 0.5
|  | SizeZ_mm | 0.6 | 0.6
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Newark | Newark
|  | Supplier 3 | Mouser | Mouser
|  | Supplier Part Number 1 | 541-3.32KLCT-ND | 541-3.32KLCT-ND
|  | Supplier Part Number 2 | 52K6942 | 52K6942
|  | Supplier Part Number 3 | 71-CRCW0402-3.32K-E3 | 71-CRCW0402-3.32K-E3
|  | Technology | Thick Film | Thick Film
|  | TempCo | 100 ppm/C | 100 ppm/C
|  | Tolerance_% | 1% | 1%
|  | Value | 3.32k | 3.32k
|  | Value1 | 1% | 1%
|  | Value2 | 0.063W | 0.063W
|  | Value_Code | 3k32 | 3k32
|  | ValueDisplayed | 3.32k | 3.32k
|  | VDC_V | 50V | 50V
R2 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | 0 | 0
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | CRCW0805470KJNEA | CRCW0805470KJNEA
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.vishay.com/docs/20035/dcrcwe3.pdf | http://www.vishay.com/docs/20035/dcrcwe3.pdf
|  | CompType | Resistor | Resistor
|  | Description | RES, 470 k, 5%, 0.125 W, AEC-Q200 Grade 0, 0805 | RES, 470 k, 5%, 0.125 W, AEC-Q200 Grade 0, 0805
|  | EIA_Code | E24 | E24
|  | Footprint | 0805_HV1 | 0805_HV1
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Manufacturer | Vishay-Dale | Vishay-Dale
|  | MountType | SMT | SMT
|  | PackageReference | 0805 | 0805
|  | PartNumber | CRCW0805470KJNEA | CRCW0805470KJNEA
|  | Power_W | 125mW | 125mW
|  | Res_ohm | 470k | 470k
|  | RoHS | E | E
|  | SizeArea_mm2 | 2.5 | 2.5
|  | SizeX_mm | 2 | 2
|  | SizeY_mm | 1.25 | 1.25
|  | SizeZ_mm | 1.45 | 1.45
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Newark | Newark
|  | Supplier 3 | Mouser | Mouser
|  | Supplier Part Number 1 | 541-470KACT-ND | 541-470KACT-ND
|  | Supplier Part Number 2 | 59M6916 | 59M6916
|  | Supplier Part Number 3 | 71-CRCW0805470KJNEA | 71-CRCW0805470KJNEA
|  | Technology | Thick Film | Thick Film
|  | TempCo | 200 ppm/C | 200 ppm/C
|  | Tolerance_% | 5% | 5%
|  | Value | 470k | 470k
|  | Value1 | 5% | 5%
|  | Value2 | 0.125W | 0.125W
|  | Value_Code | 470k | 470k
|  | ValueDisplayed | 470k | 470k
|  | VDC_V | 150V | 150V
R3 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | 0 | 0
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | CRCW120613K0JNEA | CRCW120613K0JNEA
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.vishay.com/docs/20035/dcrcwe3.pdf | http://www.vishay.com/docs/20035/dcrcwe3.pdf
|  | CompType | Resistor | Resistor
|  | Description | RES, 13 k, 5%, 0.25 W, AEC-Q200 Grade 0, 1206 | RES, 13 k, 5%, 0.25 W, AEC-Q200 Grade 0, 1206
|  | EIA_Code | E24 | E24
|  | Footprint | 1206L | 1206L
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Manufacturer | Vishay-Dale | Vishay-Dale
|  | MountType | SMT | SMT
|  | PackageReference | 1206 | 1206
|  | PartNumber | CRCW120613K0JNEA | CRCW120613K0JNEA
|  | Power_W | 250mW | 250mW
|  | Res_ohm | 13k | 13k
|  | RoHS | E | E
|  | SizeArea_mm2 | 5.12 | 5.12
|  | SizeX_mm | 3.2 | 3.2
|  | SizeY_mm | 1.6 | 1.6
|  | SizeZ_mm | 1.35 | 1.35
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 |  |
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | 541-13KECT-ND | 541-13KECT-ND
|  | Supplier Part Number 2 |  |
|  | Supplier Part Number 3 |  |
|  | Technology | Thick Film | Thick Film
|  | TempCo | 200 ppm/C | 200 ppm/C
|  | Tolerance_% | 5% | 5%
|  | Value | 13k | 13k
|  | Value1 | 5% | 5%
|  | Value2 | 0.25W | 0.25W
|  | Value_Code | 13k0 | 13k0
|  | ValueDisplayed | 13k | 13k
|  | VDC_V | 200V | 200V
R4 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | 0 | 0
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | CRCW120613K0JNEA | CRCW120613K0JNEA
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.vishay.com/docs/20035/dcrcwe3.pdf | http://www.vishay.com/docs/20035/dcrcwe3.pdf
|  | CompType | Resistor | Resistor
|  | Description | RES, 13 k, 5%, 0.25 W, AEC-Q200 Grade 0, 1206 | RES, 13 k, 5%, 0.25 W, AEC-Q200 Grade 0, 1206
|  | EIA_Code | E24 | E24
|  | Footprint | 1206L | 1206L
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Manufacturer | Vishay-Dale | Vishay-Dale
|  | MountType | SMT | SMT
|  | PackageReference | 1206 | 1206
|  | PartNumber | CRCW120613K0JNEA | CRCW120613K0JNEA
|  | Power_W | 250mW | 250mW
|  | Res_ohm | 13k | 13k
|  | RoHS | E | E
|  | SizeArea_mm2 | 5.12 | 5.12
|  | SizeX_mm | 3.2 | 3.2
|  | SizeY_mm | 1.6 | 1.6
|  | SizeZ_mm | 1.35 | 1.35
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 |  |
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | 541-13KECT-ND | 541-13KECT-ND
|  | Supplier Part Number 2 |  |
|  | Supplier Part Number 3 |  |
|  | Technology | Thick Film | Thick Film
|  | TempCo | 200 ppm/C | 200 ppm/C
|  | Tolerance_% | 5% | 5%
|  | Value | 13k | 13k
|  | Value1 | 5% | 5%
|  | Value2 | 0.25W | 0.25W
|  | Value_Code | 13k0 | 13k0
|  | ValueDisplayed | 13k | 13k
|  | VDC_V | 200V | 200V
R5 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | 0 | 0
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | CRCW080515R0JNEA | CRCW080515R0JNEA
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.vishay.com/docs/20035/dcrcwe3.pdf | http://www.vishay.com/docs/20035/dcrcwe3.pdf
|  | CompType | Resistor | Resistor
|  | Description | RES, 15, 5%, 0.125 W, AEC-Q200 Grade 0, 0805 | RES, 15, 5%, 0.125 W, AEC-Q200 Grade 0, 0805
|  | EIA_Code | E24 | E24
|  | Footprint | 0805_HV1 | 0805_HV1
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Manufacturer | Vishay-Dale | Vishay-Dale
|  | MountType | SMT | SMT
|  | PackageReference | 0805 | 0805
|  | PartNumber | CRCW080515R0JNEA | CRCW080515R0JNEA
|  | Power_W | 125mW | 125mW
|  | Res_ohm | 15 | 15
|  | RoHS | E | E
|  | SizeArea_mm2 | 2.5 | 2.5
|  | SizeX_mm | 2 | 2
|  | SizeY_mm | 1.25 | 1.25
|  | SizeZ_mm | 1.45 | 1.45
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Newark | Newark
|  | Supplier 3 | Mouser | Mouser
|  | Supplier Part Number 1 | 541-15ACT-ND | 541-15ACT-ND
|  | Supplier Part Number 2 | 59M6857 | 59M6857
|  | Supplier Part Number 3 | 71-CRCW080515R0JNEA | 71-CRCW080515R0JNEA
|  | Technology | Thick Film | Thick Film
|  | TempCo | 200 ppm/C | 200 ppm/C
|  | Tolerance_% | 5% | 5%
|  | Value | 15 | 15
|  | Value1 | 5% | 5%
|  | Value2 | 0.125W | 0.125W
|  | Value_Code | 15R0 | 15R0
|  | ValueDisplayed | 15 | 15
|  | VDC_V | 150V | 150V
R6 | HVP053B_sheet1.schdoc |  | Fitted | Not Fitted
|  | AEC Category | Q200 |
|  | AEC Grade | 0 |
|  | AEC Qualified | Y |
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | CRCW04021M00JNED |
|  | ComponentLink1Description | Datasheet link |
|  | ComponentLink1URL | http://www.vishay.com/docs/20035/dcrcwe3.pdf |
|  | CompType | Resistor |
|  | Description | RES, 1.0 M, 5%, 0.063 W, AEC-Q200 Grade 0, 0402 |
|  | EIA_Code | E24 |
|  | Footprint | 0402S |
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Manufacturer | Vishay-Dale |
|  | MountType | SMT |
|  | PackageReference | 0402 |
|  | PartNumber | CRCW04021M00JNED |
|  | Power_W | 63mW |
|  | Res_ohm | 1M |
|  | RoHS | E |
|  | SizeArea_mm2 | 0.5 |
|  | SizeX_mm | 1 |
|  | SizeY_mm | 0.5 |
|  | SizeZ_mm | 0.6 |
|  | Supplier 1 | Digi-Key |
|  | Supplier 2 | Newark |
|  | Supplier 3 | Mouser |
|  | Supplier Part Number 1 | 541-1.0MJCT-ND |
|  | Supplier Part Number 2 | 59M6694 |
|  | Supplier Part Number 3 | 71-CRCW0402J-1M-E3 |
|  | Technology | Thick Film |
|  | TempCo | 200 ppm/C |
|  | Tolerance_% | 5% |
|  | Value | 1.0Meg |
|  | Value1 | 5% |
|  | Value2 | 0.063W |
|  | Value_Code | 1M00 |
|  | ValueDisplayed | 1.0M |
|  | VDC_V | 50V |
R7 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | 0 | 0
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | CRCW080515R0JNEA | CRCW080515R0JNEA
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.vishay.com/docs/20035/dcrcwe3.pdf | http://www.vishay.com/docs/20035/dcrcwe3.pdf
|  | CompType | Resistor | Resistor
|  | Description | RES, 15, 5%, 0.125 W, AEC-Q200 Grade 0, 0805 | RES, 15, 5%, 0.125 W, AEC-Q200 Grade 0, 0805
|  | EIA_Code | E24 | E24
|  | Footprint | 0805_HV1 | 0805_HV1
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Manufacturer | Vishay-Dale | Vishay-Dale
|  | MountType | SMT | SMT
|  | PackageReference | 0805 | 0805
|  | PartNumber | CRCW080515R0JNEA | CRCW080515R0JNEA
|  | Power_W | 125mW | 125mW
|  | Res_ohm | 15 | 15
|  | RoHS | E | E
|  | SizeArea_mm2 | 2.5 | 2.5
|  | SizeX_mm | 2 | 2
|  | SizeY_mm | 1.25 | 1.25
|  | SizeZ_mm | 1.45 | 1.45
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Newark | Newark
|  | Supplier 3 | Mouser | Mouser
|  | Supplier Part Number 1 | 541-15ACT-ND | 541-15ACT-ND
|  | Supplier Part Number 2 | 59M6857 | 59M6857
|  | Supplier Part Number 3 | 71-CRCW080515R0JNEA | 71-CRCW080515R0JNEA
|  | Technology | Thick Film | Thick Film
|  | TempCo | 200 ppm/C | 200 ppm/C
|  | Tolerance_% | 5% | 5%
|  | Value | 15 | 15
|  | Value1 | 5% | 5%
|  | Value2 | 0.125W | 0.125W
|  | Value_Code | 15R0 | 15R0
|  | ValueDisplayed | 15 | 15
|  | VDC_V | 150V | 150V
R8 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | 0 | 0
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | CRCW0402169KFKED | CRCW0402169KFKED
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.vishay.com/docs/20035/dcrcwe3.pdf | http://www.vishay.com/docs/20035/dcrcwe3.pdf
|  | CompType | Resistor | Resistor
|  | Description | RES, 169 k, 1%, 0.063 W, AEC-Q200 Grade 0, 0402 | RES, 169 k, 1%, 0.063 W, AEC-Q200 Grade 0, 0402
|  | EIA_Code | E96 | E96
|  | Footprint | 0402S | 0402S
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Manufacturer | Vishay-Dale | Vishay-Dale
|  | MountType | SMT | SMT
|  | PackageReference | 0402 | 0402
|  | PartNumber | CRCW0402169KFKED | CRCW0402169KFKED
|  | Power_W | 63mW | 63mW
|  | Res_ohm | 169k | 169k
|  | RoHS | E | E
|  | SizeArea_mm2 | 0.5 | 0.5
|  | SizeX_mm | 1 | 1
|  | SizeY_mm | 0.5 | 0.5
|  | SizeZ_mm | 0.6 | 0.6
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Newark | Newark
|  | Supplier 3 | Mouser | Mouser
|  | Supplier Part Number 1 | 541-169KLCT-ND | 541-169KLCT-ND
|  | Supplier Part Number 2 | 72M6754 | 72M6754
|  | Supplier Part Number 3 | 71-CRCW0402-169K-E3 | 71-CRCW0402-169K-E3
|  | Technology | Thick Film | Thick Film
|  | TempCo | 100 ppm/C | 100 ppm/C
|  | Tolerance_% | 1% | 1%
|  | Value | 169k | 169k
|  | Value1 | 1% | 1%
|  | Value2 | 0.063W | 0.063W
|  | Value_Code | 169k | 169k
|  | ValueDisplayed | 169k | 169k
|  | VDC_V | 50V | 50V
R9 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | 0 | 0
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | CRCW040293K1FKED | CRCW040293K1FKED
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.vishay.com/docs/20035/dcrcwe3.pdf | http://www.vishay.com/docs/20035/dcrcwe3.pdf
|  | CompType | Resistor | Resistor
|  | Description | RES, 93.1 k, 1%, 0.063 W, AEC-Q200 Grade 0, 0402 | RES, 93.1 k, 1%, 0.063 W, AEC-Q200 Grade 0, 0402
|  | EIA_Code | E96 | E96
|  | Footprint | 0402S | 0402S
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Manufacturer | Vishay-Dale | Vishay-Dale
|  | MountType | SMT | SMT
|  | PackageReference | 0402 | 0402
|  | PartNumber | CRCW040293K1FKED | CRCW040293K1FKED
|  | Power_W | 63mW | 63mW
|  | Res_ohm | 93.1k | 93.1k
|  | RoHS | E | E
|  | SizeArea_mm2 | 0.5 | 0.5
|  | SizeAreaWB_mm2 |  |
|  | SizeX_mm | 1 | 1
|  | SizeY_mm | 0.5 | 0.5
|  | SizeZ_mm | 0.6 | 0.6
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Newark | Newark
|  | Supplier 3 | Mouser | Mouser
|  | Supplier Part Number 1 | 541-93.1KLCT-ND | 541-93.1KLCT-ND
|  | Supplier Part Number 2 | 52K7343 | 52K7343
|  | Supplier Part Number 3 | 71-CRCW0402-93.1K-E3 | 71-CRCW0402-93.1K-E3
|  | Technology | Thick Film | Thick Film
|  | TempCo | 100 ppm/C | 100 ppm/C
|  | Tolerance_% | 1% | 1%
|  | Value | 93.1k | 93.1k
|  | Value1 | 1% | 1%
|  | Value2 | 0.063W | 0.063W
|  | Value_Code | 93k1 | 93k1
|  | ValueDisplayed | 93.1k | 93.1k
|  | VDC_V | 50V | 50V
R10 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | 0 | 0
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | CRCW04021M00JNED | CRCW04021M00JNED
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.vishay.com/docs/20035/dcrcwe3.pdf | http://www.vishay.com/docs/20035/dcrcwe3.pdf
|  | CompType | Resistor | Resistor
|  | Description | RES, 1.0 M, 5%, 0.063 W, AEC-Q200 Grade 0, 0402 | RES, 1.0 M, 5%, 0.063 W, AEC-Q200 Grade 0, 0402
|  | EIA_Code | E24 | E24
|  | Footprint | 0402S | 0402S
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Manufacturer | Vishay-Dale | Vishay-Dale
|  | MountType | SMT | SMT
|  | PackageReference | 0402 | 0402
|  | PartNumber | CRCW04021M00JNED | CRCW04021M00JNED
|  | Power_W | 63mW | 63mW
|  | Res_ohm | 1M | 1M
|  | RoHS | E | E
|  | SizeArea_mm2 | 0.5 | 0.5
|  | SizeX_mm | 1 | 1
|  | SizeY_mm | 0.5 | 0.5
|  | SizeZ_mm | 0.6 | 0.6
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Newark | Newark
|  | Supplier 3 | Mouser | Mouser
|  | Supplier Part Number 1 | 541-1.0MJCT-ND | 541-1.0MJCT-ND
|  | Supplier Part Number 2 | 59M6694 | 59M6694
|  | Supplier Part Number 3 | 71-CRCW0402J-1M-E3 | 71-CRCW0402J-1M-E3
|  | Technology | Thick Film | Thick Film
|  | TempCo | 200 ppm/C | 200 ppm/C
|  | Tolerance_% | 5% | 5%
|  | Value | 1.0Meg | 1.0Meg
|  | Value1 | 5% | 5%
|  | Value2 | 0.063W | 0.063W
|  | Value_Code | 1M00 | 1M00
|  | ValueDisplayed | 1.0M | 1.0M
|  | VDC_V | 50V | 50V
R11 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | 0 | 0
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | CRCW040210R0JNED | CRCW040210R0JNED
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.vishay.com/docs/20035/dcrcwe3.pdf | http://www.vishay.com/docs/20035/dcrcwe3.pdf
|  | CompType | Resistor | Resistor
|  | Description | RES, 10, 5%, 0.063 W, AEC-Q200 Grade 0, 0402 | RES, 10, 5%, 0.063 W, AEC-Q200 Grade 0, 0402
|  | EIA_Code | E24 | E24
|  | Footprint | 0402S | 0402S
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Manufacturer | Vishay-Dale | Vishay-Dale
|  | MountType | SMT | SMT
|  | PackageReference | 0402 | 0402
|  | PartNumber | CRCW040210R0JNED | CRCW040210R0JNED
|  | Power_W | 63mW | 63mW
|  | Res_ohm | 10 | 10
|  | RoHS | E | E
|  | SizeArea_mm2 | 0.5 | 0.5
|  | SizeX_mm | 1 | 1
|  | SizeY_mm | 0.5 | 0.5
|  | SizeZ_mm | 0.6 | 0.6
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Newark | Newark
|  | Supplier 3 | Mouser | Mouser
|  | Supplier Part Number 1 | 541-10JCT-ND | 541-10JCT-ND
|  | Supplier Part Number 2 | 59M6698 | 59M6698
|  | Supplier Part Number 3 | 71-CRCW0402J-10-E3 | 71-CRCW0402J-10-E3
|  | Technology | Thick Film | Thick Film
|  | TempCo | 200 ppm/C | 200 ppm/C
|  | Tolerance_% | 5% | 5%
|  | Value | 10 | 10
|  | Value1 | 5% | 5%
|  | Value2 | 0.063W | 0.063W
|  | Value_Code | 10R0 | 10R0
|  | ValueDisplayed | 10 | 10
|  | VDC_V | 50V | 50V
R12 | HVP053B_sheet1.schdoc |  | Fitted | Not Fitted
|  | AEC Category | Q200 |
|  | AEC Grade | 0 |
|  | AEC Qualified | Y |
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | CRCW120610R0JNEA |
|  | ComponentLink1Description | Datasheet link |
|  | ComponentLink1URL | http://www.vishay.com/docs/20035/dcrcwe3.pdf |
|  | CompType | Resistor |
|  | Description | RES, 10, 5%, 0.25 W, AEC-Q200 Grade 0, 1206 |
|  | EIA_Code | E24 |
|  | Footprint | 1206L |
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Manufacturer | Vishay-Dale |
|  | MountType | SMT |
|  | PackageReference | 1206 |
|  | PartNumber | CRCW120610R0JNEA |
|  | Power_W | 250mW |
|  | Res_ohm | 10 |
|  | RoHS | E |
|  | SizeArea_mm2 | 5.12 |
|  | SizeX_mm | 3.2 |
|  | SizeY_mm | 1.6 |
|  | SizeZ_mm | 1.35 |
|  | Supplier 1 | Digi-Key |
|  | Supplier 2 | Newark |
|  | Supplier 3 | Mouser |
|  | Supplier Part Number 1 | 541-10ECT-ND |
|  | Supplier Part Number 2 | 53K1916 |
|  | Supplier Part Number 3 | 71-CRCW1206J-10-E3 |
|  | Technology | Thick Film |
|  | TempCo | 200 ppm/C |
|  | Tolerance_% | 5% |
|  | Value | 10 |
|  | Value1 | 5% |
|  | Value2 | 0.25W |
|  | Value_Code | 10R0 |
|  | ValueDisplayed | 10 |
|  | VDC_V | 200V |
R13 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | 0 | 0
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | CRCW040239K2FKED | CRCW040239K2FKED
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.vishay.com/docs/20035/dcrcwe3.pdf | http://www.vishay.com/docs/20035/dcrcwe3.pdf
|  | CompType | Resistor | Resistor
|  | Description | RES, 39.2 k, 1%, 0.063 W, AEC-Q200 Grade 0, 0402 | RES, 39.2 k, 1%, 0.063 W, AEC-Q200 Grade 0, 0402
|  | EIA_Code | E96 | E96
|  | Footprint | 0402S | 0402S
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Manufacturer | Vishay-Dale | Vishay-Dale
|  | MountType | SMT | SMT
|  | PackageReference | 0402 | 0402
|  | PartNumber | CRCW040239K2FKED | CRCW040239K2FKED
|  | Power_W | 63mW | 63mW
|  | Res_ohm | 39.2k | 39.2k
|  | RoHS | E | E
|  | SizeArea_mm2 | 0.5 | 0.5
|  | SizeX_mm | 1 | 1
|  | SizeY_mm | 0.5 | 0.5
|  | SizeZ_mm | 0.6 | 0.6
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Newark | Newark
|  | Supplier 3 | Mouser | Mouser
|  | Supplier Part Number 1 | 541-39.2KLCT-ND | 541-39.2KLCT-ND
|  | Supplier Part Number 2 | 52K7028 | 52K7028
|  | Supplier Part Number 3 | 71-CRCW0402-39.2K-E3 | 71-CRCW0402-39.2K-E3
|  | Technology | Thick Film | Thick Film
|  | TempCo | 100 ppm/C | 100 ppm/C
|  | Tolerance_% | 1% | 1%
|  | Value | 39.2k | 39.2k
|  | Value1 | 1% | 1%
|  | Value2 | 0.063W | 0.063W
|  | Value_Code | 39k2 | 39k2
|  | ValueDisplayed | 39.2k | 39.2k
|  | VDC_V | 50V | 50V
R14 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | 0 | 0
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | CRCW0402191KFKED | CRCW0402191KFKED
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.vishay.com/docs/20035/dcrcwe3.pdf | http://www.vishay.com/docs/20035/dcrcwe3.pdf
|  | CompType | Resistor | Resistor
|  | Description | RES, 191 k, 1%, 0.063 W, AEC-Q200 Grade 0, 0402 | RES, 191 k, 1%, 0.063 W, AEC-Q200 Grade 0, 0402
|  | EIA_Code | E96 | E96
|  | Footprint | 0402S | 0402S
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Manufacturer | Vishay-Dale | Vishay-Dale
|  | MountType | SMT | SMT
|  | PackageReference | 0402 | 0402
|  | PartNumber | CRCW0402191KFKED | CRCW0402191KFKED
|  | Power_W | 63mW | 63mW
|  | Res_ohm | 191k | 191k
|  | RoHS | E | E
|  | SizeArea_mm2 | 0.5 | 0.5
|  | SizeX_mm | 1 | 1
|  | SizeY_mm | 0.5 | 0.5
|  | SizeZ_mm | 0.6 | 0.6
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Newark | Newark
|  | Supplier 3 | Mouser | Mouser
|  | Supplier Part Number 1 | 541-191KLCT-ND | 541-191KLCT-ND
|  | Supplier Part Number 2 | 52K6780 | 52K6780
|  | Supplier Part Number 3 | 71-CRCW0402-191K-E3 | 71-CRCW0402-191K-E3
|  | Technology | Thick Film | Thick Film
|  | TempCo | 100 ppm/C | 100 ppm/C
|  | Tolerance_% | 1% | 1%
|  | Value | 191k | 191k
|  | Value1 | 1% | 1%
|  | Value2 | 0.063W | 0.063W
|  | Value_Code | 191k | 191k
|  | ValueDisplayed | 191k | 191k
|  | VDC_V | 50V | 50V
R15 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | 0 | 0
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | CRCW0805100RJNEA | CRCW0805100RJNEA
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.vishay.com/docs/20035/dcrcwe3.pdf | http://www.vishay.com/docs/20035/dcrcwe3.pdf
|  | CompType | Resistor | Resistor
|  | Description | RES, 100, 5%, 0.125 W, AEC-Q200 Grade 0, 0805 | RES, 100, 5%, 0.125 W, AEC-Q200 Grade 0, 0805
|  | EIA_Code | E24 | E24
|  | Footprint | 0805_HV1 | 0805_HV1
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Manufacturer | Vishay-Dale | Vishay-Dale
|  | MountType | SMT | SMT
|  | PackageReference | 0805 | 0805
|  | PartNumber | CRCW0805100RJNEA | CRCW0805100RJNEA
|  | Power_W | 125mW | 125mW
|  | Res_ohm | 100 | 100
|  | RoHS | E | E
|  | SizeArea_mm2 | 2.5 | 2.5
|  | SizeX_mm | 2 | 2
|  | SizeY_mm | 1.25 | 1.25
|  | SizeZ_mm | 1.45 | 1.45
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Newark | Newark
|  | Supplier 3 | Mouser | Mouser
|  | Supplier Part Number 1 | 541-100ACT-ND | 541-100ACT-ND
|  | Supplier Part Number 2 | 59M6851 | 59M6851
|  | Supplier Part Number 3 | 71-CRCW0805100RJNEA | 71-CRCW0805100RJNEA
|  | Technology | Thick Film | Thick Film
|  | TempCo | 200 ppm/C | 200 ppm/C
|  | Tolerance_% | 5% | 5%
|  | Value | 100 | 100
|  | Value1 | 5% | 5%
|  | Value2 | 0.125W | 0.125W
|  | Value_Code | 100R | 100R
|  | ValueDisplayed | 100 | 100
|  | VDC_V | 150V | 150V
R16 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | 0 | 0
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | CRCW040210K0FKED | CRCW040210K0FKED
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.vishay.com/docs/20035/dcrcwe3.pdf | http://www.vishay.com/docs/20035/dcrcwe3.pdf
|  | CompType | Resistor | Resistor
|  | Description | RES, 10.0 k, 1%, 0.063 W, AEC-Q200 Grade 0, 0402 | RES, 10.0 k, 1%, 0.063 W, AEC-Q200 Grade 0, 0402
|  | EIA_Code | E96 | E96
|  | Footprint | 0402S | 0402S
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Manufacturer | Vishay-Dale | Vishay-Dale
|  | MountType | SMT | SMT
|  | PackageReference | 0402 | 0402
|  | PartNumber | CRCW040210K0FKED | CRCW040210K0FKED
|  | Power_W | 63mW | 63mW
|  | Res_ohm | 10k | 10k
|  | RoHS | E | E
|  | SizeArea_mm2 | 0.5 | 0.5
|  | SizeX_mm | 1 | 1
|  | SizeY_mm | 0.5 | 0.5
|  | SizeZ_mm | 0.6 | 0.6
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Newark | Newark
|  | Supplier 3 | Mouser | Mouser
|  | Supplier Part Number 1 | 541-10.0KLCT-ND | 541-10.0KLCT-ND
|  | Supplier Part Number 2 | 52K6595 | 52K6595
|  | Supplier Part Number 3 | 71-CRCW0402-10K-E3 | 71-CRCW0402-10K-E3
|  | Technology | Thick Film | Thick Film
|  | TempCo | 100 ppm/C | 100 ppm/C
|  | Tolerance_% | 1% | 1%
|  | Value | 10.0k | 10.0k
|  | Value1 | 1% | 1%
|  | Value2 | 0.063W | 0.063W
|  | Value_Code | 10k0 | 10k0
|  | ValueDisplayed | 10.0k | 10.0k
|  | VDC_V | 50V | 50V
R17 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | 0 | 0
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | CRCW04020000Z0EDHP | CRCW04020000Z0EDHP
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.vishay.com/docs/20043/crcwhpe3.pdf | http://www.vishay.com/docs/20043/crcwhpe3.pdf
|  | CompType | Resistor | Resistor
|  | Description | RES, 0, 0%, 0.2 W, AEC-Q200 Grade 0, 0402 | RES, 0, 0%, 0.2 W, AEC-Q200 Grade 0, 0402
|  | EIA_Code |  |
|  | Footprint | 0402S | 0402S
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Manufacturer | Vishay-Dale | Vishay-Dale
|  | MountType | SMT | SMT
|  | PackageReference | 0402 | 0402
|  | PartNumber | CRCW04020000Z0EDHP | CRCW04020000Z0EDHP
|  | Power_W | 200mW | 200mW
|  | Res_ohm | 0 | 0
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 0.5 | 0.5
|  | SizeAreaWB_mm2 | 3 | 3
|  | SizeX_mm | 1 | 1
|  | SizeY_mm | 0.5 | 0.5
|  | SizeZ_mm | 0.6 | 0.6
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Newark | Newark
|  | Supplier 3 | Mouser | Mouser
|  | Supplier Part Number 1 | 541-0.0YBTR-ND | 541-0.0YBTR-ND
|  | Supplier Part Number 2 | 96Y9050 | 96Y9050
|  | Supplier Part Number 3 | 71-CRCW04020000Z0EDH | 71-CRCW04020000Z0EDH
|  | Technology | Thick Film | Thick Film
|  | TempCo |  |
|  | Tolerance_% | 0% | 0%
|  | Value | 0 | 0
|  | Value1 | 0% | 0%
|  | Value2 | 0.2W | 0.2W
|  | Value_Code | 0 | 0
|  | ValueDisplayed | 0 | 0
|  | VDC_V | 50V | 50V
R18 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | 0 | 0
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | CRCW0402511RFKED | CRCW0402511RFKED
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.vishay.com/docs/20035/dcrcwe3.pdf | http://www.vishay.com/docs/20035/dcrcwe3.pdf
|  | CompType | Resistor | Resistor
|  | Description | RES, 511, 1%, 0.063 W, AEC-Q200 Grade 0, 0402 | RES, 511, 1%, 0.063 W, AEC-Q200 Grade 0, 0402
|  | EIA_Code | E96 | E96
|  | Footprint | 0402S | 0402S
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Manufacturer | Vishay-Dale | Vishay-Dale
|  | MountType | SMT | SMT
|  | PackageReference | 0402 | 0402
|  | PartNumber | CRCW0402511RFKED | CRCW0402511RFKED
|  | Power_W | 63mW | 63mW
|  | Res_ohm | 511 | 511
|  | RoHS | E | E
|  | SizeArea_mm2 | 0.5 | 0.5
|  | SizeX_mm | 1 | 1
|  | SizeY_mm | 0.5 | 0.5
|  | SizeZ_mm | 0.6 | 0.6
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Newark | Newark
|  | Supplier 3 | Mouser | Mouser
|  | Supplier Part Number 1 | 541-511LCT-ND | 541-511LCT-ND
|  | Supplier Part Number 2 | 52K7136 | 52K7136
|  | Supplier Part Number 3 | 71-CRCW0402-511-E3 | 71-CRCW0402-511-E3
|  | Technology | Thick Film | Thick Film
|  | TempCo | 100 ppm/C | 100 ppm/C
|  | Tolerance_% | 1% | 1%
|  | Value | 511 | 511
|  | Value1 | 1% | 1%
|  | Value2 | 0.063W | 0.063W
|  | Value_Code | 511R | 511R
|  | ValueDisplayed | 511 | 511
|  | VDC_V | 50V | 50V
R19 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | 0 | 0
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | CRCW0402402RFKED | CRCW0402402RFKED
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.vishay.com/docs/20035/dcrcwe3.pdf | http://www.vishay.com/docs/20035/dcrcwe3.pdf
|  | CompType | Resistor | Resistor
|  | Description | RES, 402, 1%, 0.063 W, AEC-Q200 Grade 0, 0402 | RES, 402, 1%, 0.063 W, AEC-Q200 Grade 0, 0402
|  | EIA_Code | E96 | E96
|  | Footprint | 0402S | 0402S
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Manufacturer | Vishay-Dale | Vishay-Dale
|  | MountType | SMT | SMT
|  | PackageReference | 0402 | 0402
|  | PartNumber | CRCW0402402RFKED | CRCW0402402RFKED
|  | Power_W | 63mW | 63mW
|  | Res_ohm | 402 | 402
|  | RoHS | E | E
|  | SizeArea_mm2 | 0.5 | 0.5
|  | SizeX_mm | 1 | 1
|  | SizeY_mm | 0.5 | 0.5
|  | SizeZ_mm | 0.6 | 0.6
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Newark | Newark
|  | Supplier 3 | Mouser | Mouser
|  | Supplier Part Number 1 | 541-402LCT-ND | 541-402LCT-ND
|  | Supplier Part Number 2 | 52K7054 | 52K7054
|  | Supplier Part Number 3 | 71-CRCW0402-402-E3 | 71-CRCW0402-402-E3
|  | Technology | Thick Film | Thick Film
|  | TempCo | 100 ppm/C | 100 ppm/C
|  | Tolerance_% | 1% | 1%
|  | Value | 402 | 402
|  | Value1 | 1% | 1%
|  | Value2 | 0.063W | 0.063W
|  | Value_Code | 402R | 402R
|  | ValueDisplayed | 402 | 402
|  | VDC_V | 50V | 50V
R20 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | 0 | 0
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | CRCW040215K4FKED | CRCW040215K4FKED
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.vishay.com/docs/20035/dcrcwe3.pdf | http://www.vishay.com/docs/20035/dcrcwe3.pdf
|  | CompType | Resistor | Resistor
|  | Description | RES, 15.4 k, 1%, 0.063 W, AEC-Q200 Grade 0, 0402 | RES, 15.4 k, 1%, 0.063 W, AEC-Q200 Grade 0, 0402
|  | EIA_Code | E96 | E96
|  | Footprint | 0402S | 0402S
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Manufacturer | Vishay-Dale | Vishay-Dale
|  | MountType | SMT | SMT
|  | PackageReference | 0402 | 0402
|  | PartNumber | CRCW040215K4FKED | CRCW040215K4FKED
|  | Power_W | 63mW | 63mW
|  | Res_ohm | 15.4k | 15.4k
|  | RoHS | E | E
|  | SizeArea_mm2 | 0.5 | 0.5
|  | SizeX_mm | 1 | 1
|  | SizeY_mm | 0.5 | 0.5
|  | SizeZ_mm | 0.6 | 0.6
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Newark | Newark
|  | Supplier 3 | Mouser | Mouser
|  | Supplier Part Number 1 | 541-15.4KLCT-ND | 541-15.4KLCT-ND
|  | Supplier Part Number 2 | 52K6710 | 52K6710
|  | Supplier Part Number 3 | 71-CRCW0402-15.4K-E3 | 71-CRCW0402-15.4K-E3
|  | Technology | Thick Film | Thick Film
|  | TempCo | 100 ppm/C | 100 ppm/C
|  | Tolerance_% | 1% | 1%
|  | Value | 15.4k | 15.4k
|  | Value1 | 1% | 1%
|  | Value2 | 0.063W | 0.063W
|  | Value_Code | 15k4 | 15k4
|  | ValueDisplayed | 15.4k | 15.4k
|  | VDC_V | 50V | 50V
R21 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade |  |
|  | AEC Qualified | ? | ?
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | MCR25JZHFLR220 | MCR25JZHFLR220
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.rohm.com/products/databook/r/pdf/mcr25_ttk.pdf | http://www.rohm.com/products/databook/r/pdf/mcr25_ttk.pdf
|  | CompType | Resistor | Resistor
|  | Description | RES, 0.22, 1%, 0.5 W, 1210 | RES, 0.22, 1%, 0.5 W, 1210
|  | EIA_Code | E96 | E96
|  | Footprint | 1210L | 1210L
|  | LatestRevisionDate | 2017-03-09 | 2017-03-09
|  | Manufacturer | Rohm | Rohm
|  | MountType | SMT | SMT
|  | PackageReference | 1210 | 1210
|  | PartNumber | MCR25JZHFLR220 | MCR25JZHFLR220
|  | Power_W | 500mW | 500mW
|  | Published | 2008-06-26 | 2008-06-26
|  | Publisher | Texas Instruments | Texas Instruments
|  | Res_ohm | 0.22 | 0.22
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 8 | 8
|  | SizeAreaWB_mm2 | 14.7 | 14.7
|  | SizeX_mm | 3.2 | 3.2
|  | SizeY_mm | 2.5 | 2.5
|  | SizeZ_mm | 1.35 | 1.35
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 |  |
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | RHM.22SCT-ND | RHM.22SCT-ND
|  | Supplier Part Number 2 |  |
|  | Supplier Part Number 3 |  |
|  | Technology | Thick Film | Thick Film
|  | TempCo | 200 ppm/C | 200 ppm/C
|  | Tolerance_% | 1% | 1%
|  | U/M | EA | EA
|  | Value | 0.22 | 0.22
|  | Value1 | 1% | 1%
|  | Value2 | 0.5W | 0.5W
|  | Value_Code | R220 | R220
|  | ValueDisplayed | 0.22 | 0.22
|  | VDC_V | 0V | 0V
R22 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade |  |
|  | AEC Qualified | ? | ?
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | RC0402JR-070RL | RC0402JR-070RL
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.yageo.com/pdf/Pu-RC0402_51_PbFree_L_2.pdf | http://www.yageo.com/pdf/Pu-RC0402_51_PbFree_L_2.pdf
|  | CompType | Resistor | Resistor
|  | Description | RES, 0, 5%, 0.063 W, 0402 | RES, 0, 5%, 0.063 W, 0402
|  | EIA_Code | E24 | E24
|  | Footprint | 0402S | 0402S
|  | LatestRevisionDate | 2017-03-09 | 2017-03-09
|  | Manufacturer | Yageo America | Yageo America
|  | MountType | SMT | SMT
|  | PackageReference | 0402 | 0402
|  | PartNumber | RC0402JR-070RL | RC0402JR-070RL
|  | Power_W | 63mW | 63mW
|  | Published | 2008-06-26 | 2008-06-26
|  | Publisher | Texas Instruments | Texas Instruments
|  | Res_ohm | 0 | 0
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 0.5 | 0.5
|  | SizeX_mm | 1 | 1
|  | SizeY_mm | 0.5 | 0.5
|  | SizeZ_mm | 0.6 | 0.6
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Mouser | Mouser
|  | Supplier 3 | Farnell | Farnell
|  | Supplier Part Number 1 | 311-0.0JRCT-ND | 311-0.0JRCT-ND
|  | Supplier Part Number 2 | 603-RC0402JR-070RL | 603-RC0402JR-070RL
|  | Supplier Part Number 3 | 9232516 | 9232516
|  | Technology | Thick Film | Thick Film
|  | TempCo | 200 ppm/C | 200 ppm/C
|  | Tolerance_% | 5% | 5%
|  | U/M | EA | EA
|  | Value | 0 | 0
|  | Value1 | 5% | 5%
|  | Value2 | 0.063W | 0.063W
|  | Value_Code | 0000 | 0000
|  | ValueDisplayed | 0 | 0
|  | VDC_V | 50V | 50V
R23 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | 0 | 0
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | CRCW04026K98FKED | CRCW04026K98FKED
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.vishay.com/docs/20035/dcrcwe3.pdf | http://www.vishay.com/docs/20035/dcrcwe3.pdf
|  | CompType | Resistor | Resistor
|  | Description | RES, 6.98 k, 1%, 0.063 W, AEC-Q200 Grade 0, 0402 | RES, 6.98 k, 1%, 0.063 W, AEC-Q200 Grade 0, 0402
|  | EIA_Code | E96 | E96
|  | Footprint | 0402S | 0402S
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Manufacturer | Vishay-Dale | Vishay-Dale
|  | MountType | SMT | SMT
|  | PackageReference | 0402 | 0402
|  | PartNumber | CRCW04026K98FKED | CRCW04026K98FKED
|  | Power_W | 63mW | 63mW
|  | Res_ohm | 6.98k | 6.98k
|  | RoHS | E | E
|  | SizeArea_mm2 | 0.5 | 0.5
|  | SizeX_mm | 1 | 1
|  | SizeY_mm | 0.5 | 0.5
|  | SizeZ_mm | 0.6 | 0.6
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Newark | Newark
|  | Supplier 3 | Mouser | Mouser
|  | Supplier Part Number 1 | 541-6.98KLCT-ND | 541-6.98KLCT-ND
|  | Supplier Part Number 2 | 52K7189 | 52K7189
|  | Supplier Part Number 3 | 71-CRCW0402-6.98K-E3 | 71-CRCW0402-6.98K-E3
|  | Technology | Thick Film | Thick Film
|  | TempCo | 100 ppm/C | 100 ppm/C
|  | Tolerance_% | 1% | 1%
|  | Value | 6.98k | 6.98k
|  | Value1 | 1% | 1%
|  | Value2 | 0.063W | 0.063W
|  | Value_Code | 6k98 | 6k98
|  | ValueDisplayed | 6.98k | 6.98k
|  | VDC_V | 50V | 50V
R24 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | 0 | 0
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | CRCW04021M00JNED | CRCW04021M00JNED
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.vishay.com/docs/20035/dcrcwe3.pdf | http://www.vishay.com/docs/20035/dcrcwe3.pdf
|  | CompType | Resistor | Resistor
|  | Description | RES, 1.0 M, 5%, 0.063 W, AEC-Q200 Grade 0, 0402 | RES, 1.0 M, 5%, 0.063 W, AEC-Q200 Grade 0, 0402
|  | EIA_Code | E24 | E24
|  | Footprint | 0402S | 0402S
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Manufacturer | Vishay-Dale | Vishay-Dale
|  | MountType | SMT | SMT
|  | PackageReference | 0402 | 0402
|  | PartNumber | CRCW04021M00JNED | CRCW04021M00JNED
|  | Power_W | 63mW | 63mW
|  | Res_ohm | 1M | 1M
|  | RoHS | E | E
|  | SizeArea_mm2 | 0.5 | 0.5
|  | SizeX_mm | 1 | 1
|  | SizeY_mm | 0.5 | 0.5
|  | SizeZ_mm | 0.6 | 0.6
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Newark | Newark
|  | Supplier 3 | Mouser | Mouser
|  | Supplier Part Number 1 | 541-1.0MJCT-ND | 541-1.0MJCT-ND
|  | Supplier Part Number 2 | 59M6694 | 59M6694
|  | Supplier Part Number 3 | 71-CRCW0402J-1M-E3 | 71-CRCW0402J-1M-E3
|  | Technology | Thick Film | Thick Film
|  | TempCo | 200 ppm/C | 200 ppm/C
|  | Tolerance_% | 5% | 5%
|  | Value | 1.0Meg | 1.0Meg
|  | Value1 | 5% | 5%
|  | Value2 | 0.063W | 0.063W
|  | Value_Code | 1M00 | 1M00
|  | ValueDisplayed | 1.0M | 1.0M
|  | VDC_V | 50V | 50V
R25 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | 0 | 0
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | ERJ-2RKF1503X | ERJ-2RKF1503X
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000CE2.pdf | http://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000CE2.pdf
|  | CompType | Resistor | Resistor
|  | Description | RES, 150 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0402 | RES, 150 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0402
|  | EIA_Code | E96 | E96
|  | Footprint | 0402S | 0402S
|  | LatestRevisionDate | 2017-03-09 | 2017-03-09
|  | Manufacturer | Panasonic | Panasonic
|  | MountType | SMT | SMT
|  | PackageReference | 0402 | 0402
|  | PartNumber | ERJ-2RKF1503X | ERJ-2RKF1503X
|  | Power_W | 100mW | 100mW
|  | Published | 2008-06-26 | 2008-06-26
|  | Publisher | Texas Instruments | Texas Instruments
|  | Res_ohm | 150k | 150k
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 0.5 | 0.5
|  | SizeX_mm | 1 | 1
|  | SizeY_mm | 0.5 | 0.5
|  | SizeZ_mm | 0.6 | 0.6
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Newark | Newark
|  | Supplier 3 | Mouser | Mouser
|  | Supplier Part Number 1 | P150KLCT-ND | P150KLCT-ND
|  | Supplier Part Number 2 | 64R5260 | 64R5260
|  | Supplier Part Number 3 | 667-ERJ-2RKF1503X | 667-ERJ-2RKF1503X
|  | Technology | Thick Film | Thick Film
|  | TempCo | 100 ppm/C | 100 ppm/C
|  | Tolerance_% | 1% | 1%
|  | U/M | EA | EA
|  | Value | 150k | 150k
|  | Value1 | 1% | 1%
|  | Value2 | 0.1W | 0.1W
|  | Value_Code | 150k | 150k
|  | ValueDisplayed | 150k | 150k
|  | VDC_V | 50V | 50V
R26 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | 0 | 0
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | CRCW040215K0FKED | CRCW040215K0FKED
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.vishay.com/docs/20035/dcrcwe3.pdf | http://www.vishay.com/docs/20035/dcrcwe3.pdf
|  | CompType | Resistor | Resistor
|  | Description | RES, 15.0 k, 1%, 0.063 W, AEC-Q200 Grade 0, 0402 | RES, 15.0 k, 1%, 0.063 W, AEC-Q200 Grade 0, 0402
|  | EIA_Code | E96 | E96
|  | Footprint | 0402S | 0402S
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Manufacturer | Vishay-Dale | Vishay-Dale
|  | MountType | SMT | SMT
|  | PackageReference | 0402 | 0402
|  | PartNumber | CRCW040215K0FKED | CRCW040215K0FKED
|  | Power_W | 63mW | 63mW
|  | Res_ohm | 15k | 15k
|  | RoHS | E | E
|  | SizeArea_mm2 | 0.5 | 0.5
|  | SizeX_mm | 1 | 1
|  | SizeY_mm | 0.5 | 0.5
|  | SizeZ_mm | 0.6 | 0.6
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Newark | Newark
|  | Supplier 3 | Mouser | Mouser
|  | Supplier Part Number 1 | 541-15.0KLCT-ND | 541-15.0KLCT-ND
|  | Supplier Part Number 2 | 52K6708 | 52K6708
|  | Supplier Part Number 3 | 71-CRCW0402-15K-E3 | 71-CRCW0402-15K-E3
|  | Technology | Thick Film | Thick Film
|  | TempCo | 100 ppm/C | 100 ppm/C
|  | Tolerance_% | 1% | 1%
|  | Value | 15.0k | 15.0k
|  | Value1 | 1% | 1%
|  | Value2 | 0.063W | 0.063W
|  | Value_Code | 15k0 | 15k0
|  | ValueDisplayed | 15.0k | 15.0k
|  | VDC_V | 50V | 50V
R27 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | 0 | 0
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | CRCW0402511RFKED | CRCW0402511RFKED
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.vishay.com/docs/20035/dcrcwe3.pdf | http://www.vishay.com/docs/20035/dcrcwe3.pdf
|  | CompType | Resistor | Resistor
|  | Description | RES, 511, 1%, 0.063 W, AEC-Q200 Grade 0, 0402 | RES, 511, 1%, 0.063 W, AEC-Q200 Grade 0, 0402
|  | EIA_Code | E96 | E96
|  | Footprint | 0402S | 0402S
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Manufacturer | Vishay-Dale | Vishay-Dale
|  | MountType | SMT | SMT
|  | PackageReference | 0402 | 0402
|  | PartNumber | CRCW0402511RFKED | CRCW0402511RFKED
|  | Power_W | 63mW | 63mW
|  | Res_ohm | 511 | 511
|  | RoHS | E | E
|  | SizeArea_mm2 | 0.5 | 0.5
|  | SizeX_mm | 1 | 1
|  | SizeY_mm | 0.5 | 0.5
|  | SizeZ_mm | 0.6 | 0.6
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Newark | Newark
|  | Supplier 3 | Mouser | Mouser
|  | Supplier Part Number 1 | 541-511LCT-ND | 541-511LCT-ND
|  | Supplier Part Number 2 | 52K7136 | 52K7136
|  | Supplier Part Number 3 | 71-CRCW0402-511-E3 | 71-CRCW0402-511-E3
|  | Technology | Thick Film | Thick Film
|  | TempCo | 100 ppm/C | 100 ppm/C
|  | Tolerance_% | 1% | 1%
|  | Value | 511 | 511
|  | Value1 | 1% | 1%
|  | Value2 | 0.063W | 0.063W
|  | Value_Code | 511R | 511R
|  | ValueDisplayed | 511 | 511
|  | VDC_V | 50V | 50V
R28 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | 0 | 0
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | ERJ-6RQFR68V | ERJ-6RQFR68V
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | https://industrial.panasonic.com/cdbs/www-data/pdf/RDN0000/AOA0000C313.pdf | https://industrial.panasonic.com/cdbs/www-data/pdf/RDN0000/AOA0000C313.pdf
|  | CompType | Resistor | Resistor
|  | Description | RES, 0.68, 1%, 0.125 W, AEC-Q200 Grade 0, 0805 | RES, 0.68, 1%, 0.125 W, AEC-Q200 Grade 0, 0805
|  | EIA_Code | E96 | E96
|  | Footprint | 0805_HV1 | 0805_HV1
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Manufacturer | Panasonic | Panasonic
|  | MountType | SMT | SMT
|  | PackageReference | 0805 | 0805
|  | PartNumber | ERJ-6RQFR68V | ERJ-6RQFR68V
|  | Power_W | 125mW | 125mW
|  | Res_ohm | 0.68 | 0.68
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 2.5 | 2.5
|  | SizeAreaWB_mm2 | 6.75 | 6.75
|  | SizeX_mm | 2 | 2
|  | SizeY_mm | 1.25 | 1.25
|  | SizeZ_mm | 1.45 | 1.45
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Mouser | Mouser
|  | Supplier 3 | Farnell | Farnell
|  | Supplier Part Number 1 | P.68DCT-ND | P.68DCT-ND
|  | Supplier Part Number 2 | 667-ERJ-6RQFR68V | 667-ERJ-6RQFR68V
|  | Supplier Part Number 3 | 1717797 | 1717797
|  | Technology | Thick Film | Thick Film
|  | TempCo | 250 ppm/C | 250 ppm/C
|  | Tolerance_% | 1% | 1%
|  | Value | 0.68 | 0.68
|  | Value1 | 1% | 1%
|  | Value2 | 0.125W | 0.125W
|  | Value_Code | R680 | R680
|  | ValueDisplayed | 0.68 | 0.68
|  | VDC_V |  |
R29 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | 0 | 0
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | CRCW040210K0FKED | CRCW040210K0FKED
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.vishay.com/docs/20035/dcrcwe3.pdf | http://www.vishay.com/docs/20035/dcrcwe3.pdf
|  | CompType | Resistor | Resistor
|  | Description | RES, 10.0 k, 1%, 0.063 W, AEC-Q200 Grade 0, 0402 | RES, 10.0 k, 1%, 0.063 W, AEC-Q200 Grade 0, 0402
|  | EIA_Code | E96 | E96
|  | Footprint | 0402S | 0402S
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Manufacturer | Vishay-Dale | Vishay-Dale
|  | MountType | SMT | SMT
|  | PackageReference | 0402 | 0402
|  | PartNumber | CRCW040210K0FKED | CRCW040210K0FKED
|  | Power_W | 63mW | 63mW
|  | Res_ohm | 10k | 10k
|  | RoHS | E | E
|  | SizeArea_mm2 | 0.5 | 0.5
|  | SizeX_mm | 1 | 1
|  | SizeY_mm | 0.5 | 0.5
|  | SizeZ_mm | 0.6 | 0.6
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Newark | Newark
|  | Supplier 3 | Mouser | Mouser
|  | Supplier Part Number 1 | 541-10.0KLCT-ND | 541-10.0KLCT-ND
|  | Supplier Part Number 2 | 52K6595 | 52K6595
|  | Supplier Part Number 3 | 71-CRCW0402-10K-E3 | 71-CRCW0402-10K-E3
|  | Technology | Thick Film | Thick Film
|  | TempCo | 100 ppm/C | 100 ppm/C
|  | Tolerance_% | 1% | 1%
|  | Value | 10.0k | 10.0k
|  | Value1 | 1% | 1%
|  | Value2 | 0.063W | 0.063W
|  | Value_Code | 10k0 | 10k0
|  | ValueDisplayed | 10.0k | 10.0k
|  | VDC_V | 50V | 50V
R30 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | 0 | 0
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | CRCW040220K0FKED | CRCW040220K0FKED
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.vishay.com/docs/20035/dcrcwe3.pdf | http://www.vishay.com/docs/20035/dcrcwe3.pdf
|  | CompType | Resistor | Resistor
|  | Description | RES, 20.0 k, 1%, 0.063 W, AEC-Q200 Grade 0, 0402 | RES, 20.0 k, 1%, 0.063 W, AEC-Q200 Grade 0, 0402
|  | EIA_Code | E96 | E96
|  | Footprint | 0402S | 0402S
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Manufacturer | Vishay-Dale | Vishay-Dale
|  | MountType | SMT | SMT
|  | PackageReference | 0402 | 0402
|  | PartNumber | CRCW040220K0FKED | CRCW040220K0FKED
|  | Power_W | 63mW | 63mW
|  | Res_ohm | 20k | 20k
|  | RoHS | E | E
|  | SizeArea_mm2 | 0.5 | 0.5
|  | SizeX_mm | 1 | 1
|  | SizeY_mm | 0.5 | 0.5
|  | SizeZ_mm | 0.6 | 0.6
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Newark | Newark
|  | Supplier 3 | Mouser | Mouser
|  | Supplier Part Number 1 | 541-20.0KLCT-ND | 541-20.0KLCT-ND
|  | Supplier Part Number 2 | 52K6817 | 52K6817
|  | Supplier Part Number 3 | 71-CRCW0402-20K-E3 | 71-CRCW0402-20K-E3
|  | Technology | Thick Film | Thick Film
|  | TempCo | 100 ppm/C | 100 ppm/C
|  | Tolerance_% | 1% | 1%
|  | Value | 20.0k | 20.0k
|  | Value1 | 1% | 1%
|  | Value2 | 0.063W | 0.063W
|  | Value_Code | 20k0 | 20k0
|  | ValueDisplayed | 20.0k | 20.0k
|  | VDC_V | 50V | 50V
R31 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | 0 | 0
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | CRCW040230K0FKED | CRCW040230K0FKED
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.vishay.com/docs/20035/dcrcwe3.pdf | http://www.vishay.com/docs/20035/dcrcwe3.pdf
|  | CompType | Resistor | Resistor
|  | Description | RES, 30.0 k, 1%, 0.063 W, AEC-Q200 Grade 0, 0402 | RES, 30.0 k, 1%, 0.063 W, AEC-Q200 Grade 0, 0402
|  | EIA_Code |  |
|  | Footprint | 0402S | 0402S
|  | Green_EU RoHS | Passed with Exemption | Passed with Exemption
|  | Green_EU RoHS-2 | Passed | Passed
|  | Green_Lifecycle | Active | Active
|  | Green_REACh | Passed | Passed
|  | Manufacturer | Vishay-Dale | Vishay-Dale
|  | MountType | SMT | SMT
|  | PackageReference | 0402 | 0402
|  | PartNumber | CRCW040230K0FKED | CRCW040230K0FKED
|  | Power_W | 63mW | 63mW
|  | Res_ohm | 30k | 30k
|  | RoHS | E | E
|  | SizeArea_mm2 | 0.5 | 0.5
|  | SizeX_mm | 1 | 1
|  | SizeY_mm | 0.5 | 0.5
|  | SizeZ_mm | 0.6 | 0.6
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Newark | Newark
|  | Supplier 3 | Mouser | Mouser
|  | Supplier Part Number 1 | 541-30.0KLCT-ND | 541-30.0KLCT-ND
|  | Supplier Part Number 2 | 52K6953 | 52K6953
|  | Supplier Part Number 3 | 71-CRCW0402-30K-E3 | 71-CRCW0402-30K-E3
|  | Technology | Thick Film | Thick Film
|  | TempCo | 100 ppm/C | 100 ppm/C
|  | Tolerance_% | 1% | 1%
|  | Value | 30.0k | 30.0k
|  | Value1 | 1% | 1%
|  | Value2 | 0.063W | 0.063W
|  | Value_Code | 30k0 | 30k0
|  | ValueDisplayed | 30.0k | 30.0k
|  | VDC_V | 50V | 50V
R32 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | 0 | 0
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | CRCW04025K62FKED | CRCW04025K62FKED
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.vishay.com/docs/20035/dcrcwe3.pdf | http://www.vishay.com/docs/20035/dcrcwe3.pdf
|  | CompType | Resistor | Resistor
|  | Description | RES, 5.62 k, 1%, 0.063 W, AEC-Q200 Grade 0, 0402 | RES, 5.62 k, 1%, 0.063 W, AEC-Q200 Grade 0, 0402
|  | EIA_Code | E96 | E96
|  | Footprint | 0402S | 0402S
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Manufacturer | Vishay-Dale | Vishay-Dale
|  | MountType | SMT | SMT
|  | PackageReference | 0402 | 0402
|  | PartNumber | CRCW04025K62FKED | CRCW04025K62FKED
|  | Power_W | 63mW | 63mW
|  | Res_ohm | 5.62k | 5.62k
|  | RoHS | E | E
|  | SizeArea_mm2 | 0.5 | 0.5
|  | SizeX_mm | 1 | 1
|  | SizeY_mm | 0.5 | 0.5
|  | SizeZ_mm | 0.6 | 0.6
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Newark | Newark
|  | Supplier 3 | Mouser | Mouser
|  | Supplier Part Number 1 | 541-5.62KLCT-ND | 541-5.62KLCT-ND
|  | Supplier Part Number 2 | 52K7126 | 52K7126
|  | Supplier Part Number 3 | 71-CRCW0402-5.62K-E3 | 71-CRCW0402-5.62K-E3
|  | Technology | Thick Film | Thick Film
|  | TempCo | 100 ppm/C | 100 ppm/C
|  | Tolerance_% | 1% | 1%
|  | Value | 5.62k | 5.62k
|  | Value1 | 1% | 1%
|  | Value2 | 0.063W | 0.063W
|  | Value_Code | 5k62 | 5k62
|  | ValueDisplayed | 5.62k | 5.62k
|  | VDC_V | 50V | 50V
R33 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | 0 | 0
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | CRCW1206220KJNEA | CRCW1206220KJNEA
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.vishay.com/docs/20035/dcrcwe3.pdf | http://www.vishay.com/docs/20035/dcrcwe3.pdf
|  | CompType | Resistor | Resistor
|  | Description | RES, 220 k, 5%, 0.25 W, AEC-Q200 Grade 0, 1206 | RES, 220 k, 5%, 0.25 W, AEC-Q200 Grade 0, 1206
|  | EIA_Code | E24 | E24
|  | Footprint | 1206 | 1206
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Manufacturer | Vishay-Dale | Vishay-Dale
|  | MountType | SMT | SMT
|  | PackageReference | 1206 | 1206
|  | PartNumber | CRCW1206220KJNEA | CRCW1206220KJNEA
|  | Power_W | 250mW | 250mW
|  | Res_ohm | 220k | 220k
|  | RoHS | E | E
|  | SizeArea_mm2 | 5.12 | 5.12
|  | SizeX_mm | 3.2 | 3.2
|  | SizeY_mm | 1.6 | 1.6
|  | SizeZ_mm | 1.35 | 1.35
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Newark | Newark
|  | Supplier 3 | Mouser | Mouser
|  | Supplier Part Number 1 | 541-220KECT-ND | 541-220KECT-ND
|  | Supplier Part Number 2 | 59M6969 | 59M6969
|  | Supplier Part Number 3 | 71-CRCW1206J-220K-E3 | 71-CRCW1206J-220K-E3
|  | Technology | Thick Film | Thick Film
|  | TempCo | 200 ppm/C | 200 ppm/C
|  | Tolerance_% | 5% | 5%
|  | Value | 220k | 220k
|  | Value1 | 5% | 5%
|  | Value2 | 0.25W | 0.25W
|  | Value_Code | 220k | 220k
|  | ValueDisplayed | 220k | 220k
|  | VDC_V | 200V | 200V
R34 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | 0 | 0
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | CRCW1206220KJNEA | CRCW1206220KJNEA
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.vishay.com/docs/20035/dcrcwe3.pdf | http://www.vishay.com/docs/20035/dcrcwe3.pdf
|  | CompType | Resistor | Resistor
|  | Description | RES, 220 k, 5%, 0.25 W, AEC-Q200 Grade 0, 1206 | RES, 220 k, 5%, 0.25 W, AEC-Q200 Grade 0, 1206
|  | EIA_Code | E24 | E24
|  | Footprint | 1206 | 1206
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Manufacturer | Vishay-Dale | Vishay-Dale
|  | MountType | SMT | SMT
|  | PackageReference | 1206 | 1206
|  | PartNumber | CRCW1206220KJNEA | CRCW1206220KJNEA
|  | Power_W | 250mW | 250mW
|  | Res_ohm | 220k | 220k
|  | RoHS | E | E
|  | SizeArea_mm2 | 5.12 | 5.12
|  | SizeX_mm | 3.2 | 3.2
|  | SizeY_mm | 1.6 | 1.6
|  | SizeZ_mm | 1.35 | 1.35
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Newark | Newark
|  | Supplier 3 | Mouser | Mouser
|  | Supplier Part Number 1 | 541-220KECT-ND | 541-220KECT-ND
|  | Supplier Part Number 2 | 59M6969 | 59M6969
|  | Supplier Part Number 3 | 71-CRCW1206J-220K-E3 | 71-CRCW1206J-220K-E3
|  | Technology | Thick Film | Thick Film
|  | TempCo | 200 ppm/C | 200 ppm/C
|  | Tolerance_% | 5% | 5%
|  | Value | 220k | 220k
|  | Value1 | 5% | 5%
|  | Value2 | 0.25W | 0.25W
|  | Value_Code | 220k | 220k
|  | ValueDisplayed | 220k | 220k
|  | VDC_V | 200V | 200V
R35 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | 0 | 0
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | CRCW1206220KJNEA | CRCW1206220KJNEA
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.vishay.com/docs/20035/dcrcwe3.pdf | http://www.vishay.com/docs/20035/dcrcwe3.pdf
|  | CompType | Resistor | Resistor
|  | Description | RES, 220 k, 5%, 0.25 W, AEC-Q200 Grade 0, 1206 | RES, 220 k, 5%, 0.25 W, AEC-Q200 Grade 0, 1206
|  | EIA_Code | E24 | E24
|  | Footprint | 1206 | 1206
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Manufacturer | Vishay-Dale | Vishay-Dale
|  | MountType | SMT | SMT
|  | PackageReference | 1206 | 1206
|  | PartNumber | CRCW1206220KJNEA | CRCW1206220KJNEA
|  | Power_W | 250mW | 250mW
|  | Res_ohm | 220k | 220k
|  | RoHS | E | E
|  | SizeArea_mm2 | 5.12 | 5.12
|  | SizeX_mm | 3.2 | 3.2
|  | SizeY_mm | 1.6 | 1.6
|  | SizeZ_mm | 1.35 | 1.35
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Newark | Newark
|  | Supplier 3 | Mouser | Mouser
|  | Supplier Part Number 1 | 541-220KECT-ND | 541-220KECT-ND
|  | Supplier Part Number 2 | 59M6969 | 59M6969
|  | Supplier Part Number 3 | 71-CRCW1206J-220K-E3 | 71-CRCW1206J-220K-E3
|  | Technology | Thick Film | Thick Film
|  | TempCo | 200 ppm/C | 200 ppm/C
|  | Tolerance_% | 5% | 5%
|  | Value | 220k | 220k
|  | Value1 | 5% | 5%
|  | Value2 | 0.25W | 0.25W
|  | Value_Code | 220k | 220k
|  | ValueDisplayed | 220k | 220k
|  | VDC_V | 200V | 200V
R36 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | 0 | 0
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | CRCW0402102RFKED | CRCW0402102RFKED
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.vishay.com/docs/20035/dcrcwe3.pdf | http://www.vishay.com/docs/20035/dcrcwe3.pdf
|  | CompType | Resistor | Resistor
|  | Description | RES, 102, 1%, 0.063 W, AEC-Q200 Grade 0, 0402 | RES, 102, 1%, 0.063 W, AEC-Q200 Grade 0, 0402
|  | EIA_Code | E96 | E96
|  | Footprint | 0402S | 0402S
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Manufacturer | Vishay-Dale | Vishay-Dale
|  | MountType | SMT | SMT
|  | PackageReference | 0402 | 0402
|  | PartNumber | CRCW0402102RFKED | CRCW0402102RFKED
|  | Power_W | 63mW | 63mW
|  | Res_ohm | 102 | 102
|  | RoHS | E | E
|  | SizeArea_mm2 | 0.5 | 0.5
|  | SizeX_mm | 1 | 1
|  | SizeY_mm | 0.5 | 0.5
|  | SizeZ_mm | 0.6 | 0.6
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Newark | Newark
|  | Supplier 3 | Mouser | Mouser
|  | Supplier Part Number 1 | 541-102LCT-ND | 541-102LCT-ND
|  | Supplier Part Number 2 | 52K6613 | 52K6613
|  | Supplier Part Number 3 | 71-CRCW0402-102-E3 | 71-CRCW0402-102-E3
|  | Technology | Thick Film | Thick Film
|  | TempCo | 100 ppm/C | 100 ppm/C
|  | Tolerance_% | 1% | 1%
|  | Value | 102 | 102
|  | Value1 | 1% | 1%
|  | Value2 | 0.063W | 0.063W
|  | Value_Code | 102R | 102R
|  | ValueDisplayed | 102 | 102
|  | VDC_V | 50V | 50V
R37 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | 0 | 0
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | CRCW04022K10FKED | CRCW04022K10FKED
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.vishay.com/docs/20035/dcrcwe3.pdf | http://www.vishay.com/docs/20035/dcrcwe3.pdf
|  | CompType | Resistor | Resistor
|  | Description | RES, 2.10 k, 1%, 0.063 W, AEC-Q200 Grade 0, 0402 | RES, 2.10 k, 1%, 0.063 W, AEC-Q200 Grade 0, 0402
|  | EIA_Code | E96 | E96
|  | Footprint | 0402S | 0402S
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Manufacturer | Vishay-Dale | Vishay-Dale
|  | MountType | SMT | SMT
|  | PackageReference | 0402 | 0402
|  | PartNumber | CRCW04022K10FKED | CRCW04022K10FKED
|  | Power_W | 63mW | 63mW
|  | Res_ohm | 2.1k | 2.1k
|  | RoHS | E | E
|  | SizeArea_mm2 | 0.5 | 0.5
|  | SizeX_mm | 1 | 1
|  | SizeY_mm | 0.5 | 0.5
|  | SizeZ_mm | 0.6 | 0.6
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Newark | Newark
|  | Supplier 3 | Mouser | Mouser
|  | Supplier Part Number 1 | 541-2.10KLCT-ND | 541-2.10KLCT-ND
|  | Supplier Part Number 2 | 52K6791 | 52K6791
|  | Supplier Part Number 3 | 71-CRCW0402-2.1K-E3 | 71-CRCW0402-2.1K-E3
|  | Technology | Thick Film | Thick Film
|  | TempCo | 100 ppm/C | 100 ppm/C
|  | Tolerance_% | 1% | 1%
|  | Value | 2.10k | 2.10k
|  | Value1 | 1% | 1%
|  | Value2 | 0.063W | 0.063W
|  | Value_Code | 2k10 | 2k10
|  | ValueDisplayed | 2.10k | 2.10k
|  | VDC_V | 50V | 50V
R38 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | 0 | 0
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | CRCW04022K10FKED | CRCW04022K10FKED
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.vishay.com/docs/20035/dcrcwe3.pdf | http://www.vishay.com/docs/20035/dcrcwe3.pdf
|  | CompType | Resistor | Resistor
|  | Description | RES, 2.10 k, 1%, 0.063 W, AEC-Q200 Grade 0, 0402 | RES, 2.10 k, 1%, 0.063 W, AEC-Q200 Grade 0, 0402
|  | EIA_Code | E96 | E96
|  | Footprint | 0402S | 0402S
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Manufacturer | Vishay-Dale | Vishay-Dale
|  | MountType | SMT | SMT
|  | PackageReference | 0402 | 0402
|  | PartNumber | CRCW04022K10FKED | CRCW04022K10FKED
|  | Power_W | 63mW | 63mW
|  | Res_ohm | 2.1k | 2.1k
|  | RoHS | E | E
|  | SizeArea_mm2 | 0.5 | 0.5
|  | SizeX_mm | 1 | 1
|  | SizeY_mm | 0.5 | 0.5
|  | SizeZ_mm | 0.6 | 0.6
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Newark | Newark
|  | Supplier 3 | Mouser | Mouser
|  | Supplier Part Number 1 | 541-2.10KLCT-ND | 541-2.10KLCT-ND
|  | Supplier Part Number 2 | 52K6791 | 52K6791
|  | Supplier Part Number 3 | 71-CRCW0402-2.1K-E3 | 71-CRCW0402-2.1K-E3
|  | Technology | Thick Film | Thick Film
|  | TempCo | 100 ppm/C | 100 ppm/C
|  | Tolerance_% | 1% | 1%
|  | Value | 2.10k | 2.10k
|  | Value1 | 1% | 1%
|  | Value2 | 0.063W | 0.063W
|  | Value_Code | 2k10 | 2k10
|  | ValueDisplayed | 2.10k | 2.10k
|  | VDC_V | 50V | 50V
R39 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | 0 | 0
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | CRCW040227K4FKED | CRCW040227K4FKED
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.vishay.com/docs/20035/dcrcwe3.pdf | http://www.vishay.com/docs/20035/dcrcwe3.pdf
|  | CompType | Resistor | Resistor
|  | Description | RES, 27.4 k, 1%, 0.063 W, AEC-Q200 Grade 0, 0402 | RES, 27.4 k, 1%, 0.063 W, AEC-Q200 Grade 0, 0402
|  | EIA_Code | E96 | E96
|  | Footprint | 0402S | 0402S
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Manufacturer | Vishay-Dale | Vishay-Dale
|  | MountType | SMT | SMT
|  | PackageReference | 0402 | 0402
|  | PartNumber | CRCW040227K4FKED | CRCW040227K4FKED
|  | Power_W | 63mW | 63mW
|  | Res_ohm | 27.4k | 27.4k
|  | RoHS | E | E
|  | SizeArea_mm2 | 0.5 | 0.5
|  | SizeX_mm | 1 | 1
|  | SizeY_mm | 0.5 | 0.5
|  | SizeZ_mm | 0.6 | 0.6
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Newark | Newark
|  | Supplier 3 | Mouser | Mouser
|  | Supplier Part Number 1 | 541-27.4KLCT-ND | 541-27.4KLCT-ND
|  | Supplier Part Number 2 | 52K6909 | 52K6909
|  | Supplier Part Number 3 | 71-CRCW0402-27.4K-E3 | 71-CRCW0402-27.4K-E3
|  | Technology | Thick Film | Thick Film
|  | TempCo | 100 ppm/C | 100 ppm/C
|  | Tolerance_% | 1% | 1%
|  | Value | 27.4k | 27.4k
|  | Value1 | 1% | 1%
|  | Value2 | 0.063W | 0.063W
|  | Value_Code | 27k4 | 27k4
|  | ValueDisplayed | 27.4k | 27.4k
|  | VDC_V | 50V | 50V
R40 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | 0 | 0
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | CRCW04021K00FKED | CRCW04021K00FKED
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.vishay.com/docs/20035/dcrcwe3.pdf | http://www.vishay.com/docs/20035/dcrcwe3.pdf
|  | CompType | Resistor | Resistor
|  | Description | RES, 1.00 k, 1%, 0.063 W, AEC-Q200 Grade 0, 0402 | RES, 1.00 k, 1%, 0.063 W, AEC-Q200 Grade 0, 0402
|  | EIA_Code | E96 | E96
|  | Footprint | 0402S | 0402S
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Manufacturer | Vishay-Dale | Vishay-Dale
|  | MountType | SMT | SMT
|  | PackageReference | 0402 | 0402
|  | PartNumber | CRCW04021K00FKED | CRCW04021K00FKED
|  | Power_W | 63mW | 63mW
|  | Res_ohm | 1k | 1k
|  | RoHS | E | E
|  | SizeArea_mm2 | 0.5 | 0.5
|  | SizeX_mm | 1 | 1
|  | SizeY_mm | 0.5 | 0.5
|  | SizeZ_mm | 0.6 | 0.6
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Newark | Newark
|  | Supplier 3 | Mouser | Mouser
|  | Supplier Part Number 1 | 541-1.00KLCT-ND | 541-1.00KLCT-ND
|  | Supplier Part Number 2 | 52K6545 | 52K6545
|  | Supplier Part Number 3 | 71-CRCW0402-1.0K-E3 | 71-CRCW0402-1.0K-E3
|  | Technology | Thick Film | Thick Film
|  | TempCo | 100 ppm/C | 100 ppm/C
|  | Tolerance_% | 1% | 1%
|  | Value | 1.00k | 1.00k
|  | Value1 | 1% | 1%
|  | Value2 | 0.063W | 0.063W
|  | Value_Code | 1k00 | 1k00
|  | ValueDisplayed | 1.00k | 1.00k
|  | VDC_V | 50V | 50V
R41 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Grade | 0 | 0
|  | AEC Qualified | Y | Y
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | CRCW040210K0FKED | CRCW040210K0FKED
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.vishay.com/docs/20035/dcrcwe3.pdf | http://www.vishay.com/docs/20035/dcrcwe3.pdf
|  | CompType | Resistor | Resistor
|  | Description | RES, 10.0 k, 1%, 0.063 W, AEC-Q200 Grade 0, 0402 | RES, 10.0 k, 1%, 0.063 W, AEC-Q200 Grade 0, 0402
|  | EIA_Code | E96 | E96
|  | Footprint | 0402S | 0402S
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Manufacturer | Vishay-Dale | Vishay-Dale
|  | MountType | SMT | SMT
|  | PackageReference | 0402 | 0402
|  | PartNumber | CRCW040210K0FKED | CRCW040210K0FKED
|  | Power_W | 63mW | 63mW
|  | Res_ohm | 10k | 10k
|  | RoHS | E | E
|  | SizeArea_mm2 | 0.5 | 0.5
|  | SizeX_mm | 1 | 1
|  | SizeY_mm | 0.5 | 0.5
|  | SizeZ_mm | 0.6 | 0.6
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Newark | Newark
|  | Supplier 3 | Mouser | Mouser
|  | Supplier Part Number 1 | 541-10.0KLCT-ND | 541-10.0KLCT-ND
|  | Supplier Part Number 2 | 52K6595 | 52K6595
|  | Supplier Part Number 3 | 71-CRCW0402-10K-E3 | 71-CRCW0402-10K-E3
|  | Technology | Thick Film | Thick Film
|  | TempCo | 100 ppm/C | 100 ppm/C
|  | Tolerance_% | 1% | 1%
|  | Value | 10.0k | 10.0k
|  | Value1 | 1% | 1%
|  | Value2 | 0.063W | 0.063W
|  | Value_Code | 10k0 | 10k0
|  | ValueDisplayed | 10.0k | 10.0k
|  | VDC_V | 50V | 50V
RT1 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | NCP18WB473J03RB | NCP18WB473J03RB
|  | ComponentLink1Description | Datasheet link | Datasheet link
|  | ComponentLink1URL | http://www.murata.com/products/catalog/pdf/r44e.pdf | http://www.murata.com/products/catalog/pdf/r44e.pdf
|  | CompType | ThermistorNTC | ThermistorNTC
|  | Description | Thermistor NTC, 47k ohm, 5%, 0603 | Thermistor NTC, 47k ohm, 5%, 0603
|  | Footprint | 0603S | 0603S
|  | LatestRevisionDate | 09/03/2017 | 09/03/2017
|  | Manufacturer | MuRata | MuRata
|  | MountType | SMT | SMT
|  | PackageReference | 0603 | 0603
|  | PartNumber | NCP18WB473J03RB | NCP18WB473J03RB
|  | Power_W | 100mW | 100mW
|  | Published | 22/09/2009 | 22/09/2009
|  | Publisher | Texas Instruments | Texas Instruments
|  | RoHS | Y | Y
|  | Series | NCP18 | NCP18
|  | SizeArea_mm2 | 1.28 | 1.28
|  | SizeAreaWB_mm2 | 4.68 | 4.68
|  | SizeX_mm | 1.6 | 1.6
|  | SizeY_mm | 0.8 | 0.8
|  | SizeZ_mm | 1 | 1
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 |  |
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | 490-2428-1-ND | 490-2428-1-ND
|  | Supplier Part Number 2 |  |
|  | Supplier Part Number 3 |  |
|  | TaMax_C | 125°C | 125°C
|  | TaMin_C | -40°C | -40°C
|  | Tolerance_% | 5% | 5%
|  | U/M | EA | EA
|  | Value | 47k | 47k
|  | Vault Folder |  |
SH-J1 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Cert_CSA |  |
|  | Cert_CULUS |  |
|  | Cert_UL | Y | Y
|  | Cert_VDE |  |
|  | ClassName |  |
|  | Color | Black | Black
|  | Comment | SNT-100-BK-T-H | SNT-100-BK-T-H
|  | ComponentLink1Description | Datasheet URL | Datasheet URL
|  | ComponentLink1URL | http://suddendocs.samtec.com/prints/snt-100-xx-x-x-mkt.pdf | http://suddendocs.samtec.com/prints/snt-100-xx-x-x-mkt.pdf
|  | CompType | Shunt | Shunt
|  | ContactFinish | Tin | Tin
|  | Current_A | 4.3A | 4.3A
|  | Description | Shunt, 100mil, Tin plated, Black | Shunt, 100mil, Tin plated, Black
|  | Footprint | SNT-100-BK-x-H | SNT-100-BK-x-H
|  | Gender | Female | Female
|  | Green_EU RoHS | Passed | Passed
|  | Green_EU RoHS-2 | Passed | Passed
|  | Green_Lifecycle | Active | Active
|  | Green_REACh | Passed | Passed
|  | Manufacturer | Samtec | Samtec
|  | MountType | N/A | N/A
|  | Note |  |
|  | Orientation |  |
|  | PackageReference | Shunt Connector Black Open Top, 2x1 | Shunt Connector Black Open Top, 2x1
|  | PartNumber | SNT-100-BK-T-H | SNT-100-BK-T-H
|  | PinCount |  |
|  | Pitch_mm |  |
|  | RoHS | Y | Y
|  | Row_Count |  |
|  | RowSpacing_mm |  |
|  | Shrouded |  |
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Newark | Newark
|  | Supplier 3 | Farnell | Farnell
|  | Supplier Part Number 1 | SAM8972-ND | SAM8972-ND
|  | Supplier Part Number 2 | 95H6926 | 95H6926
|  | Supplier Part Number 3 | 1803187 | 1803187
|  | Voltage_V |  |
T1 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category |  |
|  | AEC Grade |  |
|  | AEC Qualified | No | No
|  | Comment | RLTI-1431 | RLTI-1431
|  | ComponentLink1Description |  |
|  | ComponentLink1URL |  |
|  | CompType |  |
|  | Datasheet Path | datasheets/Trans-RLTI-1431.pdf | datasheets/Trans-RLTI-1431.pdf
|  | DCR_ohm | 0.24 | 0.24
|  | Description | Transformer FLYBACK for UCC28781EVM-053 | Transformer FLYBACK for UCC28781EVM-053
|  | Footprint | FP-RLTI-1431_PTH8_1IN0_0IN91-MFG | FP-RLTI-1431_PTH8_1IN0_0IN91-MFG
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | helpURL | https://upverter.com/upn/revision/bb4accb8eb6b1c49/ | https://upverter.com/upn/revision/bb4accb8eb6b1c49/
|  | Ind_H | 160µH | 160µH
|  | Lead Free | Yes | Yes
|  | LeakageInd_H |  |
|  | Lp |  |
|  | Manufacturer | Renco | Renco
|  | MountType |  |
|  | Ns1toNp | 1:0.151 | 1:0.151
|  | Ns2toNp |  |
|  | Ns3toNp |  |
|  | Operating Temperature Range | to | to
|  | PackageReference | PTH8_1IN0_0IN91 | PTH8_1IN0_0IN91
|  | Part Number | RLTI-1431 | RLTI-1431
|  | PartNumber | RLTI-1431 | RLTI-1431
|  | RoHS | TRUE | TRUE
|  | Rsec1_ohm | 7m | 7m
|  | Rsec2_ohm |  |
|  | Rsec3_ohm |  |
|  | SizeArea_mm2 |  |
|  | SizeAreaWB_mm2 |  |
|  | SizeX_mm |  |
|  | SizeY_mm |  |
|  | SizeZ_mm | 0.66inch | 0.66inch
|  | Supplier 1 |  |
|  | Supplier 2 |  |
|  | Supplier Part Number 1 |  |
|  | Supplier Part Number 2 |  |
|  | Value |  |
|  | ValueDisplayed |  |
|  | Voltage_Isolation_Vrms | 3kV | 3kV
TP1 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Cert_CSA |  |
|  | Cert_CULUS |  |
|  | Cert_UL |  |
|  | Cert_VDE |  |
|  | ClassName |  |
|  | CNHeader | FALSE | FALSE
|  | Color | Black | Black
|  | Comment | LINE | LINE
|  | ComponentLink1Description | Datasheet URL | Datasheet URL
|  | ComponentLink1URL | http://www.keyelco.com/userAssets/file/M60-2p60.pdf | http://www.keyelco.com/userAssets/file/M60-2p60.pdf
|  | CompType | Test Point | Test Point
|  | ContactFinish | Silver | Silver
|  | CT | TRUE | TRUE
|  | Current_A |  |
|  | Description | Test Point, Multipurpose, Black, TH | Test Point, Multipurpose, Black, TH
|  | Footprint | Keystone5011 | Keystone5011
|  | Gender |  |
|  | Green_EU RoHS | Passed | Passed
|  | Green_EU RoHS-2 | Incomplete | Incomplete
|  | Green_Lifecycle | Active | Active
|  | Green_REACh | Passed | Passed
|  | LatestRevisionDate | 26/05/2017 | 26/05/2017
|  | Manufacturer | Keystone | Keystone
|  | MountType | TH | TH
|  | Note |  |
|  | Orientation |  |
|  | PackageReference | Black Multipurpose Testpoint | Black Multipurpose Testpoint
|  | PartNumber | 5011 | 5011
|  | PinCount |  |
|  | Pitch_mm |  |
|  | Publisher | Texas Instruments | Texas Instruments
|  | RoHS | Y | Y
|  | Row_Count |  |
|  | RowSpacing_mm |  |
|  | Shrouded |  |
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Mouser | Mouser
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | 36-5011-ND | 36-5011-ND
|  | Supplier Part Number 2 | 534-5011 | 534-5011
|  | Supplier Part Number 3 |  |
|  | Voltage_V |  |
TP2 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Cert_CSA |  |
|  | Cert_CULUS |  |
|  | Cert_UL |  |
|  | Cert_VDE |  |
|  | ClassName |  |
|  | CNHeader | FALSE | FALSE
|  | Color | White | White
|  | Comment | NEUTRAL | NEUTRAL
|  | ComponentLink1Description | Datasheet URL | Datasheet URL
|  | ComponentLink1URL | http://www.keyelco.com/userAssets/file/M60-2p60.pdf | http://www.keyelco.com/userAssets/file/M60-2p60.pdf
|  | CompType | Test Point | Test Point
|  | ContactFinish | Silver | Silver
|  | CT | TRUE | TRUE
|  | Current_A |  |
|  | Description | Test Point, Multipurpose, White, TH | Test Point, Multipurpose, White, TH
|  | Footprint | Keystone5012 | Keystone5012
|  | Gender |  |
|  | Green_EU RoHS | Passed | Passed
|  | Green_EU RoHS-2 | Incomplete | Incomplete
|  | Green_Lifecycle | Active | Active
|  | Green_REACh | Passed | Passed
|  | LatestRevisionDate | 26/05/2017 | 26/05/2017
|  | Manufacturer | Keystone | Keystone
|  | MountType | TH | TH
|  | Note |  |
|  | Orientation |  |
|  | PackageReference | White Multipurpose Testpoint | White Multipurpose Testpoint
|  | PartNumber | 5012 | 5012
|  | PinCount |  |
|  | Pitch_mm |  |
|  | Publisher | Texas Instruments | Texas Instruments
|  | RoHS | Y | Y
|  | Row_Count |  |
|  | RowSpacing_mm |  |
|  | Shrouded |  |
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Mouser | Mouser
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | 36-5012-ND | 36-5012-ND
|  | Supplier Part Number 2 | 534-5012 | 534-5012
|  | Supplier Part Number 3 |  |
|  | Voltage_V |  |
TP3 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Cert_CSA |  |
|  | Cert_CULUS |  |
|  | Cert_UL |  |
|  | Cert_VDE |  |
|  | ClassName |  |
|  | CNHeader | FALSE | FALSE
|  | Color | Black | Black
|  | Comment | GND_S | GND_S
|  | ComponentLink1Description | Datasheet URL | Datasheet URL
|  | ComponentLink1URL | http://www.keyelco.com/userAssets/file/M60-2p60.pdf | http://www.keyelco.com/userAssets/file/M60-2p60.pdf
|  | CompType | Test Point | Test Point
|  | ContactFinish | Silver | Silver
|  | CT | TRUE | TRUE
|  | Current_A |  |
|  | Description | Test Point, Multipurpose, Black, TH | Test Point, Multipurpose, Black, TH
|  | Footprint | Keystone5011 | Keystone5011
|  | Gender |  |
|  | Green_EU RoHS | Passed | Passed
|  | Green_EU RoHS-2 | Incomplete | Incomplete
|  | Green_Lifecycle | Active | Active
|  | Green_REACh | Passed | Passed
|  | LatestRevisionDate | 26/05/2017 | 26/05/2017
|  | Manufacturer | Keystone | Keystone
|  | MountType | TH | TH
|  | Note |  |
|  | Orientation |  |
|  | PackageReference | Black Multipurpose Testpoint | Black Multipurpose Testpoint
|  | PartNumber | 5011 | 5011
|  | PinCount |  |
|  | Pitch_mm |  |
|  | Publisher | Texas Instruments | Texas Instruments
|  | RoHS | Y | Y
|  | Row_Count |  |
|  | RowSpacing_mm |  |
|  | Shrouded |  |
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Mouser | Mouser
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | 36-5011-ND | 36-5011-ND
|  | Supplier Part Number 2 | 534-5011 | 534-5011
|  | Supplier Part Number 3 |  |
|  | Voltage_V |  |
TP4 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Cert_CSA |  |
|  | Cert_CULUS |  |
|  | Cert_UL |  |
|  | Cert_VDE |  |
|  | ClassName |  |
|  | CNHeader | FALSE | FALSE
|  | Color | White | White
|  | Comment | VOUT | VOUT
|  | ComponentLink1Description | Datasheet URL | Datasheet URL
|  | ComponentLink1URL | http://www.keyelco.com/userAssets/file/M60-2p60.pdf | http://www.keyelco.com/userAssets/file/M60-2p60.pdf
|  | CompType | Test Point | Test Point
|  | ContactFinish | Silver | Silver
|  | CT | TRUE | TRUE
|  | Current_A |  |
|  | Description | Test Point, Multipurpose, White, TH | Test Point, Multipurpose, White, TH
|  | Footprint | Keystone5012 | Keystone5012
|  | Gender |  |
|  | Green_EU RoHS | Passed | Passed
|  | Green_EU RoHS-2 | Incomplete | Incomplete
|  | Green_Lifecycle | Active | Active
|  | Green_REACh | Passed | Passed
|  | LatestRevisionDate | 26/05/2017 | 26/05/2017
|  | Manufacturer | Keystone | Keystone
|  | MountType | TH | TH
|  | Note |  |
|  | Orientation |  |
|  | PackageReference | White Multipurpose Testpoint | White Multipurpose Testpoint
|  | PartNumber | 5012 | 5012
|  | PinCount |  |
|  | Pitch_mm |  |
|  | Publisher | Texas Instruments | Texas Instruments
|  | RoHS | Y | Y
|  | Row_Count |  |
|  | RowSpacing_mm |  |
|  | Shrouded |  |
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Mouser | Mouser
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | 36-5012-ND | 36-5012-ND
|  | Supplier Part Number 2 | 534-5012 | 534-5012
|  | Supplier Part Number 3 |  |
|  | Voltage_V |  |
TP5 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Cert_CSA |  |
|  | Cert_CULUS |  |
|  | Cert_UL |  |
|  | Cert_VDE |  |
|  | ClassName |  |
|  | CNHeader | FALSE | FALSE
|  | Color | White | White
|  | Comment | VOUT_A | VOUT_A
|  | ComponentLink1Description | Datasheet URL | Datasheet URL
|  | ComponentLink1URL | http://www.keyelco.com/userAssets/file/M60-2p60.pdf | http://www.keyelco.com/userAssets/file/M60-2p60.pdf
|  | CompType | Test Point | Test Point
|  | ContactFinish | Silver | Silver
|  | CT | TRUE | TRUE
|  | Current_A |  |
|  | Description | Test Point, Multipurpose, White, TH | Test Point, Multipurpose, White, TH
|  | Footprint | Keystone5012 | Keystone5012
|  | Gender |  |
|  | Green_EU RoHS | Passed | Passed
|  | Green_EU RoHS-2 | Incomplete | Incomplete
|  | Green_Lifecycle | Active | Active
|  | Green_REACh | Passed | Passed
|  | LatestRevisionDate | 26/05/2017 | 26/05/2017
|  | Manufacturer | Keystone | Keystone
|  | MountType | TH | TH
|  | Note |  |
|  | Orientation |  |
|  | PackageReference | White Multipurpose Testpoint | White Multipurpose Testpoint
|  | PartNumber | 5012 | 5012
|  | PinCount |  |
|  | Pitch_mm |  |
|  | Publisher | Texas Instruments | Texas Instruments
|  | RoHS | Y | Y
|  | Row_Count |  |
|  | RowSpacing_mm |  |
|  | Shrouded |  |
|  | Supplier 1 | Digi-Key | Digi-Key
|  | Supplier 2 | Mouser | Mouser
|  | Supplier 3 |  |
|  | Supplier Part Number 1 | 36-5012-ND | 36-5012-ND
|  | Supplier Part Number 2 | 534-5012 | 534-5012
|  | Supplier Part Number 3 |  |
|  | Voltage_V |  |
U1 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Grade | Grade 1 | Grade 1
|  | AEC Qualified | Yes | Yes
|  | Comment | UCC28781QRTWRQ1 | UCC28781QRTWRQ1
|  | Datasheet Path | datasheets/IC-UCC28781QRTWRQ1.pdf | datasheets/IC-UCC28781QRTWRQ1.pdf
|  | Description | Zero-Voltage-Switching Flyback Controller with Dedicated Synchronous Rectifier Gate-Drive | Zero-Voltage-Switching Flyback Controller with Dedicated Synchronous Rectifier Gate-Drive
|  | Footprint | RTW0024B-MFG | RTW0024B-MFG
|  | helpURL | https://upverter.com/upn/revision/7acca52f8211efa0/ | https://upverter.com/upn/revision/7acca52f8211efa0/
|  | Lead Free | Yes | Yes
|  | Manufacturer | Texas Instruments | Texas Instruments
|  | Max Supply Voltage | 34V | 34V
|  | Min Supply Voltage | 14V | 14V
|  | Nominal Supply Current | 235-3000uA | 235-3000uA
|  | Number Of Outputs | 1 | 1
|  | Operating Temperature Range | -40°C to +125°C | -40°C to +125°C
|  | Output Type | Other | Other
|  | PackageReference | WQFN24 | WQFN24
|  | Part Number | UCC28781QRTWRQ1 | UCC28781QRTWRQ1
|  | PartNumber | UCC28781QRTWRQ1 | UCC28781QRTWRQ1
|  | RoHS | TRUE | TRUE
|  | SizeZ_mm | 0.8mm | 0.8mm
|  | Standoff Height | 0mm | 0mm
|  | Switching Frequency | 1.5kHz | 1.5kHz
|  | Switching Topology | Flyback | Flyback
|  | TaMax_C | +125°C | +125°C
|  | TaMin_C | -40°C | -40°C
|  | TJmax_C | +140°C | +140°C
U2 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | AEC Category | Q200 | Q200
|  | AEC Qualified | N | N
|  | Alternate Manufacturer | Texas Instruments | Texas Instruments
|  | Alternate PartNumber |  |
|  | Comment | UCC5304DWV | UCC5304DWV
|  | ComponentLink1Description | Datasheet Link | Datasheet Link
|  | ComponentLink1URL | http://www.ti.com/lit/ds/symlink/ucc5304.pdf | http://www.ti.com/lit/ds/symlink/ucc5304.pdf
|  | ComponentLink2Description | Product Folder | Product Folder
|  | ComponentLink2URL | http://www.ti.com/product/ucc5304 | http://www.ti.com/product/ucc5304
|  | ComponentLink3Description | Online Datasheet | Online Datasheet
|  | ComponentLink3URL | http://www.ti.com/product/ucc5304/datasheet | http://www.ti.com/product/ucc5304/datasheet
|  | CompType | IC | IC
|  | Description | 4-A/6-A, Single-Channel Reinforced Isolation Gate Driver with High Noise Immunity, DWV0008A (SOIC-8) | 4-A/6-A, Single-Channel Reinforced Isolation Gate Driver with High Noise Immunity, DWV0008A (SOIC-8)
|  | Footprint | DWV0008A | DWV0008A
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Manufacturer | Texas Instruments | Texas Instruments
|  | MountType | SMT | SMT
|  | Operating Temperature Range |  |
|  | PackageDescription | SOIC-8 | SOIC-8
|  | PackageReference | DWV0008A | DWV0008A
|  | PartNumber | UCC5304DWV | UCC5304DWV
|  | Rating |  |
|  | RoHS |  |
|  | SizeArea_mm2 | 67.275 | 67.275
|  | SizeAreaWB_mm2 | 105.975 | 105.975
|  | SizeX_mm | 11.5 | 11.5
|  | SizeY_mm | 5.85 | 5.85
|  | SizeZ_mm | 2.8 | 2.8
U3 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | Alternate Manufacturer | Texas Instruments | Texas Instruments
|  | Alternate PartNumber |  |
|  | Comment | ATL431AIDBZR | ATL431AIDBZR
|  | ComponentLink1Description | Datasheet Link | Datasheet Link
|  | ComponentLink1URL | http://www.ti.com/lit/ds/symlink/atl431.pdf | http://www.ti.com/lit/ds/symlink/atl431.pdf
|  | CompType | IC | IC
|  | Description | 2.5V Low Iq Adjustable Precision Shunt Regulator, DBZ0003A (SOT-23-3) | 2.5V Low Iq Adjustable Precision Shunt Regulator, DBZ0003A (SOT-23-3)
|  | Footprint | DBZ0003A_L | DBZ0003A_L
|  | Footprint Path 6 | C:\AltiumLibraries\Footprints\TI\.PcbLib | C:\AltiumLibraries\Footprints\TI\.PcbLib
|  | LatestRevisionDate | 2017-06-09 | 2017-06-09
|  | Manufacturer | Texas Instruments | Texas Instruments
|  | MountType | SMT | SMT
|  | PackageDescription | SOT-23-3 | SOT-23-3
|  | PackageReference | DBZ0003A | DBZ0003A
|  | PartNumber | ATL431AIDBZR | ATL431AIDBZR
|  | Publisher | Texas Instruments | Texas Instruments
|  | RoHS | Y | Y
|  | SizeArea_mm2 | 7.5 | 7.5
|  | SizeAreaWB_mm2 | 14.0 | 14.0
|  | SizeX_mm | 2.5 | 2.5
|  | SizeY_mm | 3.0 | 3.0
|  | SizeZ_mm | 1.12 | 1.12
|  | U/M | EA | EA
U4 | HVP053B_sheet1.schdoc |  | Fitted | Fitted
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | Comment | TLP383(GR-TPL,E | TLP383(GR-TPL,E
|  | ComponentLink1Description | Datasheet | Datasheet
|  | ComponentLink1URL | https://toshiba.semicon-storage.com/info/docget.jsp?did=28831&prodName=TLP383 | https://toshiba.semicon-storage.com/info/docget.jsp?did=28831&prodName=TLP383
|  | CompType |  |
|  | CTR (Max) | 300% | 300%
|  | CTR (Min) | 100% | 100%
|  | Description | Optoisolator Transistor Output 5000Vrms 1 Channel 6-SO | Optoisolator Transistor Output 5000Vrms 1 Channel 6-SO
|  | Footprint | FP-TLP383(GR-TPL,E_SO6-4-MFG | FP-TLP383(GR-TPL,E_SO6-4-MFG
|  | Green_EU RoHS |  |
|  | Green_EU RoHS-2 |  |
|  | Green_Lifecycle |  |
|  | Green_REACh |  |
|  | Manufacturer | Toshiba | Toshiba
|  | MountType |  |
|  | PackageReference | SO6-4 | SO6-4
|  | PartNumber | TLP383(GR-TPL,E | TLP383(GR-TPL,E
|  | RoHS | TRUE | TRUE
|  | SizeArea_mm2 |  |
|  | SizeAreaWB_mm2 |  |
|  | SizeX_mm |  |
|  | SizeY_mm |  |
|  | SizeZ_mm | 2.3mm | 2.3mm
|  | Supplier 1 |  |
|  | Supplier 2 |  |
|  | Supplier 3 |  |
|  | Supplier Part Number 1 |  |
|  | Supplier Part Number 2 |  |
|  | Supplier Part Number 3 |  |
|  | Symbol Name | SYM-TLP383(GR-TPL,E | SYM-TLP383(GR-TPL,E
|  | Voltage_Isolation_Vrms |  |
ZZ1 | HVP053B_Hardware.SchDoc |  | Fitted | Fitted
|  | ClassName | AssemblyNote | AssemblyNote
|  | Comment | These assemblies are ESD sensitive, ESD precautions shall be observed. | These assemblies are ESD sensitive, ESD precautions shall be observed.
|  | CompType | AssemblyNote | AssemblyNote
|  | Description | These assemblies are ESD sensitive, ESD precautions shall be observed. | These assemblies are ESD sensitive, ESD precautions shall be observed.
|  | Footprint | AssemblyNote | AssemblyNote
|  | Key | AssemblyNote | AssemblyNote
|  | LatestRevisionDate | 2017-08-10 | 2017-08-10
|  | Publisher | Texas Instruments | Texas Instruments
ZZ2 | HVP053B_Hardware.SchDoc |  | Fitted | Fitted
|  | ClassName | AssemblyNote | AssemblyNote
|  | Comment | These assemblies must be clean and free from flux and all contaminants. Use of no clean flux is not acceptable. | These assemblies must be clean and free from flux and all contaminants. Use of no clean flux is not acceptable.
|  | CompType | AssemblyNote | AssemblyNote
|  | Description | These assemblies must be clean and free from flux and all contaminants. Use of no clean flux is not acceptable. | These assemblies must be clean and free from flux and all contaminants. Use of no clean flux is not acceptable.
|  | Footprint | AssemblyNote | AssemblyNote
|  | Key | AssemblyNote | AssemblyNote
|  | LatestRevisionDate | 2017-08-10 | 2017-08-10
|  | Publisher | Texas Instruments | Texas Instruments
ZZ3 | HVP053B_Hardware.SchDoc |  | Fitted | Fitted
|  | ClassName | AssemblyNote | AssemblyNote
|  | Comment | These assemblies must comply with workmanship standards IPC-A-610 Class 2, unless otherwise specified. | These assemblies must comply with workmanship standards IPC-A-610 Class 2, unless otherwise specified.
|  | CompType | AssemblyNote | AssemblyNote
|  | Description | These assemblies must comply with workmanship standards IPC-A-610 Class 2, unless otherwise specified. | These assemblies must comply with workmanship standards IPC-A-610 Class 2, unless otherwise specified.
|  | Footprint | AssemblyNote | AssemblyNote
|  | Key | AssemblyNote | AssemblyNote
|  | LatestRevisionDate | 2017-08-10 | 2017-08-10
|  | Publisher | Texas Instruments | Texas Instruments
ZZ4 | HVP053B_Hardware.SchDoc |  | Fitted | Fitted
|  | Alternate Manufacturer |  |
|  | Alternate PartNumber |  |
|  | ClassName | AssemblyNote | AssemblyNote
|  | Comment | Default installation of XCD configuration jumper SH-J1 to be in "XCD Disabled" position on J5 (across pins 2-3). | Default installation of XCD configuration jumper SH-J1 to be in "XCD Disabled" position on J5 (across pins 2-3).
|  | ComponentLink1Description |  |
|  | ComponentLink1URL |  |
|  | CompType | AssemblyNote | AssemblyNote
|  | Description | This Assembly Note will show in the PcbDoc and associated outputs | This Assembly Note will show in the PcbDoc and associated outputs
|  | Footprint | AssemblyNote | AssemblyNote
|  | Key | AssemblyNote | AssemblyNote
|  | LatestRevisionDate | 2017-03-09 | 2017-03-09
|  | Manufacturer |  |
|  | MountType |  |
|  | Note |  |
|  | PackageReference |  |
|  | PartNumber |  |
|  | Publisher | Texas Instruments | Texas Instruments
|  | RoHS |  |
|  | Supplier 1 |  |
|  | Supplier 2 |  |
|  | Supplier 3 |  |
|  | Supplier Part Number 1 |  |
|  | Supplier Part Number 2 |  |
|  | Supplier Part Number 3 |  |
|  | Value |  |

Back to top