Error Report for  - Users\x0213103\AppData\Local\Temp\Pro94FB.tmp
9/22/2014 5:21:03 PM

Warning pad shape change for U4-1 from rounded 13.78mil,66.929mil to rectangular 13.78mil,53.15mil
Warning pad shape change for U4-6 from rounded 13.78mil,66.929mil to rectangular 13.78mil,53.15mil
Warning pad shape change for U4-14 from rounded 13.78mil,66.929mil to rectangular 13.78mil,53.15mil
Warning pad shape change for U4-10 from rounded 13.78mil,66.929mil to rectangular 13.78mil,53.15mil
Warning pad shape change for J1-2 from rounded 40mil,50mil to rounded 40mil,40mil
Warning pad shape change for J1-3 from rounded 40mil,50mil to rounded 40mil,40mil
Warning pad shape change for U4-8 from rounded 13.78mil,66.929mil to rectangular 13.78mil,53.15mil
Warning pad shape change for U2-11 from rounded 13.78mil,66.929mil to rectangular 13.78mil,53.15mil
Warning pad shape change for U2-6 from rounded 13.78mil,66.929mil to rectangular 13.78mil,53.15mil
Warning pad shape change for U4-2 from rounded 13.78mil,66.929mil to rectangular 13.78mil,53.15mil
Warning pad shape change for U4-9 from rounded 13.78mil,66.929mil to rectangular 13.78mil,53.15mil
Warning pad shape change for U2-7 from rounded 13.78mil,66.929mil to rectangular 13.78mil,53.15mil
Warning pad shape change for U2-10 from rounded 13.78mil,66.929mil to rectangular 13.78mil,53.15mil
Warning pad shape change for U2-1 from rounded 13.78mil,66.929mil to rectangular 13.78mil,53.15mil
Warning pad shape change for U4-13 from rounded 13.78mil,66.929mil to rectangular 13.78mil,53.15mil
Warning pad shape change for U2-2 from rounded 13.78mil,66.929mil to rectangular 13.78mil,53.15mil
Warning pad shape change for U2-3 from rounded 13.78mil,66.929mil to rectangular 13.78mil,53.15mil
Warning pad shape change for U2-5 from rounded 13.78mil,66.929mil to rectangular 13.78mil,53.15mil
Warning pad shape change for U2-13 from rounded 13.78mil,66.929mil to rectangular 13.78mil,53.15mil
Warning pad shape change for U2-14 from rounded 13.78mil,66.929mil to rectangular 13.78mil,53.15mil
Warning pad shape change for U4-3 from rounded 13.78mil,66.929mil to rectangular 13.78mil,53.15mil
Warning pad shape change for U4-5 from rounded 13.78mil,66.929mil to rectangular 13.78mil,53.15mil
Warning pad shape change for U2-12 from rounded 13.78mil,66.929mil to rectangular 13.78mil,53.15mil
Warning pad shape change for U2-8 from rounded 13.78mil,66.929mil to rectangular 13.78mil,53.15mil
Warning pad shape change for U2-9 from rounded 13.78mil,66.929mil to rectangular 13.78mil,53.15mil
Warning pad shape change for U4-4 from rounded 13.78mil,66.929mil to rectangular 13.78mil,53.15mil
Warning pad shape change for U4-11 from rounded 13.78mil,66.929mil to rectangular 13.78mil,53.15mil
Warning pad shape change for J2-2 from rounded 40mil,50mil to rounded 40mil,40mil
Warning pad shape change for U4-12 from rounded 13.78mil,66.929mil to rectangular 13.78mil,53.15mil
Warning pad shape change for U2-4 from rounded 13.78mil,66.929mil to rectangular 13.78mil,53.15mil
Warning pad shape change for U4-7 from rounded 13.78mil,66.929mil to rectangular 13.78mil,53.15mil
Warning pad shape change for J2-3 from rounded 40mil,50mil to rounded 40mil,40mil
