Field=Fitted~String~Fitted~100|Field=Description~String~Description~100|Field=Designator~String~Designator~100|Field=PartNumber~String~PartNumber~100|Field=Quantity~Integer~Quantity~100|Field=Manufacturer~String~Manufacturer~100|Field=Alternate Manufacturer~String~Alternate Manufacturer~100|Field=Alternate PartNumber~String~Alternate PartNumber~100|Field=PackageReference~String~PackageReference~100|Field=Value~String~Value~100|ReportField=Currency~USD|ReportField=ProductionQuantity~100|ReportField=ProjectFileName~TIDA-00316.PrjPcb|ReportField=ProjectFullPath~C:\Users\Public\Documents\Altium\AD\Examples\2015-projects\TIDA-00316\8-5-2015\Final _database_TIDA-00316\TIDA-00316.PrjPcb|ReportField=Title~BOM For Variant [001] of Project [TIDA-00316.PrjPcb] (No PCB Document Selected)|ReportField=TotalQuantity~189|ReportField=ReportTime~10:18:59 AM|ReportField=ReportDate~5/14/2015|ReportField=ReportDateTime~5/14/2015 10:18:59 AM|ReportField=OutputName~BOM|ReportField=OutputType~BOM_PartType|ReportField=GeneratorName~BOM|ReportField=GeneratorDescription~Bill of Materials|ReportField=VariantName~001|ReportField=CopyrightYear~2015|ReportField=EVM_Orderable~N/A|ReportField=PCB_Layout~Avinash N|ReportField=PCB_Rev~E1|ReportField=PRJ_Customer~Public Release|ReportField=PRJ_Engineer~Sanjay Pithadia|ReportField=PRJ_Number~TIDA-00316|ReportField=PRJ_Title~Motor Current Measurement using Hall Sensors|ReportField=SCH_Rev~E1|ReportField=TechSupport~http://www.ti.com/support|ReportField=TID~ChangeMe!|ReportField=Address1~Not shown in title block|ReportField=Address2~Not shown in title block|ReportField=Address3~Not shown in title block|ReportField=Address4~Not shown in title block|ReportField=Application_BuildNumber~|ReportField=ApprovedBy~Not shown in title block|ReportField=Author~Not shown in title block|ReportField=CheckedBy~Not shown in title block|ReportField=CompanyName~Not shown in title block|ReportField=ConfigurationParameters~|ReportField=ConfiguratorName~|ReportField=CurrentDate~5/14/2015|ReportField=CurrentTime~10:17:33 AM|ReportField=Date~Not shown in title block|ReportField=DocumentFullPathAndName~C:\Users\Public\Documents\Altium\AD\Examples\2015-projects\TIDA-00316\8-5-2015\Final _database_TIDA-00316\SH01_CoverSheet.SchDoc|ReportField=DocumentName~SH01_CoverSheet.SchDoc|ReportField=DocumentNumber~1|ReportField=DrawnBy~Sanjay Pithadia|ReportField=Engineer~Sanjay Pithadia|ReportField=ImagePath~Not shown in title block|ReportField=IsUserConfigurable~|ReportField=ModifiedDate~5/14/2015|ReportField=Organization~Not shown in title block|ReportField=PageSetup~Record=PageOptions|CenterHorizontal=True|CenterVertical=True|PrintScale=1.00|XCorrection=1.00|YCorrection=1.00|PrintKind=0|BorderSize=5000000|LeftOffset=0|BottomOffset=0|Orientation=2|PaperLength=1000|PaperWidth=1000|Scale=100|PaperSource=15|PrintQuality=600|MediaType=1|DitherType=10|PaperKind=Letter|PrintScaleMode=1|ReportField=ProjectName~TIDA-00316.PrjPcb|ReportField=Revision~Use project parameter SCH_Rev|ReportField=Rule~|ReportField=SheetNumber~1|ReportField=SheetTotal~6|ReportField=Time~Not shown in title block|ReportField=Title~Block Diagram|ReportField=VersionControl_RevNumber~|ReportField=DataSourceFileName~TIDA-00316.PrjPcb|ReportField=DataSourceFullPath~C:\Users\Public\Documents\Altium\AD\Examples\2015-projects\TIDA-00316\8-5-2015\Final _database_TIDA-00316\TIDA-00316.PrjPcb
Fitted|Printed Circuit Board|!PCB1|TIDA-00316|1|Any|-|-||
Fitted|CAP, CERM, 10 µF, 35 V, +/- 20%, X7R, 1206_190|C1|C3216X7R1V106M160AC|1|TDK|||1206_190|10uF
Fitted|CAP, CERM, 3300 pF, 50 V, +/- 10%, X7R, 0805|C2|C0805C332K5RACTU|1|Kemet|||0805|3300pF
Fitted|CAP, CERM, 100 pF, 100 V, +/- 5%, C0G/NP0, 0603|C3, C4, C5, C10, C11, C23, C27, C28|C1608C0G2A101J|8|TDK|||0603|100pF
Fitted|CAP, CERM, 10 µF, 25 V, +/- 10%, X5R, 0805_140|C6, C8, C20, C21, C29, C36, C38, C54, C56|GRM21BR61E106KA73L|9|MuRata|||0805_140|10uF
Fitted|CAP, CERM, 0.1 µF, 50 V, +/- 10%, X7R, 0603|C7, C13, C18, C22, C30, C31, C32, C33, C34, C35, C37, C53, C55|GRM188R71H104KA93D|13|MuRata|||0603|0.1uF
Fitted|CAP, CERM, 22 µF, 16 V, +/- 10%, X5R, 0805|C9|C2012X5R1C226K125AC|1|TDK|||0805|22uF
Fitted|CAP, CERM, 2700 pF, 50 V, +/- 5%, C0G/NP0, 0603|C14|C1608C0G1H272J|1|TDK|||0603|2700pF
Fitted|CAP, CERM, 0.01 µF, 25 V, +/- 5%, C0G/NP0, 0603|C15, C16, C58, C59|C1608C0G1E103J|4|TDK|||0603|0.01uF
Fitted|CAP, CERM, 1uF, 10V, +/-10%, X7R, 0805|C17, C24, C25, C47, C48, C49, C50, C51, C52|C0805C105K8RACTU|9|Kemet|||0805|1uF
Fitted|CAP, CERM, 470 pF, 50 V, +/- 5%, C0G/NP0, 0603|C19|06035A471JAT2A|1|AVX|||0603|470pF
Fitted|CAP, CERM, 200 pF, 100 V, +/- 5%, C0G/NP0, 0603|C26, C57|GRM1885C2A201JA01D|2|MuRata|||0603|200pF
Fitted|CAP, CERM, 4.7 µF, 10 V, +/- 10%, X5R, 0603|C42, C43|0603ZD475KAT2A|2|AVX|||0603|4.7uF
Fitted|CAP, CERM, 330 pF, 50 V, +/- 1%, C0G/NP0, 0603|C44, C45, C46, C61|C1608C0G1H331F080AA|4|TDK|||0603|330pF
Fitted|CAP, CERM, 0.01 µF, 50 V, +/- 5%, X7R, 0402|C60|C0402C103J5RACTU|1|Kemet|||0402|0.01uF
Fitted|Diode, Schottky, 40 V, 0.015 A, SOD-123|D1, D2, D5, D6, D7, D8, D9|SD101CW-7-F|7|Diodes Inc.|||SOD-123|40V
Fitted|Diode, Schottky, 60V, 1A, SMA|D3, D4|MBRA160T3G|2|ON Semiconductor|||SMA|60V
Fitted|Diode, Zener, 3.6V, 500mW, SOD-123|D10, D11, D12, D13|MMSZ5227B-7-F|4|Diodes Inc.|||SOD-123|3.6V
Fitted|Machine Screw, Round, #4-40 x 1/4, Nylon, Philips panhead|H1, H2, H3, H4|NY PMS 440 0025 PH|4|B&F Fastener Supply|-|-|Screw|
Fitted|Standoff, Hex, 0.5"L #4-40 Nylon|H9, H10, H11, H12|1902C|4|Keystone|-|-|Standoff|
Fitted|Conn Term Block, 2POS, 5.08mm, TH|J1|1715721|1|Phoenix Contact|||2POS Terminal Block|2x1
Fitted|Terminal Block, 3.5 mm, 2x1, Tin, TH|J2|39357-0002|1|Molex|||Terminal Block, 3.5 mm, 2x1, TH|
Fitted|Terminal Block, 3.5 mm, 3x1, Tin, TH|J3|39357-0003|1|Molex|||Terminal Block, 3.5 mm, 3x1, TH|
Fitted|Header, 2.54 mm, 6x1, Gold, TH|J4, J12|61300611121|2|Wurth Elektronik|||Header, 2.54mm, 6x1, TH|
Fitted|Connector, TH, SMA|J5, J6, J7, J8|142-0701-201|4|Emerson Network Power|||SMA|
Fitted|Header, 100mil, 2x1, Tin, TH|J9|90120-0122|1|Molex|||Header 2x1|
Fitted|CONN HIGH SPD CARD EDGE 60 POS|J10|SPD08-060-RB-TR|1|3M|-|-|28.6x7mm|
Fitted|CONN HIGH SPD CARD EDGE 120 POS|J11|SPD08-120-L-RB|1|3M|||7x56mm|SPD08-120-L-RB
Fitted|Inductor, Shielded, Composite, 2.2 µH, 3.7 A, 0.02 ohm, SMD|L1|XFL4020-222MEB|1|Coilcraft|||4x2x4mm|2.2uH
Fitted|LED SmartLED Green 570NM|LD1, LD2|LG L29K-G2J1-24-Z|2|OSRAM|LED||0603|Green
Fitted|RES, 0, 5%, 0.1 W, 0603|R2|CRCW06030000Z0EA|1|Vishay-Dale|||0603|0
Fitted|RES, 0 ohm, 5%, 0.1W, 0603|R3, R4, R7, R9, R25, R38, R39, R41, R46, R47, R50, R51, R53, R60, R62, R63, R64, R65, R66, R67, R68, R69, R70, R71, R72, R73, R74, R75, R76, R77, R78, R79, R80, R81, R82, R83, R84, R92|CRCW06030000Z0EA|38|Vishay-Dale|||0603|0
Fitted|RES, 154 k, 1%, 0.1 W, 0603|R5|CRCW0603154KFKEA|1|Vishay-Dale|||0603|154k
Fitted|RES, 42.2, 1%, 0.125 W, 0805|R6|CRCW080542R2FKEA|1|Vishay-Dale|||0805|42.2
Fitted|RES, 1.00 k, 1%, 0.1 W, 0603|R8, R55, R93|CRCW06031K00FKEA|3|Vishay-Dale|||0603|1.00k
Fitted|RES, 2.00 k, 1%, 0.1 W, 0603|R10, R11, R12, R14, R15, R16, R17, R18, R19, R21, R23, R91|RC0603FR-072KL|12|Yageo America|||0603|2.00k
Fitted|RES, 1.0 M, 5%, 0.1 W, 0603|R13|CRCW06031M00JNEA|1|Vishay-Dale|||0603|1.0Meg
Fitted|RES, 673, 0.1%, 0.1 W, 0603|R22, R34|RT0603BRD07673RL|2|Yageo America|||0603|673
Fitted|RES, 5.23 k, 1%, 0.1 W, 0603|R26|CRCW06035K23FKEA|1|Vishay-Dale|||0603|5.23k
Fitted|RES, 2.00 k, 1%, 0.1 W, 0603|R28, R29|CRCW06032K00FKEA|2|Vishay-Dale|||0603|2.00k
Fitted|RES, 18.2 k, 1%, 0.1 W, 0603|R30, R32|CRCW060318K2FKEA|2|Vishay-Dale|||0603|18.2k
Fitted|RES, 2.00 k, 0.1%, 0.1 W, 0603|R31, R33, R37, R40|RG1608P-202-B-T5|4|Susumu Co Ltd|||0603|2.00k
Fitted|RES, 1.15 k, 1%, 0.1 W, 0603|R35|CRCW06031K15FKEA|1|Vishay-Dale|||0603|1.15k
Fitted|RES, 9.76 k, 1%, 0.1 W, 0603|R42|CRCW06039K76FKEA|1|Vishay-Dale|||0603|9.76k
Fitted|RES, 43.2 k, 1%, 0.1 W, 0603|R43, R45|CRCW060343K2FKEA|2|Vishay-Dale|||0603|43.2k
Fitted|RES, 20.0 k, 1%, 0.1 W, 0603|R44|RC0603FR-0720KL|1|Yageo America|||0603|20.0k
Fitted|RES, 24.9, 1%, 0.1 W, 0603|R48, R49|CRCW060324R9FKEA|2|Vishay-Dale|||0603|24.9
Fitted|RES, 10.0 k, 1%, 0.1 W, 0603|R52|CRCW060310K0FKEA|1|Vishay-Dale|||0603|10.0k
Fitted|RES, 2.49 k, 1%, 0.1 W, 0603|R56|CRCW06032K49FKEA|1|Vishay-Dale|||0603|2.49k
Fitted|RES, 22, 5%, 0.1 W, 0603|R57, R58, R59, R61|CRCW060322R0JNEA|4|Vishay-Dale|||0603|22
Fitted|RES, 0, 5%, 0.125 W, 0805|R85, R90|CRCW08050000Z0EA|2|Vishay-Dale|||0805|0
Fitted|Buck Step Down Regulator with 3 to 17 V Input and 0.9 to 6 V Output, -40 to 85 degC, 16-Pin QFN (RGT), Green (RoHS & no Sb/Br)|U1|TPS62150RGTT|1|Texas Instruments|None|Equivalent|RGT0016C|
Fitted|Current Transducer, 25A, TH|U2|LAH 25-NP|1|LEM|||14.93x33.3mm|
Fitted|20 MHz, Low Noise, RRIO, CMOS Operational Amplifier with Shutdown, 1.8 to 5.5 V, -40 to 125 degC, 5-pin SOT23 (DBV0005A), Green (RoHS & no Sb/Br)|U3|OPA322AIDBVR|1|Texas Instruments|None|Equivalent|DBV0005A|
Fitted|Single Output High PSRR LDO, 200 mA, Adjustable -1.18 to -33 V Output, -3 to -36 V Input, with Ultra-Low Noise, 8-pin MSOP (DGN), -40 to 125 degC, Green (RoHS & no Sb/Br)|U4|TPS7A3001DGNR|1|Texas Instruments|None|Equivalent|DGN0008D|
Fitted|Single Output High PSRR LDO, 150 mA, Adjustable 1.2 to 33 V Output, 3 to 36 V Input, with Ultra-Low Noise, 8-pin MSOP (DGN), -40 to 125 degC, Green (RoHS & no Sb/Br)|U5|TPS7A4901DGNR|1|Texas Instruments|None|Equivalent|DGN0008D|
Fitted|High Voltage, Rail-to-Rail Input/Output, Precision Operational Amplifiers, e-trim™ Series, D0008A|U6|OPA2192IDR|1|Texas Instruments|Texas Instruments|OPA2192ID|D0008A|
Fitted|20 MHz, Low Noise, RRIO, CMOS Operational Amplifier, 1.8 to 5.5 V, -40 to 125 degC, 8-pin SOIC (D0008A), Green (RoHS & no Sb/Br)|U7|OPA2322AIDR|1|Texas Instruments|None|Equivalent|D0008A|
Fitted|Ultra Low Power, Rail-to-Rail Output, Fully-Differential Amplifier, DGK0008A|U8|THS4531AIDGK|1|Texas Instruments|Texas Instruments||DGK0008A|
Fitted|Dual Comparator, D0008A|U9|LM393AD|1|Texas Instruments|Texas Instruments||D0008A|
Fitted|Micropower 250 mA Low-Noise Ultra Low-Dropout Regulator, 6-pin LLP, Pb-Free|U10|LP2992AILD-5.0/NOPB|1|Texas Instruments|||LDE06A|
Fitted|Low-Drift, Low-Power, Dual-Output, VREF and VREF / 2 Voltage References, DDC0005A|U11|REF2033AIDDCR|1|Texas Instruments|Texas Instruments|REF2033AIDDCT|DDC0005A|
Fitted|DUAL OUTPUT VOLTAGE REFERENCE 2.5V, DBV0005A|U12|REF2025DBV|1|Texas Instruments|None||DBV0005A|
Not Fitted|CAP, CERM, 22 µF, 16 V, +/- 10%, X5R, 0805|C12|C2012X5R1C226K125AC|0|TDK|||0805|22uF
Not Fitted|CAP, CERM, 330 pF, 50 V, +/- 1%, C0G/NP0, 0603|C39, C40, C41|C1608C0G1H331F080AA|0|TDK|||0603|330pF
Not Fitted|Fiducial mark.  There is nothing to buy or mount.|FID1, FID2, FID3, FID4, FID5, FID6|N/A|0|N/A|||Fiducial|
Not Fitted|RES, 0, 5%, 0.1 W, 0603|R1|CRCW06030000Z0EA|0|Vishay-Dale|||0603|0
Not Fitted|RES, 2.00 k, 1%, 0.1 W, 0603|R20, R27|RC0603FR-072KL|0|Yageo America|||0603|2.00k
Not Fitted|RES, 0 ohm, 5%, 0.1W, 0603|R24, R36, R54|CRCW06030000Z0EA|0|Vishay-Dale|||0603|0
Not Fitted|RES, 0, 5%, 0.125 W, 0805|R86, R87, R88, R89|CRCW08050000Z0EA|0|Vishay-Dale|||0805|0
