
                              SILKSCREEN GENERATOR
                              --------------------

                       04:54 PM Tuesday, February 03, 2015
         Job Name: C:\TempLayouts\PP-CMBEVM_RevF\PCB\PP-CMBEVM_RevF.pcb


    Silkscreen Side To Process           : BOTH

    Process All Cell Types               : YES

    Top Silkscreen For Selected Cells    : Silkscreen Reference Designator Top
                                         : Silkscreen Outline Top

    Bottom Silkscreen For Selected Cells : Silkscreen Reference Designator Bottom
                                         : Silkscreen Outline Bottom

    Break Silkscreen Using               : Conductive Pads

    Break Graphics Pad Clearance         : 0.025mm

    Break Graphics Via Clearance         : 0.025mm

    Break Text Pad Clearance             : 0.025mm

    Break Text Via Clearance             : 0.025mm

    Broken Graphics Line Width           : 0.075mm

    Broken Text Line Width               : 0.1mm
    


    TOP Silkscreen Data Created Successfully (2245 Geometries).


    BOTTOM Silkscreen Data Created Successfully (1681 Geometries).