
                             XE Neutral File Export
                             ----------------------

                       04:55 PM Tuesday, February 03, 2015
         Job Name: C:\TempLayouts\PP-CMBEVM_RevF\PCB\PP-CMBEVM_RevF.pcb


Output: C:\TempLayouts\PP-CMBEVM_RevE\PCB\Output\XEneutralFile.txt
Processing Board
Unable to obtain hole information from board
Unable to obtain hole information from board
Unable to obtain hole information from board
Unable to obtain hole information from board
Unable to obtain hole information from board
Unable to obtain hole information from board
Processing Nets

Processing Geometries
DIODE_SMA
    Placement outline for mount side has been changed to top layer
HDR_1x2-2mm
    Placement outline for mount side has been changed to top layer
HDR_2X2
    Placement outline for mount side has been changed to top layer
HDR_2x5
    Placement outline for mount side has been changed to top layer
HTQFP64-PAP
    Placement outline for mount side has been changed to top layer
HTSSOP56-DCA_0.75-Vias
    Placement outline for mount side has been changed to top layer
IND_SDR0403
    Placement outline for mount side has been changed to top layer
IND_XAL-40xx
    Placement outline for mount side has been changed to top layer
LED0402
    Placement outline for mount side has been changed to top layer
LED0603
    Placement outline for mount side has been changed to top layer
LQFP48-PT
    Placement outline for mount side has been changed to top layer
MicroSD_3M-2900
    Placement outline for mount side has been changed to top layer
MiniAudio_SJ-3523-SMT
    Placement outline for mount side has been changed to top layer
OptoReceiver_PLR135
    Placement outline for mount side has been changed to top layer
OptoTransmitter_PLT133
    Placement outline for mount side has been changed to top layer
QFN12-RUE
    Placement outline for mount side has been changed to top layer
QFN32-RGJ
    Placement outline for mount side has been changed to top layer
QFN48-RGZ_VIA25
    Placement outline for mount side has been changed to top layer
    Placement outline for mount side has been changed to top layer
    More than one height attribute has been found for this geometry.  Only the first one has been used.
QSS-050-D-A
    Placement outline for mount side has been changed to top layer
RCA_PJRAN1X
    Unable to get pad information for pin 1 cell 'RCA_PJRAN1X'
    Unable to get pad information for pin 2 cell 'RCA_PJRAN1X'
    Unable to get pad information for pin 3 cell 'RCA_PJRAN1X'
    Placement outline for mount side has been changed to top layer
Unable to obtain hole information from board
Unable to obtain hole information from board
RC0402
    Placement outline for mount side has been changed to top layer
RC0402_Reflow
    Placement outline for mount side has been changed to top layer
RC0603
    Placement outline for mount side has been changed to top layer
RC0805_ReFlow
    Placement outline for mount side has been changed to top layer
RC1210
    Placement outline for mount side has been changed to top layer
SCKT-HDR_1x4-RA_50LS
    Placement outline for mount side has been changed to top layer
SOD-128_M-FLAT
    Placement outline for mount side has been changed to top layer
SOP8-D
    Placement outline for mount side has been changed to top layer
SOP14-D
    Placement outline for mount side has been changed to top layer
SOT23-DBV3
    Placement outline for mount side has been changed to top layer
SOT23-DBV5
    Placement outline for mount side has been changed to top layer
SOT553-DRL5
    Placement outline for mount side has been changed to top layer
SOT553-DRL6
    Placement outline for mount side has been changed to top layer
SO8-DDA
    Placement outline for mount side has been changed to top layer
StandoffPad_5.5x3.25mm_M3
    Placement outline for mount side has been changed to top layer
StandoffPad_6.5x3.25mm_M3
    Placement outline for mount side has been changed to top layer
SW_TL015
    Placement outline for mount side has been changed to top layer
Testpoint_TH_Round_30x15
    Placement outline for mount side has been changed to top layer
TP-040
    Placement outline for mount side has been changed to top layer
TQFP48-PFB
    Placement outline for mount side has been changed to top layer
TSSOP8-ST_4.4mm
    Placement outline for mount side has been changed to top layer
UDFN8-8MA1
    Placement outline for mount side has been changed to top layer
UQFN16-RSV
    Placement outline for mount side has been changed to top layer
USB_MICRO-B_47346-0001
    Placement outline for mount side has been changed to top layer
VSSOP8-DCU
    Placement outline for mount side has been changed to top layer
WCSP81-YZF
    Placement outline for mount side has been changed to top layer
WSON6-NGG0006A
    Placement outline for mount side has been changed to top layer
WSON10-NGZ
    Placement outline for mount side has been changed to top layer
XTAL_ABM10_2.5x2.0mm
    Placement outline for mount side has been changed to top layer
XTAL_ABRACOM-ABM8G
    Placement outline for mount side has been changed to top layer
XTAL_CTS-625
    Placement outline for mount side has been changed to top layer
Processing Components

Processing Holes
Unable to obtain hole information from board
Unable to obtain hole information from board

Processing Pads
BGA Pad 10x6
Gnd Via 0.3mm
Pad Rectangle 12x24
Pad Rectangle 12x40
Pad Rectangle 15x60
Pad Rectangle 30x22
Pad Rectangle 40x44
Pad Rectangle 45x22
Pad Rectangle 50x60
Pad Rectangle 55x20
Pad Rectangle 60x12
Pad Rectangle 60x110
Pad Rectangle 80x30
Pad Rectangle 100x80
Pad Square 32
PowerPad Via 0.3mm
Round 6.5x3.25mm
Round 30x15
Round 40x25 SocketPin
Round 56x32
Round 65x35
Round 65x40
Round 75x35
Round 75x45
Slot 1.0x3.5mm  2.0x4.5mm Pad
    Converting radius corner rectangle pad to rectangle
    Converting radius corner rectangle pad to rectangle
    Converting radius corner rectangle pad to rectangle
Slot 1.3x2.5mm  2.3x3.5mm Pad
    Converting radius corner rectangle pad to rectangle
    Converting radius corner rectangle pad to rectangle
    Converting radius corner rectangle pad to rectangle
SMD Finger 0.28x0.85mm
    Converting round finger pad to rectangle
    Converting round finger pad to rectangle
SMD Finger 0.28x1.75mm
    Converting round finger pad to rectangle
    Converting round finger pad to rectangle
SMD Oblong 0.45x1.10mm
    Converting oblong pad to rectangle
    Converting oblong pad to rectangle
SMD PowerPad 1.6x2.1mm
SMD PowerPad 2.0x2.2mm
SMD PowerPad 3.15mm
SMD PowerPad 3.61x6.35mm
SMD PowerPad 4.51x5.36mm
SMD PowerPad 6.5mm
SMD Rectangle 0.2x0.6mm RUE12
SMD Rectangle 0.3x1.6mm PAP
SMD Rectangle 0.3x1.6mm PWP
SMD Rectangle 0.5x0.6mm
SMD Rectangle 0.6x0.9mm
SMD Rectangle 0.6x1.55mm
SMD Rectangle 0.7x1.3mm
SMD Rectangle 0.8x1.5mm
SMD Rectangle 0.9x0.8mm
SMD Rectangle 0.20x0.65mm
SMD Rectangle 0.20x0.75mm
SMD Rectangle 0.25x0.5mm
SMD Rectangle 0.35x0.6mm
SMD Rectangle 1.0x0.85mm
SMD Rectangle 1.0x3.7mm
SMD Rectangle 1.2x1.9mm
SMD Rectangle 1.4x1.2mm
SMD Rectangle 1.4x1.9mm
SMD Rectangle 1.4x2.1mm
SMD Rectangle 1.5x2.1mm
SMD Rectangle 1.8x1.4mm
SMD Rectangle 1.8x4.5mm
SMD Rectangle 2.2x2.8mm
SMD Rectangle 2.4x1.9mm
SMD Rectangle 2x2.5mm
SMD Rectangle 3.4x4.0mm
SMD Rectangle 16x90
SMD Rectangle 20x22
SMD Rectangle 40x35
SMD Rectangle 110x17
SMD Rectangle 185x17
SMD Round 10
SMD Square 2.8mm
Square 56x32
Square 65x40
StandoffPad 5.5x3.25mm
Template Via 20
Via 25x10
Via20x10
Via35x20
Via40x20
Via50x25
Via60x36
VIia30x15
 Processing Test Points

The following geometries have been renamed to conform to legal BoardStation names
	"SMD Rectangle 16x90"  ->  SMD_Rectangle_16x90
	"SMD Rectangle 40x35"  ->  SMD_Rectangle_40x35
	"SMD Rectangle 20x22"  ->  SMD_Rectangle_20x22
	"SMD Round 10"  ->  SMD_Round_10
	"BGA Pad 10x6"  ->  BGA_Pad_10x6
	"Pad Rectangle 45x22"  ->  Pad_Rectangle_45x22
	"Via 25x10"  ->  Via_25x10
	"Template Via 20"  ->  Template_Via_20
	"Pad Rectangle 12x24"  ->  Pad_Rectangle_12x24
	"Pad Rectangle 30x22"  ->  Pad_Rectangle_30x22
	"SMD Rectangle 0.20x0.65mm"  ->  SMD_Rectangle_0.20x0.65mm
	"Pad Rectangle 60x12"  ->  Pad_Rectangle_60x12
	"Pad Rectangle 12x40"  ->  Pad_Rectangle_12x40
	"Round 65x35"  ->  Round_65x35
	"Pad Rectangle 80x30"  ->  Pad_Rectangle_80x30
	"SMD Finger 0.28x0.85mm"  ->  SMD_Finger_0.28x0.85mm
	"SMD Rectangle 0.3x1.6mm PWP"  ->  SMD_Rectangle_0.3x1.6mm_PWP
	"SMD Rectangle 0.8x1.5mm"  ->  SMD_Rectangle_0.8x1.5mm
	"SMD Rectangle 0.3x1.6mm PAP"  ->  SMD_Rectangle_0.3x1.6mm_PAP
	"SMD Finger 0.28x1.75mm"  ->  SMD_Finger_0.28x1.75mm
	"SMD Rectangle 0.2x0.6mm RUE12"  ->  SMD_Rectangle_0.2x0.6mm_RUE12
	"Pad Rectangle 15x60"  ->  Pad_Rectangle_15x60
	"SMD Rectangle 0.5x0.6mm"  ->  SMD_Rectangle_0.5x0.6mm
	"SMD Oblong 0.45x1.10mm"  ->  SMD_Oblong_0.45x1.10mm
	"SMD Rectangle 1.0x0.85mm"  ->  SMD_Rectangle_1.0x0.85mm
	"SMD Rectangle 0.6x0.9mm"  ->  SMD_Rectangle_0.6x0.9mm
	"Round 75x35"  ->  Round_75x35
	"Pad Rectangle 100x80"  ->  Pad_Rectangle_100x80
	"SMD Rectangle 0.35x0.6mm"  ->  SMD_Rectangle_0.35x0.6mm
	"SMD Rectangle 0.6x1.55mm"  ->  SMD_Rectangle_0.6x1.55mm
	"SMD Rectangle 2.2x2.8mm"  ->  SMD_Rectangle_2.2x2.8mm
	"Round 56x32"  ->  Round_56x32
	"PowerPad Via 0.3mm"  ->  PowerPad_Via_0.3mm
	"SMD PowerPad 6.5mm"  ->  SMD_PowerPad_6.5mm
	"SMD PowerPad 2.0x2.2mm"  ->  SMD_PowerPad_2.0x2.2mm
	"SMD Rectangle 0.25x0.5mm"  ->  SMD_Rectangle_0.25x0.5mm
	"Gnd Via 0.3mm"  ->  Gnd_Via_0.3mm
	"Square 56x32"  ->  Square_56x32
	"SMD Rectangle 185x17"  ->  SMD_Rectangle_185x17
	"SMD Rectangle 110x17"  ->  SMD_Rectangle_110x17
	"Round 65x40"  ->  Round_65x40
	"Pad Rectangle 50x60"  ->  Pad_Rectangle_50x60
	"SMD Rectangle 0.9x0.8mm"  ->  SMD_Rectangle_0.9x0.8mm
	"Round 75x45"  ->  Round_75x45
	"Pad Rectangle 40x44"  ->  Pad_Rectangle_40x44
	"Round 6.5x3.25mm"  ->  Round_6.5x3.25mm
	"Pad Rectangle 60x110"  ->  Pad_Rectangle_60x110
	"SMD PowerPad 3.15mm"  ->  SMD_PowerPad_3.15mm
	"SMD PowerPad 3.61x6.35mm"  ->  SMD_PowerPad_3.61x6.35mm
	"SMD Rectangle 0.7x1.3mm"  ->  SMD_Rectangle_0.7x1.3mm
	"SMD Rectangle 1.8x1.4mm"  ->  SMD_Rectangle_1.8x1.4mm
	"SMD Rectangle 1.4x1.9mm"  ->  SMD_Rectangle_1.4x1.9mm
	"StandoffPad 5.5x3.25mm"  ->  StandoffPad_5.5x3.25mm
	"SMD Rectangle 1.4x1.2mm"  ->  SMD_Rectangle_1.4x1.2mm
	"Round 40x25 SocketPin"  ->  Round_40x25_SocketPin
	"Square 65x40"  ->  Square_65x40
	"SMD PowerPad 4.51x5.36mm"  ->  SMD_PowerPad_4.51x5.36mm
	"SMD PowerPad 1.6x2.1mm"  ->  SMD_PowerPad_1.6x2.1mm
	"SMD Rectangle 2x2.5mm"  ->  SMD_Rectangle_2x2.5mm
	"SMD Rectangle 3.4x4.0mm"  ->  SMD_Rectangle_3.4x4.0mm
	"Round 30x15"  ->  Round_30x15
	"SMD Rectangle 0.20x0.75mm"  ->  SMD_Rectangle_0.20x0.75mm
	"Pad Rectangle 55x20"  ->  Pad_Rectangle_55x20
	"SMD Rectangle 2.4x1.9mm"  ->  SMD_Rectangle_2.4x1.9mm
	"SMD Rectangle 1.2x1.9mm"  ->  SMD_Rectangle_1.2x1.9mm
	"SMD Rectangle 1.5x2.1mm"  ->  SMD_Rectangle_1.5x2.1mm
	"Slot 1.0x3.5mm  2.0x4.5mm Pad"  ->  Slot_1.0x3.5mm__2.0x4.5mm_Pad
	"Slot 1.3x2.5mm  2.3x3.5mm Pad"  ->  Slot_1.3x2.5mm__2.3x3.5mm_Pad
	"SMD Square 2.8mm"  ->  SMD_Square_2.8mm
	"Pad Square 32"  ->  Pad_Square_32
	"SMD Rectangle 1.0x3.7mm"  ->  SMD_Rectangle_1.0x3.7mm
	"SMD Rectangle 1.4x2.1mm"  ->  SMD_Rectangle_1.4x2.1mm
	"SMD Rectangle 1.8x4.5mm"  ->  SMD_Rectangle_1.8x4.5mm
	"StandoffPad 5.5x3.25mm_M3"  ->  StandoffPad_5.5x3.25mm_M3
	"StandoffPad 6.5x3.25mm_M3"  ->  StandoffPad_6.5x3.25mm_M3
	"Testpoint TH Round 30x15"  ->  Testpoint_TH_Round_30x15

The following device types have been renamed to conform to legal BoardStation names
	"SWITCHCRAFT_PHONE JACK"  ->  SWITCHCRAFT_PHONE_JACK
	"DIODES INC_SMA"  ->  DIODES_INC_SMA