
                                PLANES PROCESSOR
                                ----------------

                          04:22 PM Monday, May 06, 2013
Job Name: X:\AdapterAndControlerBoards\ControlConsoleBoard\PurePath-ConsoleMotherBoard_RevD\PCB\PurePath-ConsoleMotherBoard_RevD.pcb




    POSITIVE PLANE LAYER : 1

        Plane Shapes Found On This Layer : 10
        Plane Holes  Found On This Layer : 2


        PLANE NET : AGND

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 0.200mm
            Plane To Other Metal Clearance    : 0.000mm
            Mounting Hole / Contour Clearance : 0.152mm
            Minimum Plane Gap Distance        : NA
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : YES
            Default Via Tie Properties
                Tie Leg Width                 : 0.500mm
                Thermal Clearance             : 0.300mm
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Default Thru Tie Properties
                Tie Leg Width                 : 0.750mm
                Thermal Clearance             : 0.300mm
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Default SMD Tie Properties
                Tie Leg Width                 : 0.750mm
                Thermal Clearance             : 0.300mm
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 0.250mm
            Default Hatch Distance            : 0.250mm
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 91
            Total Thru Pads Of This Net       : 48
            Total SMD  Pads Of This Net       : 37

            Plane Created : Layer 1 - Net AGND

                Via Pads In This Plane           : 91
                Thru Pads In This Plane          : 48
                SMD Pads In This Plane           : 37
                     
                Pads To Be Buried In Plane       : 176
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0


        PLANE NET : GND

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 0.200mm
            Plane To Other Metal Clearance    : 0.000mm
            Mounting Hole / Contour Clearance : 0.152mm
            Minimum Plane Gap Distance        : NA
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : YES
            Default Via Tie Properties
                Tie Leg Width                 : 0.500mm
                Thermal Clearance             : 0.300mm
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Default Thru Tie Properties
                Tie Leg Width                 : 0.750mm
                Thermal Clearance             : 0.300mm
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Default SMD Tie Properties
                Tie Leg Width                 : 0.500mm
                Thermal Clearance             : 0.300mm
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 0.250mm
            Default Hatch Distance            : 0.250mm
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 346
            Total Thru Pads Of This Net       : 136
            Total SMD  Pads Of This Net       : 144

            Plane Created : Layer 1 - Net GND

                Via Pads In This Plane           : 346
                Thru Pads In This Plane          : 125
                SMD Pads In This Plane           : 139
                     
                Pads To Be Buried In Plane       : 590
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0
                Pads With 4/4 Tie Connections    : 12
                Pads With 3/4 Tie Connections    : 3
                Pads With 2/4 Tie Connections    : 4
                Pads With 1/4 Tie Connection     : 1

                    Pads With 3 Tie Legs : 3
                        Coordinates (mm) :
                                1) X=54.291      Y=97.375        Pin: C502-2  
                                2) X=65.709      Y=42.250        Pin: C412-2  
                                3) X=71.000      Y=87.000        Pin: S3-1  

                    Pads With 2 Tie Legs : 4
                        Coordinates (mm) :
                                1) X=14.250      Y=73.925        Pin: Y2-2  
                                2) X=15.500      Y=75.575        Pin: Y2-4  
                                3) X=29.375      Y=90.584        Pin: C103-2  
                                4) X=54.300      Y=80.100        Pin: OSC2-2  

                    Pads With 1 Tie Legs : 1
                        Coordinates (mm) :
                                1) X=26.525      Y=90.675        Pin: OSC1-2  


    POSITIVE PLANE LAYER : 2

        Plane Shapes Found On This Layer : 10
        Plane Holes  Found On This Layer : 2


        PLANE NET : AGND

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 0.200mm
            Plane To Other Metal Clearance    : 0.000mm
            Mounting Hole / Contour Clearance : 0.152mm
            Minimum Plane Gap Distance        : NA
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : YES
            Default Via Tie Properties
                Tie Leg Width                 : 0.500mm
                Thermal Clearance             : 0.300mm
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Default Thru Tie Properties
                Tie Leg Width                 : 0.750mm
                Thermal Clearance             : 0.300mm
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Default SMD Tie Properties
                Tie Leg Width                 : 0.500mm
                Thermal Clearance             : 0.300mm
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 0.250mm
            Default Hatch Distance            : 0.250mm
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 91
            Total Thru Pads Of This Net       : 48
            Total SMD  Pads Of This Net       : 0

            Plane Created : Layer 2 - Net AGND

                Via Pads In This Plane           : 91
                Thru Pads In This Plane          : 48
                SMD Pads In This Plane           : 0
                     
                Pads To Be Buried In Plane       : 139
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0


        PLANE NET : GND

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 0.200mm
            Plane To Other Metal Clearance    : 0.000mm
            Mounting Hole / Contour Clearance : 0.152mm
            Minimum Plane Gap Distance        : NA
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : YES
            Default Via Tie Properties
                Tie Leg Width                 : 0.500mm
                Thermal Clearance             : 0.300mm
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Default Thru Tie Properties
                Tie Leg Width                 : 0.750mm
                Thermal Clearance             : 0.300mm
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Default SMD Tie Properties
                Tie Leg Width                 : 0.750mm
                Thermal Clearance             : 0.300mm
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 0.250mm
            Default Hatch Distance            : 0.250mm
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 346
            Total Thru Pads Of This Net       : 136
            Total SMD  Pads Of This Net       : 0

            Plane Created : Layer 2 - Net GND

                Via Pads In This Plane           : 346
                Thru Pads In This Plane          : 128
                SMD Pads In This Plane           : 0
                     
                Pads To Be Buried In Plane       : 468
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0
                Pads With 4/4 Tie Connections    : 6


    POSITIVE PLANE LAYER : 4

        Plane Shapes Found On This Layer : 13
        Plane Holes  Found On This Layer : 2


        PLANE NET : AGND

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 0.250mm
            Plane To Other Metal Clearance    : 0.000mm
            Mounting Hole / Contour Clearance : 0.152mm
            Minimum Plane Gap Distance        : NA
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : YES
            Default Via Tie Properties
                Tie Leg Width                 : 0.500mm
                Thermal Clearance             : 0.300mm
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Default Thru Tie Properties
                Tie Leg Width                 : 0.750mm
                Thermal Clearance             : 0.300mm
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Default SMD Tie Properties
                Tie Leg Width                 : 0.500mm
                Thermal Clearance             : 0.300mm
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 0.200mm
            Default Hatch Distance            : 0.200mm
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 91
            Total Thru Pads Of This Net       : 48
            Total SMD  Pads Of This Net       : 21

            Plane Created : Layer 4 - Net AGND

                Via Pads In This Plane           : 91
                Thru Pads In This Plane          : 48
                SMD Pads In This Plane           : 21
                     
                Pads To Be Buried In Plane       : 158
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0
                Pads With 4/4 Tie Connections    : 2


        PLANE NET : GND

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 0.250mm
            Plane To Other Metal Clearance    : 0.000mm
            Mounting Hole / Contour Clearance : 0.152mm
            Minimum Plane Gap Distance        : NA
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : YES
            Default Via Tie Properties
                Tie Leg Width                 : 0.500mm
                Thermal Clearance             : 0.300mm
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Default Thru Tie Properties
                Tie Leg Width                 : 0.750mm
                Thermal Clearance             : 0.300mm
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Default SMD Tie Properties
                Tie Leg Width                 : 0.500mm
                Thermal Clearance             : 0.300mm
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 0.250mm
            Default Hatch Distance            : 0.250mm
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 346
            Total Thru Pads Of This Net       : 136
            Total SMD  Pads Of This Net       : 135

            Plane Created : Layer 4 - Net GND

                Via Pads In This Plane           : 346
                Thru Pads In This Plane          : 125
                SMD Pads In This Plane           : 135
                     
                Pads To Be Buried In Plane       : 595
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0
                Pads With 4/4 Tie Connections    : 6
                Pads With 3/4 Tie Connections    : 3
                Pads With 2/4 Tie Connections    : 2

                    Pads With 3 Tie Legs : 3
                        Coordinates (mm) :
                                1) X=12.625      Y=56.334        Pin: C135-2  
                                2) X=14.875      Y=96.291        Pin: C111-2  
                                3) X=22.250      Y=96.291        Pin: C109-2  

                    Pads With 2 Tie Legs : 2
                        Coordinates (mm) :
                                1) X=39.375      Y=96.625        Pin: S7-3  
                                2) X=79.825      Y=42.125        Pin: Q3-2  



                        04:22 PM Monday, May 06, 2013