
                                PLANES PROCESSOR
                                ----------------

                      12:46 PM Thursday, September 27, 2012
      Job Name: C:\ILS Projects\AFE5809_RevX1_EVM\PCB\AFE5809_RevX1_EVM.pcb




    POSITIVE PLANE LAYER : 1

        Plane Shapes Found On This Layer : 15
        Plane Holes  Found On This Layer : 0


        PLANE NET : GND

            Total Plane Shapes For This Net   : 3
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 15th
            Plane To Other Metal Clearance    : 0th
            Mounting Hole / Contour Clearance : 10th
            Minimum Plane Gap Distance        : NA
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : NO
            Default Via Tie Properties
                Number Tie Legs               : BURIED
            Default Thru Tie Properties
                Number Tie Legs               : BURIED
            Default SMD Tie Properties
                Number Tie Legs               : BURIED
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 5th
            Default Hatch Distance            : 5th
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 407
            Total Thru Pads Of This Net       : 84
            Total SMD  Pads Of This Net       : 232

            Plane Created : Layer 1 - Net GND

                Via Pads In This Plane           : 23
                Thru Pads In This Plane          : 0
                SMD Pads In This Plane           : 1
                     
                Pads To Be Buried In Plane       : 24
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0

            Plane Created : Layer 1 - Net GND

                Via Pads In This Plane           : 20
                Thru Pads In This Plane          : 0
                SMD Pads In This Plane           : 1
                     
                Pads To Be Buried In Plane       : 21
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0

            Plane Created : Layer 1 - Net GND

                Via Pads In This Plane           : 23
                Thru Pads In This Plane          : 0
                SMD Pads In This Plane           : 1
                     
                Pads To Be Buried In Plane       : 24
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0


        PLANE NET : +5V

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 15th
            Plane To Other Metal Clearance    : 0th
            Mounting Hole / Contour Clearance : 10th
            Minimum Plane Gap Distance        : NA
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : NO
            Default Via Tie Properties
                Number Tie Legs               : BURIED
            Default Thru Tie Properties
                Number Tie Legs               : BURIED
            Default SMD Tie Properties
                Number Tie Legs               : BURIED
            Eliminate Untied Areas            : NO
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 6.9th
            Default Hatch Distance            : 6.9th
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 14
            Total Thru Pads Of This Net       : 0
            Total SMD  Pads Of This Net       : 19

            Plane Created : Layer 1 - Net +5V

                Via Pads In This Plane           : 4
                Thru Pads In This Plane          : 0
                SMD Pads In This Plane           : 1
                     
                Pads To Be Buried In Plane       : 5
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0


        PLANE NET : +5VA

            Total Plane Shapes For This Net   : 3
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 15th
            Plane To Other Metal Clearance    : 0th
            Mounting Hole / Contour Clearance : 10th
            Minimum Plane Gap Distance        : NA
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : NO
            Default Via Tie Properties
                Number Tie Legs               : BURIED
            Default Thru Tie Properties
                Number Tie Legs               : BURIED
            Default SMD Tie Properties
                Number Tie Legs               : BURIED
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 5th
            Default Hatch Distance            : 5th
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 35
            Total Thru Pads Of This Net       : 3
            Total SMD  Pads Of This Net       : 3

            Plane Created : Layer 1 - Net +5VA

                Via Pads In This Plane           : 12
                Thru Pads In This Plane          : 0
                SMD Pads In This Plane           : 1
                     
                Pads To Be Buried In Plane       : 13
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0

            Plane Created : Layer 1 - Net +5VA

                Via Pads In This Plane           : 6
                Thru Pads In This Plane          : 0
                SMD Pads In This Plane           : 1
                     
                Pads To Be Buried In Plane       : 7
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0

            Plane Created : Layer 1 - Net +5VA

                Via Pads In This Plane           : 6
                Thru Pads In This Plane          : 0
                SMD Pads In This Plane           : 1
                     
                Pads To Be Buried In Plane       : 7
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0


        PLANE NET : AVDD_ADC

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 15th
            Plane To Other Metal Clearance    : 0th
            Mounting Hole / Contour Clearance : 10th
            Minimum Plane Gap Distance        : NA
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : NO
            Default Via Tie Properties
                Number Tie Legs               : BURIED
            Default Thru Tie Properties
                Number Tie Legs               : BURIED
            Default SMD Tie Properties
                Number Tie Legs               : BURIED
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 5th
            Default Hatch Distance            : 5th
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 10
            Total Thru Pads Of This Net       : 0
            Total SMD  Pads Of This Net       : 7

            Plane Created : Layer 1 - Net AVDD_ADC

                Via Pads In This Plane           : 6
                Thru Pads In This Plane          : 0
                SMD Pads In This Plane           : 1
                     
                Pads To Be Buried In Plane       : 7
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0


        PLANE NET : DVDD

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 15th
            Plane To Other Metal Clearance    : 0th
            Mounting Hole / Contour Clearance : 10th
            Minimum Plane Gap Distance        : NA
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : NO
            Default Via Tie Properties
                Number Tie Legs               : BURIED
            Default Thru Tie Properties
                Number Tie Legs               : BURIED
            Default SMD Tie Properties
                Number Tie Legs               : BURIED
            Eliminate Untied Areas            : NO
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 6.9th
            Default Hatch Distance            : 6.9th
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 8
            Total Thru Pads Of This Net       : 0
            Total SMD  Pads Of This Net       : 3

            Plane Created : Layer 1 - Net DVDD

                Via Pads In This Plane           : 6
                Thru Pads In This Plane          : 0
                SMD Pads In This Plane           : 1
                     
                Pads To Be Buried In Plane       : 7
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0


        PLANE NET : +3.3VD

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 15th
            Plane To Other Metal Clearance    : 0th
            Mounting Hole / Contour Clearance : 10th
            Minimum Plane Gap Distance        : NA
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : NO
            Default Via Tie Properties
                Number Tie Legs               : BURIED
            Default Thru Tie Properties
                Number Tie Legs               : BURIED
            Default SMD Tie Properties
                Number Tie Legs               : BURIED
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 5th
            Default Hatch Distance            : 5th
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 0
            Total Thru Pads Of This Net       : 2
            Total SMD  Pads Of This Net       : 3

            Plane Created : Layer 1 - Net +3.3VD

                Via Pads In This Plane           : 0
                Thru Pads In This Plane          : 2
                SMD Pads In This Plane           : 3
                     
                Pads To Be Buried In Plane       : 5
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0


        PLANE NET : +3.3VA

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 15th
            Plane To Other Metal Clearance    : 0th
            Mounting Hole / Contour Clearance : 10th
            Minimum Plane Gap Distance        : NA
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : NO
            Default Via Tie Properties
                Number Tie Legs               : BURIED
            Default Thru Tie Properties
                Number Tie Legs               : BURIED
            Default SMD Tie Properties
                Number Tie Legs               : BURIED
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 5th
            Default Hatch Distance            : 5th
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 0
            Total Thru Pads Of This Net       : 5
            Total SMD  Pads Of This Net       : 3

            Plane Created : Layer 1 - Net +3.3VA

                Via Pads In This Plane           : 0
                Thru Pads In This Plane          : 5
                SMD Pads In This Plane           : 3
                     
                Pads To Be Buried In Plane       : 8
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0


        PLANE NET : +1.8VD

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 15th
            Plane To Other Metal Clearance    : 0th
            Mounting Hole / Contour Clearance : 10th
            Minimum Plane Gap Distance        : NA
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : NO
            Default Via Tie Properties
                Number Tie Legs               : BURIED
            Default Thru Tie Properties
                Number Tie Legs               : BURIED
            Default SMD Tie Properties
                Number Tie Legs               : BURIED
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 5th
            Default Hatch Distance            : 5th
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 0
            Total Thru Pads Of This Net       : 3
            Total SMD  Pads Of This Net       : 3

            Plane Created : Layer 1 - Net +1.8VD

                Via Pads In This Plane           : 0
                Thru Pads In This Plane          : 3
                SMD Pads In This Plane           : 3
                     
                Pads To Be Buried In Plane       : 6
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0


        PLANE NET : XSIG011079

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 15th
            Plane To Other Metal Clearance    : 0th
            Mounting Hole / Contour Clearance : 10th
            Minimum Plane Gap Distance        : NA
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : NO
            Default Via Tie Properties
                Number Tie Legs               : BURIED
            Default Thru Tie Properties
                Number Tie Legs               : BURIED
            Default SMD Tie Properties
                Number Tie Legs               : BURIED
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 5th
            Default Hatch Distance            : 5th
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 0
            Total Thru Pads Of This Net       : 0
            Total SMD  Pads Of This Net       : 5

            Plane Created : Layer 1 - Net XSIG011079

                Via Pads In This Plane           : 0
                Thru Pads In This Plane          : 0
                SMD Pads In This Plane           : 5
                     
                Pads To Be Buried In Plane       : 5
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0


        PLANE NET : XSIG011087

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 15th
            Plane To Other Metal Clearance    : 0th
            Mounting Hole / Contour Clearance : 10th
            Minimum Plane Gap Distance        : NA
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : NO
            Default Via Tie Properties
                Number Tie Legs               : BURIED
            Default Thru Tie Properties
                Number Tie Legs               : BURIED
            Default SMD Tie Properties
                Number Tie Legs               : BURIED
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 5th
            Default Hatch Distance            : 5th
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 0
            Total Thru Pads Of This Net       : 0
            Total SMD  Pads Of This Net       : 5

            Plane Created : Layer 1 - Net XSIG011087

                Via Pads In This Plane           : 0
                Thru Pads In This Plane          : 0
                SMD Pads In This Plane           : 5
                     
                Pads To Be Buried In Plane       : 5
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0


        PLANE NET : XSIG011095

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 15th
            Plane To Other Metal Clearance    : 0th
            Mounting Hole / Contour Clearance : 10th
            Minimum Plane Gap Distance        : NA
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : NO
            Default Via Tie Properties
                Number Tie Legs               : BURIED
            Default Thru Tie Properties
                Number Tie Legs               : BURIED
            Default SMD Tie Properties
                Number Tie Legs               : BURIED
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 5th
            Default Hatch Distance            : 5th
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 0
            Total Thru Pads Of This Net       : 0
            Total SMD  Pads Of This Net       : 5

            Plane Created : Layer 1 - Net XSIG011095

                Via Pads In This Plane           : 0
                Thru Pads In This Plane          : 0
                SMD Pads In This Plane           : 5
                     
                Pads To Be Buried In Plane       : 5
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0


    POSITIVE PLANE LAYER : 2

        Plane Shapes Found On This Layer : 2
        Plane Holes  Found On This Layer : 0


        PLANE NET : GND

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 10th
            Plane To Other Metal Clearance    : 0th
            Mounting Hole / Contour Clearance : 20th
            Minimum Plane Gap Distance        : NA
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : NO
            Default Via Tie Properties
                Number Tie Legs               : BURIED
            Default Thru Tie Properties
                Tie Leg Width                 : 25th
                Thermal Clearance             : 15th
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Default SMD Tie Properties
                Number Tie Legs               : BURIED
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 6th
            Default Hatch Distance            : 6th
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 407
            Total Thru Pads Of This Net       : 84
            Total SMD  Pads Of This Net       : 0

            Plane Created : Layer 2 - Net GND

                Via Pads In This Plane           : 407
                Thru Pads In This Plane          : 84
                SMD Pads In This Plane           : 0
                     
                Pads To Be Buried In Plane       : 407
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0
                Pads With 4/4 Tie Connections    : 84


        PLANE NET : DGND

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 10th
            Plane To Other Metal Clearance    : 0th
            Mounting Hole / Contour Clearance : 20th
            Minimum Plane Gap Distance        : NA
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : NO
            Default Via Tie Properties
                Number Tie Legs               : BURIED
            Default Thru Tie Properties
                Tie Leg Width                 : 25th
                Thermal Clearance             : 15th
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Default SMD Tie Properties
                Number Tie Legs               : BURIED
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 6th
            Default Hatch Distance            : 6th
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 29
            Total Thru Pads Of This Net       : 2
            Total SMD  Pads Of This Net       : 0

            Plane Created : Layer 2 - Net DGND

                Via Pads In This Plane           : 29
                Thru Pads In This Plane          : 2
                SMD Pads In This Plane           : 0
                     
                Pads To Be Buried In Plane       : 29
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0
                Pads With 4/4 Tie Connections    : 2


    POSITIVE PLANE LAYER : 3

        Plane Shapes Found On This Layer : 9
        Plane Holes  Found On This Layer : 1


        PLANE NET : +5V

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 10th
            Plane To Other Metal Clearance    : 0th
            Mounting Hole / Contour Clearance : 20th
            Minimum Plane Gap Distance        : 20th
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : NO
            Default Via Tie Properties
                Number Tie Legs               : BURIED
            Default Thru Tie Properties
                Tie Leg Width                 : 25th
                Thermal Clearance             : 15th
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Default SMD Tie Properties
                Number Tie Legs               : BURIED
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 6th
            Default Hatch Distance            : 6th
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 14
            Total Thru Pads Of This Net       : 0
            Total SMD  Pads Of This Net       : 0

            Plane Created : Layer 3 - Net +5V

                Via Pads In This Plane           : 12
                Thru Pads In This Plane          : 0
                SMD Pads In This Plane           : 0
                     
                Pads To Be Buried In Plane       : 12
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0


        PLANE NET : +5VA

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 10th
            Plane To Other Metal Clearance    : 0th
            Mounting Hole / Contour Clearance : 20th
            Minimum Plane Gap Distance        : 20th
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : NO
            Default Via Tie Properties
                Number Tie Legs               : BURIED
            Default Thru Tie Properties
                Tie Leg Width                 : 25th
                Thermal Clearance             : 15th
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Default SMD Tie Properties
                Number Tie Legs               : BURIED
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 6th
            Default Hatch Distance            : 6th
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 35
            Total Thru Pads Of This Net       : 3
            Total SMD  Pads Of This Net       : 0

            Plane Created : Layer 3 - Net +5VA

                Via Pads In This Plane           : 23
                Thru Pads In This Plane          : 3
                SMD Pads In This Plane           : 0
                     
                Pads To Be Buried In Plane       : 23
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0
                Pads With 4/4 Tie Connections    : 3


        PLANE NET : AVDD

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 10th
            Plane To Other Metal Clearance    : 0th
            Mounting Hole / Contour Clearance : 20th
            Minimum Plane Gap Distance        : 20th
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : NO
            Default Via Tie Properties
                Number Tie Legs               : BURIED
            Default Thru Tie Properties
                Tie Leg Width                 : 25th
                Thermal Clearance             : 15th
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Default SMD Tie Properties
                Number Tie Legs               : BURIED
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 6th
            Default Hatch Distance            : 6th
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 23
            Total Thru Pads Of This Net       : 6
            Total SMD  Pads Of This Net       : 0

            Plane Created : Layer 3 - Net AVDD

                Via Pads In This Plane           : 23
                Thru Pads In This Plane          : 6
                SMD Pads In This Plane           : 0
                     
                Pads To Be Buried In Plane       : 23
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0
                Pads With 4/4 Tie Connections    : 6


        PLANE NET : 3.3V_USB

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 10th
            Plane To Other Metal Clearance    : 5th
            Mounting Hole / Contour Clearance : 20th
            Minimum Plane Gap Distance        : 20th
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : NO
            Default Via Tie Properties
                Number Tie Legs               : BURIED
            Default Thru Tie Properties
                Tie Leg Width                 : 25th
                Thermal Clearance             : 15th
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Default SMD Tie Properties
                Number Tie Legs               : BURIED
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 6th
            Default Hatch Distance            : 6th
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 3
            Total Thru Pads Of This Net       : 0
            Total SMD  Pads Of This Net       : 0

            Plane Created : Layer 3 - Net 3.3V_USB

                Via Pads In This Plane           : 3
                Thru Pads In This Plane          : 0
                SMD Pads In This Plane           : 0
                     
                Pads To Be Buried In Plane       : 3
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0


        PLANE NET : CLKBUF_AVCC

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 10th
            Plane To Other Metal Clearance    : 0th
            Mounting Hole / Contour Clearance : 20th
            Minimum Plane Gap Distance        : 20th
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : NO
            Default Via Tie Properties
                Number Tie Legs               : BURIED
            Default Thru Tie Properties
                Tie Leg Width                 : 25th
                Thermal Clearance             : 15th
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Default SMD Tie Properties
                Number Tie Legs               : BURIED
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 6th
            Default Hatch Distance            : 6th
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 17
            Total Thru Pads Of This Net       : 0
            Total SMD  Pads Of This Net       : 0

            Plane Created : Layer 3 - Net CLKBUF_AVCC

                Via Pads In This Plane           : 17
                Thru Pads In This Plane          : 0
                SMD Pads In This Plane           : 0
                     
                Pads To Be Buried In Plane       : 17
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0


        PLANE NET : CLKBUF_VCC

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 10th
            Plane To Other Metal Clearance    : 5th
            Mounting Hole / Contour Clearance : 20th
            Minimum Plane Gap Distance        : 20th
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : NO
            Default Via Tie Properties
                Number Tie Legs               : BURIED
            Default Thru Tie Properties
                Tie Leg Width                 : 25th
                Thermal Clearance             : 15th
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Default SMD Tie Properties
                Number Tie Legs               : BURIED
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 6th
            Default Hatch Distance            : 6th
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 30
            Total Thru Pads Of This Net       : 0
            Total SMD  Pads Of This Net       : 0

            Plane Created : Layer 3 - Net CLKBUF_VCC

                Via Pads In This Plane           : 27
                Thru Pads In This Plane          : 0
                SMD Pads In This Plane           : 0
                     
                Pads To Be Buried In Plane       : 27
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0


        PLANE NET : +5V_USB

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 10th
            Plane To Other Metal Clearance    : 0th
            Mounting Hole / Contour Clearance : 20th
            Minimum Plane Gap Distance        : 10th
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : NO
            Default Via Tie Properties
                Number Tie Legs               : BURIED
            Default Thru Tie Properties
                Tie Leg Width                 : 25th
                Thermal Clearance             : 15th
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Default SMD Tie Properties
                Number Tie Legs               : BURIED
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 6th
            Default Hatch Distance            : 6th
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 7
            Total Thru Pads Of This Net       : 1
            Total SMD  Pads Of This Net       : 0

            Plane Created : Layer 3 - Net +5V_USB

                Via Pads In This Plane           : 7
                Thru Pads In This Plane          : 1
                SMD Pads In This Plane           : 0
                     
                Pads To Be Buried In Plane       : 7
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0
                Pads With 4/4 Tie Connections    : 1


        PLANE NET : AVDD_ADC

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 10th
            Plane To Other Metal Clearance    : 0th
            Mounting Hole / Contour Clearance : 20th
            Minimum Plane Gap Distance        : 20th
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : NO
            Default Via Tie Properties
                Number Tie Legs               : BURIED
            Default Thru Tie Properties
                Tie Leg Width                 : 25th
                Thermal Clearance             : 15th
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Default SMD Tie Properties
                Number Tie Legs               : BURIED
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 6th
            Default Hatch Distance            : 6th
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 10
            Total Thru Pads Of This Net       : 0
            Total SMD  Pads Of This Net       : 0

            Plane Created : Layer 3 - Net AVDD_ADC

                Via Pads In This Plane           : 10
                Thru Pads In This Plane          : 0
                SMD Pads In This Plane           : 0
                     
                Pads To Be Buried In Plane       : 10
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0


        PLANE NET : DVDD

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 10th
            Plane To Other Metal Clearance    : 0th
            Mounting Hole / Contour Clearance : 20th
            Minimum Plane Gap Distance        : 20th
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : NO
            Default Via Tie Properties
                Number Tie Legs               : BURIED
            Default Thru Tie Properties
                Tie Leg Width                 : 25th
                Thermal Clearance             : 15th
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Default SMD Tie Properties
                Number Tie Legs               : BURIED
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 6th
            Default Hatch Distance            : 6th
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 8
            Total Thru Pads Of This Net       : 0
            Total SMD  Pads Of This Net       : 0

            Plane Created : Layer 3 - Net DVDD

                Via Pads In This Plane           : 8
                Thru Pads In This Plane          : 0
                SMD Pads In This Plane           : 0
                     
                Pads To Be Buried In Plane       : 8
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0


    POSITIVE PLANE LAYER : 4

        Plane Shapes Found On This Layer : 3
        Plane Holes  Found On This Layer : 0


        PLANE NET : +5VA

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 15th
            Plane To Other Metal Clearance    : 0th
            Mounting Hole / Contour Clearance : 10th
            Minimum Plane Gap Distance        : NA
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : NO
            Default Via Tie Properties
                Number Tie Legs               : BURIED
            Default Thru Tie Properties
                Tie Leg Width                 : 25th
                Thermal Clearance             : 15th
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Default SMD Tie Properties
                Number Tie Legs               : BURIED
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 6.9th
            Default Hatch Distance            : 6.9th
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 35
            Total Thru Pads Of This Net       : 3
            Total SMD  Pads Of This Net       : 0

            Plane Created : Layer 4 - Net +5VA

                Via Pads In This Plane           : 20
                Thru Pads In This Plane          : 0
                SMD Pads In This Plane           : 0
                     
                Pads To Be Buried In Plane       : 20
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0


        PLANE NET : -5V

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 15th
            Plane To Other Metal Clearance    : 0th
            Mounting Hole / Contour Clearance : 20th
            Minimum Plane Gap Distance        : NA
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : NO
            Default Via Tie Properties
                Number Tie Legs               : BURIED
            Default Thru Tie Properties
                Number Tie Legs               : BURIED
            Default SMD Tie Properties
                Number Tie Legs               : BURIED
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 5th
            Default Hatch Distance            : 5th
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 10
            Total Thru Pads Of This Net       : 2
            Total SMD  Pads Of This Net       : 0

            Plane Created : Layer 4 - Net -5V

                Via Pads In This Plane           : 9
                Thru Pads In This Plane          : 1
                SMD Pads In This Plane           : 0
                     
                Pads To Be Buried In Plane       : 10
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0


        PLANE NET : CLKBUF_CP

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 15th
            Plane To Other Metal Clearance    : 0th
            Mounting Hole / Contour Clearance : 20th
            Minimum Plane Gap Distance        : NA
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : NO
            Default Via Tie Properties
                Number Tie Legs               : BURIED
            Default Thru Tie Properties
                Tie Leg Width                 : 25th
                Thermal Clearance             : 15th
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Default SMD Tie Properties
                Number Tie Legs               : BURIED
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 5th
            Default Hatch Distance            : 5th
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 14
            Total Thru Pads Of This Net       : 0
            Total SMD  Pads Of This Net       : 0

            Plane Created : Layer 4 - Net CLKBUF_CP

                Via Pads In This Plane           : 14
                Thru Pads In This Plane          : 0
                SMD Pads In This Plane           : 0
                     
                Pads To Be Buried In Plane       : 14
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0


    POSITIVE PLANE LAYER : 5

        Plane Shapes Found On This Layer : 2
        Plane Holes  Found On This Layer : 0


        PLANE NET : GND

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 10th
            Plane To Other Metal Clearance    : 0th
            Mounting Hole / Contour Clearance : 20th
            Minimum Plane Gap Distance        : NA
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : NO
            Default Via Tie Properties
                Number Tie Legs               : BURIED
            Default Thru Tie Properties
                Tie Leg Width                 : 25th
                Thermal Clearance             : 15th
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Default SMD Tie Properties
                Number Tie Legs               : BURIED
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 6th
            Default Hatch Distance            : 6th
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 407
            Total Thru Pads Of This Net       : 84
            Total SMD  Pads Of This Net       : 0

            Plane Created : Layer 5 - Net GND

                Via Pads In This Plane           : 407
                Thru Pads In This Plane          : 84
                SMD Pads In This Plane           : 0
                     
                Pads To Be Buried In Plane       : 407
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0
                Pads With 4/4 Tie Connections    : 84


        PLANE NET : DGND

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 10th
            Plane To Other Metal Clearance    : 0th
            Mounting Hole / Contour Clearance : 20th
            Minimum Plane Gap Distance        : NA
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : NO
            Default Via Tie Properties
                Number Tie Legs               : BURIED
            Default Thru Tie Properties
                Tie Leg Width                 : 25th
                Thermal Clearance             : 15th
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Default SMD Tie Properties
                Number Tie Legs               : BURIED
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 6th
            Default Hatch Distance            : 6th
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 29
            Total Thru Pads Of This Net       : 2
            Total SMD  Pads Of This Net       : 0

            Plane Created : Layer 5 - Net DGND

                Via Pads In This Plane           : 29
                Thru Pads In This Plane          : 2
                SMD Pads In This Plane           : 0
                     
                Pads To Be Buried In Plane       : 29
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0
                Pads With 4/4 Tie Connections    : 2


    POSITIVE PLANE LAYER : 6

        Plane Shapes Found On This Layer : 16
        Plane Holes  Found On This Layer : 0


        PLANE NET : GND

            Total Plane Shapes For This Net   : 5
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 15th
            Plane To Other Metal Clearance    : 0th
            Mounting Hole / Contour Clearance : 20th
            Minimum Plane Gap Distance        : NA
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : NO
            Default Via Tie Properties
                Number Tie Legs               : BURIED
            Default Thru Tie Properties
                Number Tie Legs               : BURIED
            Default SMD Tie Properties
                Number Tie Legs               : BURIED
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 5th
            Default Hatch Distance            : 5th
            Default Hatch Pattern             : (-) Horizontal
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 407
            Total Thru Pads Of This Net       : 84
            Total SMD  Pads Of This Net       : 110

            Plane Created : Layer 6 - Net GND

                Via Pads In This Plane           : 9
                Thru Pads In This Plane          : 0
                SMD Pads In This Plane           : 16
                     
                Pads To Be Buried In Plane       : 25
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0

            Plane Created : Layer 6 - Net GND

                Via Pads In This Plane           : 23
                Thru Pads In This Plane          : 0
                SMD Pads In This Plane           : 1
                     
                Pads To Be Buried In Plane       : 24
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0

            Plane Created : Layer 6 - Net GND

                Via Pads In This Plane           : 3
                Thru Pads In This Plane          : 2
                SMD Pads In This Plane           : 3
                     
                Pads To Be Buried In Plane       : 8
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0

            Plane Created : Layer 6 - Net GND

                Via Pads In This Plane           : 8
                Thru Pads In This Plane          : 0
                SMD Pads In This Plane           : 4
                     
                Pads To Be Buried In Plane       : 12
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0

            Plane Created : Layer 6 - Net GND

                Via Pads In This Plane           : 2
                Thru Pads In This Plane          : 1
                SMD Pads In This Plane           : 2
                     
                Pads To Be Buried In Plane       : 5
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0


        PLANE NET : +5V

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 15th
            Plane To Other Metal Clearance    : 0th
            Mounting Hole / Contour Clearance : 20th
            Minimum Plane Gap Distance        : NA
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : NO
            Default Via Tie Properties
                Number Tie Legs               : BURIED
            Default Thru Tie Properties
                Number Tie Legs               : BURIED
            Default SMD Tie Properties
                Number Tie Legs               : BURIED
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 5th
            Default Hatch Distance            : 5th
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 14
            Total Thru Pads Of This Net       : 0
            Total SMD  Pads Of This Net       : 11

            Plane Created : Layer 6 - Net +5V

                Via Pads In This Plane           : 4
                Thru Pads In This Plane          : 0
                SMD Pads In This Plane           : 5
                     
                Pads To Be Buried In Plane       : 9
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0


        PLANE NET : AVDD

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 15th
            Plane To Other Metal Clearance    : 0th
            Mounting Hole / Contour Clearance : 20th
            Minimum Plane Gap Distance        : NA
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : NO
            Default Via Tie Properties
                Number Tie Legs               : BURIED
            Default Thru Tie Properties
                Number Tie Legs               : BURIED
            Default SMD Tie Properties
                Number Tie Legs               : BURIED
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 5th
            Default Hatch Distance            : 5th
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 23
            Total Thru Pads Of This Net       : 6
            Total SMD  Pads Of This Net       : 10

            Plane Created : Layer 6 - Net AVDD

                Via Pads In This Plane           : 12
                Thru Pads In This Plane          : 0
                SMD Pads In This Plane           : 1
                     
                Pads To Be Buried In Plane       : 13
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0


        PLANE NET : CLKBUF_AVCC

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 15th
            Plane To Other Metal Clearance    : 0th
            Mounting Hole / Contour Clearance : 20th
            Minimum Plane Gap Distance        : NA
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : NO
            Default Via Tie Properties
                Number Tie Legs               : BURIED
            Default Thru Tie Properties
                Number Tie Legs               : BURIED
            Default SMD Tie Properties
                Number Tie Legs               : BURIED
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 5th
            Default Hatch Distance            : 5th
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 17
            Total Thru Pads Of This Net       : 0
            Total SMD  Pads Of This Net       : 8

            Plane Created : Layer 6 - Net CLKBUF_AVCC

                Via Pads In This Plane           : 9
                Thru Pads In This Plane          : 0
                SMD Pads In This Plane           : 1
                     
                Pads To Be Buried In Plane       : 10
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0


        PLANE NET : CLKBUF_VCC

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 15th
            Plane To Other Metal Clearance    : 0th
            Mounting Hole / Contour Clearance : 20th
            Minimum Plane Gap Distance        : NA
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : NO
            Default Via Tie Properties
                Number Tie Legs               : BURIED
            Default Thru Tie Properties
                Number Tie Legs               : BURIED
            Default SMD Tie Properties
                Number Tie Legs               : BURIED
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 5th
            Default Hatch Distance            : 5th
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 30
            Total Thru Pads Of This Net       : 0
            Total SMD  Pads Of This Net       : 15

            Plane Created : Layer 6 - Net CLKBUF_VCC

                Via Pads In This Plane           : 9
                Thru Pads In This Plane          : 0
                SMD Pads In This Plane           : 1
                     
                Pads To Be Buried In Plane       : 10
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0


        PLANE NET : -5V

            Total Plane Shapes For This Net   : 2
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 15th
            Plane To Other Metal Clearance    : 0th
            Mounting Hole / Contour Clearance : 20th
            Minimum Plane Gap Distance        : NA
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : NO
            Default Via Tie Properties
                Number Tie Legs               : BURIED
            Default Thru Tie Properties
                Number Tie Legs               : BURIED
            Default SMD Tie Properties
                Number Tie Legs               : BURIED
            Eliminate Untied Areas            : NO
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 6.9th
            Default Hatch Distance            : 6.9th
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 10
            Total Thru Pads Of This Net       : 2
            Total SMD  Pads Of This Net       : 7

            Plane Created : Layer 6 - Net -5V

                Via Pads In This Plane           : 2
                Thru Pads In This Plane          : 0
                SMD Pads In This Plane           : 2
                     
                Pads To Be Buried In Plane       : 4
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0

            Plane Created : Layer 6 - Net -5V

                Via Pads In This Plane           : 5
                Thru Pads In This Plane          : 1
                SMD Pads In This Plane           : 4
                     
                Pads To Be Buried In Plane       : 10
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0


        PLANE NET : +5V_SRC

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 15th
            Plane To Other Metal Clearance    : 0th
            Mounting Hole / Contour Clearance : 20th
            Minimum Plane Gap Distance        : NA
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : NO
            Default Via Tie Properties
                Number Tie Legs               : BURIED
            Default Thru Tie Properties
                Number Tie Legs               : BURIED
            Default SMD Tie Properties
                Number Tie Legs               : BURIED
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 5th
            Default Hatch Distance            : 5th
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 0
            Total Thru Pads Of This Net       : 2
            Total SMD  Pads Of This Net       : 4

            Plane Created : Layer 6 - Net +5V_SRC

                Via Pads In This Plane           : 0
                Thru Pads In This Plane          : 2
                SMD Pads In This Plane           : 4
                     
                Pads To Be Buried In Plane       : 6
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0


        PLANE NET : -5VA

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 15th
            Plane To Other Metal Clearance    : 0th
            Mounting Hole / Contour Clearance : 20th
            Minimum Plane Gap Distance        : NA
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : NO
            Default Via Tie Properties
                Number Tie Legs               : BURIED
            Default Thru Tie Properties
                Number Tie Legs               : BURIED
            Default SMD Tie Properties
                Number Tie Legs               : BURIED
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 6.9th
            Default Hatch Distance            : 6.9th
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 0
            Total Thru Pads Of This Net       : 3
            Total SMD  Pads Of This Net       : 1

            Plane Created : Layer 6 - Net -5VA

                Via Pads In This Plane           : 0
                Thru Pads In This Plane          : 2
                SMD Pads In This Plane           : 1
                     
                Pads To Be Buried In Plane       : 3
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0


        PLANE NET : CLKBUF_CP

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 15th
            Plane To Other Metal Clearance    : 0th
            Mounting Hole / Contour Clearance : 20th
            Minimum Plane Gap Distance        : NA
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : NO
            Default Via Tie Properties
                Number Tie Legs               : BURIED
            Default Thru Tie Properties
                Number Tie Legs               : BURIED
            Default SMD Tie Properties
                Number Tie Legs               : BURIED
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 5th
            Default Hatch Distance            : 5th
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 14
            Total Thru Pads Of This Net       : 0
            Total SMD  Pads Of This Net       : 3

            Plane Created : Layer 6 - Net CLKBUF_CP

                Via Pads In This Plane           : 9
                Thru Pads In This Plane          : 0
                SMD Pads In This Plane           : 1
                     
                Pads To Be Buried In Plane       : 10
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0


        PLANE NET : XSIG011460

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 15th
            Plane To Other Metal Clearance    : 0th
            Mounting Hole / Contour Clearance : 20th
            Minimum Plane Gap Distance        : NA
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : NO
            Default Via Tie Properties
                Number Tie Legs               : BURIED
            Default Thru Tie Properties
                Number Tie Legs               : BURIED
            Default SMD Tie Properties
                Number Tie Legs               : BURIED
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 6.9th
            Default Hatch Distance            : 6.9th
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 0
            Total Thru Pads Of This Net       : 0
            Total SMD  Pads Of This Net       : 5

            Plane Created : Layer 6 - Net XSIG011460

                Via Pads In This Plane           : 0
                Thru Pads In This Plane          : 0
                SMD Pads In This Plane           : 5
                     
                Pads To Be Buried In Plane       : 5
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0


        PLANE NET : XSIG011464

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 15th
            Plane To Other Metal Clearance    : 0th
            Mounting Hole / Contour Clearance : 20th
            Minimum Plane Gap Distance        : NA
            Use TieLeg Bridges If Needed      : YES
            Use Padstack Thermal Definition   : NO
            Default Via Tie Properties
                Number Tie Legs               : BURIED
            Default Thru Tie Properties
                Number Tie Legs               : BURIED
            Default SMD Tie Properties
                Number Tie Legs               : BURIED
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 6.9th
            Default Hatch Distance            : 6.9th
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 0
            Total Thru Pads Of This Net       : 1
            Total SMD  Pads Of This Net       : 4

            Plane Created : Layer 6 - Net XSIG011464

                Via Pads In This Plane           : 0
                Thru Pads In This Plane          : 1
                SMD Pads In This Plane           : 4
                     
                Pads To Be Buried In Plane       : 5
                    Unconnected To Plane         : 0
                        Connected To Trace       : 0



                        12:47 PM Thursday, September 27, 2012