Field=#~Integer~#~50|Field=Fitted~String~Fitted~150|Field=Description~String~Description~150|Field=Designator~String~Designator~150|Field=PartNumber~String~PartNumber~150|Field=Quantity~Integer~Quantity~150|Field=Manufacturer~String~Manufacturer~150|Field=PackageReference~String~PackageReference~150|Field=Value~String~Value~150|Field=Alternate Manufacturer~String~Alternate Manufacturer~150|Field=Alternate PartNumber~String~Alternate PartNumber~150|ReportField=Currency~USD|ReportField=ProductionQuantity~100|ReportField=ProjectFileName~TIDA-01432E1.PrjPcb|ReportField=ProjectFullPath~X:\TID\Sabre\TIDA-01001-TIDA-01500\TIDA-01431-TIDA-01440\TIDA-01432 - Automotive USB Redriver (general release TIDA01256)\TIDA-01432\TIDA-01432E1 (7-24-2017 10-55-15 AM)\TIDA-01432E1.PrjPcb|ReportField=Title~TIDA-01432E1_BOM (EVM format) For Variant [001] of Project [TIDA-01432E1.PrjPcb] (No PCB Document Selected)|ReportField=TotalQuantity~77|ReportField=ReportTime~5:11:32 PM|ReportField=ReportDate~8/25/2017|ReportField=ReportDateTime~8/25/2017 5:11:32 PM|ReportField=OutputName~TIDA-01432E1_BOM (EVM format)|ReportField=OutputType~BOM_PartType|ReportField=GeneratorName~BOM|ReportField=GeneratorDescription~Bill of Materials|ReportField=VariantName~001|ReportField=EVM_Orderable~ChangeMe!|ReportField=CopyrightYear~2016|ReportField=PCB_Layout~Bovenzi/Clanin|ReportField=PCB_Rev~E1|ReportField=PRJ_Customer~Not for Public Release|ReportField=PRJ_Engineer~H.Bovenzi|ReportField=PRJ_Number~TIDA-01432|ReportField=PRJ_Title~TIDA-01432|ReportField=SCH_Rev~E1|ReportField=TechSupport~http://www.ti.com/support|ReportField=TID~N/A|ReportField=Address1~Not shown in title block|ReportField=Address2~Not shown in title block|ReportField=Address3~Not shown in title block|ReportField=Address4~Not shown in title block|ReportField=Application_BuildNumber~|ReportField=ApprovedBy~Not shown in title block|ReportField=Author~Not shown in title block|ReportField=CheckedBy~Not shown in title block|ReportField=CompanyName~Not shown in title block|ReportField=ConfigurationParameters~|ReportField=ConfiguratorName~|ReportField=CurrentDate~8/25/2017|ReportField=CurrentTime~5:03:31 PM|ReportField=Date~Not shown in title block|ReportField=DocumentFullPathAndName~X:\TID\Sabre\TIDA-01001-TIDA-01500\TIDA-01431-TIDA-01440\TIDA-01432 - Automotive USB Redriver (general release TIDA01256)\TIDA-01432\TIDA-01432E1 (7-24-2017 10-55-15 AM)\TIDA-01432 E1_Hardware.SchDoc|ReportField=DocumentName~TIDA-01432 E1_Hardware.SchDoc|ReportField=DocumentNumber~1|ReportField=DrawnBy~|ReportField=Engineer~Not shown in title block|ReportField=ImagePath~Not shown in title block|ReportField=IsUserConfigurable~|ReportField=ModifiedDate~7/24/2017|ReportField=Organization~Not shown in title block|ReportField=PageSetup~Record=PageOptions:CenterHorizontal=True:CenterVertical=True:PrintScale=1.00:XCorrection=1.00:YCorrection=1.00:PrintKind=0:BorderSize=5000000:LeftOffset=0:BottomOffset=0:Orientation=2:PaperLength=1000:PaperWidth=1000:Scale=100:PaperSource=15:PrintQuality=600:MediaType=1:DitherType=10:PaperKind=Letter:PrintScaleMode=1|ReportField=ProjectName~TIDA-01432E1.PrjPcb|ReportField=Revision~Use project parameter SCH_Rev|ReportField=Rule~|ReportField=SheetNumber~3|ReportField=SheetTotal~3|ReportField=Time~Not shown in title block|ReportField=Title~|ReportField=VersionControl_RevNumber~|ReportField=DataSourceFileName~TIDA-01432E1.PrjPcb|ReportField=DataSourceFullPath~X:\TID\Sabre\TIDA-01001-TIDA-01500\TIDA-01431-TIDA-01440\TIDA-01432 - Automotive USB Redriver (general release TIDA01256)\TIDA-01432\TIDA-01432E1 (7-24-2017 10-55-15 AM)\TIDA-01432E1.PrjPcb|ReportField=PCBConfigurationName~Bare PCB|ReportField=Item~|ReportField=ItemRevision~|ReportField=ItemAndRevision~|ReportField=ItemRevisionBase~|ReportField=ItemRevisionLevel1~|ReportField=ItemRevisionLevel2~|ReportField=ItemRevisionLevel1AndBase~|ReportField=ItemRevisionLevel2AndLevel1~
1|Fitted|Printed Circuit Board|!PCB|TIDA-01432|1|Any|||-|-
2|Fitted|CAP, CERM, 2.2 µF, 50 V, +/- 10%, X5R, 0805|C1|C2012X5R1H225K125AB|1|TDK|0805|2.2uF||
3|Fitted|CAP, CERM, 10uF, 50V, +/-10%, X7R, 1210|C5|GRM32ER71H106KA12L|1|MuRata|1210|10uF||
4|Fitted|CAP, CERM, 4700 pF, 100 V, +/- 5%, C0G/NP0, 0603|C6, C9|C0603C472J1GAC7867|2|Kemet|0603|4700pF||
5|Fitted|CAP, CERM, 0.01 µF, 10 V, +/- 10%, X5R, 0402|C7|GRM155R61A103KA01D|1|MuRata|0402|0.01uF||
6|Fitted|CAP, CERM, 4.7 µF, 35 V, +/- 10%, X5R, 0603|C8|C1608X5R1V475K080AC|1|TDK|0603|4.7uF||
7|Fitted|CAP, CERM, 12 pF, 25 V, +/- 5%, C0G/NP0, AEC-Q200 Grade 1, 0402|C10|C0402C120J3GACAUTO|1|Kemet|0402|12pF||
8|Fitted|CAP, AL, 470 µF, 50 V, +/- 20%, SMD|C13|EMVA500ATR471MKG5S|1|Chemi-Con|KG5|470uF||
9|Fitted|CAP, CERM, 10 µF, 10 V, +/- 10%, X7R, AEC-Q200 Grade 1, 1206_190|C14, C16, C17|GCM31CR71A106KA64L|3|MuRata|1206_190|10uF||
10|Fitted|CAP, CERM, 0.1 µF, 50 V, +/- 10%, X7R, 0603|C15, C18, C20, C21, C22, C23|GCM188R71H104KA57D|6|MuRata|0603|0.1uF||
11|Fitted|CAP, CERM, 2.2 µF, 25 V, +/- 10%, X5R, 0402|C19|C1005X5R1E225K050BC|1|TDK|0402|2.2uF||
12|Fitted|CAP, CERM, 0.1 µF, 50 V, +/- 10%, X7R, 0402|Cbias1|C1005X7R1H104K050BB|1|TDK|0402|0.1uF||
13|Fitted|CAP, CERM, 0.47 µF, 10 V, +/- 10%, X5R, 0402|Cboot1|C1005X5R1A474K050BB|1|TDK|0402|0.47uF||
14|Fitted|CAP, AL, 47 µF, 63 V, +/- 20%, 0.65 ohm, SMD|Cin1|EEE-FK1J470P|1|Panasonic|SMT Radial F|47uF||
15|Fitted|CAP, CERM, 10 µF, 50 V, +/- 10%, X7R, 1210|Cin2, Cin3|GRM32ER71H106KA12L|2|MuRata|1210|10uF||
16|Fitted|CAP, CERM, 0.047 µF, 50 V,+/- 10%, X7R, 0603|Cin4, Cin5|GRM188R71H473KA61D|2|MuRata|0603|0.047uF||
17|Fitted|CAP, CERM, 22 µF, 25 V, +/- 10%, X5R, 1210|COUT1, COUT2|GRM32ER61E226KE15L|2|MuRata|1210|22uF||
18|Fitted|CAP, AL, 120 µF, 10 V, +/- 20%, 0.025 ohm, SMD|COUT3|APXE100ARA121MF61G|1|Chemi-Con|F61|120uF||
19|Fitted|CAP, CERM, 0.047 µF, 25 V, +/- 10%, X7R, AEC-Q200 Grade 1, 0603|COUT4|GCM188R71E473KA37D|1|MuRata|0603|0.047uF||
20|Fitted|CAP, CERM, 3300 pF, 10 V, +/- 10%, X5R, 0201|Csnub1|GRM033R61A332KA01D|1|MuRata|0201|3300pF||
21|Fitted|Diode, TVS, Bi, 28 V, 45.4 Vc, SMB|D1|SMBJ28CA-13-F|1|Diodes Inc.|SMB|28V||
22|Fitted|Diode, TVS, Bi, 16 V, 400 W, SMA|D2, D3|SMAJ16CA|2|Littelfuse|SMA|16V||
23|Fitted|Diode, TVS, Uni, 5 V, 20 W, AEC-Q101, SOT-416|D4|ESDR0502BT1G|1|ON Semiconductor|SOT-416|5V||
24|Fitted|Fiducial mark.  There is nothing to buy or mount.|FID4|N/A|1|N/A|Fiducial|||
25|Fitted|RF Coaxial Connector, Bordeaux, R/A, TH|J1|99S20D-40MA5-D|1|Rosenberger|Right Angle Plug for PCB, 6-Lead, TH|||
26|Fitted|Receptacle, USB TYPE C, R/A, SMT|J2|201267-0001|1|Molex|Receptacle, USB TYPE C, R/A, SMT|||
27|Fitted|Inductor, Shielded, Composite, 10 µH, 4.9 A, 0.05 ohm, SMD|L1|XAL5050-103MEB|1|Coilcraft|XAL5050|10uH||
28|Fitted|Inductor, Shielded, Ferrite, 8.2 µH, 4.5 A, 0.0505 ohm, SMD|L2|SRP6540-8R2M|1|Bourns|Inductor, 7.2x4x6.5mm|8.2uH||
29|Fitted|Thermal Transfer Printable Labels, 0.650" W x 0.200" H - 10,000 per roll|LBL1|THT-14-423-10|1|Brady|PCB Label 0.650"H x 0.200"W||-|-
30|Fitted|MOSFET, N-CH, 40 V, 75 A, PowerPAK_SO-8L|Q1|SQJ422EP-T1-GE3|1|Vishay-Siliconix|PowerPAK_SO-8L|40V|None|
31|Fitted|RES, 0, 5%, 0.063 W, 0402|R1|CRCW04020000Z0ED|1|Vishay-Dale|0402|0||
32|Fitted|RES, 1.00 k, 1%, 0.1 W, 0402|R2|ERJ-2RKF1001X|1|Panasonic|0402|1.00k||
33|Fitted|RES, 0, 5%, 0.063 W, 0402|R3, R20|MCR01MZPJ000|2|Rohm|0402|0||
34|Fitted|RES, 5.11 k, 1%, 0.063 W, 0402|R4|CRCW04025K11FKED|1|Vishay-Dale|0402|5.11k||
35|Fitted|RES, 100 k, 1%, 0.063 W, AEC-Q200 Grade 0, 0402|R5, R6, R7, R8, R9|RMCF0402FT100K|5|Stackpole Electronics Inc|0402|100k||
36|Fitted|RES, 2.00 k, 1%, 0.063 W, 0402|R10|CRCW04022K00FKED|1|Vishay-Dale|0402|2.00k||
37|Fitted|RES, 15.4 k, 1%, 0.063 W, 0402|R11|CRCW040215K4FKED|1|Vishay-Dale|0402|15.4k||
38|Fitted|RES, 80.6 k, 1%, 0.063 W, 0402|R12|CRCW040280K6FKED|1|Vishay-Dale|0402|80.6k||
39|Fitted|RES, 200 k, 1%, 0.063 W, 0402|R13, R14, R16|CRCW0402200KFKED|3|Vishay-Dale|0402|200k||
40|Fitted|RES, 26.1 k, 1%, 0.063 W, 0402|R15|CRCW040226K1FKED|1|Vishay-Dale|0402|26.1k||
41|Fitted|RES, 1.00 k, 1%, 0.063 W, 0402|R17|CRCW04021K00FKED|1|Vishay-Dale|0402|1.00k||
42|Fitted|RES, 10.0 k, 1%, 0.063 W, 0402|R18|CRCW040210K0FKED|1|Vishay-Dale|0402|10.0k||
43|Fitted|RES, 49.9 k, 1%, 0.063 W, 0402|R19|CRCW040249K9FKED|1|Vishay-Dale|0402|49.9k||
44|Fitted|RES, 3.0, 5%, 0.063 W, 0402|Rbias1|CRCW04023R00JNED|1|Vishay-Dale|0402|3.0||
45|Fitted|RES, 2.94 k, 1%, 0.063 W, 0402|RFA1|CRCW04022K94FKED|1|Vishay-Dale|0402|2.94k||
46|Fitted|RES, 49.9 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0402|RFB1|ERJ-2RKF4992X|1|Panasonic|0402|49.9k||
47|Fitted|RES, 12.1 k, 1%, 0.063 W, 0402|RG1|CRCW040212K1FKED|1|Vishay-Dale|0402|12.1k||
48|Fitted|RES, 8.2, 5%, 0.063 W, 0402|Rsnub1|CRCW04028R20JNED|1|Vishay-Dale|0402|8.2||
49|Fitted|Test Point, Miniature, Red, TH|TP1, TP2|5000|2|Keystone|Red Miniature Testpoint|||
50|Fitted|Test Point, Miniature, Black, TH|TP3, TP5|5001|2|Keystone|Black Miniature Testpoint|||
51|Fitted|LMS3635AQRNLRQ1, RNL0022A (VQFN-HR-22)|U1|LMS3635AQRNLRQ1|1|Texas Instruments|RNL0022A||Texas Instruments|LMS3635AQRNLTQ1
52|Fitted|Automotive USB Charging Port Controller and Power Switch with Short to BAT protection, RVC0020A|U3|TPS254900IRVCRQ1|1|Texas Instruments|RVC0020A||Texas Instruments|TPS254900IRVCTQ1
53|Fitted|USB 2.0 HIGH SPEED SIGNAL CONDITIONER, RGY0014A (VQFN-14)|U4|TUSB213RGYR|1|Texas Instruments|RGY0014A||Texas Instruments|TUSB213RGYT
54|Fitted|USB Type-C DFP Port Controller, DRF0008A|U5|TUSB319DRFRQ1|1|Texas Instruments|DRF0008A||Texas Instruments|
55|Fitted|Single Inverter Gate, DCK0005A (SOT-5)|U6|SN74AHCT1G04DCKR|1|Texas Instruments|DCK0005A||Texas Instruments|SN74AHCT1G04DCKT
56|Fitted|Zero Iq Reverse Polarity Protection Smart Diode Controller, DGK0008A (VSSOP-8)|U7|LM74610QDGKRQ1|1|Texas Instruments|DGK0008A||Texas Instruments|
57|Not Fitted|Fiducial mark.  There is nothing to buy or mount.|FID1, FID2, FID3|N/A|0|N/A|Fiducial|||
