Field=#~Integer~#~50|Field=Fitted~String~Fitted~100|Field=Description~String~Description~100|Field=Designator~String~Designator~100|Field=PartNumber~String~PartNumber~100|Field=Quantity~Integer~Quantity~100|Field=Manufacturer~String~Manufacturer~100|Field=PackageReference~String~PackageReference~100|Field=Value~String~Value~100|ReportField=Currency~USD|ReportField=ProductionQuantity~100|ReportField=ProjectFileName~TIDA01411.PrjPCB|ReportField=ProjectFullPath~C:\Users\a0226506\Desktop\PennyProject\PoE\PSE\TPS23861\6kvLightningSurgesolution\TI_DesignDoc\TIDA01411\TIDA01411\TIDA01411.PrjPCB|ReportField=Title~PDF BOM (TI Designs format) For Variant [001] of Project [TIDA01411.PrjPCB] (No PCB Document Selected)|ReportField=TotalQuantity~243|ReportField=ReportTime~7:53:20 AM|ReportField=ReportDate~12/21/2017|ReportField=ReportDateTime~12/21/2017 7:53:20 AM|ReportField=OutputName~PDF BOM (TI Designs format)|ReportField=OutputType~BOM_PartType|ReportField=GeneratorName~BOM|ReportField=GeneratorDescription~Bill of Materials|ReportField=VariantName~001|ReportField=EVM_Orderable~TIDA-01411|ReportField=CopyrightYear~2017|ReportField=EVM-orderable~TIDA-01411|ReportField=PCB_Layout~P.Xu|ReportField=PCB_Rev~A|ReportField=PRJ_Customer~Public Release|ReportField=PRJ_Engineer~P.Xu|ReportField=PRJ_Number~TIDA-01411|ReportField=PRJ_Title~TPS23861 Four-Port Lightning Surge Board|ReportField=SCH_Rev~A|ReportField=TechSupport~http://www.ti.com/support|ReportField=TID~TIDA-01411|ReportField=Address1~Not shown in title block|ReportField=Address2~Not shown in title block|ReportField=Address3~Not shown in title block|ReportField=Address4~Not shown in title block|ReportField=Application_BuildNumber~|ReportField=ApprovedBy~Not shown in title block|ReportField=Author~Not shown in title block|ReportField=CheckedBy~Not shown in title block|ReportField=CompanyName~Not shown in title block|ReportField=ConfigurationParameters~|ReportField=ConfiguratorName~|ReportField=CurrentDate~12/21/2017|ReportField=CurrentTime~7:48:41 AM|ReportField=Date~Not shown in title block|ReportField=DocumentFullPathAndName~C:\Users\a0226506\Desktop\PennyProject\PoE\PSE\TPS23861\6kvLightningSurgesolution\TI_DesignDoc\TIDA01411\TIDA01411\TIDA01411_Hardware.SchDoc|ReportField=DocumentName~TIDA01411_Hardware.SchDoc|ReportField=DocumentNumber~4|ReportField=DrawnBy~|ReportField=Engineer~Not shown in title block|ReportField=ImagePath~Not shown in title block|ReportField=IsUserConfigurable~|ReportField=ModifiedDate~11/25/2017|ReportField=Organization~Not shown in title block|ReportField=PageSetup~Record=PageOptions:CenterHorizontal=True:CenterVertical=True:PrintScale=1.00:XCorrection=1.00:YCorrection=1.00:PrintKind=0:BorderSize=5000000:LeftOffset=0:BottomOffset=0:Orientation=2:PaperLength=1000:PaperWidth=1000:Scale=100:PaperSource=15:PrintQuality=600:MediaType=1:DitherType=10:PaperKind=Letter:PrintScaleMode=1|ReportField=ProjectName~TIDA01411.PrjPCB|ReportField=Revision~Use project parameter SCH_Rev|ReportField=Rule~|ReportField=SheetNumber~4|ReportField=SheetTotal~4|ReportField=Time~Not shown in title block|ReportField=Title~|ReportField=VersionControl_RevNumber~|ReportField=DataSourceFileName~TIDA01411.PrjPCB|ReportField=DataSourceFullPath~C:\Users\a0226506\Desktop\PennyProject\PoE\PSE\TPS23861\6kvLightningSurgesolution\TI_DesignDoc\TIDA01411\TIDA01411\TIDA01411.PrjPCB
1|Fitted|Printed Circuit Board|!PCB|TIDA-01411|1|Any||
2|Fitted|CAP, CERM, 0.01uF, 100V, +/-10%, X7R, 0603|C1|06031C103KAT2A|1|AVX|0603|0.01uF
3|Fitted|CAP, AL, 22 µF, 80 V, +/- 20%, 1.3 ohm, SMD|C2, C56, C57|EEE-FK1K220P|3|Panasonic|SMT Radial F|22uF
4|Fitted|CAP, CERM, 0.1uF, 100V, +/-10%, X7R, 0805|C3, C5, C23, C33, C43, C53|C2012X7R2A104K|6|TDK|0805|0.1uF
5|Fitted|CAP, CERM, 0.1uF, 50V, +/-10%, X7R, 0603|C4, C10, C11, C12, C13, C14, C16, C18, C20, C24, C26, C28, C30, C34, C36, C38, C40, C44, C46, C48, C50|06035C104KAT2A|21|AVX|0603|0.1uF
6|Fitted|CAP, CERM, 1uF, 100V, +/-10%, X7R, 1206|C6|GRM31CR72A105KA01L|1|MuRata|1206|1uF
7|Fitted|CAP, CERM, 1uF, 10V, +/-10%, X7R, 0805|C7, C9|0805ZC105KAT2A|2|AVX|0805|1uF
8|Fitted|CAP, CERM, 4.7uF, 10V, +/-10%, X5R, 0603|C8|0603ZD475KAT2A|1|AVX|0603|4.7uF
9|Fitted|CAP, CERM, 0.01uF, 100V, +/-10%, X7R, 0603|C15, C17, C19, C21, C25, C27, C29, C31, C35, C37, C39, C41, C45, C47, C49, C51|C1608X7R2A103K|16|TDK|0603|0.01uF
10|Fitted|CAP, CERM, 1000pF, 2000V, +/-10%, X7R, 1812|C22, C32, C42, C52|1812GC102KA1|4|AVX|1812|1000pF
11|Fitted|CAP, CERM, 2200 pF, 2000 V, +/- 10%, X7R, 1812|C54, C55|C4532X7R3D222K|2|TDK|1812|2200pF
12|Fitted|Diode, TVS, Uni, 58 V, 1500 W, SMC|D1|SMLJ58A|1|Diodes Inc.|SMC|58V
13|Fitted|Diode, TVS, Bi, 5 V, 350 W, SOD323, 2-Leads, Body 1.9x1.45mm, No Polarity Mark|D2, D3, D4, D5, D8, D9, D10, D11, D14, D15, D16, D17, D20, D21, D22, D23|CDSOD323-T05C|16|Bourns|SOD323, 2-Leads, Body 1.9x1.45mm, No Polarity Mark|5V
14|Fitted|Diode, TVS, Uni, 58 V, 3000 W, SMC|D6, D12, D18|SMLJ58A|3|Bourns|SMC|58V
15|Fitted|Diode, Schottky, 100V, 1.5A, SMA|D7, D13, D19|10MQ100NTRPBF|3|International Rectifier|SMA|0.68V
16|Fitted|ESD Suppressor Diode Arrays, 7V, SMD|D24|CD143A-SR70|1|Bourns|3.04X1.22X1.4|7V
17|Fitted|Fuse, 1.25 A, 600 VAC, SMD|F1, F2|B1250T|2|Bourns|9.65x3.05mm|
18|Fitted|Fuse, 1.5A, 63V, SMD|F3, F4|C1S 1.5|2|Bel Fuse|1206|
19|Fitted|Standoff, Hex, 1"L #6-32 Nylon, M-F|H1, H2, H3, H4, H5, H6|4820|6|Keystone|1" Nylon Hex Standoff|
20|Fitted|Terminal Block, 6A, 3.5mm Pitch, 2-Pos, TH|J1|ED555/2DS|1|On-Shore Technology|7.0x8.2x6.5mm|
21|Fitted|Header (shrouded), 100mil, 5x2, High-Temperature, Gold, TH|J2|N2510-6002-RB|1|3M|5x2 Shrouded header|
22|Fitted|RJ-45, Right Angle, No LED, tab up|J3, J6, J9, J12|1-406541-1|4|AMP|16.26x14.54x15.75|
23|Fitted|Header, 100mil, 8x1, Gold, TH|J4, J7, J10, J11|TSW-108-07-G-S|4|Samtec|8x1 Header|
24|Fitted|Terminal screw, vertical, snap-in|J5, J8|7693|2|Keystone|7693|15A
25|Fitted|Inductor, Drum Core, Ferrite, 180uH, 0.38A, 1.38 ohm, SMD|L1|SDR0604-181KL|1|Bourns|5.8x4.8x5.8mm|180uH
26|Fitted|Coupled inductor, 5A, 0.01 ohm, SMD|L2, L3, L4, L5|ACM7060-301-2PL-TL|4|TDK|6x3.5x7 mm|uH
27|Fitted|MOSFET, N-CH, 100V, 3.3A, 3.3x1x3.3mm|Q1, Q2, Q3, Q4|FDMC3612|4|Fairchild Semiconductor|3.3x1x3.3mm|100V
28|Fitted|RES, 47 ohm, 5%, 0.1W, 0603|R1, R7, R9, R12|CRCW060347R0JNEA|4|Vishay-Dale|0603|47
29|Fitted|RES, 47.5k ohm, 1%, 0.1W, 0603|R2|CRCW060347K5FKEA|1|Vishay-Dale|0603|47.5k
30|Fitted|RES, 200k ohm, 1%, 0.1W, 0603|R3|CRCW0603200KFKEA|1|Vishay-Dale|0603|200k
31|Fitted|RES, 22.1 ohm, 1%, 0.1W, 0603|R4, R8, R11, R14|CRCW060322R1FKEA|4|Vishay-Dale|0603|22.1
32|Fitted|RES, 10.0k ohm, 1%, 0.1W, 0603|R5, R15, R16, R17, R19|CRCW060310K0FKEA|5|Vishay-Dale|0603|10.0k
33|Fitted|RES, 4.99 ohm, 1%, 0.1W, 0603|R6|CRCW06034R99FKEA|1|Vishay-Dale|0603|4.99
34|Fitted|RES, 13.3k ohm, 1%, 0.1W, 0603|R10|CRCW060313K3FKEA|1|Vishay-Dale|0603|13.3k
35|Fitted|RES, 6.04k ohm, 1%, 0.1W, 0603|R13|CRCW06036K04FKEA|1|Vishay-Dale|0603|6.04k
36|Fitted|RES, 4.7k ohm, 5%, 0.1W, 0603|R18, R20, R80|CRCW06034K70JNEA|3|Vishay-Dale|0603|4.7k
37|Fitted|RES, 49.9, 1%, 0.125 W, 0805|R21, R22, R23, R24, R29, R30, R31, R32, R35, R36, R37, R38, R43, R44, R45, R46, R49, R50, R51, R52, R57, R58, R59, R60, R63, R64, R65, R66, R71, R72, R73, R74|CRCW080549R9FKEA|32|Vishay-Dale|0805|49.9
38|Fitted|RES, 75.0 ohm, 1%, 0.1W, 0603|R25, R26, R27, R28, R39, R40, R41, R42, R53, R54, R55, R56, R67, R68, R69, R70|CRCW060375R0FKEA|16|Vishay-Dale|0603|75.0
39|Fitted|RES, 0.51 ohm, 1%, 0.25W, 0805|R33, R34, R47, R48, R61, R62, R75, R76|CRM0805-FX-R510ELF|8|Bourns|0805|0.51
40|Fitted|RES, 0, 5%, 0.75 W, 2010|R77|CRCW20100000Z0EF|1|Vishay-Dale|2010|0
41|Fitted|Varistor, 324V, 6KA, Disc, 14mm, TH|RV1, RV2, RV3, RV4|V14E230P|4|Littelfuse|D17mm|324 - 396 V
42|Fitted|Varistor, 324V, 3.5KA, Disc, 10mm, TH|RV5, RV6, RV7, RV8|V10E230P|4|Littelfuse|D12.5mm|324 - 396 V
43|Fitted|Varistor, 324V, 1.75KA, Disc, 7mm, TH|RV9, RV10, RV11, RV12, RV13, RV14|V07E230P|6|Littelfuse|D9mm|324 - 396 V
44|Fitted|Transformer, 0.35 mH, SMT|T1, T2, T3, T4|PT61020EL|4|Bourns|SMD, 17.62x12.2mm|0.35 mH
45|Fitted|Test Point, Multipurpose, Red, TH|TP1, TP2, TP21|5010|3|Keystone|Red Multipurpose Testpoint|Red
46|Fitted|Test Point, Miniature, SMT|TP3, TP5, TP8, TP10, TP12, TP14, TP17, TP19|5015|8|Keystone|Testpoint_Keystone_Miniature|SMT
47|Fitted|Test Point, Multipurpose, Orange, TH|TP4, TP9, TP13, TP18|5013|4|Keystone|Orange Multipurpose Testpoint|Orange
48|Fitted|Test Point, Multipurpose, Black, TH|TP7, TP16|5011|2|Keystone|Black Multipurpose Testpoint|Black
49|Fitted|100V, 100mA Constant On-Time Synchronous Buck Regulator, DDA0008B|U1|LM5019MRX/NOPB|1|Texas Instruments|DDA0008B|
50|Fitted|QUAD IEEE 802.3at POWER-OVER-ETHERNET PSE CONTROLLER, PW0028A|U2|TPS23861PW|1|Texas Instruments|PW0028A|
51|Fitted|Optocoupler, 5kV RMS, SMT|U3|FOD817DS|1|Fairchild Semiconductor|DIP-4L Gullwing|
52|Fitted|5 Mbps Dual Channels, 1 / 1, Digital Isolator, 3.3 V / 5 V, -40 to +125 degC, 8-pin SOIC (D), Green (RoHS & no Sb/Br)|U4|ISO7221BD|1|Texas Instruments|D0008A|
53|Fitted|Low-Power Bidirectional I2C Isolators, D0008A|U5|ISO1541D|1|Texas Instruments|D0008A|
54|Fitted|TCS™ Dual Transient Current Suppressor, TCS-DL004-250|U6, U7, U8, U9, U10, U11, U12, U13, U14, U15, U16, U17|TCS-DL004-250-WH|12|Bourns|SMD, 4x2.5mm|
