Field=#~Integer~#~50|Field=Fitted~String~Fitted~150|Field=Description~String~Description~150|Field=Designator~String~Designator~150|Field=PartNumber~String~PartNumber~150|Field=Quantity~Integer~Quantity~150|Field=Manufacturer~String~Manufacturer~150|Field=Alternate Manufacturer~String~Alternate Manufacturer~150|Field=Alternate PartNumber~String~Alternate PartNumber~150|Field=PackageReference~String~PackageReference~150|Field=Value~String~Value~150|ReportField=Currency~USD|ReportField=ProductionQuantity~100|ReportField=ProjectFileName~TIDA-050024.PrjPCB|ReportField=ProjectFullPath~C:\1.0 TI work\3.1 TI reference design\2.1 TIDA-050024\TIDA-050024 PCB2\TIDA-050024.PrjPCB|ReportField=Title~BOM For Variant [one cell] of Project [TIDA-050024.PrjPCB] (No PCB Document Selected)|ReportField=TotalQuantity~151|ReportField=ReportTime~10:29:48 AM|ReportField=ReportDate~12/17/2018|ReportField=ReportDateTime~12/17/2018 10:29:48 AM|ReportField=OutputName~BOM|ReportField=OutputType~BOM_PartType|ReportField=GeneratorName~BOM|ReportField=GeneratorDescription~Bill of Materials|ReportField=VariantName~one cell|ReportField=CopyrightYear~2014|ReportField=PCB_Layout~Helen Chen|ReportField=PCB_Rev~A|ReportField=PRJ_Customer~Public Release|ReportField=PRJ_Engineer~Helen Chen|ReportField=PRJ_Number~TIDA-050024|ReportField=PRJ_Title~TIDA-050024|ReportField=SCH_Rev~A|ReportField=TechSupport~http://www.ti.com/support|ReportField=Address1~Not shown in title block|ReportField=Address2~Not shown in title block|ReportField=Address3~Not shown in title block|ReportField=Address4~Not shown in title block|ReportField=Application_BuildNumber~|ReportField=ApprovedBy~Not shown in title block|ReportField=Author~Not shown in title block|ReportField=CheckedBy~Not shown in title block|ReportField=CompanyName~TI|ReportField=ConfigurationParameters~|ReportField=ConfiguratorName~|ReportField=CurrentDate~12/17/2018|ReportField=CurrentTime~10:27:36 AM|ReportField=Date~Not shown in title block|ReportField=DocumentFullPathAndName~C:\1.0 TI work\3.1 TI reference design\2.1 TIDA-050024\TIDA-050024 PCB2\TIDA050024_1.SchDoc|ReportField=DocumentName~TIDA050024_1.SchDoc|ReportField=DocumentNumber~1|ReportField=DrawnBy~Helen Chen|ReportField=Engineer~Not shown in title block|ReportField=ImagePath~Not shown in title block|ReportField=IsUserConfigurable~|ReportField=ModifiedDate~12/17/2018|ReportField=Organization~Not shown in title block|ReportField=PageSetup~Record=PageOptions:CenterHorizontal=True:CenterVertical=True:PrintScale=0.68:XCorrection=1.00:YCorrection=1.00:PrintKind=0:BorderSize=5000000:LeftOffset=0:BottomOffset=0:Orientation=2:PaperLength=1000:PaperWidth=1000:Scale=100:PaperSource=15:PrintQuality=600:MediaType=1:DitherType=10:PaperKind=Letter:PrintScaleMode=1|ReportField=ProjectName~TIDA-050024.PrjPCB|ReportField=Revision~A|ReportField=Rule~|ReportField=SheetNumber~1|ReportField=SheetTotal~3|ReportField=Time~Not shown in title block|ReportField=Title~TIDA-050024|ReportField=VersionControl_RevNumber~|ReportField=DataSourceFileName~TIDA-050024.PrjPCB|ReportField=DataSourceFullPath~C:\1.0 TI work\3.1 TI reference design\2.1 TIDA-050024\TIDA-050024 PCB2\TIDA-050024.PrjPCB|ReportField=PCBConfigurationName~Bare PCB|ReportField=Item~|ReportField=ItemRevision~|ReportField=ItemAndRevision~|ReportField=ItemRevisionBase~|ReportField=ItemRevisionLevel1~|ReportField=ItemRevisionLevel2~|ReportField=ItemRevisionLevel1AndBase~|ReportField=ItemRevisionLevel2AndLevel1~
1|Fitted|Printed Circuit Board|!PCB1|TIDA-050024|1|Any|-|-||
2|Fitted|CAP, TA, 47 µF, 25 V, +/- 20%, 0.12 ohm, SMD|C1|T495D476M025ATE120|1|Kemet|||7343-31|47uF
3|Fitted|CAP, CERM, 22 µF, 25 V, +/- 10%, X5R, 1210|C2, C6, C7, C8, C9, C25|GRM32ER61E226KE15L|6|MuRata|||1210|22uF
4|Fitted|CAP, CERM, 10 µF, 25 V, +/- 20%, X5R, 0603|C3, C4, C17, C18, C20, C21|GRM188R61E106MA73D|6|MuRata|||0603|10uF
5|Fitted|CAP, CERM, 1 µF, 25 V,+/- 10%, X5R, 0402|C5, C22|C1005X5R1E105K050BC|2|TDK|||0402|1uF
6|Fitted|CAP, CERM, 100 pF, 50 V,+/- 5%, C0G/NP0, 0402|C10, C14, C23|GRM1555C1H101JA01D|3|MuRata|||0402|100pF
7|Fitted|CAP, CERM, 0.1 µF, 50 V,+/- 10%, X7R, AEC-Q200 Grade 1, 0402|C11, C12, C15, C16, C19|CGA2B3X7R1H104K050BB|5|TDK|||0402|0.1uF
8|Fitted|CAP, CERM, 0.022 µF, 25 V,+/- 10%, X7R, AEC-Q200 Grade 1, 0402|C13|GCM155R71E223KA55D|1|MuRata|||0402|0.022uF
9|Fitted|CAP, CERM, 1 µF, 25 V, +/- 10%, X5R, 0603|C26, C27, C31, C38, C41, C42, C43|GRM188R61E105KA12D|7|MuRata|||0603|1uF
10|Fitted|CAP, CERM, 0.1 µF, 50 V, +/- 10%, X7R, 0603|C29, C34, C35, C36, C37, C55|GCM188R71H104KA57D|6|MuRata|||0603|0.1uF
11|Fitted|CAP, CERM, 1000 pF, 50 V, +/- 5%, C0G/NP0, 0603|C30, C56|GRM1885C1H102JA01D|2|MuRata|||0603|1000pF
12|Fitted|CAP, CERM, 0.68 µF, 50 V, +/- 10%, X7R, 1206|C32, C39, C44, C51|GRM31MR71H684KA88L|4|MuRata|||1206|0.68uF
13|Fitted|CAP, CERM, 0.01 µF, 50 V, +/- 10%, X7R, 0603|C33, C40, C45, C52|GRM188R71H103KA01D|4|MuRata|||0603|0.01uF
14|Fitted|CAP, CERM, 47 pF, 50 V, +/- 5%, C0G/NP0, 0603|C46|GRM1885C1H470JA01D|1|MuRata|||0603|47pF
15|Fitted|CAP, CERM, 330 pF, 50 V, +/- 5%, C0G/NP0, 0603|C47, C48, C49, C50|GRM1885C1H331JA01D|4|MuRata|||0603|330pF
16|Fitted|CAP, AL, 220 µF, 35 V, +/- 20%, 0.09 ohm, TH|C53, C54|EEU-FC1V221|2|Panasonic|||10x12.5mm|220uF
17|Fitted|Diode, Zener, 4.3 V, 225 mW, SOT-23|D1|BZX84C4V3LT1G|1|ON Semiconductor|||SOT-23|4.3V
18|Fitted|Diode, Switching, 75 V, 0.3 A, SMD, 2-Leads, Body 1.2x0.8mm|D2, D3, D4|1N4148WT|3|Fairchild Semiconductor|||SMD, 2-Leads, Body 1.2x0.8mm|75V
19|Fitted|Heatsink FOR TI MOD, 50x13.9mm|H1|ATS-TI10P-521-C1-R1|1|Advanced Thermal Solutions|||HEAT SINK, 50x13.9mm|
20|Fitted|Machine Screw, Round, #4-40 x 1/4, Nylon, Philips panhead|H1, H2, H3, H4|NY PMS 440 0025 PH|4|B&F Fastener Supply|-|-|Screw|
21|Fitted|Terminal, Turret, TH, Double|J1, J2, J3, J4|1502-2|4|Keystone|||Keystone1502-2|
22|Fitted|Header, 100mil, 3x1, Gold, TH|J5, J6, J17|TSW-103-07-G-S|3|Samtec|||3x1 Header|
23|Fitted|Header, 100mil, 2x1, Gold, TH|J7, J8, JP1, JP2, JP3|TSW-102-07-G-S|5|Samtec|||2x1 Header|
24|Fitted|RCA Jack, Red, R/A, TH|J9|971|1|Keystone|||PC Mount Phono Jack-Red, TH|
25|Fitted|RCA Jack, White, R/A, TH|J10|970|1|Keystone|||PC Mount Phono Jack-White, TH|
26|Fitted|Binding Post, RED, TH|J11, J13|7006|2|Keystone|||11.4x27.2mm|
27|Fitted|Binding Post, BLACK, TH|J12, J14|7007|2|Keystone|||11.4x27.2mm|
28|Fitted|Terminal, Turret, TH, Double|J15|1502-2|1|Keystone|||Keystone1502-2|Double
29|Fitted|Header, 100mil, 3x1, Gold, TH|J16|PBC03SAAN|1|Sullins Connector Solutions|||PBC03SAAN|
30|Fitted|Inductor, Shielded, Composite, 3 µH, 21 A, 0.0059 ohm, SMD|L1|XAL1350-302MEB|1|Coilcraft|||13x14mm|3uH
31|Fitted|Inductor, Shielded, Powdered Iron, 2.2 µH, 2.3 A, 0.082 ohm, SMD|L2|DFE252012F-2R2M=P2|1|MuRata Toko|||2.5x1.2x2mm|2.2uH
32|Fitted|Inductor, Shielded, Ferrite, 10 µH, 4.2 A, 0.037 ohm, AEC-Q200 Grade 1, SMD|L11, L12, L21, L22|SRT8045-103MEB|4|Coilcraft|||8x8.4mm|10uH
33|Fitted|MOSFET, 2-CH, N-CH, 30 V, 35 A, DQY0008A (LSON-CLIP-8)|Q1|CSD87351Q5D|1|Texas Instruments|None||DQY0008A|30V
34|Fitted|Transistor, NPN, 45 V, 0.1 A, SOT-23|Q2, Q4|BC850CLT1G|2|ON Semiconductor|||SOT-23|45 V
35|Fitted|MOSFET, N-CH, 50 V, 0.22 A, SOT-23|Q3|BSS138|1|Fairchild Semiconductor|None||SOT-23|50V
36|Fitted|RES, 0.002, 1%, 2 W, 2512|R0|CSNL2512FT2L00|1|Stackpole Electronics Inc|||2512|0.002
37|Fitted|RES, 10.0, 1%, 0.063 W, 0402|R01, R02, R5, R6|CRCW040210R0FKED|4|Vishay-Dale|||0402|10.0
38|Fitted|RES, 49.9, 1%, 0.063 W, 0402|R1|CRCW040249R9FKED|1|Vishay-Dale|||0402|49.9
39|Fitted|RES, 200 k, 1%, 0.1 W, 0402|R2|ERJ-2RKF2003X|1|Panasonic|||0402|200k
40|Fitted|RES, 56.2 k, 1%, 0.063 W, 0402|R3|CRCW040256K2FKED|1|Vishay-Dale|||0402|56.2k
41|Fitted|RES, 7.50 k, 1%, 0.063 W, 0402|R7|CRCW04027K50FKED|1|Vishay-Dale|||0402|7.50k
42|Fitted|RES, 137 k, 1%, 0.063 W, 0402|R8|CRCW0402137KFKED|1|Vishay-Dale|||0402|137k
43|Fitted|RES, 100 k, 1%, 0.063 W, 0402|R9|CRCW0402100KFKED|1|Vishay-Dale|||0402|100k
44|Fitted|RES, 0, 0%, 0.25 W, AEC-Q200 Grade 0, 0603|R10, R11|RCS06030000Z0EA|2|Vishay-Dale|||0603|0
45|Fitted|RES, 0, 5%, 0.063 W, 0402|R13, R19, R27, Rg1, Rg2|CRCW04020000Z0ED|5|Vishay-Dale|||0402|0
46|Fitted|RES, 100 k, 0.5%, 0.063 W, 0402|R14, R18, R20|CRCW0402100KDHEDP|3|Vishay-Dale|||0402|100k
47|Fitted|RES, 10.2 k, 1%, 0.063 W, 0402|R15, R16, R21, R22|CRCW040210K2FKED|4|Vishay-Dale|||0402|10.2k
48|Fitted|RES, 3.01 k, 1%, 0.063 W, 0402|R17|CRCW04023K01FKED|1|Vishay-Dale|||0402|3.01k
49|Fitted|RES, 12.1, 1%, 0.063 W, 0402|R23|CRCW040212R1FKED|1|Vishay-Dale|||0402|12.1
50|Fitted|RES, 1.00 M, 1%, 0.1 W, 0402|R24|ERJ-2RKF1004X|1|Panasonic|||0402|1.00Meg
51|Fitted|RES, 16.9 k, 1%, 0.063 W, 0402|R25, R?|CRCW040216K9FKED|2|Vishay-Dale|||0402|16.9k
52|Fitted|RES, 10.5 k, 1%, 0.1 W, 0603|R26|CRCW060310K5FKEA|1|Vishay-Dale|||0603|10.5k
53|Fitted|RES, 39 k, 5%, 0.063 W, 0402|R28|CRCW040239K0JNED|1|Vishay-Dale|||0402|39k
54|Fitted|RES, 4.70 k, 0.1%, 0.1 W, 0603|R29|RG1608P-472-B-T5|1|Susumu Co Ltd|||0603|4.70k
55|Fitted|RES, 100k ohm, 1%, 0.1W, 0603|R30, R32, R37, R38, R44|RC0603FR-07100KL|5|Yageo America|||0603|100k
56|Fitted|RES, 499 k, 1%, 0.1 W, 0603|R31|RC0603FR-07499KL|1|Yageo America|||0603|499k
57|Fitted|RES, 10, 5%, 0.125 W, 0805|R33, R34, R35, R36|CRCW080510R0JNEA|4|Vishay-Dale|||0805|10
58|Fitted|RES, 3.3, 5%, 0.1 W, 0603|R39, R40, R41, R42|CRCW06033R30JNEA|4|Vishay-Dale|||0603|3.3
59|Fitted|RES, 0, 5%, 0.063 W, 0402|R43|ERJ-2GE0R00X|1|Panasonic|||0402|0
60|Fitted|Test Point, Miniature, Orange, TH|TP2, TP3, TP5, TP6, TP7|5003|5|Keystone|||Orange Miniature Testpoint|Orange
61|Fitted|Low Iq, Synchronous Boost Controller with Wide Input Voltage and 5.5V Gate Drive for Low Qg  NexFETs, RTE0016E (WQFN-16)|U1|TPS43061RTER|1|Texas Instruments|Texas Instruments|TPS43061RTET|RTE0016E|
62|Fitted|Low-Cost, Low Noise, 5.5 MHz CMOS Operational Amplifier, 2.2 to 5.5 V, -40 to 125 degC, 14-pin SOP (PW0014A), Green (RoHS & no Sb/Br)|U2|OPA4377AIPW|1|Texas Instruments|None|Equivalent|PW0014A|
63|Fitted|6.5-μA Quiescent Current, 1.8-A Switch Current Boost Converter, DBV0005A (SOT-23-5)|U3|TPS613222ADBVR|1|Texas Instruments|Texas Instruments|TPS613222ADBVT|DBV0005A|
64|Fitted|2x30-W Class-D Amplifier With Low Idle Power Dissipation, DAP0032A (TSSOP-32)|U4|TPA3128D2DAPR|1|Texas Instruments|Texas Instruments|TPA3128D2DAP|DAP0032A|
65|Not Fitted|RES, 20.5 k, 1%, 0.063 W, 0402|R27|CRCW040220K5FKED|0|Vishay-Dale|||0402|20.5k
