## Example Summary

The following example configures TimerA0 in periodic mode and
toggles GPIO every 1s using the repeat count feature.
NOTE: The repeat count feature is specific to the TimerA0 instance, and not the
other TimerA instances.

## Peripherals & Pin Assignments
- TIMA0
- GPIOB22   

## BoosterPacks, Board Resources & Jumper Settings
- GPIOB22
    
- Jumper settings:
    + J5  ON

## Example Usage
Compile, load the image by the LFU BSL GUI
LED2 will toggle every 1s.