
## Demo Summary

The demo is the bootloader code that used for live firmware update.

## Peripherals & Pin Assignments

- GPIOA
    + Open-drain Output: PA0

## BoosterPacks, Board Resources & Jumper Settings

-LP-MSPM0G3507

## Example Usage

Compile, load and run the example.
LED0 will blink every 0.5s.
