# TRF3302/TRF3302-Q1 S-parameters

## S-Parameters of device include the matching inductor that define L1 band operation (HB) or L2/L5 operation (LB)
 - Refer to the TRF3302EVM or TRF3302Q1EVM User's Guide for the component value

## S-Parameters are the same for TRF3302 and TRF3302-Q1

## S-Parameters are provided at different bias voltages (1.8v, 2.0v, 3.3v) and different operating temperature conditions (-40C, 27C, 85C, 125C)



