-1.00%

-0.50%

0.00%

0.50%

1.00%

-10 -8 -6 -4 -2 0 2 4 6 8 10

Total Error, Simulated (%)

Load Current under Sense (A)

Effects on Error via 1-point Calibration, High Side, 25°C

Error, Pre-Calibration Error, Post-Calibration