(---------------------------------------------------------------------)
(                                                                     )
(    Dangling Line, Via and Antenna Report                            )
(                                                                     )
(    Drawing          : CC1311-R3EM-5XD7793.brd                       )
(    Software Version : 17.2S056                                      )
(    Date/Time        : Tue Feb 23 16:25:58 2021                      )
(                                                                     )
(---------------------------------------------------------------------)


Report methodology:
  - Dangling lines have at least one end not connected.
  - Dangling vias have one or no connection
      - Plus are not a test, thieving or netshort property via.
  - Antenna vias do not have connections on their start and end layers.
      - Plus they are not a thieving vias.
      - Optionally, VOLTAGE nets, testvias and through vias can be suppressed with
        the environment variable report_antennavia.
      - Section may be suppressed by variable report_noantennavia.
  - Not part of the current partition.
  - To suppress items in dangle report add the OK_DANGLE property to the via
    or connect line.



<< Antenna Vias >>
  Net                  Padstack               Location            Layers
  ---------------------------------------------------------------------------
  VDDR                 VIA                  (122.800 104.850) TOP/BOTTOM 
  VDDR                 VIA                  (128.600 113.375) TOP/BOTTOM 
  VDDR                 VIA                  (125.240 116.337) TOP/BOTTOM 
  VDDS                 VIA                  (131.475 117.075) TOP/BOTTOM 
  VDDS                 VIA                  (134.900 106.875) TOP/BOTTOM 
  VDDS                 VIA                  (134.900 104.925) TOP/BOTTOM 
  VDDS                 VIA                  (115.875 111.225) TOP/BOTTOM 
  VDDS                 VIA                  (116.700 114.250) TOP/BOTTOM 
  VDDS                 VIA                  (126.162 112.114) TOP/BOTTOM 
  VDDS                 VIA                  (124.725 108.714) TOP/BOTTOM 

<< Summary >>
  Total dangling lines:       0
  Total dangling vias:        0
  Total antenna vias:        10
