## RFC_RAT

Instance: RFC_RAT
Component: RFC_RAT
Base address: 0x40043000

Component for rat register bank

### TOP:RFC_RAT Register Summary

Register Name | Type | Register Width (Bits) | Register Reset | Address Offset | Physical Address
RATCNT | RW | 32 | 0x0000 0000 | 0x0000 0004 | 0x4004 3004

### TOP:RFC_RAT Register Descriptions

### TOP:RFC_RAT:RATCNT

Address offset | 0x0000 0004
Physical address | 0x4004 3004 | Instance | RFC_RAT
Description | Radio Timer Counter Value
Type | RW

Bits | Field Name | Description | Type | Reset
31:0 | CNT | Counter value. This is not writable while radio timer counter is enabled. | RW | 0x0000 0000