CC26xx Driver Library |

- Main Page
- Related Pages
- CC26xx APIs
- Register Descriptions
- Online Resources

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Modules Pages
Functions
aon_rtc.c File Reference
`#include <driverlib/aon_rtc.h>`

Go to the source code of this file.

## Functions
uint32_t | AONRTCStatus (void)
| Check if the AON Real Time Clock is running. More...
void | AONRTCEventClear (uint32_t ui32Channel)
| Clear event from a specified channel. More...
bool | AONRTCEventGet (uint32_t ui32Channel)
| Get event status for a specified channel. More...
void | AONRTCModeCh1Set (uint32_t ui32Mode)
| Set operational mode of channel 1. More...
uint32_t | AONRTCModeCh1Get (void)
| Get operational mode of channel 1. More...
void | AONRTCModeCh2Set (uint32_t ui32Mode)
| Set operational mode of channel 2. More...
uint32_t | AONRTCModeCh2Get (void)
| Get operational mode of channel 2. More...
void | AONRTCChannelEnable (uint32_t ui32Channel)
| Enable event operation for the specified channel. More...
void | AONRTCChannelDisable (uint32_t ui32Channel)
| Disable event operation for the specified channel. More...
void | AONRTCCompareValueSet (uint32_t ui32Channel, uint32_t ui32CompValue)
| Set the compare value for the given channel. More...
uint32_t | AONRTCCompareValueGet (uint32_t ui32Channel)
| Get the compare value for the given channel. More...