(---------------------------------------------------------------------)
(                                                                     )
(    Dangling Line, Via and Antenna Report                            )
(                                                                     )
(    Drawing          : CC1352-P7EM-XD7793-XD24-PA24_10dBm.brd        )
(    Software Version : 17.2S056                                      )
(    Date/Time        : Tue Nov 24 10:52:55 2020                      )
(                                                                     )
(---------------------------------------------------------------------)


Report methodology:
  - Dangling lines have at least one end not connected.
  - Dangling vias have one or no connection
      - Plus are not a test, thieving or netshort property via.
  - Antenna vias do not have connections on their start and end layers.
      - Plus they are not a thieving vias.
      - Optionally, VOLTAGE nets, testvias and through vias can be suppressed with
        the environment variable report_antennavia.
      - Section may be suppressed by variable report_noantennavia.
  - Not part of the current partition.
  - To suppress items in dangle report add the OK_DANGLE property to the via
    or connect line.



<< Antenna Vias >>
  Net                  Padstack               Location            Layers
  ---------------------------------------------------------------------------
  N2095595             VIA                  (115.000 89.600) TOP/BOTTOM 
  N2095595             VIA                  (137.900 88.500) TOP/BOTTOM 
  N2095595             VIA                  (115.000 88.500) TOP/BOTTOM 
  RX_TX                VIA                  (129.700 120.125) TOP/BOTTOM 
  VDDR                 VIA                  (126.025 118.945) TOP/BOTTOM 
  VDDS                 VIA                  (130.525 106.887) TOP/BOTTOM 
  VDDS                 VIA                  (128.815 107.826) TOP/BOTTOM 
  NRESET               VIA                  (138.061 107.925) TOP/BOTTOM 
  NRESET               VIA                  (139.078 101.175) TOP/BOTTOM 

<< Summary >>
  Total dangling lines:       0
  Total dangling vias:        0
  Total antenna vias:         9
