- Main Page
- Data Structures
- Files

- File List
- Globals

# data_flash.c

Go to the documentation of this file.

    00001 //******************************************************************************
    00002 //THIS PROGRAM IS PROVIDED "AS IS". TI MAKES NO WARRANTIES OR
    00003 //REPRESENTATIONS, EITHER EXPRESS, IMPLIED OR STATUTORY,
    00004 //INCLUDING ANY IMPLIED WARRANTIES OF MERCHANTABILITY, FITNESS
    00005 //FOR A PARTICULAR PURPOSE, LACK OF VIRUSES, ACCURACY OR
    00006 //COMPLETENESS OF RESPONSES, RESULTS AND LACK OF NEGLIGENCE.
    00007 //TI DISCLAIMS ANY WARRANTY OF TITLE, QUIET ENJOYMENT, QUIET
    00008 //POSSESSION, AND NON-INFRINGEMENT OF ANY THIRD PARTY
    00009 //INTELLECTUAL PROPERTY RIGHTS WITH REGARD TO THE PROGRAM OR
    00010 //YOUR USE OF THE PROGRAM.
    00011 //
    00012 //IN NO EVENT SHALL TI BE LIABLE FOR ANY SPECIAL, INCIDENTAL,
    00013 //CONSEQUENTIAL OR INDIRECT DAMAGES, HOWEVER CAUSED, ON ANY
    00014 //THEORY OF LIABILITY AND WHETHER OR NOT TI HAS BEEN ADVISED
    00015 //OF THE POSSIBILITY OF SUCH DAMAGES, ARISING IN ANY WAY OUT
    00016 //OF THIS AGREEMENT, THE PROGRAM, OR YOUR USE OF THE PROGRAM.
    00017 //EXCLUDED DAMAGES INCLUDE, BUT ARE NOT LIMITED TO, COST OF
    00018 //REMOVAL OR REINSTALLATION, COMPUTER TIME, LABOR COSTS, LOSS
    00019 //OF GOODWILL, LOSS OF PROFITS, LOSS OF SAVINGS, OR LOSS OF
    00020 //USE OR INTERRUPTION OF BUSINESS. IN NO EVENT WILL TI'S
    00021 //AGGREGATE LIABILITY UNDER THIS AGREEMENT OR ARISING OUT OF
    00022 //YOUR USE OF THE PROGRAM EXCEED FIVE HUNDRED DOLLARS
    00023 //(U.S.$500).
    00024 //
    00025 //Unless otherwise stated, the Program written and copyrighted
    00026 //by Texas Instruments is distributed as "freeware".  You may,
    00027 //only under TI's copyright in the Program, use and modify the
    00028 //Program without any charge or restriction.  You may
    00029 //distribute to third parties, provided that you transfer a
    00030 //copy of this license to the third party and the third party
    00031 //agrees to these terms by its first use of the Program. You
    00032 //must reproduce the copyright notice and any other legend of
    00033 //ownership on each copy or partial copy, of the Program.
    00034 //
    00035 //You acknowledge and agree that the Program contains
    00036 //copyrighted material, trade secrets and other TI proprietary
    00037 //information and is protected by copyright laws,
    00038 //international copyright treaties, and trade secret laws, as
    00039 //well as other intellectual property laws.  To protect TI's
    00040 //rights in the Program, you agree not to decompile, reverse
    00041 //engineer, disassemble or otherwise translate any object code
    00042 //versions of the Program to a human-readable form.  You agree
    00043 //that in no event will you alter, remove or destroy any
    00044 //copyright notice included in the Program.  TI reserves all
    00045 //rights not specifically granted under this license. Except
    00046 //as specifically provided herein, nothing in this agreement
    00047 //shall be construed as conferring by implication, estoppel,
    00048 //or otherwise, upon you, any license or other right under any
    00049 //TI patents, copyrights or trade secrets.
    00050 //
    00051 //You may not use the Program in non-TI devices.
    00052 //
    00053 //This software has been submitted to export control regulations
    00054 //The ECCN is EAR99
    00055 //*****************************************************************************
    00069 #include "msp430.h"
    00070 #include "bq_pack.h"
    00071 #include "types.h"
    00072 #include "data_flash.h"
    00073
    00074
    00075
    00079 //Constant Array that stores the battery pack info on flash memory
    00080 const DWORD DATA_FLASH[] =
    00081 {
    00082   /*Cell Voltage*/
    00083   dCOV_THRESHOLD,                  //COV_THRESHOLD           [mV]
    00084   dCOV_RECOVERY_THRESHOLD,         //COV_RECOVERY_THRESHOLD  [mV]
    00085   dCOV_TIME,                       //COV_TIME                [100ms]
    00086   dCUV_THRESHOLD,                  //CUV_THRESHOLD           [mV]
    00087   dCUV_RECOVERY_THRESHOLD,         //CUV_RECOVERY_THRESHOLD  [mV]
    00088   dCUV_TIME,                       //CUV_TIME                [100ms]
    00089
    00090   /*Temperature*/
    00091   dPACK_OVER_TEMP1, //3 PACK_OVER_TEMP1   [st C]
    00092   dPACK_OT_TIME1,   //PACK_OT_TIME1       [ms]
    00093   dPACK_OVER_TEMP2,  //3 PACK_OVER_TEMP2   [st C]
    00094   dPACK_OT_TIME2,   //PACK_OT_TIME2       [ms]
    00095
    00096   /*Charge and Discharge*/
    00097   dPACK_END_OF_CHARGE_VOLTAGE,     //PACK_END_OF_CHARGE_VOLTAGE    [mV]
    00098   dCC_CV_QUAL_TIME,                //CC_CV_QUAL_TIME               [s]
    00099   dPACK_END_OF_DISCHARGE_VOLTAGE,  //PACK_END_OF_DISCHARGE_VOLTAGE [mV]
    00100   dEND_OF_DISCHARGE_QUAL_TIME,     //END_OF_DISCHARGE_QUAL_TIME    [s]
    00101   dCHARGE_CURRENT,                 //CHARGE_CURRENT                [mA]
    00102   dCHARGE_TAPER_CURRENT,           //CHARGE_TAPER_CURRENT          [mA]
    00103   dCHARGE_TAPER_TIME,              //CHARGE_TAPER_TIME             [s]
    00104   dMAX_CHARGE_TIME,                //MAX_CHARGE_TIME               [s]
    00105   dFULL_DISCHARGE_CLEAR_VOLTS,     //FULL_DISCHARGE_CLEAR_VOLTS    [mV]
    00106   dFULL_CHARGE_CLEAR_VOLTS,        //FULL_CHARGE_CLEAR_VOLTS       [mV]
    00107   dDELTA_CHARGE_V,                 //DELTA_CHARGE_V                [mv]
    00108   dCHARGE_DISCHARGE_TIME,          //CHARGE_DISCHARGE_TIME         [s]
    00109   dDELTA_DISCHARGE_V,              //DELTA_DISCHARGE_V             [mV]
    00110
    00111   /*Safety*/
    00112   dSOV_THRESHOLD,                 //SOV_THRESHOLD                 [mV]
    00113   dSOV_RECOVERY_THRESHOLD,        //SOV_RECOVERY_THRESHOLD        [mV]
    00114   dSOV_TIME,                      //SOV_TIME                      [ms]
    00115
    00116   /*Balancing*/
    00117   dCELL_IMBALANCE_FAIL_THRESHOLD,    //CELL_IMBALANCE_FAIL_THRESHOLD [mV]
    00118   dCELL_IMBALANCE_FAIL_TIME,         //CELL_IMBALANCE_FAIL_TIME      [s]
    00119   dBALANCE_TIME,                     //BALANCE_TIME     [s] max value is 63
    00120   dBALANCE_VOLTS_THRESHOLD,          //BALANCE_VOLTS_THRESHOLD       [mV]
    00121   dMIN_BALANCE_VOLTS,                //MIN_BALANCE_VOLTS             [mV]
    00122   dMAX_BALANCE_TIME,                 //MAX_BALANCE_TIME              [s]
    00123
    00124 };
    00125
    00126
    00134 unsigned short get_u16_value(param_id_t param_id)
    00135 {
    00136
    00137   return (unsigned short)DATA_FLASH[param_id];
    00138
    00139 }
    00140
    00148 DWORD get_u32_value(param_id_t param_id)
    00149 {
    00150   return (DWORD)DATA_FLASH[param_id];
    00151 }
    00152
    00153 /*EOF*/