Defines | Functions

# TLV_descriptors.h File Reference

This file contains definitions for the Hardware Abstraction Layer (HAL) specifically created for the MSP430. More...

Go to the source code of this file.

## Defines
#define | __MSP430_HAS_TLV__
#define | TLV_START (0x1A08)
#define | TLV_END (0x1AFF)
#define | TLV_LDTAG (0x01)
#define | TLV_PDTAG (0x02)
#define | TLV_Reserved1 (0x03)
#define | TLV_Reserved2 (0x04)
#define | TLV_BLANK (0x05)
#define | TLV_Reserved3 (0x06)
#define | TLV_SERNUM (0x07)
#define | TLV_DIERECORD (0x08)
#define | TLV_ADCCAL (0x10)
#define | TLV_TAGEXT (0xFE)
#define | TLV_TAGEND (0xFF)
## Functions
void | Get_TLV_info (unsigned char tag, unsigned char *length, unsigned int *data_address)

## Detailed Description

This file contains definitions for the Hardware Abstraction Layer (HAL) specifically created for the MSP430.

Author:
  Texas Instruments, Inc

Date:
  November 2010

Version:
  1.0 Initial version

Note:
  Built with IAR for MSP430 Version: 5.10

Definition in file TLV_descriptors.h.