DRC Rules Export File for PCB: D:\PCB\Active Boards\ADC36xxEVM Refresh\ADC3644EVM\Design Data\ADC3644EVM.PcbDoc
RuleKind=Clearance|RuleName=Clearance-CMOS|Scope=Board|Minimum=5.00
RuleKind=Width|RuleName=Width|Scope=Board|Minimum=5.00
RuleKind=ShortCircuit|RuleName=ShortCircuit|Scope=Board|Allowed=0
RuleKind=SolderMaskExpansion|RuleName=SolderMaskExpansion|Scope=Board|Minimum=1.97
RuleKind=Clearance|RuleName=Clearance_Inner_Layers|Scope=Board|Minimum=5.00
RuleKind=Clearance|RuleName=Clearance_Outter_Layers|Scope=Board|Minimum=5.00
RuleKind=Clearance|RuleName=Clearance_FiducialMark|Scope=Board|Minimum=0.00
RuleKind=Clearance|RuleName=Clearance_Poly|Scope=Board|Minimum=5.00
RuleKind=Clearance|RuleName=Clearance_Keepouts|Scope=Board|Minimum=0.00
RuleKind=Clearance|RuleName=Clearance_Poly_GND|Scope=Board|Minimum=5.00
