UNITS=INCH
#
#Component attribute names
#
@0 .comp_mount_type
@1 .comp_height
@2 .no_pop
@3 .comp_ignore
@4 .comp_variant_list

#
#Component attribute text strings
#

# CMP 0
CMP 0 3.5239178 0.7207675 225 N R146 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 3.5317127 0.7129726 135 N 199 2 1
TOP 1 3.5161229 0.7285624 135 N 3 1 2
#
# CMP 1
CMP 17 1.7425155 1.6904877 315 N SW5 CHS-02TA ;0=1,1=0.1902
PRP Alt_Manufacturer ''
PRP Alt_PartNumber ''
PRP CompType 'Swtich'
PRP Manufacturer 'Nidec Components Corporation'
PRP PartNumber 'CHS-02TA'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '563-1005-1-ND'
PRP Text1 'HIGH'
PRP Text2 'LOW'
PRP Text3 ''
PRP Text4 'CTRL'
TOP 0 1.6541272 1.7435252 315 N 6 1 1
TOP 1 1.6894825 1.7788806 135 N 5 1 2
TOP 2 1.8309084 1.6374547 135 N 114 4 3
TOP 3 1.795553 1.6020994 315 N 114 3 4
#
# CMP 2
CMP 40 2.6724623 1.8888757 90 N J12 TSW-103-14-L-S ;0=2,1=0.3300
PRP Alt_Manufacturer 'Sullins Connector Solutions'
PRP Alt_PartNumber 'PBC03SAAN'
PRP Color '-'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.sullinscorp.com/catalogs/77_PAGE108-109_.100_MALE_HDR.pdf'
PRP CompType 'Header'
PRP Current_Rating_(Amps) '-'
PRP datasheet 'https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf'
PRP Length_(in) '-'
PRP Manufacturer 'Samtec'
PRP Mount_Type 'TH'
PRP PackageReference '-'
PRP PartNumber 'TSW-103-14-L-S'
PRP Pitch_(mm) '2.54'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'S1011E-03-ND'
PRP Text1 '1p8V'
PRP Text2 'SMA'
PRP Text3 'FMC'
PRP UniqueID 'cmp00015'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 2.6724623 1.9888757 90 N 12 1 1
TOP 1 2.6724623 1.8888757 90 N 11 3 2
TOP 2 2.6724623 1.7888757 90 N 115 1 3
#
# CMP 3
CMP 4 1.0089769 2.0886156 270 N C45 GRT155R71E104KE01J ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet '-'
PRP Manufacturer 'Murata'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0402'
PRP PartNumber 'GRT155R71E104KE01J'
PRP Ratings '-'
PRP Series '-'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Digi-key'
PRP Supplier_Part_Number_1 '490-GRT155R71E104KE01JCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±10%'
PRP UniqueID 'capcc09401'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '25V'
TOP 0 1.0089769 2.0689306 180 N 248 413 1
TOP 1 1.0089769 2.1083007 180 N 238 65 2
#
# CMP 4
CMP 4 1.2421659 2.3235959 0 N C44 GRT155R71E104KE01J ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet '-'
PRP Manufacturer 'Murata'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0402'
PRP PartNumber 'GRT155R71E104KE01J'
PRP Ratings '-'
PRP Series '-'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Digi-key'
PRP Supplier_Part_Number_1 '490-GRT155R71E104KE01JCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±10%'
PRP UniqueID 'capcc09401'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '25V'
TOP 0 1.2224809 2.3235959 270 N 248 414 1
TOP 1 1.261851 2.3235959 270 N 238 66 2
#
# CMP 5
CMP 10 2.8484467 0.0987195 180 N SW3 cmp00353 ;0=2,1=0.2559
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color '-'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.ckswitches.com/media/1429/1000.pdf'
PRP CompType 'Switch Slide'
PRP Current_Rating_(Amps) '-'
PRP datasheet 'https://www.mouser.com/datasheet/2/445/450301014042-1717397.pdf'
PRP Length_(in) '-'
PRP Manufacturer 'Wurth Elektronik'
PRP Mount_Type 'TH'
PRP PackageReference '-'
PRP PartNumber '450301014042'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Supplier_1 'Mouser'
PRP Supplier_Part_Number_1 '710-450301014042'
PRP Text1 'DCLKIN'
PRP Text2 'FMC'
PRP Text3 'SMA'
PRP UniqueID 'cmp00353'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 2.8484467 0.0987195 180 N 13 1 1
TOP 1 2.9484467 0.0987195 180 N 14 1 2
TOP 2 2.7484467 0.0987195 180 N 248 453 3
#
# CMP 6
CMP 44 2.1856907 1.2487976 0 N U1 ADC3644IRSB ;0=1,1=0.0315
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber 'ADC3644IRSBR'
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/adc3644.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/adc3644'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/adc3644/datasheet'
PRP CompType 'ADC'
PRP Manufacturer 'Texas Instruments'
PRP PartNumber 'ADC3644IRSBT'
TOP 0 2.0912025 1.3196638 270 N 119 1 1
TOP 1 2.0912025 1.3039158 270 N 109 5 2
TOP 2 2.0912025 1.2881677 270 N 248 401 3
TOP 3 2.0912025 1.2724197 270 N 114 2 4
TOP 4 2.0912025 1.2566717 270 N 171 8 5
TOP 5 2.0912025 1.2409236 270 N 162 2 6
TOP 6 2.0912025 1.2251756 270 N 163 2 7
TOP 7 2.0912025 1.2094276 270 N 110 11 8
TOP 8 2.0912025 1.1936795 270 N 84 1 9
TOP 9 2.0912025 1.1779315 270 N 117 1 10
TOP 10 2.1148246 1.1543094 0 N 248 402 11
TOP 11 2.1305726 1.1543094 0 N 166 1 12
TOP 12 2.1463207 1.1543094 0 N 167 1 13
TOP 13 2.1620687 1.1543094 0 N 248 403 14
TOP 14 2.1778167 1.1543094 0 N 171 9 15
TOP 15 2.1935648 1.1543094 0 N 83 1 16
TOP 16 2.2093128 1.1543094 0 N 67 1 17
TOP 17 2.2250608 1.1543094 0 N 66 1 18
TOP 18 2.2408089 1.1543094 0 N 65 1 19
TOP 19 2.2565569 1.1543094 0 N 64 1 20
TOP 20 2.2801789 1.1779315 270 N 102 7 21
TOP 21 2.2801789 1.1936795 270 N 63 1 22
TOP 22 2.2801789 1.2094276 270 N 62 1 23
TOP 23 2.2801789 1.2251756 270 N 61 1 24
TOP 24 2.2801789 1.2409236 270 N 68 1 25
TOP 25 2.2801789 1.2566717 270 N 248 404 26
TOP 26 2.2801789 1.2724197 270 N 54 1 27
TOP 27 2.2801789 1.2881677 270 N 55 1 28
TOP 28 2.2801789 1.3039158 270 N 56 1 29
TOP 29 2.2801789 1.3196638 270 N 102 8 30
TOP 30 2.2565569 1.3432858 0 N 57 1 31
TOP 31 2.2408089 1.3432858 0 N 58 1 32
TOP 32 2.2250608 1.3432858 0 N 59 1 33
TOP 33 2.2093128 1.3432858 0 N 60 1 34
TOP 34 2.1935648 1.3432858 0 N 118 1 35
TOP 35 2.1778167 1.3432858 0 N 171 10 36
TOP 36 2.1620687 1.3432858 0 N 248 405 37
TOP 37 2.1463207 1.3432858 0 N 165 1 38
TOP 38 2.1305726 1.3432858 0 N 164 1 39
TOP 39 2.1148246 1.3432858 0 N 248 406 40
TOP 40 2.1856907 1.2487977 0 N 248 407 41
TOP 41 2.1856907 1.1948606 90 N 248 484 41
TOP 42 2.1317537 1.2487976 180 N 248 485 41
TOP 43 2.1856907 1.3027346 270 N 248 486 41
TOP 44 2.2396277 1.2487976 0 N 248 487 41
TOP 45 2.1856907 1.2487976 0 N 248 488 41
#
# CMP 7
CMP 7 0.7687398 1.3558047 90 N C27 GRM188R60J476ME15D ;0=1,1=0.0394
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP Manufacturer 'Murata'
PRP Operating_Temperature '-55°C ~ 85°C'
PRP PackageReference '0603'
PRP PartNumber 'GRM188R60J476ME15D'
PRP Ratings '-'
PRP Series '-'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.81'
PRP SizeZ_mm '0.9'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '490-13247-1-ND'
PRP Temperature_Coefficient 'X5R'
PRP Tolerance '±20%'
PRP Value '47 uF'
PRP Voltage_-_Rated '6.3V'
TOP 0 0.7687398 1.3833638 0 N 248 380 1
TOP 1 0.7687398 1.3282457 0 N 102 6 2
#
# CMP 8
CMP 1 2.0511789 1.2989158 0 N C84 GRM033Z71C104ME14D ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033Z71C104ME14-01.pdf'
PRP Manufacturer 'Murata Electronics'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'GRM033Z71C104ME14D'
PRP Ratings '-'
PRP Series 'GRM'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.33'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '490-GRM033Z71C104ME14DCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±20%'
PRP UniqueID 'capcc09270'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '16V'
TOP 0 2.0401553 1.2989158 270 N 248 377 1
TOP 1 2.0622025 1.2989158 270 N 109 4 2
#
# CMP 9
CMP 0 2.6323062 1.0519467 0 N R158 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.6212826 1.0519467 270 N 43 2 1
TOP 1 2.6433298 1.0519467 270 N 28 1 2
#
# CMP 10
CMP 0 2.8829694 1.2714821 0 N R181 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.8719458 1.2714821 270 N 17 0 1
TOP 1 2.893993 1.2714821 270 N 70 2 2
#
# CMP 11
CMP 0 2.6323062 1.2714821 0 N R180 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.6212826 1.2714821 270 N 35 1 1
TOP 1 2.6433298 1.2714821 270 N 17 1 2
#
# CMP 12
CMP 0 2.9055346 1.2941671 0 N R179 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.894511 1.2941671 270 N 18 0 1
TOP 1 2.9165582 1.2941671 270 N 71 2 2
#
# CMP 13
CMP 0 2.609741 1.2941671 0 N R178 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.5987174 1.2941671 270 N 36 1 1
TOP 1 2.6207646 1.2941671 270 N 18 1 2
#
# CMP 14
CMP 0 2.8829696 1.3275372 0 N R177 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.871946 1.3275372 270 N 19 0 1
TOP 1 2.8939932 1.3275372 270 N 72 2 2
#
# CMP 15
CMP 0 2.6323062 1.3275372 0 N R176 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.6212826 1.3275372 270 N 37 1 1
TOP 1 2.6433298 1.3275372 270 N 19 1 2
#
# CMP 16
CMP 0 2.9055346 1.3835924 0 N R175 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.894511 1.3835924 270 N 20 0 1
TOP 1 2.9165582 1.3835924 270 N 74 2 2
#
# CMP 17
CMP 0 2.6323062 1.3865924 0 N R174 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.6212826 1.3865924 270 N 46 1 1
TOP 1 2.6433298 1.3865924 270 N 20 1 2
#
# CMP 18
CMP 0 2.8829694 1.4062774 0 N R173 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.8719458 1.4062774 270 N 21 0 1
TOP 1 2.893993 1.4062774 270 N 73 2 2
#
# CMP 19
CMP 0 2.609741 1.4092774 0 N R172 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.5987174 1.4092774 270 N 38 1 1
TOP 1 2.6207646 1.4092774 270 N 21 1 2
#
# CMP 20
CMP 0 2.9056033 1.4426475 0 N R171 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.8945797 1.4426475 270 N 22 0 1
TOP 1 2.9166269 1.4426475 270 N 53 2 2
#
# CMP 21
CMP 0 2.6323062 1.4456475 0 N R170 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.6212826 1.4456475 270 N 48 1 1
TOP 1 2.6433298 1.4456475 270 N 22 1 2
#
# CMP 22
CMP 0 2.8830381 1.4653325 0 N R169 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.8720145 1.4653325 270 N 23 0 1
TOP 1 2.8940617 1.4653325 270 N 75 2 2
#
# CMP 23
CMP 0 2.609741 1.4683325 0 N R168 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.5987174 1.4683325 270 N 47 1 1
TOP 1 2.6207646 1.4683325 270 N 23 1 2
#
# CMP 24
CMP 0 2.9055346 1.248797 0 N R167 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.894511 1.248797 270 N 24 0 1
TOP 1 2.9165582 1.248797 270 N 69 2 2
#
# CMP 25
CMP 0 2.609741 1.248797 0 N R166 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.5987174 1.248797 270 N 34 1 1
TOP 1 2.6207646 1.248797 270 N 24 1 2
#
# CMP 26
CMP 0 2.8829694 1.226112 0 N R165 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.8719458 1.226112 270 N 25 0 1
TOP 1 2.893993 1.226112 270 N 76 2 2
#
# CMP 27
CMP 0 2.6323062 1.226112 0 N R164 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.6212826 1.226112 270 N 39 1 1
TOP 1 2.6433298 1.226112 270 N 25 1 2
#
# CMP 28
CMP 0 2.8829694 1.1927419 0 N R163 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.8719458 1.1927419 270 N 26 0 1
TOP 1 2.893993 1.1927419 270 N 77 2 2
#
# CMP 29
CMP 0 2.609741 1.1927419 0 N R162 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.5987174 1.1927419 270 N 40 1 1
TOP 1 2.6207646 1.1927419 270 N 26 1 2
#
# CMP 30
CMP 0 2.9055346 1.1700569 0 N R161 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.894511 1.1700569 270 N 27 0 1
TOP 1 2.9165582 1.1700569 270 N 78 2 2
#
# CMP 31
CMP 0 2.6323062 1.1700569 0 N R160 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.6212826 1.1700569 270 N 41 1 1
TOP 1 2.6433298 1.1700569 270 N 27 1 2
#
# CMP 32
CMP 0 2.9055346 1.0519467 0 N R159 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.894511 1.0519467 270 N 28 0 1
TOP 1 2.9165582 1.0519467 270 N 80 2 2
#
# CMP 33
CMP 8 2.960748 1.5771087 180 N R109 ERJ-6GEY0R00V ;0=1,1=0.0571
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ6GEY0R00V'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0805'
PRP PartNumber 'ERJ-6GEY0R00V'
PRP Power_(Watts) '0.125W, 1/8W'
PRP Ratings 'AEC-Q200'
PRP Resistance '0 O'
PRP Series 'ERJ-6G'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P0.0ACT-ND'
PRP Temperature_Coefficient '-'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD080510615'
PRP Value '0 O'
TOP 0 2.9902756 1.5771087 90 N 0 218 1
TOP 1 2.9312205 1.5771087 90 N 0 219 2
#
# CMP 34
CMP 0 2.8829694 1.0746317 0 N R157 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.8719458 1.0746317 270 N 29 0 1
TOP 1 2.893993 1.0746317 270 N 79 2 2
#
# CMP 35
CMP 0 2.609741 1.0746317 0 N R156 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.5987174 1.0746317 270 N 42 1 1
TOP 1 2.6207646 1.0746317 270 N 29 1 2
#
# CMP 36
CMP 0 2.9055346 1.1110018 0 N R155 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.894511 1.1110018 270 N 30 0 1
TOP 1 2.9165582 1.1110018 270 N 81 2 2
#
# CMP 37
CMP 0 2.6323062 1.1110018 0 N R154 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.6212826 1.1110018 270 N 44 1 1
TOP 1 2.6433298 1.1110018 270 N 30 1 2
#
# CMP 38
CMP 0 2.8829694 1.1336868 0 N R153 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.8719458 1.1336868 270 N 31 0 1
TOP 1 2.893993 1.1336868 270 N 82 2 2
#
# CMP 39
CMP 0 2.609741 1.1336868 0 N R152 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.5987174 1.1336868 270 N 45 1 1
TOP 1 2.6207646 1.1336868 270 N 31 1 2
#
# CMP 40
CMP 0 2.633976 1.5102933 0 N R182 ERJ-1GNJ123C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://b2b-api.panasonic.eu/file_stream/pids/fileversion/1242'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GNJ123C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '12 kO'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P123235CT-ND'
PRP Temperature_Coefficient '±200ppm/°C'
PRP Tolerance '±5%'
PRP UniqueID 'RSMD020101206'
PRP Value '12 kO'
TOP 0 2.6229524 1.5102933 270 N 248 333 1
TOP 1 2.6449996 1.5102933 270 N 32 5 2
#
# CMP 41
CMP 0 2.6560232 1.5102933 0 N R151 ERJ-1GNJ123C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://b2b-api.panasonic.eu/file_stream/pids/fileversion/1242'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GNJ123C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '12 kO'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P123235CT-ND'
PRP Temperature_Coefficient '±200ppm/°C'
PRP Tolerance '±5%'
PRP UniqueID 'RSMD020101206'
PRP Value '12 kO'
TOP 0 2.6449996 1.5102933 270 N 32 6 1
TOP 1 2.6670468 1.5102933 270 N 33 8 2
#
# CMP 42
CMP 4 2.57 1.1208443 270 N C92 GRT155R71E104KE01J ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet '-'
PRP Manufacturer 'Murata'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0402'
PRP PartNumber 'GRT155R71E104KE01J'
PRP Ratings '-'
PRP Series '-'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Digi-key'
PRP Supplier_Part_Number_1 '490-GRT155R71E104KE01JCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±10%'
PRP UniqueID 'capcc09401'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '25V'
TOP 0 2.57 1.1011593 180 N 248 378 1
TOP 1 2.57 1.1405294 180 N 33 12 2
#
# CMP 43
CMP 4 2.9452756 1.1208443 270 N C91 GRT155R71E104KE01J ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet '-'
PRP Manufacturer 'Murata'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0402'
PRP PartNumber 'GRT155R71E104KE01J'
PRP Ratings '-'
PRP Series '-'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Digi-key'
PRP Supplier_Part_Number_1 '490-GRT155R71E104KE01JCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±10%'
PRP UniqueID 'capcc09401'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '25V'
TOP 0 2.9452756 1.1011593 180 N 248 334 1
TOP 1 2.9452756 1.1405294 180 N 33 9 2
#
# CMP 44
CMP 4 2.9402756 1.3373797 270 N C90 GRT155R71E104KE01J ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet '-'
PRP Manufacturer 'Murata'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0402'
PRP PartNumber 'GRT155R71E104KE01J'
PRP Ratings '-'
PRP Series '-'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Digi-key'
PRP Supplier_Part_Number_1 '490-GRT155R71E104KE01JCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±10%'
PRP UniqueID 'capcc09401'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '25V'
TOP 0 2.9402756 1.3176947 180 N 248 335 1
TOP 1 2.9402756 1.3570648 180 N 33 10 2
#
# CMP 45
CMP 4 2.575 1.3373797 270 N C89 GRT155R71E104KE01J ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet '-'
PRP Manufacturer 'Murata'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0402'
PRP PartNumber 'GRT155R71E104KE01J'
PRP Ratings '-'
PRP Series '-'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Digi-key'
PRP Supplier_Part_Number_1 '490-GRT155R71E104KE01JCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±10%'
PRP UniqueID 'capcc09401'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '25V'
TOP 0 2.575 1.3176947 180 N 248 336 1
TOP 1 2.575 1.3570648 180 N 33 11 2
#
# CMP 46
CMP 32 2.0050801 1.4253654 45 N J13 GRPB021VWVN-RC ;0=2,1=0.1570
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color '-'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.sullinscorp.com/catalogs/77_PAGE108-109_.100_MALE_HDR.pdf'
PRP CompType 'Header'
PRP Current_Rating_(Amps) '-'
PRP datasheet 'http://www.sullinscorp.com/catalogs/71_Page70-71_HEADER_.050_1.27mm_MALE.pdf'
PRP Length_(in) '-'
PRP Manufacturer 'Sullins Connector Solutions'
PRP Mount_Type 'TH'
PRP PackageReference '-'
PRP PartNumber 'GRPB021VWVN-RC'
PRP Pitch_(mm) '1.27'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'S9014E-02-ND'
PRP Text1 'VREF'
PRP Text2 'DUT'
PRP UniqueID 'cmp00298'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 1.9874024 1.4430431 45 N 10 1 1
TOP 1 2.0227578 1.4076877 45 N 109 6 2
#
# CMP 47
CMP 0 3.3253942 1.3082674 0 N R141 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 3.3143705 1.3082674 270 N 115 0 1
TOP 1 3.3364179 1.3082674 270 N 51 1 2
#
# CMP 48
CMP 30 0.1088189 2.2571785 90 N J3 USB4105-GF-A ;0=1,1=0.4400
PRP Alternate_PartNumber ''
PRP CompType 'USB C'
PRP Manufacturer 'GCT'
PRP PartNumber 'USB4105-GF-A'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '2073-USB4105-GF-ACT-ND'
PRP Supplier_Part_Number_2 '640-USB4105-GF-A'
TOP 0 0.2275196 2.4272572 90 N 248 465 1
TOP 1 0.2275196 2.0870998 90 N 248 464 2
TOP 2 0.0629528 2.4272572 90 N 248 467 3
TOP 3 0.0629528 2.0870998 90 N 248 466 4
TOP 4 0.2501575 2.3831628 90 N 248 389 A1
TOP 5 0.2501575 2.3516667 90 N 87 3 A4
TOP 6 0.2501575 2.3063911 90 N 0 222 A5
TOP 7 0.2501575 2.267021 90 N 86 2 A6
TOP 8 0.2501575 2.247336 90 N 85 1 A7
TOP 9 0.2501575 2.2079659 90 N 0 223 A8
TOP 10 0.2501575 2.1311942 90 N 248 388 B1
TOP 11 0.2501575 2.1626903 90 N 87 2 B4
TOP 12 0.2501575 2.1882809 90 N 0 224 B5
TOP 13 0.2501575 2.2276509 90 N 86 1 B6
TOP 14 0.2501575 2.2867061 90 N 85 2 B7
TOP 15 0.2501575 2.3260761 90 N 0 221 B8
TOP 16 0.2078346 2.370958 90 N 0 257 empty-1
TOP 17 0.2078346 2.143399 90 N 0 258 empty-2
#
# CMP 49
CMP 8 2.9595275 1.645 180 N R108 ERJ-6GEY0R00V ;0=1,1=0.0571
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ6GEY0R00V'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0805'
PRP PartNumber 'ERJ-6GEY0R00V'
PRP Power_(Watts) '0.125W, 1/8W'
PRP Ratings 'AEC-Q200'
PRP Resistance '0 O'
PRP Series 'ERJ-6G'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P0.0ACT-ND'
PRP Temperature_Coefficient '-'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD080510615'
PRP Value '0 O'
TOP 0 2.9890551 1.645 90 N 0 213 1
TOP 1 2.93 1.645 90 N 0 212 2
#
# CMP 50
CMP 8 2.96 1.715 180 N R107 ERJ-6GEY0R00V ;0=1,1=0.0571
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ6GEY0R00V'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0805'
PRP PartNumber 'ERJ-6GEY0R00V'
PRP Power_(Watts) '0.125W, 1/8W'
PRP Ratings 'AEC-Q200'
PRP Resistance '0 O'
PRP Series 'ERJ-6G'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P0.0ACT-ND'
PRP Temperature_Coefficient '-'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD080510615'
PRP Value '0 O'
TOP 0 2.9895276 1.715 90 N 0 215 1
TOP 1 2.9304725 1.715 90 N 0 214 2
#
# CMP 51
CMP 0 3.5239178 0.8207675 225 N R144 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 3.5317127 0.8129726 135 N 198 5 1
TOP 1 3.5161229 0.8285624 135 N 88 1 2
#
# CMP 52
CMP 0 3.5239178 0.9707675 225 N R142 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 3.5317127 0.9629726 135 N 191 2 1
TOP 1 3.5161229 0.9785624 135 N 90 1 2
#
# CMP 53
CMP 0 3.5239178 0.8707675 225 N R143 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 3.5317127 0.8629726 135 N 190 2 1
TOP 1 3.5161229 0.8785624 135 N 89 1 2
#
# CMP 54
CMP 37 1.1600001 2.6335827 90 N D5 LTST-C191TGKT ;0=1,1=0.0354
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color 'Green'
PRP CompType 'LED'
PRP Current_Rating_(Amps) '20mA'
PRP datasheet '-'
PRP Length_(in) '-'
PRP Manufacturer 'Lite-On Inc.'
PRP Mount_Type 'SMD'
PRP PackageReference '-'
PRP PartNumber 'LTST-C191TGKT'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '0.65'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '160-1888-1-ND'
PRP Text1 'IOVDD'
PRP UniqueID 'cmp00247'
PRP Voltage_-_Forward_(Vf)_(Typ) '3.2V'
PRP Voltage_Rating_-_DC '-'
TOP 0 1.1600001 2.6631102 90 N 237 18 1
TOP 1 1.1600001 2.6040551 90 N 91 1 2
#
# CMP 55
CMP 37 1.0650001 2.6335827 90 N D4 LTST-C191TGKT ;0=1,1=0.0354
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color 'Green'
PRP CompType 'LED'
PRP Current_Rating_(Amps) '20mA'
PRP datasheet '-'
PRP Length_(in) '-'
PRP Manufacturer 'Lite-On Inc.'
PRP Mount_Type 'SMD'
PRP PackageReference '-'
PRP PartNumber 'LTST-C191TGKT'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '0.65'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '160-1888-1-ND'
PRP Text1 'AVDD'
PRP UniqueID 'cmp00247'
PRP Voltage_-_Forward_(Vf)_(Typ) '3.2V'
PRP Voltage_Rating_-_DC '-'
TOP 0 1.0650001 2.6631102 90 N 237 16 1
TOP 1 1.0650001 2.6040551 90 N 92 1 2
#
# CMP 56
CMP 35 1.9841945 1.03026 270 N TP3 5116 ;0=2,1=0.1811
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color 'Green'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.keyelco.com/userAssets/file/M60-2p60.pdf'
PRP CompType 'TestPoint'
PRP Current_Rating_(Amps) '-'
PRP datasheet 'https://www.keyelco.com/userAssets/file/M65p56.pdf'
PRP Length_(in) '-'
PRP Manufacturer 'Keystone'
PRP Mount_Type 'TH'
PRP PackageReference '-'
PRP PartNumber '5116'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '36-5116-ND'
PRP Text1 'VCM'
PRP UniqueID 'cmp00057'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 1.9841945 1.03026 270 N 110 12 1
#
# CMP 57
CMP 0 2.1935644 1.1032858 270 N R129 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.1935644 1.0922622 180 N 113 1 1
TOP 1 2.1935644 1.1143094 180 N 83 0 2
#
# CMP 58
CMP 8 0.8442673 1.3164347 180 N FB3 BLM21SP471SN1D ;0=1,1=0.0571
PRP CompType 'FerriteBead'
PRP Current '2.5A'
PRP datasheet 'https://www.murata.com/en-us/api/pdfdownloadapi?cate=luNoiseSupprFilteChipFerriBead&partno=BLM21SP471SN1%23'
PRP DCR '-'
PRP Impedance '470 O'
PRP Manufacturer 'Murata Electronics'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0805'
PRP PartNumber 'BLM21SP471SN1D'
PRP Series 'EMIFIL®, BLM21'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '490-18594-1-ND'
PRP Temperature_Coefficient '-'
PRP Tolerance '-'
PRP UniqueID 'dcp00579'
PRP Value '-'
PRP Voltage_-_Rated '-'
TOP 0 0.8737949 1.3164347 90 N 100 2 1
TOP 1 0.8147398 1.3164347 90 N 102 5 2
#
# CMP 59
CMP 4 0.9411414 1.1507486 0 N C23 GRT155R71E104KE01J ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet '-'
PRP Manufacturer 'Murata'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0402'
PRP PartNumber 'GRT155R71E104KE01J'
PRP Ratings '-'
PRP Series '-'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Digi-key'
PRP Supplier_Part_Number_1 '490-GRT155R71E104KE01JCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±10%'
PRP UniqueID 'capcc09401'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '25V'
TOP 0 0.9214564 1.1507486 270 N 248 337 1
TOP 1 0.9608265 1.1507486 270 N 238 50 2
#
# CMP 60
CMP 2 0.7427161 1.2107882 90 N R29 ERA-2AEB1242X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thin Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDM0000/AOA0000C307.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERA-2AEB1242X'
PRP Power_(Watts) '0.063W, 1/16W'
PRP Ratings 'AEC-Q200'
PRP Resistance '12.4 kO'
PRP Series 'ERA-2A'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P12.4KDCCT-ND'
PRP Temperature_Coefficient '±25ppm/°C'
PRP Tolerance '±0.1%'
PRP UniqueID 'RSMD040200551'
PRP Value '12.4 kO'
TOP 0 0.7427161 1.2304732 0 N 248 338 1
TOP 1 0.7427161 1.1911031 0 N 99 1 2
#
# CMP 61
CMP 14 0.8584642 1.1905123 270 N R27 WSLP0603R1000FEA ;0=1,1=0.0000
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP CompType 'Resistor SMD Sense'
PRP datasheet 'https://www.seielect.com/catalog/sei-css_cssh.pdf'
PRP Manufacturer 'Vishay Dale'
PRP PartNumber 'WSLP0603R1000FEA'
PRP Power_(Watts) '0.4W, 2/5W'
PRP Resistance '3 mO'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '541-10032-1-ND'
PRP Tolerance '±1%'
PRP Value '100 mO'
TOP 0 0.8584642 1.1550793 270 N 170 25 1
TOP 1 0.8584642 1.2255517 270 N 100 3 2
#
# CMP 62
CMP 9 0.7937158 1.1755046 90 N C26 C2012X7S1E106K125AC ;0=1,1=0.0571
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://product.tdk.com/system/files/dam/doc/product/capacitor/ceramic/mlcc/catalog/mlcc_commercial_general_en.pdf'
PRP Manufacturer 'TDK Corporation'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0805'
PRP PartNumber 'C2012X7S1E106K125AC'
PRP Ratings '-'
PRP Series 'C'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.5'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '445-181600-1-ND'
PRP Temperature_Coefficient 'X7S'
PRP Tolerance '±10%'
PRP UniqueID 'capcc03511'
PRP Value '10 uF'
PRP Voltage_-_Rated '25V'
TOP 0 0.7937158 1.2050322 0 N 248 381 1
TOP 1 0.7937158 1.1459771 0 N 170 24 2
#
# CMP 63
CMP 3 0.7477158 1.0855909 270 N R30 ERJ-2RKF1202X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1202X'
PRP Power_(Watts) '0.1W, 1/10W'
PRP Ratings 'AEC-Q200'
PRP Resistance '12 kO'
PRP Series 'ERJ-2RK'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P12.0KLCT-ND'
PRP Temperature_Coefficient '±100ppm/°C'
PRP Tolerance '±1%'
PRP UniqueID 'RSMD040200519'
PRP Value '12 kO'
TOP 0 0.7477158 1.0659059 180 N 98 2 1
TOP 1 0.7477158 1.105276 180 N 101 1 2
#
# CMP 64
CMP 2 0.8014009 1.0659059 180 N R31 ERJ-U020R00X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDP0000/AOA0000C334.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-U020R00X'
PRP Power_(Watts) '0.1W, 1/10W'
PRP Ratings 'AEC-Q200'
PRP Resistance '0 O'
PRP Series 'ERJ-U02'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '10-ERJ-U020R00XCT-ND'
PRP Temperature_Coefficient '-100/ +600ppm/°C'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD040200004'
PRP Value '0 O'
TOP 0 0.8210859 1.0659059 90 N 248 339 1
TOP 1 0.7817158 1.0659059 90 N 98 1 2
#
# CMP 65
CMP 5 0.7127161 1.0855909 270 N C28 C1005X5R1E105K050BC ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://product.tdk.com/system/files/dam/doc/product/capacitor/ceramic/mlcc/catalog/mlcc_commercial_general_en.pdf'
PRP Manufacturer 'TDK Corporation'
PRP Operating_Temperature '-55°C ~ 85°C'
PRP PackageReference '0402'
PRP PartNumber 'C1005X5R1E105K050BC'
PRP Ratings '-'
PRP Series 'C'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.55'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '445-9066-1-ND'
PRP Temperature_Coefficient 'X5R'
PRP Tolerance '±10%'
PRP UniqueID 'capcc02750'
PRP Value '1 uF'
PRP Voltage_-_Rated '25V'
TOP 0 0.7127161 1.0659059 180 N 248 379 1
TOP 1 0.7127161 1.105276 180 N 101 2 2
#
# CMP 66
CMP 2 0.7091161 1.1714181 90 N R28 RT0402BRD0788K7L ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thin Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDM0000/AOA0000C307.pdf'
PRP Manufacturer 'Yageo'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'RT0402BRD0788K7L'
PRP Power_(Watts) '0.063W, 1/16W'
PRP Ratings 'AEC-Q200'
PRP Resistance '88.7 kO'
PRP Series 'ERA-2A'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'YAG1486CT-ND'
PRP Temperature_Coefficient '±25ppm/°C'
PRP Tolerance '±0.1%'
PRP UniqueID 'RSMD040203878'
PRP Value '88.7 kO'
TOP 0 0.7091161 1.1911031 0 N 99 2 1
TOP 1 0.7091161 1.151733 0 N 170 21 2
#
# CMP 67
CMP 4 2.6336438 0.7596774 270 N C55 GRT155R71E104KE01J ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet '-'
PRP Manufacturer 'Murata'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0402'
PRP PartNumber 'GRT155R71E104KE01J'
PRP Ratings '-'
PRP Series '-'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Digi-key'
PRP Supplier_Part_Number_1 '490-GRT155R71E104KE01JCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±10%'
PRP UniqueID 'capcc09401'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '25V'
TOP 0 2.6336438 0.7399924 180 N 248 340 1
TOP 1 2.6336438 0.7793625 180 N 238 51 2
#
# CMP 68
CMP 9 0.4809832 1.1981899 90 N C24 C2012X7S1E106K125AC ;0=1,1=0.0571
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://product.tdk.com/system/files/dam/doc/product/capacitor/ceramic/mlcc/catalog/mlcc_commercial_general_en.pdf'
PRP Manufacturer 'TDK Corporation'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0805'
PRP PartNumber 'C2012X7S1E106K125AC'
PRP Ratings '-'
PRP Series 'C'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.5'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '445-181600-1-ND'
PRP Temperature_Coefficient 'X7S'
PRP Tolerance '±10%'
PRP UniqueID 'capcc03511'
PRP Value '10 uF'
PRP Voltage_-_Rated '25V'
TOP 0 0.4809832 1.2277175 0 N 248 341 1
TOP 1 0.4809832 1.1686624 0 N 176 10 2
#
# CMP 69
CMP 4 0.5364093 1.1785048 90 N C25 GRT155R71E104KE01J ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet '-'
PRP Manufacturer 'Murata'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0402'
PRP PartNumber 'GRT155R71E104KE01J'
PRP Ratings '-'
PRP Series '-'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Digi-key'
PRP Supplier_Part_Number_1 '490-GRT155R71E104KE01JCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±10%'
PRP UniqueID 'capcc09401'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '25V'
TOP 0 0.5364093 1.1981898 0 N 248 342 1
TOP 1 0.5364093 1.1588197 0 N 176 11 2
#
# CMP 70
CMP 2 0.5224799 1.085591 90 N R24 ERA-2AEB103X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thin Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDM0000/AOA0000C307.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERA-2AEB103X'
PRP Power_(Watts) '0.063W, 1/16W'
PRP Ratings 'AEC-Q200'
PRP Resistance '10 kO'
PRP Series 'ERA-2A'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P10KDCCT-ND'
PRP Temperature_Coefficient '±25ppm/°C'
PRP Tolerance '±0.1%'
PRP UniqueID 'RSMD040200315'
PRP Value '10 kO'
TOP 0 0.5224799 1.105276 0 N 204 2 1
TOP 1 0.5224799 1.0659059 0 N 238 52 2
#
# CMP 71
CMP 25 0.6175274 1.1320476 0 N U8 TPS7A9601DSC ;0=1,1=0.0394
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color '-'
PRP CompType 'LDO'
PRP Current_Rating_(Amps) '-'
PRP datasheet 'https://www.ti.com/lit/gpn/tps7a96'
PRP Length_(in) '-'
PRP Manufacturer 'Texas Instruments'
PRP Mount_Type 'SMD'
PRP PackageReference '-'
PRP PartNumber 'TPS7A9601DSCR'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Supplier_1 '-'
PRP Supplier_Part_Number_1 '-'
PRP Text1 '2A, Vin 1.7V?5.5V'
PRP UniqueID 'cmp00446'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 0.5624093 1.1714177 0 N 176 17 1
TOP 1 0.5624093 1.1517327 0 N 176 16 2
TOP 2 0.5624093 1.1320476 0 N 8 4 3
TOP 3 0.5624093 1.1123626 0 N 204 3 4
TOP 4 0.5624093 1.0926775 0 N 99 3 5
TOP 5 0.6726455 1.0926775 0 N 248 387 6
TOP 6 0.6726455 1.1123625 0 N 101 3 7
TOP 7 0.6726455 1.1320476 0 N 100 4 8
TOP 8 0.6726455 1.1517326 0 N 170 27 9
TOP 9 0.6726455 1.1714177 0 N 170 26 10
TOP 10 0.6175273 1.1320476 0 N 248 386 11
TOP 11 0.6401652 1.1320476 0 N 248 456 11
TOP 12 0.6175274 1.094646 0 N 248 457 11
TOP 13 0.5948896 1.1320476 0 N 248 458 11
TOP 14 0.6175274 1.1694492 0 N 248 459 11
#
# CMP 72
CMP 41 0.8247398 1.3864347 180 N PP4 Probe_Point ;0=2,1=0.1570
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color '-'
PRP CompType 'Probe Point'
PRP Current_Rating_(Amps) '-'
PRP datasheet '-'
PRP Length_(in) '-'
PRP Manufacturer '-'
PRP Mount_Type '-'
PRP PackageReference '-'
PRP PartNumber '-'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Text1 'IOVDD'
PRP UniqueID 'cmp00025'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 0.8247398 1.3864347 180 N 102 9 1
#
# CMP 73
CMP 8 0.8442674 1.716435 180 N FB2 BLM21SP471SN1D ;0=1,1=0.0571
PRP CompType 'FerriteBead'
PRP Current '2.5A'
PRP datasheet 'https://www.murata.com/en-us/api/pdfdownloadapi?cate=luNoiseSupprFilteChipFerriBead&partno=BLM21SP471SN1%23'
PRP DCR '-'
PRP Impedance '470 O'
PRP Manufacturer 'Murata Electronics'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0805'
PRP PartNumber 'BLM21SP471SN1D'
PRP Series 'EMIFIL®, BLM21'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '490-18594-1-ND'
PRP Temperature_Coefficient '-'
PRP Tolerance '-'
PRP UniqueID 'dcp00579'
PRP Value '-'
PRP Voltage_-_Rated '-'
TOP 0 0.873795 1.716435 90 N 105 2 1
TOP 1 0.8147399 1.716435 90 N 171 6 2
#
# CMP 74
CMP 7 0.7687399 1.755805 90 N C21 GRM188R60J476ME15D ;0=1,1=0.0394
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP Manufacturer 'Murata'
PRP Operating_Temperature '-55°C ~ 85°C'
PRP PackageReference '0603'
PRP PartNumber 'GRM188R60J476ME15D'
PRP Ratings '-'
PRP Series '-'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.81'
PRP SizeZ_mm '0.9'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '490-13247-1-ND'
PRP Temperature_Coefficient 'X5R'
PRP Tolerance '±20%'
PRP Value '47 uF'
PRP Voltage_-_Rated '6.3V'
TOP 0 0.7687399 1.7833641 0 N 248 343 1
TOP 1 0.7687399 1.728246 0 N 171 7 2
#
# CMP 75
CMP 4 0.9411415 1.5507489 0 N C17 GRT155R71E104KE01J ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet '-'
PRP Manufacturer 'Murata'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0402'
PRP PartNumber 'GRT155R71E104KE01J'
PRP Ratings '-'
PRP Series '-'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Digi-key'
PRP Supplier_Part_Number_1 '490-GRT155R71E104KE01JCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±10%'
PRP UniqueID 'capcc09401'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '25V'
TOP 0 0.9214565 1.5507489 270 N 248 344 1
TOP 1 0.9608266 1.5507489 270 N 238 53 2
#
# CMP 76
CMP 2 0.7427162 1.6107885 90 N R20 ERA-2AEB1242X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thin Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDM0000/AOA0000C307.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERA-2AEB1242X'
PRP Power_(Watts) '0.063W, 1/16W'
PRP Ratings 'AEC-Q200'
PRP Resistance '12.4 kO'
PRP Series 'ERA-2A'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P12.4KDCCT-ND'
PRP Temperature_Coefficient '±25ppm/°C'
PRP Tolerance '±0.1%'
PRP UniqueID 'RSMD040200551'
PRP Value '12.4 kO'
TOP 0 0.7427162 1.6304735 0 N 248 345 1
TOP 1 0.7427162 1.5911034 0 N 104 1 2
#
# CMP 77
CMP 14 0.8584643 1.5905126 270 N R17 WSLP0603R1000FEA ;0=1,1=0.0000
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP CompType 'Resistor SMD Sense'
PRP datasheet 'https://www.seielect.com/catalog/sei-css_cssh.pdf'
PRP Manufacturer 'Vishay Dale'
PRP PartNumber 'WSLP0603R1000FEA'
PRP Power_(Watts) '0.4W, 2/5W'
PRP Resistance '3 mO'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '541-10032-1-ND'
PRP Tolerance '±1%'
PRP Value '100 mO'
TOP 0 0.8584643 1.5550796 270 N 107 2 1
TOP 1 0.8584643 1.625552 270 N 105 3 2
#
# CMP 78
CMP 9 0.7937159 1.5755049 90 N C20 C2012X7S1E106K125AC ;0=1,1=0.0571
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://product.tdk.com/system/files/dam/doc/product/capacitor/ceramic/mlcc/catalog/mlcc_commercial_general_en.pdf'
PRP Manufacturer 'TDK Corporation'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0805'
PRP PartNumber 'C2012X7S1E106K125AC'
PRP Ratings '-'
PRP Series 'C'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.5'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '445-181600-1-ND'
PRP Temperature_Coefficient 'X7S'
PRP Tolerance '±10%'
PRP UniqueID 'capcc03511'
PRP Value '10 uF'
PRP Voltage_-_Rated '25V'
TOP 0 0.7937159 1.6050325 0 N 248 346 1
TOP 1 0.7937159 1.5459774 0 N 107 3 2
#
# CMP 79
CMP 3 0.7477159 1.4855912 270 N R21 ERJ-2RKF1202X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1202X'
PRP Power_(Watts) '0.1W, 1/10W'
PRP Ratings 'AEC-Q200'
PRP Resistance '12 kO'
PRP Series 'ERJ-2RK'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P12.0KLCT-ND'
PRP Temperature_Coefficient '±100ppm/°C'
PRP Tolerance '±1%'
PRP UniqueID 'RSMD040200519'
PRP Value '12 kO'
TOP 0 0.7477159 1.4659062 180 N 103 1 1
TOP 1 0.7477159 1.5052763 180 N 106 1 2
#
# CMP 80
CMP 2 0.801401 1.4659062 180 N R22 ERJ-U020R00X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDP0000/AOA0000C334.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-U020R00X'
PRP Power_(Watts) '0.1W, 1/10W'
PRP Ratings 'AEC-Q200'
PRP Resistance '0 O'
PRP Series 'ERJ-U02'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '10-ERJ-U020R00XCT-ND'
PRP Temperature_Coefficient '-100/ +600ppm/°C'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD040200004'
PRP Value '0 O'
TOP 0 0.821086 1.4659062 90 N 248 347 1
TOP 1 0.7817159 1.4659062 90 N 103 2 2
#
# CMP 81
CMP 5 0.7127162 1.4855912 270 N C22 C1005X5R1E105K050BC ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://product.tdk.com/system/files/dam/doc/product/capacitor/ceramic/mlcc/catalog/mlcc_commercial_general_en.pdf'
PRP Manufacturer 'TDK Corporation'
PRP Operating_Temperature '-55°C ~ 85°C'
PRP PackageReference '0402'
PRP PartNumber 'C1005X5R1E105K050BC'
PRP Ratings '-'
PRP Series 'C'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.55'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '445-9066-1-ND'
PRP Temperature_Coefficient 'X5R'
PRP Tolerance '±10%'
PRP UniqueID 'capcc02750'
PRP Value '1 uF'
PRP Voltage_-_Rated '25V'
TOP 0 0.7127162 1.4659062 180 N 248 348 1
TOP 1 0.7127162 1.5052763 180 N 106 2 2
#
# CMP 82
CMP 2 0.7091162 1.5714184 90 N R19 RT0402BRD0788K7L ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thin Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDM0000/AOA0000C307.pdf'
PRP Manufacturer 'Yageo'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'RT0402BRD0788K7L'
PRP Power_(Watts) '0.063W, 1/16W'
PRP Ratings 'AEC-Q200'
PRP Resistance '88.7 kO'
PRP Series 'ERA-2A'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'YAG1486CT-ND'
PRP Temperature_Coefficient '±25ppm/°C'
PRP Tolerance '±0.1%'
PRP UniqueID 'RSMD040203878'
PRP Value '88.7 kO'
TOP 0 0.7091162 1.5911034 0 N 104 2 1
TOP 1 0.7091162 1.5517333 0 N 107 4 2
#
# CMP 83
CMP 9 0.4809833 1.5981902 90 N C18 C2012X7S1E106K125AC ;0=1,1=0.0571
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://product.tdk.com/system/files/dam/doc/product/capacitor/ceramic/mlcc/catalog/mlcc_commercial_general_en.pdf'
PRP Manufacturer 'TDK Corporation'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0805'
PRP PartNumber 'C2012X7S1E106K125AC'
PRP Ratings '-'
PRP Series 'C'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.5'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '445-181600-1-ND'
PRP Temperature_Coefficient 'X7S'
PRP Tolerance '±10%'
PRP UniqueID 'capcc03511'
PRP Value '10 uF'
PRP Voltage_-_Rated '25V'
TOP 0 0.4809833 1.6277178 0 N 248 349 1
TOP 1 0.4809833 1.5686627 0 N 176 12 2
#
# CMP 84
CMP 4 0.5364094 1.5785051 90 N C19 GRT155R71E104KE01J ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet '-'
PRP Manufacturer 'Murata'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0402'
PRP PartNumber 'GRT155R71E104KE01J'
PRP Ratings '-'
PRP Series '-'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Digi-key'
PRP Supplier_Part_Number_1 '490-GRT155R71E104KE01JCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±10%'
PRP UniqueID 'capcc09401'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '25V'
TOP 0 0.5364094 1.5981901 0 N 248 350 1
TOP 1 0.5364094 1.55882 0 N 176 13 2
#
# CMP 85
CMP 2 0.52248 1.4855913 90 N R15 ERA-2AEB103X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thin Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDM0000/AOA0000C307.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERA-2AEB103X'
PRP Power_(Watts) '0.063W, 1/16W'
PRP Ratings 'AEC-Q200'
PRP Resistance '10 kO'
PRP Series 'ERA-2A'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P10KDCCT-ND'
PRP Temperature_Coefficient '±25ppm/°C'
PRP Tolerance '±0.1%'
PRP UniqueID 'RSMD040200315'
PRP Value '10 kO'
TOP 0 0.52248 1.5052763 0 N 95 1 1
TOP 1 0.52248 1.4659062 0 N 238 54 2
#
# CMP 86
CMP 25 0.6175275 1.5320479 0 N U6 TPS7A9601DSC ;0=1,1=0.0394
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color '-'
PRP CompType 'LDO'
PRP Current_Rating_(Amps) '-'
PRP datasheet 'https://www.ti.com/lit/gpn/tps7a96'
PRP Length_(in) '-'
PRP Manufacturer 'Texas Instruments'
PRP Mount_Type 'SMD'
PRP PackageReference '-'
PRP PartNumber 'TPS7A9601DSCR'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Supplier_1 '-'
PRP Supplier_Part_Number_1 '-'
PRP Text1 '2A, Vin 1.7V?5.5V'
PRP UniqueID 'cmp00446'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 0.5624094 1.571418 0 N 176 15 1
TOP 1 0.5624094 1.551733 0 N 176 14 2
TOP 2 0.5624094 1.5320479 0 N 8 3 3
TOP 3 0.5624094 1.5123629 0 N 95 2 4
TOP 4 0.5624094 1.4926778 0 N 104 3 5
TOP 5 0.6726456 1.4926778 0 N 248 352 6
TOP 6 0.6726456 1.5123628 0 N 106 3 7
TOP 7 0.6726456 1.5320479 0 N 105 4 8
TOP 8 0.6726456 1.5517329 0 N 107 6 9
TOP 9 0.6726456 1.571418 0 N 107 5 10
TOP 10 0.6175274 1.5320479 0 N 248 351 11
TOP 11 0.6401653 1.5320479 0 N 248 416 11
TOP 12 0.6175275 1.4946463 0 N 248 417 11
TOP 13 0.5948897 1.5320479 0 N 248 418 11
TOP 14 0.6175275 1.5694495 0 N 248 419 11
#
# CMP 87
CMP 41 0.8247399 1.786435 180 N PP3 Probe_Point ;0=2,1=0.1570
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color '-'
PRP CompType 'Probe Point'
PRP Current_Rating_(Amps) '-'
PRP datasheet '-'
PRP Length_(in) '-'
PRP Manufacturer '-'
PRP Mount_Type '-'
PRP PackageReference '-'
PRP PartNumber '-'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Text1 'AVDD'
PRP UniqueID 'cmp00025'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 0.8247399 1.786435 180 N 171 11 1
#
# CMP 88
CMP 15 1.6811079 1.2330495 0 N T1 ADT1-1WT+ ;0=1,1=0.0602
PRP AEC_Qualified 'No'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.minicircuits.com/pdfs/ADT1-1WT+.pdf'
PRP datasheet 'https://www.minicircuits.com/pdfs/ADT1-1WT+.pdf'
PRP Datasheet_Path 'datasheets/Trans-ADT1-1WT+.pdf'
PRP Frequency_Fixed '0.4-800MHz'
PRP helpURL 'https://upverter.com/upn/revision/d297350a40f3aea3/'
PRP Insertion_Loss '0.68-2.44dB'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Mini-Circuits'
PRP Mouser_Part_Number '139-ADT1-1WT'
PRP Operating_Temperature_Range '-20°C to +85°C'
PRP PackageReference 'SMT_6'
PRP Part_Number 'ADT1-1WT+'
PRP PartNumber 'ADT1-1WT+'
PRP Return_Loss '9.75dB'
PRP RoHS 'TRUE'
PRP SizeZ_mm '2.84mm'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_2 '139-ADT1-1WT'
TOP 0 1.5811079 1.3330495 0 N 248 382 1
TOP 1 1.5811079 1.2330495 0 N 93 1 2
TOP 2 1.5811079 1.1330495 0 N 136 1 3
TOP 3 1.7811079 1.1330495 0 N 132 1 4
TOP 4 1.7811079 1.2330495 0 N 248 383 5
TOP 5 1.7811079 1.3330495 0 N 135 1 6
#
# CMP 89
CMP 16 2.1374623 1.8788757 180 N T3 ADT1-6T+ ;0=1,1=0.0602
PRP AEC_Qualified 'No'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.minicircuits.com/pdfs/ADT1-6T+.pdf'
PRP DCR_ohm '50'
PRP Manufacturer 'Mini-Circuits'
PRP Ns1toNp '1:1'
PRP PackageReference 'SMD6'
PRP PartNumber 'ADT1-6T+'
PRP RoHS 'TRUE'
PRP Rsec1_ohm '50'
PRP SizeZ_mm '.206inch'
PRP Symbol_Name 'SYM-ADT1-6T+'
TOP 0 2.2374623 1.9788757 180 N 145 1 1
TOP 1 2.1374623 1.9788757 180 N 248 385 2
TOP 2 2.0374623 1.9788757 180 N 248 384 3
TOP 3 2.0374623 1.7788757 180 N 140 1 4
TOP 4 2.1374623 1.7788757 180 N 144 1 5
TOP 5 2.2374623 1.7788757 180 N 147 1 6
#
# CMP 90
CMP 16 2.1384467 0.6187195 0 N T2 ADT1-6T+ ;0=1,1=0.0602
PRP AEC_Qualified 'No'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.minicircuits.com/pdfs/ADT1-6T+.pdf'
PRP DCR_ohm '50'
PRP Manufacturer 'Mini-Circuits'
PRP Ns1toNp '1:1'
PRP PackageReference 'SMD6'
PRP PartNumber 'ADT1-6T+'
PRP RoHS 'TRUE'
PRP Rsec1_ohm '50'
PRP SizeZ_mm '.206inch'
PRP Symbol_Name 'SYM-ADT1-6T+'
TOP 0 2.0384467 0.5187195 0 N 157 0 1
TOP 1 2.1384467 0.5187195 0 N 248 354 2
TOP 2 2.2384467 0.5187195 0 N 248 353 3
TOP 3 2.2384467 0.7187195 0 N 152 0 4
TOP 4 2.1384467 0.7187195 0 N 156 0 5
TOP 5 2.0384467 0.7187195 0 N 159 0 6
#
# CMP 91
CMP 0 2.3262025 1.2718958 0 N R117 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.3151789 1.2718958 270 N 54 0 1
TOP 1 2.3372261 1.2718958 270 N 35 2 2
#
# CMP 92
CMP 0 2.1935644 1.3943094 90 N R125 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.1935644 1.405333 0 N 195 1 1
TOP 1 2.1935644 1.3832858 0 N 118 0 2
#
# CMP 93
CMP 0 2.3262025 1.2949958 0 N R116 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.3151789 1.2949958 270 N 55 0 1
TOP 1 2.3372261 1.2949958 270 N 36 2 2
#
# CMP 94
CMP 0 2.3262025 1.3180953 0 N R115 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.3151789 1.3180953 270 N 56 0 1
TOP 1 2.3372261 1.3180953 270 N 37 2 2
#
# CMP 95
CMP 0 2.2859569 1.3943095 270 N R114 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.2859569 1.3832859 180 N 57 0 1
TOP 1 2.2859569 1.4053331 180 N 38 2 2
#
# CMP 96
CMP 0 2.2628579 1.3943095 270 N R113 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.2628579 1.3832859 180 N 58 0 1
TOP 1 2.2628579 1.4053331 180 N 46 2 2
#
# CMP 97
CMP 0 2.2397599 1.3943095 270 N R112 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.2397599 1.3832859 180 N 59 0 1
TOP 1 2.2397599 1.4053331 180 N 52 0 2
#
# CMP 98
CMP 0 2.2166614 1.3943095 270 N R111 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.2166614 1.3832859 180 N 60 0 1
TOP 1 2.2166614 1.4053331 180 N 47 2 2
#
# CMP 99
CMP 0 2.3262025 1.2256978 0 N R106 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.3151789 1.2256978 270 N 61 0 1
TOP 1 2.3372261 1.2256978 270 N 39 2 2
#
# CMP 100
CMP 0 2.3262025 1.2025988 0 N R105 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.3151789 1.2025988 270 N 62 0 1
TOP 1 2.3372261 1.2025988 270 N 40 2 2
#
# CMP 101
CMP 0 2.3262025 1.1795007 0 N R104 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.3151789 1.1795007 270 N 63 0 1
TOP 1 2.3372261 1.1795007 270 N 41 2 2
#
# CMP 102
CMP 0 2.2859584 1.1032857 90 N R103 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.2859584 1.1143093 0 N 64 0 1
TOP 1 2.2859584 1.0922621 0 N 42 2 2
#
# CMP 103
CMP 0 2.2628594 1.1032857 90 N R102 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.2628594 1.1143093 0 N 65 0 1
TOP 1 2.2628594 1.0922621 0 N 43 1 2
#
# CMP 104
CMP 0 2.2397604 1.1032857 90 N R100 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.2397604 1.1143093 0 N 66 0 1
TOP 1 2.2397604 1.0922621 0 N 44 2 2
#
# CMP 105
CMP 0 2.2166614 1.1032857 90 N R99 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.2166614 1.1143093 0 N 67 0 1
TOP 1 2.2166614 1.0922621 0 N 45 2 2
#
# CMP 106
CMP 0 2.3262025 1.2487968 0 N R98 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.3151789 1.2487968 270 N 68 0 1
TOP 1 2.3372261 1.2487968 270 N 34 2 2
#
# CMP 107
CMP 0 2.7202187 0.8362917 90 N R72 ERJ-1GNF1001C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GNF1001C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '1 kO'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P122413CT-ND'
PRP Temperature_Coefficient '±200ppm/°C'
PRP Tolerance '±1%'
PRP UniqueID 'RSMD020100143'
PRP Value '1 kO'
TOP 0 2.7202187 0.8473152 0 N 248 355 1
TOP 1 2.7202187 0.825268 0 N 131 0 2
#
# CMP 108
CMP 0 2.3582497 1.4414995 180 N R123 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.3692733 1.4414995 90 N 48 2 1
TOP 1 2.3472261 1.4414995 90 N 52 1 2
#
# CMP 109
CMP 0 2.6902187 0.8142443 90 N R70 ERJ-1GNF1001C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GNF1001C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '1 kO'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P122413CT-ND'
PRP Temperature_Coefficient '±200ppm/°C'
PRP Tolerance '±1%'
PRP UniqueID 'RSMD020100143'
PRP Value '1 kO'
TOP 0 2.6902187 0.825268 0 N 131 1 1
TOP 1 2.6902187 0.8032208 0 N 170 22 2
#
# CMP 110
CMP 0 2.3472261 1.4304759 270 N R127 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.3472261 1.4194523 180 N 50 0 1
TOP 1 2.3472261 1.4414995 180 N 52 2 2
#
# CMP 111
CMP 0 2.8932895 0.795268 180 N R71 ERJ-1GNF49R9C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GNF49R9C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '49.9 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P123049CT-ND'
PRP Temperature_Coefficient '±200ppm/°C'
PRP Tolerance '±1%'
PRP UniqueID 'RSMD020100177'
PRP Value '49.9 O'
TOP 0 2.9043131 0.795268 90 N 248 356 1
TOP 1 2.8822659 0.795268 90 N 130 0 2
#
# CMP 112
CMP 0 1.8831551 1.1885044 270 N R69 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 1.8831551 1.1774808 180 N 120 0 1
TOP 1 1.8831551 1.199528 180 N 133 0 2
#
# CMP 113
CMP 0 1.4721315 0.9580495 0 N R68 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 1.4611079 0.9580495 270 N 112 0 1
TOP 1 1.4831551 0.9580495 270 N 120 1 2
#
# CMP 114
CMP 0 1.9221317 1.2217505 180 N R67 ERJ-1GNF49R9C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GNF49R9C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '49.9 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P123049CT-ND'
PRP Temperature_Coefficient '±200ppm/°C'
PRP Tolerance '±1%'
PRP UniqueID 'RSMD020100177'
PRP Value '49.9 O'
TOP 0 1.9331553 1.2217505 90 N 133 1 1
TOP 1 1.9111081 1.2217505 90 N 134 1 2
#
# CMP 115
CMP 0 2.0012025 1.233325 270 N R66 ERJ-1GNF1001C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GNF1001C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '1 kO'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P122413CT-ND'
PRP Temperature_Coefficient '±200ppm/°C'
PRP Tolerance '±1%'
PRP UniqueID 'RSMD020100143'
PRP Value '1 kO'
TOP 0 2.0012025 1.2223014 180 N 163 0 1
TOP 1 2.0012025 1.2443486 180 N 162 0 2
#
# CMP 116
CMP 0 1.9221317 1.2443486 0 N R65 ERJ-1GNF49R9C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GNF49R9C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '49.9 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P123049CT-ND'
PRP Temperature_Coefficient '±200ppm/°C'
PRP Tolerance '±1%'
PRP UniqueID 'RSMD020100177'
PRP Value '49.9 O'
TOP 0 1.9111081 1.2443486 270 N 134 2 1
TOP 1 1.9331553 1.2443486 270 N 137 0 2
#
# CMP 117
CMP 0 1.4721315 1.5080495 0 N R64 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 1.4611079 1.5080495 270 N 111 0 1
TOP 1 1.4831551 1.5080495 270 N 121 0 2
#
# CMP 118
CMP 0 1.8831551 1.2775946 90 N R63 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 1.8831551 1.2886182 0 N 121 1 1
TOP 1 1.8831551 1.266571 0 N 137 1 2
#
# CMP 119
CMP 0 2.1271476 1.4443094 90 N R97 ERJ-1GNF10R0C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GNF10R0C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '10 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P122669CT-ND'
PRP Temperature_Coefficient '±200ppm/°C'
PRP Tolerance '±1%'
PRP UniqueID 'RSMD020100179'
PRP Value '10 O'
TOP 0 2.1271476 1.455333 0 N 122 0 1
TOP 1 2.1271476 1.4332858 0 N 164 0 2
#
# CMP 120
CMP 0 2.0769251 1.5143561 90 N R96 ERJ-1GNF33R0C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GNF33R0C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '33 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P122944CT-ND'
PRP Temperature_Coefficient '±200ppm/°C'
PRP Tolerance '±1%'
PRP UniqueID 'RSMD020100013'
PRP Value '33 O'
TOP 0 2.0769251 1.5253797 0 N 143 0 1
TOP 1 2.0769251 1.5033325 0 N 122 1 2
#
# CMP 121
CMP 0 2.1049251 1.6428049 90 N R95 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.1049251 1.6538285 0 N 141 0 1
TOP 1 2.1049251 1.6317813 0 N 143 1 2
#
# CMP 122
CMP 0 2.0939015 1.6768285 0 N R94 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.0828779 1.6768285 270 N 138 0 1
TOP 1 2.1049251 1.6768285 270 N 141 1 2
#
# CMP 123
CMP 0 2.1049251 1.5143561 90 N R93 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.1049251 1.5253797 0 N 126 0 1
TOP 1 2.1049251 1.5033325 0 N 122 2 2
#
# CMP 124
CMP 0 2.1159487 1.478944 0 N R92 ERJ-1GNF24R9C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GNF24R9C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '24.9 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P122870CT-ND'
PRP Temperature_Coefficient '±200ppm/°C'
PRP Tolerance '±1%'
PRP UniqueID 'RSMD020100010'
PRP Value '24.9 O'
TOP 0 2.1049251 1.478944 270 N 122 3 1
TOP 1 2.1269723 1.478944 270 N 110 5 2
#
# CMP 125
CMP 0 2.1609445 1.478944 0 N R91 ERJ-1GNF24R9C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GNF24R9C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '24.9 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P122870CT-ND'
PRP Temperature_Coefficient '±200ppm/°C'
PRP Tolerance '±1%'
PRP UniqueID 'RSMD020100010'
PRP Value '24.9 O'
TOP 0 2.1499209 1.478944 270 N 110 6 1
TOP 1 2.1719681 1.478944 270 N 123 0 2
#
# CMP 126
CMP 0 2.1719681 1.5143561 90 N R90 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.1719681 1.5253797 0 N 127 0 1
TOP 1 2.1719681 1.5033325 0 N 123 1 2
#
# CMP 127
CMP 0 2.1497457 1.4443094 90 N R89 ERJ-1GNF10R0C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GNF10R0C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '10 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P122669CT-ND'
PRP Temperature_Coefficient '±200ppm/°C'
PRP Tolerance '±1%'
PRP UniqueID 'RSMD020100179'
PRP Value '10 O'
TOP 0 2.1497457 1.455333 0 N 123 2 1
TOP 1 2.1497457 1.4332858 0 N 165 0 2
#
# CMP 128
CMP 0 2.1999681 1.5143561 90 N R88 ERJ-1GNF33R0C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GNF33R0C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '33 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P122944CT-ND'
PRP Temperature_Coefficient '±200ppm/°C'
PRP Tolerance '±1%'
PRP UniqueID 'RSMD020100013'
PRP Value '33 O'
TOP 0 2.1999681 1.5253797 0 N 142 0 1
TOP 1 2.1999681 1.5033325 0 N 123 3 2
#
# CMP 129
CMP 0 2.1719681 1.6428049 90 N R87 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.1719681 1.6538285 0 N 146 0 1
TOP 1 2.1719681 1.6317813 0 N 142 1 2
#
# CMP 130
CMP 0 2.1829917 1.6768285 180 N R86 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.1940153 1.6768285 90 N 148 0 1
TOP 1 2.1719681 1.6768285 90 N 146 1 2
#
# CMP 131
CMP 0 2.1497457 1.0532858 270 N R85 ERJ-1GNF10R0C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GNF10R0C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '10 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P122669CT-ND'
PRP Temperature_Coefficient '±200ppm/°C'
PRP Tolerance '±1%'
PRP UniqueID 'RSMD020100179'
PRP Value '10 O'
TOP 0 2.1497457 1.0422622 180 N 124 0 1
TOP 1 2.1497457 1.0643094 180 N 167 0 2
#
# CMP 132
CMP 0 2.1999682 0.9832391 270 N R84 ERJ-1GNF33R0C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GNF33R0C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '33 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P122944CT-ND'
PRP Temperature_Coefficient '±200ppm/°C'
PRP Tolerance '±1%'
PRP UniqueID 'RSMD020100013'
PRP Value '33 O'
TOP 0 2.1999682 0.9722155 180 N 155 0 1
TOP 1 2.1999682 0.9942627 180 N 124 1 2
#
# CMP 133
CMP 0 2.1729525 0.8547903 270 N R83 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.1729525 0.8437667 180 N 153 0 1
TOP 1 2.1729525 0.8658139 180 N 155 1 2
#
# CMP 134
CMP 0 2.1839761 0.8207667 180 N R82 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.1949997 0.8207667 90 N 150 0 1
TOP 1 2.1729525 0.8207667 90 N 153 1 2
#
# CMP 135
CMP 0 2.1719682 0.9832391 270 N R81 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.1719682 0.9722155 180 N 128 0 1
TOP 1 2.1719682 0.9942627 180 N 124 2 2
#
# CMP 136
CMP 0 2.1609446 1.0172627 180 N R80 ERJ-1GNF24R9C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GNF24R9C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '24.9 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P122870CT-ND'
PRP Temperature_Coefficient '±200ppm/°C'
PRP Tolerance '±1%'
PRP UniqueID 'RSMD020100010'
PRP Value '24.9 O'
TOP 0 2.1719682 1.0172627 90 N 124 3 1
TOP 1 2.149921 1.0172627 90 N 110 7 2
#
# CMP 137
CMP 0 2.1159488 1.0172627 180 N R79 ERJ-1GNF24R9C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GNF24R9C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '24.9 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P122870CT-ND'
PRP Temperature_Coefficient '±200ppm/°C'
PRP Tolerance '±1%'
PRP UniqueID 'RSMD020100010'
PRP Value '24.9 O'
TOP 0 2.1269724 1.0172627 90 N 110 8 1
TOP 1 2.1049252 1.0172627 90 N 125 0 2
#
# CMP 138
CMP 0 2.1049252 0.9832391 270 N R78 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.1049252 0.9722155 180 N 129 0 1
TOP 1 2.1049252 0.9942627 180 N 125 1 2
#
# CMP 139
CMP 0 2.1271476 1.0532858 270 N R77 ERJ-1GNF10R0C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GNF10R0C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '10 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P122669CT-ND'
PRP Temperature_Coefficient '±200ppm/°C'
PRP Tolerance '±1%'
PRP UniqueID 'RSMD020100179'
PRP Value '10 O'
TOP 0 2.1271476 1.0422622 180 N 125 2 1
TOP 1 2.1271476 1.0643094 180 N 166 0 2
#
# CMP 140
CMP 0 2.0769252 0.9832391 270 N R76 ERJ-1GNF33R0C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GNF33R0C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '33 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P122944CT-ND'
PRP Temperature_Coefficient '±200ppm/°C'
PRP Tolerance '±1%'
PRP UniqueID 'RSMD020100013'
PRP Value '33 O'
TOP 0 2.0769252 0.9722155 180 N 154 0 1
TOP 1 2.0769252 0.9942627 180 N 125 3 2
#
# CMP 141
CMP 0 2.1049252 0.8547903 270 N R75 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.1049252 0.8437667 180 N 158 0 1
TOP 1 2.1049252 0.8658139 180 N 154 1 2
#
# CMP 142
CMP 0 2.0939016 0.8207667 0 N R74 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 2.082878 0.8207667 270 N 160 0 1
TOP 1 2.1049252 0.8207667 270 N 158 1 2
#
# CMP 143
CMP 33 2.1049251 1.5700805 90 N L4 180_nH ;0=1,1=0.0217
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/PDF/ENG/L0075S0083LQG15HS.pdf'
PRP CompType 'Inductor'
PRP DCR_ohm '3.38'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP Imax_A '140mA'
PRP Ind_H '180nH'
PRP Irms '0.14A @ C rise'
PRP Isat '0.14A @ % inductance drop'
PRP LatestRevisionDate '2017-06-02'
PRP Manufacturer 'MuRata'
PRP Material 'Air Core'
PRP MountType 'SMT'
PRP PackageReference '0402 polarized'
PRP PartNumber 'LQG15HSR18J02D'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.55'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-2638-1-ND'
PRP Supplier_Part_Number_2 '81-LQG15HSR18J02D'
PRP Supplier_Part_Number_3 ''
PRP SymbolVersion '2008-07-23'
PRP Technology 'Multilayer'
PRP Value ''
PRP Value1 '3.38 ohm'
PRP Value2 '0.14A'
PRP ValueDisplayed '180nH'
TOP 0 2.1049251 1.5887813 90 N 143 3 1
TOP 1 2.1049251 1.5513797 90 N 126 1 2
#
# CMP 144
CMP 33 2.1719681 1.5700805 90 N L3 180_nH ;0=1,1=0.0217
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/PDF/ENG/L0075S0083LQG15HS.pdf'
PRP CompType 'Inductor'
PRP DCR_ohm '3.38'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP Imax_A '140mA'
PRP Ind_H '180nH'
PRP Irms '0.14A @ C rise'
PRP Isat '0.14A @ % inductance drop'
PRP LatestRevisionDate '2017-06-02'
PRP Manufacturer 'MuRata'
PRP Material 'Air Core'
PRP MountType 'SMT'
PRP PackageReference '0402 polarized'
PRP PartNumber 'LQG15HSR18J02D'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.55'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-2638-1-ND'
PRP Supplier_Part_Number_2 '81-LQG15HSR18J02D'
PRP Supplier_Part_Number_3 ''
PRP SymbolVersion '2008-07-23'
PRP Technology 'Multilayer'
PRP Value ''
PRP Value1 '3.38 ohm'
PRP Value2 '0.14A'
PRP ValueDisplayed '180nH'
TOP 0 2.1719681 1.5887813 90 N 142 2 1
TOP 1 2.1719681 1.5513797 90 N 127 1 2
#
# CMP 145
CMP 33 2.1719682 0.9275147 270 N L2 180_nH ;0=1,1=0.0217
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/PDF/ENG/L0075S0083LQG15HS.pdf'
PRP CompType 'Inductor'
PRP DCR_ohm '3.38'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP Imax_A '140mA'
PRP Ind_H '180nH'
PRP Irms '0.14A @ C rise'
PRP Isat '0.14A @ % inductance drop'
PRP LatestRevisionDate '2017-06-02'
PRP Manufacturer 'MuRata'
PRP Material 'Air Core'
PRP MountType 'SMT'
PRP PackageReference '0402 polarized'
PRP PartNumber 'LQG15HSR18J02D'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.55'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-2638-1-ND'
PRP Supplier_Part_Number_2 '81-LQG15HSR18J02D'
PRP Supplier_Part_Number_3 ''
PRP SymbolVersion '2008-07-23'
PRP Technology 'Multilayer'
PRP Value ''
PRP Value1 '3.38 ohm'
PRP Value2 '0.14A'
PRP ValueDisplayed '180nH'
TOP 0 2.1719682 0.9088139 270 N 155 2 1
TOP 1 2.1719682 0.9462155 270 N 128 1 2
#
# CMP 146
CMP 33 2.1049252 0.9275147 270 N L1 180_nH ;0=1,1=0.0217
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/PDF/ENG/L0075S0083LQG15HS.pdf'
PRP CompType 'Inductor'
PRP DCR_ohm '3.38'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP Imax_A '140mA'
PRP Ind_H '180nH'
PRP Irms '0.14A @ C rise'
PRP Isat '0.14A @ % inductance drop'
PRP LatestRevisionDate '2017-06-02'
PRP Manufacturer 'MuRata'
PRP Material 'Air Core'
PRP MountType 'SMT'
PRP PackageReference '0402 polarized'
PRP PartNumber 'LQG15HSR18J02D'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.55'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-2638-1-ND'
PRP Supplier_Part_Number_2 '81-LQG15HSR18J02D'
PRP Supplier_Part_Number_3 ''
PRP SymbolVersion '2008-07-23'
PRP Technology 'Multilayer'
PRP Value ''
PRP Value1 '3.38 ohm'
PRP Value2 '0.14A'
PRP ValueDisplayed '180nH'
TOP 0 2.1049252 0.9088139 270 N 154 2 1
TOP 1 2.1049252 0.9462155 270 N 129 1 2
#
# CMP 147
CMP 29 2.9724623 2.2388757 0 N J11 132134-15 ;0=1,1=0.0602
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color '-'
PRP CompType 'RF Connector'
PRP Current_Rating_(Amps) '-'
PRP datasheet 'https://media.digikey.com/pdf/Data%20Sheets/Amphenol%20PDFs/SMA625IAI-147-3GT5GP-50.pdf'
PRP Length_(in) '-'
PRP Manufacturer 'Amphenol RF'
PRP Mount_Type 'SMD'
PRP PackageReference '-'
PRP PartNumber '132134-15'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'ACX1962-ND'
PRP Text1 'PDN/SYNC'
PRP UniqueID 'cmp00028'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 2.9724623 2.2388757 0 N 11 2 1
TOP 1 2.8724623 2.3388757 0 N 248 463 2
TOP 2 3.0724623 2.3388757 0 N 248 462 3
TOP 3 2.8724623 2.1388757 0 N 248 461 4
TOP 4 3.0724623 2.1388757 0 N 248 460 5
#
# CMP 148
CMP 29 2.8822659 0.625268 0 N J6 132134-15 ;0=1,1=0.0602
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color '-'
PRP CompType 'RF Connector'
PRP Current_Rating_(Amps) '-'
PRP datasheet 'https://media.digikey.com/pdf/Data%20Sheets/Amphenol%20PDFs/SMA625IAI-147-3GT5GP-50.pdf'
PRP Length_(in) '-'
PRP Manufacturer 'Amphenol RF'
PRP Mount_Type 'SMD'
PRP PackageReference '-'
PRP PartNumber '132134-15'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'ACX1962-ND'
PRP Text1 'DCLKIN'
PRP UniqueID 'cmp00028'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 2.8822659 0.625268 0 N 130 1 1
TOP 1 2.7822659 0.725268 0 N 248 420 2
TOP 2 2.9822659 0.725268 0 N 248 421 3
TOP 3 2.7822659 0.525268 0 N 248 422 4
TOP 4 2.9822659 0.525268 0 N 248 423 5
#
# CMP 149
CMP 29 1.2611079 0.9580495 0 N J5 132134-15 ;0=1,1=0.0602
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color '-'
PRP CompType 'RF Connector'
PRP Current_Rating_(Amps) '-'
PRP datasheet 'https://media.digikey.com/pdf/Data%20Sheets/Amphenol%20PDFs/SMA625IAI-147-3GT5GP-50.pdf'
PRP Length_(in) '-'
PRP Manufacturer 'Amphenol RF'
PRP Mount_Type 'SMD'
PRP PackageReference '-'
PRP PartNumber '132134-15'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'ACX1962-ND'
PRP Text1 'CLKn'
PRP UniqueID 'cmp00028'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 1.2611079 0.9580495 0 N 112 1 1
TOP 1 1.1611079 1.0580495 0 N 248 424 2
TOP 2 1.3611079 1.0580495 0 N 248 425 3
TOP 3 1.1611079 0.8580495 0 N 248 426 4
TOP 4 1.3611079 0.8580495 0 N 248 427 5
#
# CMP 150
CMP 29 1.2611079 1.5080495 0 N J4 132134-15 ;0=1,1=0.0602
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color '-'
PRP CompType 'RF Connector'
PRP Current_Rating_(Amps) '-'
PRP datasheet 'https://media.digikey.com/pdf/Data%20Sheets/Amphenol%20PDFs/SMA625IAI-147-3GT5GP-50.pdf'
PRP Length_(in) '-'
PRP Manufacturer 'Amphenol RF'
PRP Mount_Type 'SMD'
PRP PackageReference '-'
PRP PartNumber '132134-15'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'ACX1962-ND'
PRP Text1 'CLKp'
PRP UniqueID 'cmp00028'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 1.2611079 1.5080495 0 N 111 1 1
TOP 1 1.1611079 1.6080495 0 N 248 428 2
TOP 2 1.3611079 1.6080495 0 N 248 429 3
TOP 3 1.1611079 1.4080495 0 N 248 430 4
TOP 4 1.3611079 1.4080495 0 N 248 431 5
#
# CMP 151
CMP 29 1.8624623 2.2988757 0 N J10 132134-15 ;0=1,1=0.0602
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color '-'
PRP CompType 'RF Connector'
PRP Current_Rating_(Amps) '-'
PRP datasheet 'https://media.digikey.com/pdf/Data%20Sheets/Amphenol%20PDFs/SMA625IAI-147-3GT5GP-50.pdf'
PRP Length_(in) '-'
PRP Manufacturer 'Amphenol RF'
PRP Mount_Type 'SMD'
PRP PackageReference '-'
PRP PartNumber '132134-15'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'ACX1962-ND'
PRP Text1 'CHBp'
PRP UniqueID 'cmp00028'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 1.8624623 2.2988757 0 N 139 0 1
TOP 1 1.7624623 2.3988757 0 N 248 435 2
TOP 2 1.9624623 2.3988757 0 N 248 434 3
TOP 3 1.7624623 2.1988757 0 N 248 433 4
TOP 4 1.9624623 2.1988757 0 N 248 432 5
#
# CMP 152
CMP 29 2.4124623 2.2988757 0 N J9 132134-15 ;0=1,1=0.0602
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color '-'
PRP CompType 'RF Connector'
PRP Current_Rating_(Amps) '-'
PRP datasheet 'https://media.digikey.com/pdf/Data%20Sheets/Amphenol%20PDFs/SMA625IAI-147-3GT5GP-50.pdf'
PRP Length_(in) '-'
PRP Manufacturer 'Amphenol RF'
PRP Mount_Type 'SMD'
PRP PackageReference '-'
PRP PartNumber '132134-15'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'ACX1962-ND'
PRP Text1 'CHBn'
PRP UniqueID 'cmp00028'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 2.4124623 2.2988757 0 N 149 0 1
TOP 1 2.3124623 2.3988757 0 N 248 436 2
TOP 2 2.5124623 2.3988757 0 N 248 437 3
TOP 3 2.3124623 2.1988757 0 N 248 438 4
TOP 4 2.5124623 2.1988757 0 N 248 439 5
#
# CMP 153
CMP 29 2.4134467 0.1987195 0 N J8 132134-15 ;0=1,1=0.0602
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color '-'
PRP CompType 'RF Connector'
PRP Current_Rating_(Amps) '-'
PRP datasheet 'https://media.digikey.com/pdf/Data%20Sheets/Amphenol%20PDFs/SMA625IAI-147-3GT5GP-50.pdf'
PRP Length_(in) '-'
PRP Manufacturer 'Amphenol RF'
PRP Mount_Type 'SMD'
PRP PackageReference '-'
PRP PartNumber '132134-15'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'ACX1962-ND'
PRP Text1 'CHAn'
PRP UniqueID 'cmp00028'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 2.4134467 0.1987195 0 N 151 0 1
TOP 1 2.3134467 0.2987195 0 N 248 440 2
TOP 2 2.5134467 0.2987195 0 N 248 441 3
TOP 3 2.3134467 0.0987195 0 N 248 442 4
TOP 4 2.5134467 0.0987195 0 N 248 443 5
#
# CMP 154
CMP 29 1.8634467 0.1987195 0 N J7 132134-15 ;0=1,1=0.0602
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color '-'
PRP CompType 'RF Connector'
PRP Current_Rating_(Amps) '-'
PRP datasheet 'https://media.digikey.com/pdf/Data%20Sheets/Amphenol%20PDFs/SMA625IAI-147-3GT5GP-50.pdf'
PRP Length_(in) '-'
PRP Manufacturer 'Amphenol RF'
PRP Mount_Type 'SMD'
PRP PackageReference '-'
PRP PartNumber '132134-15'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'ACX1962-ND'
PRP Text1 'CHAp'
PRP UniqueID 'cmp00028'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 1.8634467 0.1987195 0 N 161 0 1
TOP 1 1.7634467 0.2987195 0 N 248 444 2
TOP 2 1.9634467 0.2987195 0 N 248 445 3
TOP 3 1.7634467 0.0987195 0 N 248 446 4
TOP 4 1.9634467 0.0987195 0 N 248 447 5
#
# CMP 155
CMP 1 2.7712422 0.825268 0 N C56 GRM033Z71C104ME14D ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033Z71C104ME14-01.pdf'
PRP Manufacturer 'Murata Electronics'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'GRM033Z71C104ME14D'
PRP Ratings '-'
PRP Series 'GRM'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.33'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '490-GRM033Z71C104ME14DCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±20%'
PRP UniqueID 'capcc09270'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '16V'
TOP 0 2.7602187 0.825268 270 N 131 2 1
TOP 1 2.7822659 0.825268 270 N 130 2 2
#
# CMP 156
CMP 1 1.9671789 1.2217505 0 N C54 GRM033Z71C104ME14D ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033Z71C104ME14-01.pdf'
PRP Manufacturer 'Murata Electronics'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'GRM033Z71C104ME14D'
PRP Ratings '-'
PRP Series 'GRM'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.33'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '490-GRM033Z71C104ME14DCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±20%'
PRP UniqueID 'capcc09270'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '16V'
TOP 0 1.9561553 1.2217505 270 N 133 2 1
TOP 1 1.9782025 1.2217505 270 N 163 1 2
#
# CMP 157
CMP 1 1.8721315 1.199528 180 N C53 GRM033Z71C104ME14D ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033Z71C104ME14-01.pdf'
PRP Manufacturer 'Murata Electronics'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'GRM033Z71C104ME14D'
PRP Ratings '-'
PRP Series 'GRM'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.33'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '490-GRM033Z71C104ME14DCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±20%'
PRP UniqueID 'capcc09270'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '16V'
TOP 0 1.8831551 1.199528 90 N 133 3 1
TOP 1 1.8611079 1.199528 90 N 132 0 2
#
# CMP 158
CMP 1 1.8770845 1.2330495 0 N C51 GRM033Z71C104ME14D ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033Z71C104ME14-01.pdf'
PRP Manufacturer 'Murata Electronics'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'GRM033Z71C104ME14D'
PRP Ratings '-'
PRP Series 'GRM'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.33'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '490-GRM033Z71C104ME14DCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±20%'
PRP UniqueID 'capcc09270'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '16V'
TOP 0 1.8660609 1.2330495 270 N 248 357 1
TOP 1 1.8881081 1.2330495 270 N 134 3 2
#
# CMP 159
CMP 1 1.4950843 1.2330495 180 N C50 GRM033Z71C104ME14D ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033Z71C104ME14-01.pdf'
PRP Manufacturer 'Murata Electronics'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'GRM033Z71C104ME14D'
PRP Ratings '-'
PRP Series 'GRM'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.33'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '490-GRM033Z71C104ME14DCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±20%'
PRP UniqueID 'capcc09270'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '16V'
TOP 0 1.5061079 1.2330495 90 N 93 0 1
TOP 1 1.4840607 1.2330495 90 N 248 358 2
#
# CMP 160
CMP 1 1.8721315 1.266571 0 N C49 GRM033Z71C104ME14D ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033Z71C104ME14-01.pdf'
PRP Manufacturer 'Murata Electronics'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'GRM033Z71C104ME14D'
PRP Ratings '-'
PRP Series 'GRM'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.33'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '490-GRM033Z71C104ME14DCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±20%'
PRP UniqueID 'capcc09270'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '16V'
TOP 0 1.8611079 1.266571 270 N 135 0 1
TOP 1 1.8831551 1.266571 270 N 137 2 2
#
# CMP 161
CMP 1 1.4611079 0.9690731 90 N C52 GRM033Z71C104ME14D ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033Z71C104ME14-01.pdf'
PRP Manufacturer 'Murata Electronics'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'GRM033Z71C104ME14D'
PRP Ratings '-'
PRP Series 'GRM'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.33'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '490-GRM033Z71C104ME14DCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±20%'
PRP UniqueID 'capcc09270'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '16V'
TOP 0 1.4611079 0.9800967 0 N 136 0 1
TOP 1 1.4611079 0.9580495 0 N 112 2 2
#
# CMP 162
CMP 1 1.9671789 1.2443486 0 N C48 GRM033Z71C104ME14D ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033Z71C104ME14-01.pdf'
PRP Manufacturer 'Murata Electronics'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'GRM033Z71C104ME14D'
PRP Ratings '-'
PRP Series 'GRM'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.33'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '490-GRM033Z71C104ME14DCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±20%'
PRP UniqueID 'capcc09270'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '16V'
TOP 0 1.9561553 1.2443486 270 N 137 3 1
TOP 1 1.9782025 1.2443486 270 N 162 1 2
#
# CMP 163
CMP 1 1.8624623 2.0878521 90 N C72 GRM033Z71C104ME14D ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033Z71C104ME14-01.pdf'
PRP Manufacturer 'Murata Electronics'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'GRM033Z71C104ME14D'
PRP Ratings '-'
PRP Series 'GRM'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.33'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '490-GRM033Z71C104ME14DCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±20%'
PRP UniqueID 'capcc09270'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '16V'
TOP 0 1.8624623 2.0988757 0 N 139 1 1
TOP 1 1.8624623 2.0768285 0 N 138 1 2
#
# CMP 164
CMP 1 2.1049251 1.6878521 270 N C71 GRM033Z71C104ME14D ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033Z71C104ME14-01.pdf'
PRP Manufacturer 'Murata Electronics'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'GRM033Z71C104ME14D'
PRP Ratings '-'
PRP Series 'GRM'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.33'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '490-GRM033Z71C104ME14DCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±20%'
PRP UniqueID 'capcc09270'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '16V'
TOP 0 2.1049251 1.6768285 180 N 141 2 1
TOP 1 2.1049251 1.6988757 180 N 140 0 2
#
# CMP 165
CMP 1 2.1379445 1.6117813 0 N C70 CGA1A2X7R1E101M030BA ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://product.tdk.com/system/files/dam/doc/product/capacitor/ceramic/mlcc/catalog/mlcc_automotive_general_en.pdf'
PRP Manufacturer 'TDK Corporation'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'CGA1A2X7R1E101M030BA'
PRP Ratings 'AEC-Q200'
PRP Series 'CGA'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.33'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '445-12088-1-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±20%'
PRP UniqueID 'capcc06388'
PRP Value '100 pF'
PRP Voltage_-_Rated '25V'
TOP 0 2.1269209 1.6117813 270 N 143 2 1
TOP 1 2.1489681 1.6117813 270 N 142 3 2
#
# CMP 166
CMP 1 2.1374623 1.6928521 90 N C69 GRM033Z71C104ME14D ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033Z71C104ME14-01.pdf'
PRP Manufacturer 'Murata Electronics'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'GRM033Z71C104ME14D'
PRP Ratings '-'
PRP Series 'GRM'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.33'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '490-GRM033Z71C104ME14DCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±20%'
PRP UniqueID 'capcc09270'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '16V'
TOP 0 2.1374623 1.7038757 0 N 144 0 1
TOP 1 2.1374623 1.6818285 0 N 248 359 2
#
# CMP 167
CMP 1 2.1384464 1.5129676 90 N C68 GRM033Z71C104ME14D ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033Z71C104ME14-01.pdf'
PRP Manufacturer 'Murata Electronics'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'GRM033Z71C104ME14D'
PRP Ratings '-'
PRP Series 'GRM'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.33'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '490-GRM033Z71C104ME14DCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±20%'
PRP UniqueID 'capcc09270'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '16V'
TOP 0 2.1384464 1.5239912 0 N 248 360 1
TOP 1 2.1384464 1.501944 0 N 110 9 2
#
# CMP 168
CMP 1 2.4014387 2.0988757 180 N C66 GRM033Z71C104ME14D ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033Z71C104ME14-01.pdf'
PRP Manufacturer 'Murata Electronics'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'GRM033Z71C104ME14D'
PRP Ratings '-'
PRP Series 'GRM'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.33'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '490-GRM033Z71C104ME14DCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±20%'
PRP UniqueID 'capcc09270'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '16V'
TOP 0 2.4124623 2.0988757 90 N 149 1 1
TOP 1 2.3904151 2.0988757 90 N 145 0 2
#
# CMP 169
CMP 1 2.1719681 1.6878521 90 N C67 GRM033Z71C104ME14D ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033Z71C104ME14-01.pdf'
PRP Manufacturer 'Murata Electronics'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'GRM033Z71C104ME14D'
PRP Ratings '-'
PRP Series 'GRM'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.33'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '490-GRM033Z71C104ME14DCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±20%'
PRP UniqueID 'capcc09270'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '16V'
TOP 0 2.1719681 1.6988757 0 N 147 0 1
TOP 1 2.1719681 1.6768285 0 N 146 2 2
#
# CMP 170
CMP 1 2.4124623 2.0878521 90 N C65 GRM033Z71C104ME14D ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033Z71C104ME14-01.pdf'
PRP Manufacturer 'Murata Electronics'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'GRM033Z71C104ME14D'
PRP Ratings '-'
PRP Series 'GRM'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.33'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '490-GRM033Z71C104ME14DCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±20%'
PRP UniqueID 'capcc09270'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '16V'
TOP 0 2.4124623 2.0988757 0 N 149 2 1
TOP 1 2.4124623 2.0768285 0 N 148 1 2
#
# CMP 171
CMP 1 2.4134467 0.4097431 270 N C64 GRM033Z71C104ME14D ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033Z71C104ME14-01.pdf'
PRP Manufacturer 'Murata Electronics'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'GRM033Z71C104ME14D'
PRP Ratings '-'
PRP Series 'GRM'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.33'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '490-GRM033Z71C104ME14DCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±20%'
PRP UniqueID 'capcc09270'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '16V'
TOP 0 2.4134467 0.3987195 180 N 151 1 1
TOP 1 2.4134467 0.4207667 180 N 150 1 2
#
# CMP 172
CMP 1 2.1729525 0.8097431 90 N C63 GRM033Z71C104ME14D ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033Z71C104ME14-01.pdf'
PRP Manufacturer 'Murata Electronics'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'GRM033Z71C104ME14D'
PRP Ratings '-'
PRP Series 'GRM'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.33'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '490-GRM033Z71C104ME14DCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±20%'
PRP UniqueID 'capcc09270'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '16V'
TOP 0 2.1729525 0.8207667 0 N 153 2 1
TOP 1 2.1729525 0.7987195 0 N 152 1 2
#
# CMP 173
CMP 1 2.1389488 0.8858139 180 N C62 CGA1A2X7R1E101M030BA ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://product.tdk.com/system/files/dam/doc/product/capacitor/ceramic/mlcc/catalog/mlcc_automotive_general_en.pdf'
PRP Manufacturer 'TDK Corporation'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'CGA1A2X7R1E101M030BA'
PRP Ratings 'AEC-Q200'
PRP Series 'CGA'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.33'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '445-12088-1-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±20%'
PRP UniqueID 'capcc06388'
PRP Value '100 pF'
PRP Voltage_-_Rated '25V'
TOP 0 2.1499724 0.8858139 90 N 155 3 1
TOP 1 2.1279252 0.8858139 90 N 154 3 2
#
# CMP 174
CMP 1 2.1384467 0.8047431 270 N C60 GRM033Z71C104ME14D ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033Z71C104ME14-01.pdf'
PRP Manufacturer 'Murata Electronics'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'GRM033Z71C104ME14D'
PRP Ratings '-'
PRP Series 'GRM'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.33'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '490-GRM033Z71C104ME14DCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±20%'
PRP UniqueID 'capcc09270'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '16V'
TOP 0 2.1384467 0.7937195 180 N 156 1 1
TOP 1 2.1384467 0.8157667 180 N 248 361 2
#
# CMP 175
CMP 1 2.1384469 0.9832391 270 N C61 GRM033Z71C104ME14D ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033Z71C104ME14-01.pdf'
PRP Manufacturer 'Murata Electronics'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'GRM033Z71C104ME14D'
PRP Ratings '-'
PRP Series 'GRM'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.33'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '490-GRM033Z71C104ME14DCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±20%'
PRP UniqueID 'capcc09270'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '16V'
TOP 0 2.1384469 0.9722155 180 N 248 362 1
TOP 1 2.1384469 0.9942627 180 N 110 10 2
#
# CMP 176
CMP 1 1.8744703 0.3987195 0 N C58 GRM033Z71C104ME14D ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033Z71C104ME14-01.pdf'
PRP Manufacturer 'Murata Electronics'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'GRM033Z71C104ME14D'
PRP Ratings '-'
PRP Series 'GRM'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.33'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '490-GRM033Z71C104ME14DCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±20%'
PRP UniqueID 'capcc09270'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '16V'
TOP 0 1.8634467 0.3987195 270 N 161 1 1
TOP 1 1.8854939 0.3987195 270 N 157 1 2
#
# CMP 177
CMP 1 2.1049252 0.8097431 270 N C59 GRM033Z71C104ME14D ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033Z71C104ME14-01.pdf'
PRP Manufacturer 'Murata Electronics'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'GRM033Z71C104ME14D'
PRP Ratings '-'
PRP Series 'GRM'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.33'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '490-GRM033Z71C104ME14DCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±20%'
PRP UniqueID 'capcc09270'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '16V'
TOP 0 2.1049252 0.7987195 180 N 159 1 1
TOP 1 2.1049252 0.8207667 180 N 158 2 2
#
# CMP 178
CMP 1 1.8634467 0.4097431 270 N C57 GRM033Z71C104ME14D ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033Z71C104ME14-01.pdf'
PRP Manufacturer 'Murata Electronics'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'GRM033Z71C104ME14D'
PRP Ratings '-'
PRP Series 'GRM'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.33'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '490-GRM033Z71C104ME14DCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±20%'
PRP UniqueID 'capcc09270'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '16V'
TOP 0 1.8634467 0.3987195 180 N 161 2 1
TOP 1 1.8634467 0.4207667 180 N 160 1 2
#
# CMP 179
CMP 37 0.3251442 0.1198529 0 N D1 LTST-C191TGKT ;0=1,1=0.0354
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color 'Green'
PRP CompType 'LED'
PRP Current_Rating_(Amps) '20mA'
PRP datasheet '-'
PRP Length_(in) '-'
PRP Manufacturer 'Lite-On Inc.'
PRP Mount_Type 'SMD'
PRP PackageReference '-'
PRP PartNumber 'LTST-C191TGKT'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '0.65'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '160-1888-1-ND'
PRP Text1 '12V'
PRP UniqueID 'cmp00247'
PRP Voltage_-_Forward_(Vf)_(Typ) '3.2V'
PRP Voltage_Rating_-_DC '-'
TOP 0 0.2956167 0.1198529 0 N 237 17 1
TOP 1 0.3546718 0.1198529 0 N 184 1 2
#
# CMP 180
CMP 41 0.9524967 0.7209945 180 N PP1 Probe_Point ;0=2,1=0.1570
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color '-'
PRP CompType 'Probe Point'
PRP Current_Rating_(Amps) '-'
PRP datasheet '-'
PRP Length_(in) '-'
PRP Manufacturer '-'
PRP Mount_Type '-'
PRP PackageReference '-'
PRP PartNumber '-'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Text1 '3p3V'
PRP UniqueID 'cmp00025'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 0.9524967 0.7209945 180 N 238 67 1
#
# CMP 181
CMP 36 0.4663254 0.70079 0 N TP2 5125 ;0=2,1=0.3200
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color 'Brown'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.keyelco.com/userAssets/file/M60-2p60.pdf'
PRP CompType 'TestPoint'
PRP Current_Rating_(Amps) '-'
PRP datasheet 'https://www.keyelco.com/userAssets/file/M65p56.pdf'
PRP Length_(in) '-'
PRP Manufacturer 'Keystone'
PRP Mount_Type 'TH'
PRP PackageReference '-'
PRP PartNumber '5125'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '36-5125-ND'
PRP Text1 'EXT GND'
PRP UniqueID 'cmp00047'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 0.4663254 0.70079 0 N 182 10 1
#
# CMP 182
CMP 34 0.7860498 0.6480012 0 N TP1 5010 ;0=2,1=0.3200
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color 'Red'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.keyelco.com/userAssets/file/M60-2p60.pdf'
PRP CompType 'TestPoint'
PRP Current_Rating_(Amps) '-'
PRP datasheet 'https://www.keyelco.com/userAssets/file/M65p56.pdf'
PRP Length_(in) '-'
PRP Manufacturer 'Keystone'
PRP Mount_Type 'TH'
PRP PackageReference '-'
PRP PartNumber '5010'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '36-5010-ND'
PRP Text1 'EXT 12V'
PRP UniqueID 'cmp00040'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 0.7860498 0.6480012 0 N 183 2 1
#
# CMP 183
CMP 11 1.0888057 0.2983161 90 N SW1 500ASSP1M2QE ;0=2,1=0.5244
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color '-'
PRP CompType 'Switch Slide'
PRP Current_Rating_(Amps) '3A'
PRP datasheet 'https://sten-eswitch-13110800-production.s3.amazonaws.com/system/asset/product_line/data_sheet/116/500A.pdf'
PRP Length_(in) '-'
PRP Manufacturer 'E-Switch'
PRP Mount_Type 'TH'
PRP PackageReference '-'
PRP PartNumber '500ASSP1M2QE'
PRP Pitch_(mm) '2.54'
PRP Series '500A'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'EG2481-ND'
PRP Text1 'JACK'
PRP Text2 '12V'
PRP Text3 'FMC'
PRP UniqueID 'cmp00460'
PRP Voltage_Rating_-_DC '120V'
TOP 0 1.0888057 0.3983161 90 N 189 4 1
TOP 1 1.0888057 0.2983161 90 N 181 5 2
TOP 2 1.0888057 0.1983161 90 N 251 3 3
#
# CMP 184
CMP 42 -0.1484062 0.4430007 0 N J2 RAPC722X ;0=2,1=0.4400
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color '-'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.switchcraft.com/Drawings/rapc722x_cd.pdf'
PRP CompType 'Power'
PRP Current_Rating_(Amps) '-'
PRP datasheet '-'
PRP Length_(in) '-'
PRP Manufacturer 'Switchcraft'
PRP Mount_Type 'TH'
PRP PackageReference '-'
PRP PartNumber 'RAPC722X'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'SC1313-ND'
PRP Text1 '12V 2A'
PRP UniqueID 'cmp00022'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 0.4104278 0.4430007 90 N 183 3 1
TOP 1 0.1644278 0.4430007 270 N 182 11 2
TOP 2 0.2924278 0.2579613 0 N 182 12 3
#
# CMP 185
CMP 28 0.734475 0.319576 270 N F1 BNX002-11 ;0=2,1=0.0000
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color '-'
PRP CompType 'Filter'
PRP Current_Rating_(Amps) '-'
PRP datasheet 'https://www.mouser.com/datasheet/2/281/1/ENFH0011-3074219.pdf'
PRP Length_(in) '-'
PRP Manufacturer 'Murata Electronics'
PRP Mount_Type 'TH'
PRP PackageReference '-'
PRP PartNumber 'BNX002-11'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Supplier_1 'Mouser'
PRP Supplier_Part_Number_1 '81-BNX002-11'
PRP Text1 'EMI Filter 40DB 50V 10A'
PRP UniqueID 'cmp00325'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 0.6360498 0.4180012 270 N 183 1 1
TOP 1 0.8329002 0.4180012 270 N 189 5 2
TOP 2 0.6360498 0.2211508 270 N 182 9 3
TOP 3 0.734475 0.5164264 270 N 188 8 4
TOP 4 0.734475 0.319576 270 N 188 9 4
TOP 5 0.8329002 0.2211508 270 N 188 10 4
#
# CMP 186
CMP 2 1.094843 2.1920409 0 N R55 ERA-2AEB103X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thin Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDM0000/AOA0000C307.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERA-2AEB103X'
PRP Power_(Watts) '0.063W, 1/16W'
PRP Ratings 'AEC-Q200'
PRP Resistance '10 kO'
PRP Series 'ERA-2A'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P10KDCCT-ND'
PRP Temperature_Coefficient '±25ppm/°C'
PRP Tolerance '±0.1%'
PRP UniqueID 'RSMD040200315'
PRP Value '10 kO'
TOP 0 1.075158 2.1920409 270 N 248 415 1
TOP 1 1.1145281 2.1920409 270 N 7 2 2
#
# CMP 187
CMP 41 1.385 2.185965 0 N PP9 Probe_Point ;0=2,1=0.1570
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color '-'
PRP CompType 'Probe Point'
PRP Current_Rating_(Amps) '-'
PRP datasheet '-'
PRP Length_(in) '-'
PRP Manufacturer '-'
PRP Mount_Type '-'
PRP PackageReference '-'
PRP PartNumber '-'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Text1 'SDIO'
PRP UniqueID 'cmp00025'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 1.385 2.185965 0 N 192 2 1
#
# CMP 188
CMP 41 1.385 2.245965 0 N PP8 Probe_Point ;0=2,1=0.1570
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color '-'
PRP CompType 'Probe Point'
PRP Current_Rating_(Amps) '-'
PRP datasheet '-'
PRP Length_(in) '-'
PRP Manufacturer '-'
PRP Mount_Type '-'
PRP PackageReference '-'
PRP PartNumber '-'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Text1 'CS'
PRP UniqueID 'cmp00025'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 1.385 2.245965 0 N 113 2 1
#
# CMP 189
CMP 41 1.385 2.125965 0 N PP7 Probe_Point ;0=2,1=0.1570
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color '-'
PRP CompType 'Probe Point'
PRP Current_Rating_(Amps) '-'
PRP datasheet '-'
PRP Length_(in) '-'
PRP Manufacturer '-'
PRP Mount_Type '-'
PRP PackageReference '-'
PRP PartNumber '-'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Text1 'SCLK'
PRP UniqueID 'cmp00025'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 1.385 2.125965 0 N 195 2 1
#
# CMP 190
CMP 4 1.0995281 2.0886156 270 N C46 GRT155R71E104KE01J ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet '-'
PRP Manufacturer 'Murata'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0402'
PRP PartNumber 'GRT155R71E104KE01J'
PRP Ratings '-'
PRP Series '-'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Digi-key'
PRP Supplier_Part_Number_1 '490-GRT155R71E104KE01JCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±10%'
PRP UniqueID 'capcc09401'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '25V'
TOP 0 1.0995281 2.0689306 180 N 248 363 1
TOP 1 1.0995281 2.1083007 180 N 170 23 2
#
# CMP 191
CMP 31 1.5636081 0.5296063 270 N SW4 FSMSM ;0=1,1=0.2500
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color '-'
PRP CompType 'Push Button'
PRP Current_Rating_(Amps) '-'
PRP datasheet 'https://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=1437566-3&DocType=Customer+Drawing&DocLang=English'
PRP Length_(in) '-'
PRP Manufacturer 'TE Connectivity'
PRP Mount_Type '-'
PRP PackageReference '-'
PRP PartNumber 'FSMSM'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'A101402CT-ND'
PRP Text1 'RESET'
PRP UniqueID 'cmp00234'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 1.5636081 0.3485039 270 N 202 2 1
TOP 1 1.5636081 0.7107087 270 N 248 390 2
#
# CMP 192
CMP 10 0.10748 1.815 90 N SW2 cmp00353 ;0=2,1=0.2559
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color '-'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.ckswitches.com/media/1429/1000.pdf'
PRP CompType 'Switch Slide'
PRP Current_Rating_(Amps) '-'
PRP datasheet 'https://www.mouser.com/datasheet/2/445/450301014042-1717397.pdf'
PRP Length_(in) '-'
PRP Manufacturer 'Wurth Elektronik'
PRP Mount_Type 'TH'
PRP PackageReference '-'
PRP PartNumber '450301014042'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Supplier_1 'Mouser'
PRP Supplier_Part_Number_1 '710-450301014042'
PRP Text1 'COMM MUX'
PRP Text2 'FMC'
PRP Text3 'USB'
PRP UniqueID 'cmp00353'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 0.10748 1.815 90 N 205 3 1
TOP 1 0.10748 1.915 90 N 1 1 2
TOP 2 0.10748 1.715 90 N 248 452 3
#
# CMP 193
CMP 41 1.4582067 0.710709 180 N PP10 Probe_Point ;0=2,1=0.1570
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color '-'
PRP CompType 'Probe Point'
PRP Current_Rating_(Amps) '-'
PRP datasheet '-'
PRP Length_(in) '-'
PRP Manufacturer '-'
PRP Mount_Type '-'
PRP PackageReference '-'
PRP PartNumber '-'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Text1 'RESET'
PRP UniqueID 'cmp00025'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 1.4582067 0.710709 180 N 203 6 1
#
# CMP 194
CMP 4 1.2293312 2.1653873 0 N C47 GRT155R71E104KE01J ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet '-'
PRP Manufacturer 'Murata'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0402'
PRP PartNumber 'GRT155R71E104KE01J'
PRP Ratings '-'
PRP Series '-'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Digi-key'
PRP Supplier_Part_Number_1 '490-GRT155R71E104KE01JCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±10%'
PRP UniqueID 'capcc09401'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '25V'
TOP 0 1.2096462 2.1653873 270 N 248 364 1
TOP 1 1.2490163 2.1653873 270 N 238 55 2
#
# CMP 195
CMP 45 2.6336439 0.8547956 180 N U17 TMUX136RSE ;0=1,1=0.0236
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color '-'
PRP CompType 'Switch'
PRP Current_Rating_(Amps) '-'
PRP datasheet 'https://www.ti.com/lit/gpn/TMUX136'
PRP Length_(in) '-'
PRP Manufacturer 'Texas Instruments'
PRP Mount_Type 'SMD'
PRP PackageReference '-'
PRP PartNumber 'TMUX136RSER'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Supplier_1 '-'
PRP Supplier_Part_Number_1 '-'
PRP Text1 'SEL: LOW A?COM, HIGH B?COM'
PRP UniqueID 'cmp00385'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 2.6602187 0.825268 90 N 131 3 1
TOP 1 2.6602187 0.8449531 90 N 0 252 2
TOP 2 2.6602187 0.8646381 90 N 49 1 3
TOP 3 2.6602187 0.8843231 90 N 0 253 4
TOP 4 2.6336438 0.8902287 180 N 248 409 5
TOP 5 2.6070691 0.8843231 90 N 248 408 6
TOP 6 2.6070691 0.8646381 90 N 0 254 7
TOP 7 2.6070691 0.8449531 90 N 50 1 8
TOP 8 2.6070691 0.825268 90 N 13 0 9
TOP 9 2.6336438 0.8193625 180 N 238 64 10
#
# CMP 196
CMP 37 0.31 2.05 0 N D6 LTST-C191TGKT ;0=1,1=0.0354
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color 'Green'
PRP CompType 'LED'
PRP Current_Rating_(Amps) '20mA'
PRP datasheet '-'
PRP Length_(in) '-'
PRP Manufacturer 'Lite-On Inc.'
PRP Mount_Type 'SMD'
PRP PackageReference '-'
PRP PartNumber 'LTST-C191TGKT'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '0.65'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '160-1888-1-ND'
PRP Text1 'USB'
PRP UniqueID 'cmp00247'
PRP Voltage_-_Forward_(Vf)_(Typ) '3.2V'
PRP Voltage_Rating_-_DC '-'
TOP 0 0.2804725 2.05 0 N 221 1 1
TOP 1 0.3395276 2.05 0 N 213 1 2
#
# CMP 197
CMP 0 0.4039769 2.0701706 180 N R36 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 0.4150005 2.0701706 90 N 232 0 1
TOP 1 0.3929533 2.0701706 90 N 210 2 2
#
# CMP 198
CMP 54 0.4031825 2.5222216 315 N Y1 ABM3-12.000MHZ-D2Y-T ;0=1,1=0.0512
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color '-'
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.abracon.com/Resonators/abm3.pdf'
PRP CompType 'XO'
PRP Current_Rating_(Amps) '-'
PRP datasheet 'https://abracon.com/Resonators/ABM3.pdf'
PRP Length_(in) '-'
PRP Manufacturer 'Abracon LLC'
PRP Mount_Type 'SMD'
PRP PackageReference '-'
PRP PartNumber 'ABM3-12.000MHZ-D2Y-T'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Supplier_1 'Mouser'
PRP Supplier_Part_Number_1 '815-ABM3-12-D2Y-T'
PRP Text1 '12MHz'
PRP UniqueID 'cmp00323'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 0.3461129 2.465152 315 N 234 2 1
TOP 1 0.4602522 2.5792913 315 N 233 2 2
#
# CMP 199
CMP 1 0.5080471 2.6114964 225 N C43 GJM0336C1E180JB01J ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GJM0336C1E180JB01-01.pdf'
PRP Manufacturer 'Murata Electronics'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'GJM0336C1E180JB01J'
PRP Ratings '-'
PRP Series 'GJM'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.33'
PRP Supplier_1 'Digi-Key'
PRP Temperature_Coefficient 'C0H'
PRP Tolerance '±5%'
PRP UniqueID 'capcc08580'
PRP Value '18 pF'
PRP Voltage_-_Rated '25V'
TOP 0 0.515842 2.6037015 135 N 248 365 1
TOP 1 0.5002522 2.6192913 135 N 233 0 2
#
# CMP 200
CMP 1 0.3139078 2.4173571 225 N C42 GJM0336C1E180JB01J ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GJM0336C1E180JB01-01.pdf'
PRP Manufacturer 'Murata Electronics'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'GJM0336C1E180JB01J'
PRP Ratings '-'
PRP Series 'GJM'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.33'
PRP Supplier_1 'Digi-Key'
PRP Temperature_Coefficient 'C0H'
PRP Tolerance '±5%'
PRP UniqueID 'capcc08580'
PRP Value '18 pF'
PRP Voltage_-_Rated '25V'
TOP 0 0.3217027 2.4095622 135 N 248 366 1
TOP 1 0.3061129 2.425152 135 N 234 0 2
#
# CMP 201
CMP 4 0.3760009 2.3260762 90 N C33 C1005X5R1A475K050BC ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://product.tdk.com/system/files/dam/doc/product/capacitor/ceramic/mlcc/catalog/mlcc_commercial_general_en.pdf'
PRP Manufacturer 'TDK Corporation'
PRP Operating_Temperature '-55°C ~ 85°C'
PRP PackageReference '0402'
PRP PartNumber 'C1005X5R1A475K050BC'
PRP Ratings '-'
PRP Series 'C'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.65'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '445-13820-1-ND'
PRP Temperature_Coefficient 'X5R'
PRP Tolerance '±10%'
PRP UniqueID 'capcc03298'
PRP Value '4.7 uF'
PRP Voltage_-_Rated '10V'
TOP 0 0.3760009 2.3457612 0 N 248 367 1
TOP 1 0.3760009 2.3063911 0 N 235 1 2
#
# CMP 202
CMP 3 0.34 2.3260762 90 N FB5 NFZ15SG151SN11D ;0=1,1=0.0236
PRP CompType 'FerriteBead'
PRP Current '1A'
PRP datasheet 'https://www.murata.com/en-us/products/productdata/8796735995934/ENFJ0010.pdf'
PRP DCR '120 mO'
PRP Impedance '-'
PRP Manufacturer 'Murata Electronics'
PRP Operating_Temperature '-40°C ~ 85°C'
PRP PackageReference '0402'
PRP PartNumber 'NFZ15SG151SN11D'
PRP Series 'NFZ'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '490-18375-1-ND'
PRP Temperature_Coefficient '-'
PRP Tolerance '-'
PRP UniqueID 'dcp00209'
PRP Value '-'
PRP Voltage_-_Rated '-'
TOP 0 0.34 2.3457612 0 N 238 56 1
TOP 1 0.34 2.3063911 0 N 235 2 2
#
# CMP 203
CMP 4 0.4100009 2.3260762 90 N C34 GRT155R71E104KE01J ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet '-'
PRP Manufacturer 'Murata'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0402'
PRP PartNumber 'GRT155R71E104KE01J'
PRP Ratings '-'
PRP Series '-'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Digi-key'
PRP Supplier_Part_Number_1 '490-GRT155R71E104KE01JCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±10%'
PRP UniqueID 'capcc09401'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '25V'
TOP 0 0.4100009 2.3457612 0 N 248 368 1
TOP 1 0.4100009 2.3063911 0 N 235 3 2
#
# CMP 204
CMP 2 0.3498425 2.2547415 0 N R43 ERJ-2GEJ100X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://b2b-api.panasonic.eu/file_stream/pids/fileversion/1242'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GEJ100X'
PRP Power_(Watts) '0.1W, 1/10W'
PRP Ratings 'AEC-Q200'
PRP Resistance '10 O'
PRP Series 'ERJ-2G'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P10JCT-ND'
PRP Temperature_Coefficient '±200ppm/°C'
PRP Tolerance '±5%'
PRP UniqueID 'RSMD040200327'
PRP Value '10 O'
TOP 0 0.3301575 2.2547415 270 N 85 0 1
TOP 1 0.3695276 2.2547415 270 N 229 0 2
#
# CMP 205
CMP 2 0.3498425 2.2202455 0 N R44 ERJ-2GEJ100X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://b2b-api.panasonic.eu/file_stream/pids/fileversion/1242'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GEJ100X'
PRP Power_(Watts) '0.1W, 1/10W'
PRP Ratings 'AEC-Q200'
PRP Resistance '10 O'
PRP Series 'ERJ-2G'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P10JCT-ND'
PRP Temperature_Coefficient '±200ppm/°C'
PRP Tolerance '±5%'
PRP UniqueID 'RSMD040200327'
PRP Value '10 O'
TOP 0 0.3301575 2.2202455 270 N 86 0 1
TOP 1 0.3695276 2.2202455 270 N 228 0 2
#
# CMP 206
CMP 4 0.4113719 2.1605599 270 N C32 GRT155R71E104KE01J ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet '-'
PRP Manufacturer 'Murata'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0402'
PRP PartNumber 'GRT155R71E104KE01J'
PRP Ratings '-'
PRP Series '-'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Digi-key'
PRP Supplier_Part_Number_1 '490-GRT155R71E104KE01JCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±10%'
PRP UniqueID 'capcc09401'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '25V'
TOP 0 0.4113719 2.1408749 180 N 248 369 1
TOP 1 0.4113719 2.180245 180 N 236 1 2
#
# CMP 207
CMP 4 0.3773719 2.1605599 270 N C31 C1005X5R1A475K050BC ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet 'https://product.tdk.com/system/files/dam/doc/product/capacitor/ceramic/mlcc/catalog/mlcc_commercial_general_en.pdf'
PRP Manufacturer 'TDK Corporation'
PRP Operating_Temperature '-55°C ~ 85°C'
PRP PackageReference '0402'
PRP PartNumber 'C1005X5R1A475K050BC'
PRP Ratings '-'
PRP Series 'C'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.65'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '445-13820-1-ND'
PRP Temperature_Coefficient 'X5R'
PRP Tolerance '±10%'
PRP UniqueID 'capcc03298'
PRP Value '4.7 uF'
PRP Voltage_-_Rated '10V'
TOP 0 0.3773719 2.1408749 180 N 248 370 1
TOP 1 0.3773719 2.180245 180 N 236 2 2
#
# CMP 208
CMP 2 0.3903155 2.1092207 180 N R41 ERJ-2GEJ100X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://b2b-api.panasonic.eu/file_stream/pids/fileversion/1242'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GEJ100X'
PRP Power_(Watts) '0.1W, 1/10W'
PRP Ratings 'AEC-Q200'
PRP Resistance '10 O'
PRP Series 'ERJ-2G'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P10JCT-ND'
PRP Temperature_Coefficient '±200ppm/°C'
PRP Tolerance '±5%'
PRP UniqueID 'RSMD040200327'
PRP Value '10 O'
TOP 0 0.4100005 2.1092207 90 N 230 0 1
TOP 1 0.3706304 2.1092207 90 N 238 57 2
#
# CMP 209
CMP 3 0.341371 2.1605599 270 N FB4 NFZ15SG151SN11D ;0=1,1=0.0236
PRP CompType 'FerriteBead'
PRP Current '1A'
PRP datasheet 'https://www.murata.com/en-us/products/productdata/8796735995934/ENFJ0010.pdf'
PRP DCR '120 mO'
PRP Impedance '-'
PRP Manufacturer 'Murata Electronics'
PRP Operating_Temperature '-40°C ~ 85°C'
PRP PackageReference '0402'
PRP PartNumber 'NFZ15SG151SN11D'
PRP Series 'NFZ'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '490-18375-1-ND'
PRP Temperature_Coefficient '-'
PRP Tolerance '-'
PRP UniqueID 'dcp00209'
PRP Value '-'
PRP Voltage_-_Rated '-'
TOP 0 0.341371 2.1408749 180 N 238 58 1
TOP 1 0.341371 2.180245 180 N 236 3 2
#
# CMP 210
CMP 38 0.6894887 2.2178084 0 N U11 FT4232HL-REEL ;0=1,1=0.7900
PRP Alt_Manufacturer 'FTDI'
PRP Alt_PartNumber 'FT4232HL-TRAY'
PRP Color '-'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT4232H.pdf'
PRP CompType 'uC'
PRP Current_Rating_(Amps) '-'
PRP datasheet 'https://www.mouser.com/datasheet/2/163/DS_FT4232H-1621254.pdf'
PRP Length_(in) '-'
PRP Manufacturer 'FTDI'
PRP Mount_Type 'SMD'
PRP PackageReference 'LQFP-64'
PRP PartNumber 'FT4232HL-REEL'
PRP Pitch_(mm) '-'
PRP RoHS 'TRUE'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '768-1026-1-ND'
PRP Symbol_Name 'SYM-FT4232HL-REEL'
PRP Text1 '-'
PRP UniqueID 'cmp00204'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 0.4700005 2.3654462 0 N 248 396 1
TOP 1 0.4700005 2.3457612 0 N 234 1 2
TOP 2 0.4700005 2.3260761 0 N 233 1 3
TOP 3 0.4700005 2.3063911 0 N 235 4 4
TOP 4 0.4700005 2.286706 0 N 248 395 5
TOP 5 0.4700005 2.267021 0 N 227 1 6
TOP 6 0.4700005 2.247336 0 N 229 1 7
TOP 7 0.4700005 2.2276509 0 N 228 1 8
TOP 8 0.4700005 2.2079659 0 N 236 4 9
TOP 9 0.4700005 2.1882808 0 N 248 393 10
TOP 10 0.4700005 2.1685958 0 N 248 394 11
TOP 11 0.4700005 2.1489108 0 N 217 4 12
TOP 12 0.4700005 2.1292257 0 N 248 392 13
TOP 13 0.4700005 2.1095407 0 N 230 1 14
TOP 14 0.4700005 2.0898556 0 N 248 391 15
TOP 15 0.4700005 2.0701706 0 N 232 1 16
TOP 16 0.5418509 1.9983202 0 N 211 2 17
TOP 17 0.5615359 1.9983202 0 N 207 1 18
TOP 18 0.581221 1.9983202 0 N 208 2 19
TOP 19 0.600906 1.9983202 0 N 238 62 20
TOP 20 0.6205911 1.9983202 0 N 0 239 21
TOP 21 0.6402761 1.9983202 0 N 0 238 22
TOP 22 0.6599611 1.9983202 0 N 0 237 23
TOP 23 0.6796462 1.9983202 0 N 0 236 24
TOP 24 0.6993312 1.9983202 0 N 248 397 25
TOP 25 0.7190163 1.9983202 0 N 231 1 26
TOP 26 0.7387013 1.9983202 0 N 218 2 27
TOP 27 0.7583863 1.9983202 0 N 219 3 28
TOP 28 0.7780714 1.9983202 0 N 0 235 29
TOP 29 0.7977564 1.9983202 0 N 0 234 30
TOP 30 0.8174415 1.9983202 0 N 238 61 31
TOP 31 0.8371265 1.9983202 0 N 0 233 32
TOP 32 0.9089769 2.0701706 0 N 0 251 33
TOP 33 0.9089769 2.0898556 0 N 0 250 34
TOP 34 0.9089769 2.1095407 0 N 248 398 35
TOP 35 0.9089769 2.1292257 0 N 0 249 36
TOP 36 0.9089769 2.1489108 0 N 217 5 37
TOP 37 0.9089769 2.1685958 0 N 0 248 38
TOP 38 0.9089769 2.1882808 0 N 0 247 39
TOP 39 0.9089769 2.2079659 0 N 0 246 40
TOP 40 0.9089769 2.2276509 0 N 0 245 41
TOP 41 0.9089769 2.247336 0 N 238 63 42
TOP 42 0.9089769 2.267021 0 N 0 244 43
TOP 43 0.9089769 2.286706 0 N 0 243 44
TOP 44 0.9089769 2.3063911 0 N 0 242 45
TOP 45 0.9089769 2.3260761 0 N 0 241 46
TOP 46 0.9089769 2.3457612 0 N 248 400 47
TOP 47 0.9089769 2.3654462 0 N 0 240 48
TOP 48 0.8371265 2.4372966 0 N 217 6 49
TOP 49 0.8174415 2.4372966 0 N 238 60 50
TOP 50 0.7977564 2.4372966 0 N 248 399 51
TOP 51 0.7780714 2.4372966 0 N 0 232 52
TOP 52 0.7583863 2.4372966 0 N 0 231 53
TOP 53 0.7387013 2.4372966 0 N 0 230 54
TOP 54 0.7190163 2.4372966 0 N 0 229 55
TOP 55 0.6993312 2.4372966 0 N 238 59 56
TOP 56 0.6796462 2.4372966 0 N 0 228 57
TOP 57 0.6599611 2.4372966 0 N 0 227 58
TOP 58 0.6402761 2.4372966 0 N 0 226 59
TOP 59 0.6205911 2.4372966 0 N 0 225 60
TOP 60 0.600906 2.4372966 0 N 223 2 61
TOP 61 0.581221 2.4372966 0 N 226 2 62
TOP 62 0.5615359 2.4372966 0 N 224 2 63
TOP 63 0.5418509 2.4372966 0 N 217 7 64
#
# CMP 211
CMP 41 1.351851 2.2842259 0 N PP5 Probe_Point ;0=2,1=0.1570
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color '-'
PRP CompType 'Probe Point'
PRP Current_Rating_(Amps) '-'
PRP datasheet '-'
PRP Length_(in) '-'
PRP Manufacturer '-'
PRP Mount_Type '-'
PRP PackageReference '-'
PRP PartNumber '-'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Text1 'SDA'
PRP UniqueID 'cmp00025'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 1.351851 2.2842259 0 N 194 3 1
#
# CMP 212
CMP 41 1.351851 2.362966 0 N PP6 Probe_Point ;0=2,1=0.1570
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color '-'
PRP CompType 'Probe Point'
PRP Current_Rating_(Amps) '-'
PRP datasheet '-'
PRP Length_(in) '-'
PRP Manufacturer '-'
PRP Mount_Type '-'
PRP PackageReference '-'
PRP PartNumber '-'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Text1 'SCL'
PRP UniqueID 'cmp00025'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 1.351851 2.362966 0 N 196 3 1
#
# CMP 213
CMP 13 0.125 0.125 0 N H3 CBTS130A ;0=2,1=0.0000
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color '-'
PRP CompType 'Standoff'
PRP Current_Rating_(Amps) '-'
PRP Length_(in) '5MM'
PRP Manufacturer 'Essentra Components'
PRP Mount_Type '-'
PRP PackageReference '-'
PRP PartNumber 'CBTS130A'
PRP Pitch_(mm) 'M3'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'RPC3620-ND'
PRP Text1 '-'
PRP UniqueID 'CBTS010A'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 0.125 0.125 0 N 0 256 empty-1
#
# CMP 214
CMP 13 0.13 2.595 0 N H1 CBTS130A ;0=2,1=0.0000
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color '-'
PRP CompType 'Standoff'
PRP Current_Rating_(Amps) '-'
PRP Length_(in) '5MM'
PRP Manufacturer 'Essentra Components'
PRP Mount_Type '-'
PRP PackageReference '-'
PRP PartNumber 'CBTS130A'
PRP Pitch_(mm) 'M3'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'RPC3620-ND'
PRP Text1 '-'
PRP UniqueID 'CBTS010A'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 0.13 2.595 0 N 0 255 empty-1
#
# CMP 215
CMP 52 3.26 0.254521 180 N U21 24LC64FT-I/MNY ;0=1,1=0.0000
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color '-'
PRP CompType 'EEPROM'
PRP Current_Rating_(Amps) '-'
PRP datasheet 'https://www.mouser.com/datasheet/2/268/24AA64_24FC64_24LC64_64_Kbit_I2C_Serial_EEPROM_200-2934388.pdf'
PRP Length_(in) '-'
PRP Manufacturer 'Microchip'
PRP Mount_Type 'SMD'
PRP PackageReference 'TDFN-8'
PRP PartNumber '24LC64FT-I/MNY'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 '24LC64FT-I/MNYCT-ND'
PRP Text1 '-'
PRP UniqueID 'cmp00154'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 3.3190551 0.2249934 180 N 250 2 1
TOP 1 3.3190551 0.2446785 180 N 249 2 2
TOP 2 3.3190551 0.2643635 180 N 216 1 3
TOP 3 3.3190551 0.2840486 180 N 248 412 4
TOP 4 3.2018032 0.2840486 180 N 194 2 5
TOP 5 3.2018032 0.2643635 180 N 196 2 6
TOP 6 3.2018032 0.2446785 180 N 248 411 7
TOP 7 3.2018032 0.2249934 180 N 212 3 8
TOP 8 3.26 0.254521 180 N 248 410 9
TOP 9 3.2460806 0.2406016 135 N 248 493 9
TOP 10 3.2739194 0.2684404 135 N 248 494 9
TOP 11 3.2739194 0.2406016 135 N 248 495 9
TOP 12 3.2460806 0.2684404 135 N 248 496 9
#
# CMP 216
CMP 0 3.7026486 0.8744982 315 N R139 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 3.6948537 0.8667033 225 N 240 1 1
TOP 1 3.7104435 0.8822931 225 N 215 1 2
#
# CMP 217
CMP 0 3.7026486 0.8244982 315 N R140 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 3.6948537 0.8167033 225 N 239 1 1
TOP 1 3.7104435 0.8322931 225 N 214 1 2
#
# CMP 218
CMP 0 3.7371068 0.3832674 0 N R145 ERJ-1GNF2200C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GNF2200C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '220 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P122831CT-ND'
PRP Temperature_Coefficient '±200ppm/°C'
PRP Tolerance '±1%'
PRP UniqueID 'RSMD020100147'
PRP Value '220 O'
TOP 0 3.7260832 0.3832674 270 N 248 371 1
TOP 1 3.7481304 0.3832674 270 N 246 1 2
#
# CMP 219
CMP 0 3.3650787 0.2446785 180 N R135 ERJ-1GNJ103C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://b2b-api.panasonic.eu/file_stream/pids/fileversion/1242'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GNJ103C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '10 kO'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P123222CT-ND'
PRP Temperature_Coefficient '±200ppm/°C'
PRP Tolerance '±5%'
PRP UniqueID 'RSMD020101186'
PRP Value '10 kO'
TOP 0 3.3761023 0.2446785 90 N 248 372 1
TOP 1 3.3540551 0.2446785 90 N 249 1 2
#
# CMP 220
CMP 0 3.3650787 0.2693635 180 N R136 ERJ-1GNJ103C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://b2b-api.panasonic.eu/file_stream/pids/fileversion/1242'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GNJ103C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '10 kO'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P123222CT-ND'
PRP Temperature_Coefficient '±200ppm/°C'
PRP Tolerance '±5%'
PRP UniqueID 'RSMD020101186'
PRP Value '10 kO'
TOP 0 3.3761023 0.2693635 90 N 248 373 1
TOP 1 3.3540551 0.2693635 90 N 216 0 2
#
# CMP 221
CMP 0 3.6614179 0.8589563 270 N R138 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 3.6614179 0.8479327 180 N 241 1 1
TOP 1 3.6614179 0.8699799 180 N 242 1 2
#
# CMP 222
CMP 2 3.4614179 2.2582673 270 N R150 ERJ-2RKF1000X ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 155°C'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1000X'
PRP Power_(Watts) '0.1W, 1/10W'
PRP Ratings 'AEC-Q200'
PRP Resistance '100 O'
PRP Series 'ERJ-2RK'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P100LCT-ND'
PRP Temperature_Coefficient '±100ppm/°C'
PRP Tolerance '±1%'
PRP UniqueID 'RSMD040200375'
PRP Value '100 O'
TOP 0 3.4614179 2.2385823 180 N 248 374 1
TOP 1 3.4614179 2.2779524 180 N 243 1 2
#
# CMP 223
CMP 0 3.3650787 0.2199934 180 N R134 ERJ-1GNJ103C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://b2b-api.panasonic.eu/file_stream/pids/fileversion/1242'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GNJ103C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '10 kO'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P123222CT-ND'
PRP Temperature_Coefficient '±200ppm/°C'
PRP Tolerance '±5%'
PRP UniqueID 'RSMD020101186'
PRP Value '10 kO'
TOP 0 3.3761023 0.2199934 90 N 248 375 1
TOP 1 3.3540551 0.2199934 90 N 250 1 2
#
# CMP 224
CMP 0 3.6114179 2.36 0 N R137 ERJ-1GN0R00C ;0=1,1=0.0102
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP Composition 'Thick Film'
PRP CompType 'Resistor SMD'
PRP datasheet 'https://industrial.panasonic.com/ww/products/pt/general-purpose-chip-resistors/models/ERJ1GN0R00C'
PRP Manufacturer 'Panasonic Electronic Components'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GN0R00C'
PRP Power_(Watts) '0.05W, 1/20W'
PRP Resistance '0 O'
PRP Series 'ERJ-1GN'
PRP Supplier_1 'Digi-Key'
PRP Supplier_Part_Number_1 'P15979CT-ND'
PRP Tolerance 'Jumper'
PRP UniqueID 'RSMD020101699'
PRP Value '0 O'
TOP 0 3.6003943 2.36 270 N 244 1 1
TOP 1 3.6224415 2.36 270 N 245 1 2
#
# CMP 225
CMP 27 3.3614179 2.5982675 270 N FID3 Fiducial_Mark ;0=1,1=0.0000
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color '-'
PRP CompType '-'
PRP Current_Rating_(Amps) '-'
PRP datasheet '-'
PRP Length_(in) '-'
PRP Manufacturer '-'
PRP Mount_Type '-'
PRP PackageReference '-'
PRP PartNumber '-'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP SymbolCreator 'a0412235'
PRP SymbolVersion '2009-11-4'
PRP Text1 '-'
PRP UniqueID 'cmp00099'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 3.3614179 2.5982675 270 N 0 220 1
#
# CMP 226
CMP 27 0.2818766 0.05 270 N FID1 Fiducial_Mark ;0=1,1=0.0000
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color '-'
PRP CompType '-'
PRP Current_Rating_(Amps) '-'
PRP datasheet '-'
PRP Length_(in) '-'
PRP Manufacturer '-'
PRP Mount_Type '-'
PRP PackageReference '-'
PRP PartNumber '-'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP SymbolCreator 'a0412235'
PRP SymbolVersion '2009-11-4'
PRP Text1 '-'
PRP UniqueID 'cmp00099'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 0.2818766 0.05 270 N 0 216 1
#
# CMP 227
CMP 27 3.72 0.11 270 N FID2 Fiducial_Mark ;0=1,1=0.0000
PRP Alt_Manufacturer '-'
PRP Alt_PartNumber '-'
PRP Color '-'
PRP CompType '-'
PRP Current_Rating_(Amps) '-'
PRP datasheet '-'
PRP Length_(in) '-'
PRP Manufacturer '-'
PRP Mount_Type '-'
PRP PackageReference '-'
PRP PartNumber '-'
PRP Pitch_(mm) '-'
PRP Series '-'
PRP SizeX_mm '-'
PRP SizeY_mm '-'
PRP SizeZ_mm '-'
PRP SymbolCreator 'a0412235'
PRP SymbolVersion '2009-11-4'
PRP Text1 '-'
PRP UniqueID 'cmp00099'
PRP Voltage_-_Forward_(Vf)_(Typ) '-'
PRP Voltage_Rating_-_DC '-'
TOP 0 3.72 0.11 270 N 0 217 1
#
# CMP 228
CMP 4 3.2214883 0.1949934 180 N C88 GRT155R71E104KE01J ;0=1,1=0.0236
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL ''
PRP ComponentLink2Description 'New link'
PRP ComponentLink2URL ''
PRP CompType 'Capacitor Ceramic'
PRP datasheet '-'
PRP Manufacturer 'Murata'
PRP Operating_Temperature '-55°C ~ 125°C'
PRP PackageReference '0402'
PRP PartNumber 'GRT155R71E104KE01J'
PRP Ratings '-'
PRP Series '-'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Digi-key'
PRP Supplier_Part_Number_1 '490-GRT155R71E104KE01JCT-ND'
PRP Temperature_Coefficient 'X7R'
PRP Tolerance '±10%'
PRP UniqueID 'capcc09401'
PRP Value '0.1 uF'
PRP Voltage_-_Rated '25V'
TOP 0 3.2411733 0.1949934 90 N 248 376 1
TOP 1 3.2018032 0.1949934 90 N 212 2 2
#
